#

##

##

    礦ision Build Log
    Project:
    E:\学习\全动电子液晶测试程序\液晶模块配套资料整理\最新模块代码资料制作\3.2寸\3.2寸ILI9341带触摸模块配套资料Rev3.1\STM32综合测试程序3.2寸ILI9341_240X320_IO模拟\USER\TOUCH.uvproj
    Project File Date:  03/13/2015

    Output:
    Build target 'Target 1'
    compiling main.c...
    linking...
    Program Size: Code=17378 RO-data=8854 RW-data=112 ZI-data=1648
    FromELF: creating hex file...
    "..\OBJ\TOUCH.axf" - 0 Error(s), 0 Warning(s).
    Load "..\\OBJ\\TOUCH.axf"
    Set JLink Project File to "E:\学习\全动电子液晶测试程序\液晶模块配套资料整理\最新模块代码资料制作\3.2寸\3.2寸ILI9341带触摸模块配套资料Rev3.1\STM32综合测试程序3.2寸ILI9341_240X320_IO模拟\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103RC" selected (256 KB flash, 48 KB RAM).

    JLink info:
    ------------
    DLL: V4.80g, compiled Feb 13 2014 20:50:02
    Firmware: J-Link ARM V8 compiled Jan 31 2018 18:34:52
    Hardware: V8.00
    S/N : 20080643
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103RC
    VTarget = 3.313V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...