#

##

##

    礦ision Build Log
    Project:
    D:\学习\全动电子液晶测试程序\液晶模块配套资料整理\最新模块代码资料制作\3.2寸ILI9341B_6颗灯模块配套资料Rev2.1\STM32综合测试程序3.2寸ILI9341_240X320_FSMC\USER\TOUCH.uvproj
    Project File Date:  12/03/2014

    Output:
    Build target 'Target 1'
    compiling main.c...
    main.c(52): warning:  #177-D: variable "i" was declared but never referenced
      {     u16 i=0;
    main.c: 1 warning, 0 errors
    linking...
    Program Size: Code=5848 RO-data=336 RW-data=52 ZI-data=1652
    FromELF: creating hex file...
    "..\OBJ\TOUCH.axf" - 0 Error(s), 1 Warning(s).
    Load "..\\OBJ\\TOUCH.axf"
    Set JLink Project File to "D:\学习\全动电子液晶测试程序\液晶模块配套资料整理\最新模块代码资料制作\3.2寸ILI9341B_6颗灯模块配套资料Rev2.1\STM32综合测试程序3.2寸ILI9341_240X320_FSMC\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103ZE" selected (512 KB flash, 64 KB RAM).

    JLink info:
    ------------
    DLL: V4.80g, compiled Feb 13 2014 20:50:02
    Firmware: J-Link ARM V8 compiled Jan 31 2018 18:34:52
    Hardware: V8.00
    S/N : 20080643
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103ZE
    VTarget = 3.319V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...