Static Call Graph - [.\output\test.axf]

# Static Call Graph for image .\output\test.axf

#<CALLGRAPH># ARM Linker, 5060750: Last Updated: Fri Feb 22 15:54:22 2019

### Maximum Stack Usage = 112668 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ MLX90640_GetFrameData ⇒ MLX90640_I2CWrite ⇒ MLX90640_I2CRead ⇒ I2CSendByte ⇒ I2CReceiveAck

### Mutually Recursive functions

- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - BusFault_Handler from stm32f4xx_it.o(i.BusFault_Handler) referenced from startup_stm32f4xx.o(RESET)
  - CAN1_RX0_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN1_TX_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN2_RX0_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN2_RX1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN2_SCE_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CAN2_TX_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - CRYP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DCMI_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - DebugMon_Handler from stm32f4xx_it.o(i.DebugMon_Handler) referenced from startup_stm32f4xx.o(RESET)
  - ETH_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - ETH_WKUP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - FLASH_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - FPU_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - FSMC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - HASH_RNG_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - HardFault_Handler from stm32f4xx_it.o(i.HardFault_Handler) referenced from startup_stm32f4xx.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - MemManage_Handler from stm32f4xx_it.o(i.MemManage_Handler) referenced from startup_stm32f4xx.o(RESET)
  - NMI_Handler from stm32f4xx_it.o(i.NMI_Handler) referenced from startup_stm32f4xx.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_HS_EP1_IN_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_HS_EP1_OUT_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_HS_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - OTG_HS_WKUP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - PVD_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - PendSV_Handler from stm32f4xx_it.o(i.PendSV_Handler) referenced from startup_stm32f4xx.o(RESET)
  - RCC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - Reset_Handler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SDIO_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SPI1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SPI2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SPI3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - SVC_Handler from stm32f4xx_it.o(i.SVC_Handler) referenced from startup_stm32f4xx.o(RESET)
  - SysTick_Handler from stm32f4xx_it.o(i.SysTick_Handler) referenced from startup_stm32f4xx.o(RESET)
  - SystemInit from system_stm32f4xx.o(i.SystemInit) referenced from startup_stm32f4xx.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM4_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM5_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM7_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM8_BRK_TIM12_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM8_TRG_COM_TIM14_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - TIM8_UP_TIM13_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - UART4_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - UART5_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - USART1_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - USART2_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - USART3_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - USART6_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - UsageFault_Handler from stm32f4xx_it.o(i.UsageFault_Handler) referenced from startup_stm32f4xx.o(RESET)
  - WWDG_IRQHandler from startup_stm32f4xx.o(.text) referenced from startup_stm32f4xx.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f4xx.o(.text)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 18 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(RESET)

  CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN2_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN2_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN2_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CAN2_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CRYP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DCMI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  HASH_RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_HS_EP1_IN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_HS_EP1_OUT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_HS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  OTG_HS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM8_BRK_TIM12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM8_TRG_COM_TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  TIM8_UP_TIM13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> MLX90640_I2CRead

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_dadd (Thumb, 322 bytes, Stack size 48 bytes, dadd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_lasr
  - >> __aeabi_llsl
  - >> _double_round
  - >> _double_epilogue
  [Called By]
  - >> MLX90640_GetTa
  - >> MLX90640_CalculateTo
  - >> __kernel_poly
  - >> __mathlib_dbl_infnan2
  - >> __hardfp_pow
  - >> __aeabi_dsub
  - >> __aeabi_drsub
  - >> MLX90640_GetVdd
  - >> ExtractPTATParameters

  __aeabi_dsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dsub ⇒ __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dadd
  [Called By]
  - >> MLX90640_GetTa
  - >> MLX90640_CalculateTo
  - >> __hardfp_pow

  __aeabi_drsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_drsub ⇒ __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dadd
  [Called By]
  - >> MLX90640_CalculateTo
  - >> __hardfp_pow

  __aeabi_dmul (Thumb, 228 bytes, Stack size 48 bytes, dmul.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> MLX90640_GetTa
  - >> MLX90640_CalculateTo
  - >> __kernel_poly
  - >> __mathlib_dbl_underflow
  - >> __mathlib_dbl_overflow
  - >> __hardfp_pow

  __aeabi_ddiv (Thumb, 222 bytes, Stack size 32 bytes, ddiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_ddiv ⇒ _double_round
  [Calls]
  - >> _double_round
  [Called By]
  - >> MLX90640_GetTa
  - >> MLX90640_CalculateTo
  - >> MLX90640_BadPixelsCorrection
  - >> __mathlib_dbl_invalid
  - >> __mathlib_dbl_divzero
  - >> __hardfp_pow
  - >> MLX90640_GetVdd
  - >> GetMedian
  - >> ExtractPTATParameters
  - >> ExtractKvPixelParameters
  - >> ExtractKtaPixelParameters
  - >> ExtractCPParameters
  - >> ExtractAlphaParameters

  __aeabi_i2d (Thumb, 34 bytes, Stack size 16 bytes, dflti.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = __aeabi_i2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> __hardfp_pow
  - >> MLX90640_GetVdd
  - >> ExtractPTATParameters

  __aeabi_ui2d (Thumb, 26 bytes, Stack size 16 bytes, dfltui.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = __aeabi_ui2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> MLX90640_GetTa
  - >> MLX90640_GetVdd
  - >> ExtractKvPixelParameters
  - >> ExtractKtaPixelParameters
  - >> ExtractCPParameters
  - >> ExtractAlphaParameters

  __aeabi_f2d (Thumb, 38 bytes, Stack size 0 bytes, f2d.o(.text))
  [Called By]

  - >> MLX90640_GetTa
  - >> MLX90640_CalculateTo
  - >> MLX90640_BadPixelsCorrection
  - >> MLX90640_GetVdd
  - >> GetMedian
  - >> ExtractKvPixelParameters
  - >> ExtractKtaPixelParameters
  - >> ExtractCPParameters
  - >> ExtractAlphaParameters

  __aeabi_cdrcmple (Thumb, 48 bytes, Stack size 0 bytes, cdrcmple.o(.text))
  [Called By]

  - >> MLX90640_BadPixelsCorrection
  - >> __hardfp_pow

  __aeabi_d2f (Thumb, 56 bytes, Stack size 8 bytes, d2f.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_d2f
  [Calls]
  - >> _float_round
  [Called By]
  - >> MLX90640_GetTa
  - >> MLX90640_CalculateTo
  - >> MLX90640_BadPixelsCorrection
  - >> MLX90640_GetVdd
  - >> GetMedian
  - >> ExtractPTATParameters
  - >> ExtractKvPixelParameters
  - >> ExtractKtaPixelParameters
  - >> ExtractCPParameters
  - >> ExtractAlphaParameters

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> _double_epilogue
  - >> __aeabi_dadd

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_lasr (Thumb, 36 bytes, Stack size 0 bytes, llsshr.o(.text))
  [Called By]

  - >> __aeabi_dadd

  _ll_sshift_r (Thumb, 0 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)

  __I$use$fp (Thumb, 0 bytes, Stack size 0 bytes, iusefp.o(.text), UNUSED)

  _float_round (Thumb, 18 bytes, Stack size 0 bytes, fepilogue.o(.text))
  [Called By]

  - >> __aeabi_d2f

  _float_epilogue (Thumb, 92 bytes, Stack size 4 bytes, fepilogue.o(.text), UNUSED)

  _double_round (Thumb, 30 bytes, Stack size 8 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = _double_round
  [Called By]
  - >> _double_epilogue
  - >> _dsqrt
  - >> __aeabi_ddiv
  - >> __aeabi_dadd

  _double_epilogue (Thumb, 156 bytes, Stack size 32 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_llsl
  - >> _double_round
  - >> __aeabi_llsr
  [Called By]
  - >> __aeabi_ui2d
  - >> __aeabi_i2d
  - >> __aeabi_dmul
  - >> __aeabi_dadd

  __ARM_scalbn (Thumb, 46 bytes, Stack size 16 bytes, dscalb.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = __ARM_scalbn
  [Called By]
  - >> __hardfp_pow

  scalbn (Thumb, 0 bytes, Stack size 16 bytes, dscalb.o(.text), UNUSED)

  _dsqrt (Thumb, 162 bytes, Stack size 32 bytes, dsqrt.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _dsqrt ⇒ _double_round
  [Calls]
  - >> _double_round
  - >> __aeabi_llsr
  [Called By]
  - >> sqrt
  - >> __hardfp_sqrt

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> _double_epilogue
  - >> _dsqrt

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  MLX90640_CalculateTo (Thumb, 2740 bytes, Stack size 240 bytes, mlx90640_api.o(RAMCODE))
  [Stack]

  - Max Depth = 720
  - Call Chain = MLX90640_CalculateTo ⇒ MLX90640_GetTa ⇒ MLX90640_GetVdd ⇒ __hardfp_pow ⇒ __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> MLX90640_GetTa
  - >> __hardfp_sqrt
  - >> __hardfp_pow
  - >> __aeabi_f2d
  - >> __aeabi_dsub
  - >> __aeabi_drsub
  - >> __aeabi_dmul
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> __aeabi_d2f
  - >> MLX90640_GetVdd
  [Called By]
  - >> main

  ALL_Config (Thumb, 30 bytes, Stack size 8 bytes, main.o(i.ALL_Config))
  [Stack]

  - Max Depth = 120
  - Call Chain = ALL_Config ⇒ LCD_init ⇒ TFT_FSMCConf
  [Calls]
  - >> delay_ms
  - >> LCD_init
  - >> IIC_GPIO_Init
  - >> Delay_Init
  - >> MX_GPIO_Init
  [Called By]
  - >> main

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.BusFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  CheckAdjacentPixels (Thumb, 58 bytes, Stack size 0 bytes, mlx90640_api.o(i.CheckAdjacentPixels))
  [Called By]

  - >> ExtractDeviatingPixels

  CheckEEPROMValid (Thumb, 20 bytes, Stack size 0 bytes, mlx90640_api.o(i.CheckEEPROMValid))
  [Called By]

  - >> MLX90640_ExtractParameters

  CoefficientInit (Thumb, 322 bytes, Stack size 0 bytes, temptocolor.o(i.CoefficientInit))
  [Called By]

  - >> main

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  Delay_Init (Thumb, 66 bytes, Stack size 0 bytes, delay.o(i.Delay_Init))
  [Called By]

  - >> ALL_Config

  ExtractAlphaParameters (Thumb, 616 bytes, Stack size 304 bytes, mlx90640_api.o(i.ExtractAlphaParameters))
  [Stack]

  - Max Depth = 608
  - Call Chain = ExtractAlphaParameters ⇒ __hardfp_pow ⇒ __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __hardfp_pow
  - >> __aeabi_ui2d
  - >> __aeabi_f2d
  - >> __aeabi_ddiv
  - >> __aeabi_d2f
  [Called By]
  - >> MLX90640_ExtractParameters

  ExtractCILCParameters (Thumb, 268 bytes, Stack size 16 bytes, mlx90640_api.o(i.ExtractCILCParameters))
  [Stack]

  - Max Depth = 16
  - Call Chain = ExtractCILCParameters
  [Called By]
  - >> MLX90640_ExtractParameters

  ExtractCPParameters (Thumb, 598 bytes, Stack size 80 bytes, mlx90640_api.o(i.ExtractCPParameters))
  [Stack]

  - Max Depth = 384
  - Call Chain = ExtractCPParameters ⇒ __hardfp_pow ⇒ __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __hardfp_pow
  - >> __aeabi_ui2d
  - >> __aeabi_f2d
  - >> __aeabi_ddiv
  - >> __aeabi_d2f
  [Called By]
  - >> MLX90640_ExtractParameters

  ExtractDeviatingPixels (Thumb, 350 bytes, Stack size 32 bytes, mlx90640_api.o(i.ExtractDeviatingPixels))
  [Stack]

  - Max Depth = 32
  - Call Chain = ExtractDeviatingPixels
  [Calls]
  - >> CheckAdjacentPixels
  [Called By]
  - >> MLX90640_ExtractParameters

  ExtractGainParameters (Thumb, 20 bytes, Stack size 0 bytes, mlx90640_api.o(i.ExtractGainParameters))
  [Called By]

  - >> MLX90640_ExtractParameters

  ExtractKsTaParameters (Thumb, 62 bytes, Stack size 0 bytes, mlx90640_api.o(i.ExtractKsTaParameters))
  [Called By]

  - >> MLX90640_ExtractParameters

  ExtractKsToParameters (Thumb, 262 bytes, Stack size 12 bytes, mlx90640_api.o(i.ExtractKsToParameters))
  [Stack]

  - Max Depth = 12
  - Call Chain = ExtractKsToParameters
  [Called By]
  - >> MLX90640_ExtractParameters

  ExtractKtaPixelParameters (Thumb, 512 bytes, Stack size 88 bytes, mlx90640_api.o(i.ExtractKtaPixelParameters))
  [Stack]

  - Max Depth = 392
  - Call Chain = ExtractKtaPixelParameters ⇒ __hardfp_pow ⇒ __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __hardfp_pow
  - >> __aeabi_ui2d
  - >> __aeabi_f2d
  - >> __aeabi_ddiv
  - >> __aeabi_d2f
  [Called By]
  - >> MLX90640_ExtractParameters

  ExtractKvPixelParameters (Thumb, 348 bytes, Stack size 88 bytes, mlx90640_api.o(i.ExtractKvPixelParameters))
  [Stack]

  - Max Depth = 392
  - Call Chain = ExtractKvPixelParameters ⇒ __hardfp_pow ⇒ __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __hardfp_pow
  - >> __aeabi_ui2d
  - >> __aeabi_f2d
  - >> __aeabi_ddiv
  - >> __aeabi_d2f
  [Called By]
  - >> MLX90640_ExtractParameters

  ExtractOffsetParameters (Thumb, 448 bytes, Stack size 252 bytes, mlx90640_api.o(i.ExtractOffsetParameters))
  [Stack]

  - Max Depth = 252
  - Call Chain = ExtractOffsetParameters
  [Called By]
  - >> MLX90640_ExtractParameters

  ExtractPTATParameters (Thumb, 216 bytes, Stack size 64 bytes, mlx90640_api.o(i.ExtractPTATParameters))
  [Stack]

  - Max Depth = 368
  - Call Chain = ExtractPTATParameters ⇒ __hardfp_pow ⇒ __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __hardfp_pow
  - >> __aeabi_i2d
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> __aeabi_d2f
  [Called By]
  - >> MLX90640_ExtractParameters

  ExtractResolutionParameters (Thumb, 14 bytes, Stack size 0 bytes, mlx90640_api.o(i.ExtractResolutionParameters))
  [Called By]

  - >> MLX90640_ExtractParameters

  ExtractTgcParameters (Thumb, 60 bytes, Stack size 0 bytes, mlx90640_api.o(i.ExtractTgcParameters))
  [Called By]

  - >> MLX90640_ExtractParameters

  ExtractVDDParameters (Thumb, 52 bytes, Stack size 12 bytes, mlx90640_api.o(i.ExtractVDDParameters))
  [Stack]

  - Max Depth = 12
  - Call Chain = ExtractVDDParameters
  [Called By]
  - >> MLX90640_ExtractParameters

  FSMC_NORSRAMCmd (Thumb, 46 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(i.FSMC_NORSRAMCmd))
  [Called By]

  - >> TFT_FSMCConf

  FSMC_NORSRAMInit (Thumb, 230 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(i.FSMC_NORSRAMInit))
  [Called By]

  - >> TFT_FSMCConf

  FindMaxMinTemp (Thumb, 172 bytes, Stack size 0 bytes, imagehandle.o(i.FindMaxMinTemp))
  [Called By]

  - >> main

  GPIO_Init (Thumb, 144 bytes, Stack size 20 bytes, stm32f4xx_gpio.o(i.GPIO_Init))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> IIC_GPIO_Init
  - >> MX_GPIO_Init
  - >> LCD_GPIO_Init

  GPIO_PinAFConfig (Thumb, 70 bytes, Stack size 20 bytes, stm32f4xx_gpio.o(i.GPIO_PinAFConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_PinAFConfig
  [Called By]
  - >> LCD_GPIO_Init

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(i.GPIO_SetBits))
  [Called By]

  - >> LCD_GPIO_Init

  GetMedian (Thumb, 208 bytes, Stack size 48 bytes, mlx90640_api.o(i.GetMedian))
  [Stack]

  - Max Depth = 88
  - Call Chain = GetMedian ⇒ __aeabi_ddiv ⇒ _double_round
  [Calls]
  - >> __aeabi_f2d
  - >> __aeabi_ddiv
  - >> __aeabi_d2f
  [Called By]
  - >> MLX90640_BadPixelsCorrection

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.HardFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  I2CReadBytes (Thumb, 156 bytes, Stack size 24 bytes, mlx90640_swi2c_driver.o(i.I2CReadBytes))
  [Stack]

  - Max Depth = 28
  - Call Chain = I2CReadBytes ⇒ I2CSendNack
  [Calls]
  - >> Wait
  - >> I2CSendNack
  - >> I2CSendACK
  [Called By]
  - >> MLX90640_I2CRead

  I2CReceiveAck (Thumb, 92 bytes, Stack size 8 bytes, mlx90640_swi2c_driver.o(i.I2CReceiveAck))
  [Stack]

  - Max Depth = 8
  - Call Chain = I2CReceiveAck
  [Calls]
  - >> Wait
  [Called By]
  - >> I2CSendByte

  I2CRepeatedStart (Thumb, 88 bytes, Stack size 4 bytes, mlx90640_swi2c_driver.o(i.I2CRepeatedStart))
  [Stack]

  - Max Depth = 4
  - Call Chain = I2CRepeatedStart
  [Calls]
  - >> Wait
  [Called By]
  - >> MLX90640_I2CRead

  I2CSendACK (Thumb, 80 bytes, Stack size 4 bytes, mlx90640_swi2c_driver.o(i.I2CSendACK))
  [Stack]

  - Max Depth = 4
  - Call Chain = I2CSendACK
  [Calls]
  - >> Wait
  [Called By]
  - >> I2CReadBytes

  I2CSendByte (Thumb, 124 bytes, Stack size 20 bytes, mlx90640_swi2c_driver.o(i.I2CSendByte))
  [Stack]

  - Max Depth = 28
  - Call Chain = I2CSendByte ⇒ I2CReceiveAck
  [Calls]
  - >> Wait
  - >> I2CReceiveAck
  [Called By]
  - >> MLX90640_I2CWrite
  - >> MLX90640_I2CRead

  I2CSendNack (Thumb, 80 bytes, Stack size 4 bytes, mlx90640_swi2c_driver.o(i.I2CSendNack))
  [Stack]

  - Max Depth = 4
  - Call Chain = I2CSendNack
  [Calls]
  - >> Wait
  [Called By]
  - >> I2CReadBytes

  I2CStart (Thumb, 76 bytes, Stack size 4 bytes, mlx90640_swi2c_driver.o(i.I2CStart))
  [Stack]

  - Max Depth = 4
  - Call Chain = I2CStart
  [Calls]
  - >> Wait
  [Called By]
  - >> MLX90640_I2CWrite
  - >> MLX90640_I2CRead

  I2CStop (Thumb, 68 bytes, Stack size 4 bytes, mlx90640_swi2c_driver.o(i.I2CStop))
  [Stack]

  - Max Depth = 4
  - Call Chain = I2CStop
  [Calls]
  - >> Wait
  [Called By]
  - >> MLX90640_I2CWrite
  - >> MLX90640_I2CRead

  IIC_GPIO_Init (Thumb, 48 bytes, Stack size 16 bytes, mlx90640_swi2c_driver.o(i.IIC_GPIO_Init))
  [Stack]

  - Max Depth = 36
  - Call Chain = IIC_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> ALL_Config

  IsPixelBad (Thumb, 50 bytes, Stack size 0 bytes, mlx90640_api.o(i.IsPixelBad))
  [Called By]

  - >> MLX90640_BadPixelsCorrection

  LCD_Fill (Thumb, 62 bytes, Stack size 32 bytes, lcd.o(i.LCD_Fill))
  [Stack]

  - Max Depth = 44
  - Call Chain = LCD_Fill ⇒ LCD_setwindow
  [Calls]
  - >> LCD_setwindow
  [Called By]
  - >> LCD_init

  LCD_GPIO_Init (Thumb, 372 bytes, Stack size 16 bytes, lcd.o(i.LCD_GPIO_Init))
  [Stack]

  - Max Depth = 36
  - Call Chain = LCD_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  - >> GPIO_SetBits
  - >> GPIO_PinAFConfig
  [Called By]
  - >> LCD_init

  LCD_Reset (Thumb, 48 bytes, Stack size 8 bytes, lcd.o(i.LCD_Reset))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_Reset
  [Calls]
  - >> delay_ms
  [Called By]
  - >> LCD_init

  LCD_init (Thumb, 506 bytes, Stack size 16 bytes, lcd.o(i.LCD_init))
  [Stack]

  - Max Depth = 112
  - Call Chain = LCD_init ⇒ TFT_FSMCConf
  [Calls]
  - >> delay_ms
  - >> TFT_FSMCConf
  - >> LCD_Reset
  - >> LCD_GPIO_Init
  - >> LCD_Fill
  [Called By]
  - >> ALL_Config

  LCD_setwindow (Thumb, 68 bytes, Stack size 12 bytes, lcd.o(i.LCD_setwindow))
  [Stack]

  - Max Depth = 12
  - Call Chain = LCD_setwindow
  [Called By]
  - >> SetDispBuf
  - >> LCD_Fill

  MLX90640_BadPixelsCorrection (Thumb, 1076 bytes, Stack size 72 bytes, mlx90640_api.o(i.MLX90640_BadPixelsCorrection))
  [Stack]

  - Max Depth = 160
  - Call Chain = MLX90640_BadPixelsCorrection ⇒ GetMedian ⇒ __aeabi_ddiv ⇒ _double_round
  [Calls]
  - >> __hardfp_fabs
  - >> __aeabi_f2d
  - >> __aeabi_ddiv
  - >> __aeabi_d2f
  - >> __aeabi_cdrcmple
  - >> IsPixelBad
  - >> GetMedian
  [Called By]
  - >> main

  MLX90640_DumpEE (Thumb, 24 bytes, Stack size 16 bytes, mlx90640_api.o(i.MLX90640_DumpEE))
  [Stack]

  - Max Depth = 1764
  - Call Chain = MLX90640_DumpEE ⇒ MLX90640_I2CRead ⇒ I2CSendByte ⇒ I2CReceiveAck
  [Calls]
  - >> MLX90640_I2CRead
  [Called By]
  - >> main

  MLX90640_ExtractParameters (Thumb, 136 bytes, Stack size 16 bytes, mlx90640_api.o(i.MLX90640_ExtractParameters))
  [Stack]

  - Max Depth = 624
  - Call Chain = MLX90640_ExtractParameters ⇒ ExtractAlphaParameters ⇒ __hardfp_pow ⇒ __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> ExtractVDDParameters
  - >> ExtractTgcParameters
  - >> ExtractResolutionParameters
  - >> ExtractPTATParameters
  - >> ExtractOffsetParameters
  - >> ExtractKvPixelParameters
  - >> ExtractKtaPixelParameters
  - >> ExtractKsToParameters
  - >> ExtractKsTaParameters
  - >> ExtractGainParameters
  - >> ExtractDeviatingPixels
  - >> ExtractCPParameters
  - >> ExtractCILCParameters
  - >> ExtractAlphaParameters
  - >> CheckEEPROMValid
  [Called By]
  - >> main

  MLX90640_GetCurMode (Thumb, 38 bytes, Stack size 24 bytes, mlx90640_api.o(i.MLX90640_GetCurMode))
  [Stack]

  - Max Depth = 1772
  - Call Chain = MLX90640_GetCurMode ⇒ MLX90640_I2CRead ⇒ I2CSendByte ⇒ I2CReceiveAck
  [Calls]
  - >> MLX90640_I2CRead
  [Called By]
  - >> main

  MLX90640_GetFrameData (Thumb, 196 bytes, Stack size 32 bytes, mlx90640_api.o(i.MLX90640_GetFrameData))
  [Stack]

  - Max Depth = 1812
  - Call Chain = MLX90640_GetFrameData ⇒ MLX90640_I2CWrite ⇒ MLX90640_I2CRead ⇒ I2CSendByte ⇒ I2CReceiveAck
  [Calls]
  - >> MLX90640_I2CWrite
  - >> MLX90640_I2CRead
  [Called By]
  - >> main

  MLX90640_GetTa (Thumb, 356 bytes, Stack size 112 bytes, mlx90640_api.o(i.MLX90640_GetTa))
  [Stack]

  - Max Depth = 480
  - Call Chain = MLX90640_GetTa ⇒ MLX90640_GetVdd ⇒ __hardfp_pow ⇒ __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __hardfp_pow
  - >> __aeabi_ui2d
  - >> __aeabi_f2d
  - >> __aeabi_dsub
  - >> __aeabi_dmul
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> __aeabi_d2f
  - >> MLX90640_GetVdd
  [Called By]
  - >> MLX90640_CalculateTo
  - >> main

  MLX90640_GetVdd (Thumb, 238 bytes, Stack size 64 bytes, mlx90640_api.o(i.MLX90640_GetVdd))
  [Stack]

  - Max Depth = 368
  - Call Chain = MLX90640_GetVdd ⇒ __hardfp_pow ⇒ __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __hardfp_pow
  - >> __aeabi_ui2d
  - >> __aeabi_i2d
  - >> __aeabi_f2d
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> __aeabi_d2f
  [Called By]
  - >> MLX90640_GetTa
  - >> MLX90640_CalculateTo

  MLX90640_I2CRead (Thumb, 246 bytes, Stack size 1720 bytes, mlx90640_swi2c_driver.o(i.MLX90640_I2CRead))
  [Stack]

  - Max Depth = 1748
  - Call Chain = MLX90640_I2CRead ⇒ I2CSendByte ⇒ I2CReceiveAck
  [Calls]
  - >> __aeabi_memclr4
  - >> Wait
  - >> I2CStop
  - >> I2CStart
  - >> I2CSendByte
  - >> I2CRepeatedStart
  - >> I2CReadBytes
  [Called By]
  - >> MLX90640_SetRefreshRate
  - >> MLX90640_SetChessMode
  - >> MLX90640_GetFrameData
  - >> MLX90640_GetCurMode
  - >> MLX90640_DumpEE
  - >> MLX90640_I2CWrite

  MLX90640_I2CWrite (Thumb, 154 bytes, Stack size 32 bytes, mlx90640_swi2c_driver.o(i.MLX90640_I2CWrite))
  [Stack]

  - Max Depth = 1780
  - Call Chain = MLX90640_I2CWrite ⇒ MLX90640_I2CRead ⇒ I2CSendByte ⇒ I2CReceiveAck
  [Calls]
  - >> Wait
  - >> MLX90640_I2CRead
  - >> I2CStop
  - >> I2CStart
  - >> I2CSendByte
  [Called By]
  - >> MLX90640_SetRefreshRate
  - >> MLX90640_SetChessMode
  - >> MLX90640_GetFrameData

  MLX90640_SetChessMode (Thumb, 48 bytes, Stack size 24 bytes, mlx90640_api.o(i.MLX90640_SetChessMode))
  [Stack]

  - Max Depth = 1804
  - Call Chain = MLX90640_SetChessMode ⇒ MLX90640_I2CWrite ⇒ MLX90640_I2CRead ⇒ I2CSendByte ⇒ I2CReceiveAck
  [Calls]
  - >> MLX90640_I2CWrite
  - >> MLX90640_I2CRead
  [Called By]
  - >> main

  MLX90640_SetRefreshRate (Thumb, 58 bytes, Stack size 24 bytes, mlx90640_api.o(i.MLX90640_SetRefreshRate))
  [Stack]

  - Max Depth = 1804
  - Call Chain = MLX90640_SetRefreshRate ⇒ MLX90640_I2CWrite ⇒ MLX90640_I2CRead ⇒ I2CSendByte ⇒ I2CReceiveAck
  [Calls]
  - >> MLX90640_I2CWrite
  - >> MLX90640_I2CRead
  [Called By]
  - >> main

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.MemManage_Handler))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  RCC_AHB1PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_AHB1PeriphClockCmd))
  [Called By]

  - >> IIC_GPIO_Init
  - >> MX_GPIO_Init
  - >> LCD_GPIO_Init

  RCC_AHB3PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_AHB3PeriphClockCmd))
  [Called By]

  - >> TFT_FSMCConf

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SetDispBuf (Thumb, 42 bytes, Stack size 16 bytes, imagehandle.o(i.SetDispBuf))
  [Stack]

  - Max Depth = 28
  - Call Chain = SetDispBuf ⇒ LCD_setwindow
  [Calls]
  - >> LCD_setwindow
  [Called By]
  - >> main

  SysTick_Handler (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.SysTick_Handler))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  SystemInit (Thumb, 88 bytes, Stack size 8 bytes, system_stm32f4xx.o(i.SystemInit))
  [Stack]

  - Max Depth = 20
  - Call Chain = SystemInit ⇒ SetSysClock
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_stm32f4xx.o(.text)

  TFT_FSMCConf (Thumb, 94 bytes, Stack size 96 bytes, lcd.o(i.TFT_FSMCConf))
  [Stack]

  - Max Depth = 96
  - Call Chain = TFT_FSMCConf
  [Calls]
  - >> FSMC_NORSRAMInit
  - >> FSMC_NORSRAMCmd
  - >> RCC_AHB3PeriphClockCmd
  [Called By]
  - >> LCD_init

  TempToColor (Thumb, 386 bytes, Stack size 64 bytes, temptocolor.o(i.TempToColor))
  [Stack]

  - Max Depth = 64
  - Call Chain = TempToColor
  [Calls]
  - >> Tmp2Color
  [Called By]
  - >> main

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.UsageFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f4xx.o(RESET)

  Wait (Thumb, 14 bytes, Stack size 0 bytes, mlx90640_swi2c_driver.o(i.Wait))
  [Called By]

  - >> MLX90640_I2CWrite
  - >> MLX90640_I2CRead
  - >> I2CStop
  - >> I2CStart
  - >> I2CSendNack
  - >> I2CSendByte
  - >> I2CSendACK
  - >> I2CRepeatedStart
  - >> I2CReceiveAck
  - >> I2CReadBytes

  __ARM_fpclassify (Thumb, 48 bytes, Stack size 8 bytes, fpclassify.o(i.__ARM_fpclassify))
  [Stack]

  - Max Depth = 8
  - Call Chain = __ARM_fpclassify
  [Called By]
  - >> __hardfp_pow

  __hardfp_fabs (Thumb, 20 bytes, Stack size 8 bytes, fabs.o(i.__hardfp_fabs))
  [Stack]

  - Max Depth = 8
  - Call Chain = __hardfp_fabs
  [Called By]
  - >> MLX90640_BadPixelsCorrection

  __hardfp_pow (Thumb, 3072 bytes, Stack size 192 bytes, pow.o(i.__hardfp_pow))
  [Stack]

  - Max Depth = 304
  - Call Chain = __hardfp_pow ⇒ __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __kernel_poly
  - >> __ARM_fpclassify
  - >> __mathlib_dbl_underflow
  - >> __mathlib_dbl_overflow
  - >> __mathlib_dbl_invalid
  - >> __mathlib_dbl_infnan2
  - >> __mathlib_dbl_divzero
  - >> sqrt
  - >> __ARM_scalbn
  - >> fabs
  - >> __aeabi_i2d
  - >> __aeabi_dsub
  - >> __aeabi_drsub
  - >> __aeabi_dmul
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> __aeabi_cdrcmple
  - >> __set_errno
  [Called By]
  - >> MLX90640_GetTa
  - >> MLX90640_CalculateTo
  - >> MLX90640_GetVdd
  - >> ExtractPTATParameters
  - >> ExtractKvPixelParameters
  - >> ExtractKtaPixelParameters
  - >> ExtractCPParameters
  - >> ExtractAlphaParameters

  __hardfp_sqrt (Thumb, 122 bytes, Stack size 32 bytes, sqrt.o(i.__hardfp_sqrt))
  [Stack]

  - Max Depth = 72
  - Call Chain = __hardfp_sqrt ⇒ _dsqrt ⇒ _double_round
  [Calls]
  - >> _dsqrt
  - >> __set_errno
  [Called By]
  - >> MLX90640_CalculateTo

  __kernel_poly (Thumb, 248 bytes, Stack size 24 bytes, poly.o(i.__kernel_poly))
  [Stack]

  - Max Depth = 112
  - Call Chain = __kernel_poly ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dmul
  - >> __aeabi_dadd
  [Called By]
  - >> __hardfp_pow

  __mathlib_dbl_divzero (Thumb, 28 bytes, Stack size 8 bytes, dunder.o(i.__mathlib_dbl_divzero))
  [Stack]

  - Max Depth = 48
  - Call Chain = __mathlib_dbl_divzero ⇒ __aeabi_ddiv ⇒ _double_round
  [Calls]
  - >> __aeabi_ddiv
  [Called By]
  - >> __hardfp_pow

  __mathlib_dbl_infnan2 (Thumb, 20 bytes, Stack size 8 bytes, dunder.o(i.__mathlib_dbl_infnan2))
  [Stack]

  - Max Depth = 96
  - Call Chain = __mathlib_dbl_infnan2 ⇒ __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dadd
  [Called By]
  - >> __hardfp_pow

  __mathlib_dbl_invalid (Thumb, 24 bytes, Stack size 8 bytes, dunder.o(i.__mathlib_dbl_invalid))
  [Stack]

  - Max Depth = 48
  - Call Chain = __mathlib_dbl_invalid ⇒ __aeabi_ddiv ⇒ _double_round
  [Calls]
  - >> __aeabi_ddiv
  [Called By]
  - >> __hardfp_pow

  __mathlib_dbl_overflow (Thumb, 24 bytes, Stack size 8 bytes, dunder.o(i.__mathlib_dbl_overflow))
  [Stack]

  - Max Depth = 96
  - Call Chain = __mathlib_dbl_overflow ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dmul
  [Called By]
  - >> __hardfp_pow

  __mathlib_dbl_underflow (Thumb, 24 bytes, Stack size 8 bytes, dunder.o(i.__mathlib_dbl_underflow))
  [Stack]

  - Max Depth = 96
  - Call Chain = __mathlib_dbl_underflow ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dmul
  [Called By]
  - >> __hardfp_pow

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  __set_errno (Thumb, 6 bytes, Stack size 0 bytes, errno.o(i.__set_errno))
  [Called By]

  - >> sqrt
  - >> __hardfp_sqrt
  - >> __hardfp_pow

  delay_ms (Thumb, 62 bytes, Stack size 0 bytes, delay.o(i.delay_ms))
  [Called By]

  - >> LCD_init
  - >> main
  - >> ALL_Config
  - >> LCD_Reset

  fabs (Thumb, 24 bytes, Stack size 8 bytes, fabs.o(i.fabs))
  [Stack]

  - Max Depth = 8
  - Call Chain = fabs
  [Called By]
  - >> __hardfp_pow

  main (Thumb, 214 bytes, Stack size 110856 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 112668
  - Call Chain = main ⇒ MLX90640_GetFrameData ⇒ MLX90640_I2CWrite ⇒ MLX90640_I2CRead ⇒ I2CSendByte ⇒ I2CReceiveAck
  [Calls]
  - >> delay_ms
  - >> TempToColor
  - >> SetDispBuf
  - >> MLX90640_SetRefreshRate
  - >> MLX90640_SetChessMode
  - >> MLX90640_GetTa
  - >> MLX90640_GetFrameData
  - >> MLX90640_GetCurMode
  - >> MLX90640_ExtractParameters
  - >> MLX90640_DumpEE
  - >> MLX90640_CalculateTo
  - >> MLX90640_BadPixelsCorrection
  - >> FindMaxMinTemp
  - >> CoefficientInit
  - >> ALL_Config
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  sqrt (Thumb, 110 bytes, Stack size 32 bytes, sqrt.o(i.sqrt))
  [Stack]

  - Max Depth = 72
  - Call Chain = sqrt ⇒ _dsqrt ⇒ _double_round
  [Calls]
  - >> _dsqrt
  - >> __set_errno
  [Called By]
  - >> __hardfp_pow

  ### Local Symbols

  MX_GPIO_Init (Thumb, 64 bytes, Stack size 16 bytes, main.o(i.MX_GPIO_Init))
  [Stack]

  - Max Depth = 36
  - Call Chain = MX_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> ALL_Config

  SetSysClock (Thumb, 220 bytes, Stack size 12 bytes, system_stm32f4xx.o(i.SetSysClock))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClock
  [Called By]
  - >> SystemInit

  Tmp2Color (Thumb, 118 bytes, Stack size 0 bytes, temptocolor.o(i.Tmp2Color))
  [Called By]

  - >> TempToColor

  ### Undefined Global Symbols