Static Call Graph - [..\OBJ\test.axf]

# Static Call Graph for image ..\OBJ\test.axf

#<CALLGRAPH># ARM Linker, 5.03 [Build 24]: Last Updated: Thu May 25 15:10:46 2017

### Maximum Stack Usage = 372 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

usmart_cmd_rec ⇒ usmart_get_fparam ⇒ usmart_str2num ⇒ usmart_pow

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - ADC3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - AT24CXX_ReadOneByte from 24cxx.o(.text) referenced 2 times from usmart_config.o(.data)
  - AT24CXX_WriteOneByte from 24cxx.o(.text) referenced 2 times from usmart_config.o(.data)
  - BusFault_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel4_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - Dac1_Set_Vol from dac.o(.text) referenced 2 times from usmart_config.o(.data)
  - DebugMon_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI0_IRQHandler from wkup.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI2_IRQHandler from exti.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI3_IRQHandler from exti.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI4_IRQHandler from exti.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FLASH_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FSMC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - HardFault_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - MemManage_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - NMI_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - PVD_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - PendSV_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RCC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTCAlarm_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTC_IRQHandler from rtc.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTC_Set from rtc.o(.text) referenced 2 times from usmart_config.o(.data)
  - Reset_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SDIO_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SVC_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SysTick_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SystemInit_ExtMemCtl from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(.text)
  - TAMPER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM2_IRQHandler from usmart.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM3_IRQHandler from timer.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM5_IRQHandler from timer.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TP_Adjust from touch.o(.text) referenced 2 times from touch.o(.data)
  - TP_Init from touch.o(.text) referenced 2 times from touch.o(.data)
  - TP_Scan from touch.o(.text) referenced 2 times from touch.o(.data)
  - UART4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART1_IRQHandler from usart.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART2_IRQHandler from rs485.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UsageFault_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - WWDG_IRQHandler from wdg.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32f10x_hd.o(.text)
  - _printf_input_char from _printf_char_common.o(.text) referenced from _printf_char_common.o(.text)
  - delay_ms from delay.o(.text) referenced 2 times from usmart_config.o(.data)
  - delay_us from delay.o(.text) referenced 2 times from usmart_config.o(.data)
  - fputc from usart.o(.text) referenced from _printf_char_file.o(.text)
  - read_addr from usmart.o(.text) referenced 2 times from usmart_config.o(.data)
  - usmart_cmd_rec from usmart.o(.text) referenced 2 times from usmart_config.o(.data)
  - usmart_exe from usmart.o(.text) referenced 2 times from usmart_config.o(.data)
  - usmart_init from usmart.o(.text) referenced 2 times from usmart_config.o(.data)
  - usmart_scan from usmart.o(.text) referenced 2 times from usmart_config.o(.data)
  - write_addr from usmart.o(.text) referenced 2 times from usmart_config.o(.data)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __decompress (Thumb, 90 bytes, Stack size unknown bytes, __dczerorl2.o(!!dczerorl2), UNUSED)

  __decompress1 (Thumb, 0 bytes, Stack size unknown bytes, __dczerorl2.o(!!dczerorl2), UNUSED)

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  _printf_d (Thumb, 0 bytes, Stack size unknown bytes, _printf_d.o(.ARM.Collect$$_printf_percent$$00000009))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = _printf_d ⇒ _printf_int_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_dec

  _printf_percent (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent.o(.ARM.Collect$$_printf_percent$$00000000))
  [Called By]

  - >> __printf

  _printf_u (Thumb, 0 bytes, Stack size unknown bytes, _printf_u.o(.ARM.Collect$$_printf_percent$$0000000A))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = _printf_u ⇒ _printf_int_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_dec

  _printf_x (Thumb, 0 bytes, Stack size unknown bytes, _printf_x.o(.ARM.Collect$$_printf_percent$$0000000C))
  [Stack]

  - Max Depth = 64 + Unknown Stack Size
  - Call Chain = _printf_x ⇒ _printf_int_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_hex

  _printf_c (Thumb, 0 bytes, Stack size unknown bytes, _printf_c.o(.ARM.Collect$$_printf_percent$$00000013))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = _printf_c ⇒ _printf_char ⇒ _printf_cs_common ⇒ _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_char

  _printf_s (Thumb, 0 bytes, Stack size unknown bytes, _printf_s.o(.ARM.Collect$$_printf_percent$$00000014))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = _printf_s ⇒ _printf_string ⇒ _printf_cs_common ⇒ _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_string

  _printf_percent_end (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent_end.o(.ARM.Collect$$_printf_percent$$00000017))

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002A))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000008))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000F))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000031))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000006))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000009))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000003))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000B))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 268 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ TP_Adjust ⇒ TP_Adj_Info_Show ⇒ LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  WFI_SET (Thumb, 2 bytes, Stack size 0 bytes, sys.o(.emb_text))
  [Called By]

  - >> Sys_Standby

  INTX_DISABLE (Thumb, 2 bytes, Stack size 0 bytes, sys.o(.emb_text), UNUSED)

  INTX_ENABLE (Thumb, 2 bytes, Stack size 0 bytes, sys.o(.emb_text), UNUSED)

  MSR_MSP (Thumb, 6 bytes, Stack size 0 bytes, sys.o(.emb_text), UNUSED)

  SystemInit_ExtMemCtl (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(.text)

  Reset_Handler (Thumb, 14 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  ADC3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f10x_hd.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  Load_Drow_Dialog (Thumb, 52 bytes, Stack size 16 bytes, test.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = Load_Drow_Dialog ⇒ LCD_ShowString ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor
  [Calls]
  - >> LCD_ShowString
  - >> LCD_Clear
  [Called By]
  - >> main

  main (Thumb, 326 bytes, Stack size 16 bytes, test.o(.text))
  [Stack]

  - Max Depth = 268 + Unknown Stack Size
  - Call Chain = main ⇒ TP_Adjust ⇒ TP_Adj_Info_Show ⇒ LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor
  [Calls]
  - >> uart_init
  - >> delay_ms
  - >> delay_init
  - >> TP_Save_Adjdata
  - >> TP_Draw_Big_Point
  - >> TP_Adjust
  - >> Stm32_Clock_Init
  - >> LED_Init
  - >> LCD_ShowString
  - >> LCD_Init
  - >> LCD_Clear
  - >> KEY_Scan
  - >> KEY_Init
  - >> Load_Drow_Dialog
  [Called By]
  - >> __rt_entry_main

  delay_init (Thumb, 54 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> main

  delay_us (Thumb, 54 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> TP_Read_AD
  - >> IIC_Read_Byte
  - >> IIC_Send_Byte
  - >> IIC_NAck
  - >> IIC_Ack
  - >> IIC_Wait_Ack
  - >> IIC_Stop
  - >> IIC_Start
  - >> LCD_ReadReg
  [Address Reference Count : 1]
  - usmart_config.o(.data)

  delay_ms (Thumb, 54 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> RS485_Receive_Data
  - >> AT24CXX_WriteOneByte
  - >> Check_WKUP
  - >> RTC_Init
  - >> EXTI4_IRQHandler
  - >> EXTI3_IRQHandler
  - >> EXTI2_IRQHandler
  - >> TP_Adjust
  - >> LCD_Init
  - >> KEY_Scan
  - >> main
  [Address Reference Count : 1]
  - usmart_config.o(.data)

  MY_NVIC_SetVectorTable (Thumb, 12 bytes, Stack size 0 bytes, sys.o(.text))
  [Called By]

  - >> MYRCC_DeInit

  MY_NVIC_PriorityGroupConfig (Thumb, 36 bytes, Stack size 0 bytes, sys.o(.text))
  [Called By]

  - >> MY_NVIC_Init

  MY_NVIC_Init (Thumb, 156 bytes, Stack size 32 bytes, sys.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = MY_NVIC_Init
  [Calls]
  - >> MY_NVIC_PriorityGroupConfig
  [Called By]
  - >> Timer2_Init
  - >> RS485_Init
  - >> WKUP_Init
  - >> RTC_Init
  - >> TIM5_Cap_Init
  - >> TIM3_Int_Init
  - >> WWDG_Init
  - >> EXTIX_Init
  - >> uart_init

  Ex_NVIC_Config (Thumb, 144 bytes, Stack size 16 bytes, sys.o(.text), UNUSED)
  [Called By]

  - >> WKUP_Init
  - >> EXTIX_Init

  MYRCC_DeInit (Thumb, 90 bytes, Stack size 4 bytes, sys.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = MYRCC_DeInit
  [Calls]
  - >> MY_NVIC_SetVectorTable
  [Called By]
  - >> Stm32_Clock_Init

  Sys_Standby (Thumb, 68 bytes, Stack size 8 bytes, sys.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Sys_Standby
  [Calls]
  - >> WFI_SET
  [Called By]
  - >> WKUP_Init
  - >> Sys_Enter_Standby

  Sys_Soft_Reset (Thumb, 12 bytes, Stack size 0 bytes, sys.o(.text), UNUSED)

  JTAG_Set (Thumb, 42 bytes, Stack size 0 bytes, sys.o(.text), UNUSED)

  Stm32_Clock_Init (Thumb, 130 bytes, Stack size 12 bytes, sys.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = Stm32_Clock_Init ⇒ MYRCC_DeInit
  [Calls]
  - >> MYRCC_DeInit
  [Called By]
  - >> main

  _sys_exit (Thumb, 6 bytes, Stack size 0 bytes, usart.o(.text))
  [Called By]

  - >> __rt_exit_exit

  fputc (Thumb, 22 bytes, Stack size 0 bytes, usart.o(.text))
  [Address Reference Count : 1]

  - _printf_char_file.o(.text)

  USART1_IRQHandler (Thumb, 118 bytes, Stack size 0 bytes, usart.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  uart_init (Thumb, 214 bytes, Stack size 40 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = uart_init ⇒ MY_NVIC_Init
  [Calls]
  - >> MY_NVIC_Init
  - >> __aeabi_fmul
  - >> __aeabi_ui2f
  - >> __aeabi_f2uiz
  - >> __aeabi_fdiv
  - >> __aeabi_frsub
  [Called By]
  - >> main

  LED_Init (Thumb, 100 bytes, Stack size 0 bytes, led.o(.text))
  [Called By]

  - >> main

  KEY_Init (Thumb, 86 bytes, Stack size 0 bytes, key.o(.text))
  [Called By]

  - >> EXTIX_Init
  - >> main

  KEY_Scan (Thumb, 138 bytes, Stack size 8 bytes, key.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = KEY_Scan
  [Calls]
  - >> delay_ms
  [Called By]
  - >> main

  EXTI2_IRQHandler (Thumb, 40 bytes, Stack size 8 bytes, exti.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = EXTI2_IRQHandler
  [Calls]
  - >> delay_ms
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  EXTI3_IRQHandler (Thumb, 40 bytes, Stack size 8 bytes, exti.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = EXTI3_IRQHandler
  [Calls]
  - >> delay_ms
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  EXTI4_IRQHandler (Thumb, 58 bytes, Stack size 8 bytes, exti.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = EXTI4_IRQHandler
  [Calls]
  - >> delay_ms
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  EXTIX_Init (Thumb, 96 bytes, Stack size 8 bytes, exti.o(.text), UNUSED)
  [Calls]

  - >> Ex_NVIC_Config
  - >> MY_NVIC_Init
  - >> KEY_Init

  IWDG_Init (Thumb, 28 bytes, Stack size 0 bytes, wdg.o(.text), UNUSED)

  IWDG_Feed (Thumb, 10 bytes, Stack size 0 bytes, wdg.o(.text), UNUSED)

  WWDG_Init (Thumb, 124 bytes, Stack size 16 bytes, wdg.o(.text), UNUSED)
  [Calls]

  - >> MY_NVIC_Init

  WWDG_Set_Counter (Thumb, 12 bytes, Stack size 0 bytes, wdg.o(.text))
  [Called By]

  - >> WWDG_IRQHandler

  WWDG_IRQHandler (Thumb, 36 bytes, Stack size 4 bytes, wdg.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = WWDG_IRQHandler
  [Calls]
  - >> WWDG_Set_Counter
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TIM3_IRQHandler (Thumb, 40 bytes, Stack size 0 bytes, timer.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM3_Int_Init (Thumb, 74 bytes, Stack size 16 bytes, timer.o(.text), UNUSED)
  [Calls]

  - >> MY_NVIC_Init

  TIM3_PWM_Init (Thumb, 150 bytes, Stack size 0 bytes, timer.o(.text), UNUSED)

  TIM5_Cap_Init (Thumb, 176 bytes, Stack size 16 bytes, timer.o(.text), UNUSED)
  [Calls]

  - >> MY_NVIC_Init

  TIM5_IRQHandler (Thumb, 184 bytes, Stack size 0 bytes, timer.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM4_PWM_Init (Thumb, 124 bytes, Stack size 0 bytes, timer.o(.text), UNUSED)

  LCD_WR_REG (Thumb, 6 bytes, Stack size 0 bytes, ili93xx.o(.text))
  [Called By]

  - >> LCD_Fast_DrawPoint
  - >> LCD_Scan_Dir
  - >> LCD_DisplayOff
  - >> LCD_DisplayOn
  - >> LCD_ReadPoint
  - >> LCD_SetCursor
  - >> LCD_ReadReg
  - >> LCD_Init

  LCD_WR_DATA (Thumb, 8 bytes, Stack size 0 bytes, ili93xx.o(.text))
  [Called By]

  - >> LCD_Fill
  - >> LCD_Fast_DrawPoint
  - >> LCD_Scan_Dir
  - >> LCD_SetCursor
  - >> LCD_Init

  LCD_RD_DATA (Thumb, 8 bytes, Stack size 0 bytes, ili93xx.o(.text))
  [Called By]

  - >> LCD_ReadReg
  - >> LCD_Init

  LCD_WriteReg (Thumb, 10 bytes, Stack size 0 bytes, ili93xx.o(.text))
  [Called By]

  - >> LCD_Fast_DrawPoint
  - >> LCD_Scan_Dir
  - >> LCD_DisplayOff
  - >> LCD_DisplayOn
  - >> LCD_SetCursor
  - >> LCD_Init

  LCD_ReadReg (Thumb, 22 bytes, Stack size 8 bytes, ili93xx.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_ReadReg
  [Calls]
  - >> LCD_RD_DATA
  - >> LCD_WR_REG
  - >> delay_us
  [Called By]
  - >> LCD_Init

  LCD_WriteRAM_Prepare (Thumb, 10 bytes, Stack size 0 bytes, ili93xx.o(.text))
  [Called By]

  - >> LCD_Color_Fill
  - >> LCD_Fill
  - >> LCD_DrawPoint
  - >> LCD_Clear

  LCD_WriteRAM (Thumb, 8 bytes, Stack size 0 bytes, ili93xx.o(.text), UNUSED)

  LCD_BGR2RGB (Thumb, 26 bytes, Stack size 12 bytes, ili93xx.o(.text), UNUSED)
  [Called By]

  - >> LCD_ReadPoint

  opt_delay (Thumb, 14 bytes, Stack size 0 bytes, ili93xx.o(.text), UNUSED)
  [Called By]

  - >> LCD_ReadPoint

  LCD_SetCursor (Thumb, 172 bytes, Stack size 8 bytes, ili93xx.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_SetCursor
  [Calls]
  - >> LCD_WriteReg
  - >> LCD_WR_DATA
  - >> LCD_WR_REG
  [Called By]
  - >> LCD_Color_Fill
  - >> LCD_Fill
  - >> LCD_DrawPoint
  - >> LCD_ReadPoint
  - >> LCD_Clear

  LCD_ReadPoint (Thumb, 278 bytes, Stack size 24 bytes, ili93xx.o(.text), UNUSED)
  [Calls]

  - >> LCD_SetCursor
  - >> opt_delay
  - >> LCD_BGR2RGB
  - >> LCD_WR_REG

  LCD_DisplayOn (Thumb, 46 bytes, Stack size 4 bytes, ili93xx.o(.text), UNUSED)
  [Calls]

  - >> LCD_WriteReg
  - >> LCD_WR_REG

  LCD_DisplayOff (Thumb, 44 bytes, Stack size 4 bytes, ili93xx.o(.text), UNUSED)
  [Calls]

  - >> LCD_WriteReg
  - >> LCD_WR_REG

  LCD_Scan_Dir (Thumb, 472 bytes, Stack size 20 bytes, ili93xx.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = LCD_Scan_Dir
  [Calls]
  - >> LCD_WriteReg
  - >> LCD_WR_DATA
  - >> LCD_WR_REG
  [Called By]
  - >> LCD_Display_Dir

  LCD_DrawPoint (Thumb, 28 bytes, Stack size 12 bytes, ili93xx.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = LCD_DrawPoint ⇒ LCD_SetCursor
  [Calls]
  - >> LCD_SetCursor
  - >> LCD_WriteRAM_Prepare
  [Called By]
  - >> TP_Drow_Touch_Point
  - >> LCD_ShowChar
  - >> Draw_Circle
  - >> LCD_DrawLine
  - >> TP_Draw_Big_Point

  LCD_Fast_DrawPoint (Thumb, 188 bytes, Stack size 12 bytes, ili93xx.o(.text), UNUSED)
  [Calls]

  - >> LCD_WriteReg
  - >> LCD_WR_DATA
  - >> LCD_WR_REG

  LCD_Display_Dir (Thumb, 266 bytes, Stack size 8 bytes, ili93xx.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = LCD_Display_Dir ⇒ LCD_Scan_Dir
  [Calls]
  - >> LCD_Scan_Dir
  [Called By]
  - >> LCD_Init

  LCD_Clear (Thumb, 100 bytes, Stack size 16 bytes, ili93xx.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = LCD_Clear ⇒ LCD_SetCursor
  [Calls]
  - >> LCD_SetCursor
  - >> LCD_WriteRAM_Prepare
  [Called By]
  - >> TP_Init
  - >> TP_Adjust
  - >> LCD_Init
  - >> main
  - >> Load_Drow_Dialog

  LCD_Init (Thumb, 6300 bytes, Stack size 8 bytes, ili93xx.o(.text))
  [Stack]

  - Max Depth = 152 + Unknown Stack Size
  - Call Chain = LCD_Init ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> LCD_Display_Dir
  - >> LCD_ReadReg
  - >> LCD_WriteReg
  - >> LCD_RD_DATA
  - >> LCD_WR_DATA
  - >> LCD_WR_REG
  - >> delay_ms
  - >> LCD_Clear
  - >> __2printf
  [Called By]
  - >> main

  LCD_Fill (Thumb, 178 bytes, Stack size 44 bytes, ili93xx.o(.text), UNUSED)
  [Calls]

  - >> LCD_Fill
  - >> LCD_SetCursor
  - >> LCD_WriteRAM_Prepare
  - >> LCD_WR_DATA
  [Called By]
  - >> LCD_Fill

  LCD_Color_Fill (Thumb, 100 bytes, Stack size 40 bytes, ili93xx.o(.text), UNUSED)
  [Calls]

  - >> LCD_SetCursor
  - >> LCD_WriteRAM_Prepare

  LCD_DrawLine (Thumb, 176 bytes, Stack size 68 bytes, ili93xx.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = LCD_DrawLine ⇒ LCD_DrawPoint ⇒ LCD_SetCursor
  [Calls]
  - >> LCD_DrawPoint
  [Called By]
  - >> TP_Drow_Touch_Point
  - >> LCD_DrawRectangle

  LCD_DrawRectangle (Thumb, 60 bytes, Stack size 20 bytes, ili93xx.o(.text), UNUSED)
  [Calls]

  - >> LCD_DrawLine

  Draw_Circle (Thumb, 152 bytes, Stack size 28 bytes, ili93xx.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = Draw_Circle ⇒ LCD_DrawPoint ⇒ LCD_SetCursor
  [Calls]
  - >> LCD_DrawPoint
  [Called By]
  - >> TP_Drow_Touch_Point

  LCD_ShowChar (Thumb, 340 bytes, Stack size 40 bytes, ili93xx.o(.text))
  [Stack]

  - Max Depth = 60
  - Call Chain = LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor
  [Calls]
  - >> LCD_DrawPoint
  [Called By]
  - >> LCD_ShowxNum
  - >> LCD_ShowNum
  - >> LCD_ShowString

  LCD_Pow (Thumb, 22 bytes, Stack size 8 bytes, ili93xx.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_Pow
  [Called By]
  - >> LCD_ShowxNum
  - >> LCD_ShowNum

  LCD_ShowNum (Thumb, 148 bytes, Stack size 56 bytes, ili93xx.o(.text))
  [Stack]

  - Max Depth = 116
  - Call Chain = LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor
  [Calls]
  - >> LCD_Pow
  - >> LCD_ShowChar
  [Called By]
  - >> TP_Adj_Info_Show

  LCD_ShowxNum (Thumb, 218 bytes, Stack size 60 bytes, ili93xx.o(.text), UNUSED)
  [Calls]

  - >> LCD_Pow
  - >> LCD_ShowChar

  LCD_ShowString (Thumb, 102 bytes, Stack size 36 bytes, ili93xx.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = LCD_ShowString ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor
  [Calls]
  - >> LCD_ShowChar
  [Called By]
  - >> TP_Adj_Info_Show
  - >> TP_Adjust
  - >> main
  - >> Load_Drow_Dialog

  RTC_Get_Week (Thumb, 114 bytes, Stack size 20 bytes, rtc.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = RTC_Get_Week
  [Called By]
  - >> RTC_Get

  Is_Leap_Year (Thumb, 58 bytes, Stack size 0 bytes, rtc.o(.text))
  [Called By]

  - >> RTC_Set
  - >> RTC_Get

  RTC_Get (Thumb, 246 bytes, Stack size 16 bytes, rtc.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = RTC_Get ⇒ RTC_Get_Week
  [Calls]
  - >> Is_Leap_Year
  - >> RTC_Get_Week
  [Called By]
  - >> RTC_IRQHandler
  - >> RTC_Init
  - >> RTC_Set

  RTC_Set (Thumb, 254 bytes, Stack size 36 bytes, rtc.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = RTC_Set ⇒ RTC_Get ⇒ RTC_Get_Week
  [Calls]
  - >> RTC_Get
  - >> Is_Leap_Year
  [Called By]
  - >> RTC_Init
  [Address Reference Count : 1]
  - usmart_config.o(.data)

  RTC_Init (Thumb, 368 bytes, Stack size 16 bytes, rtc.o(.text), UNUSED)
  [Calls]

  - >> RTC_Set
  - >> RTC_Get
  - >> MY_NVIC_Init
  - >> delay_ms
  - >> __2printf

  RTC_IRQHandler (Thumb, 80 bytes, Stack size 4 bytes, rtc.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = RTC_IRQHandler ⇒ RTC_Get ⇒ RTC_Get_Week
  [Calls]
  - >> RTC_Get
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  Sys_Enter_Standby (Thumb, 20 bytes, Stack size 8 bytes, wkup.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = Sys_Enter_Standby ⇒ Sys_Standby
  [Calls]
  - >> Sys_Standby
  [Called By]
  - >> EXTI0_IRQHandler

  Check_WKUP (Thumb, 72 bytes, Stack size 16 bytes, wkup.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = Check_WKUP
  [Calls]
  - >> delay_ms
  [Called By]
  - >> WKUP_Init
  - >> EXTI0_IRQHandler

  EXTI0_IRQHandler (Thumb, 20 bytes, Stack size 8 bytes, wkup.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = EXTI0_IRQHandler ⇒ Check_WKUP
  [Calls]
  - >> Check_WKUP
  - >> Sys_Enter_Standby
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  WKUP_Init (Thumb, 80 bytes, Stack size 8 bytes, wkup.o(.text), UNUSED)
  [Calls]

  - >> Check_WKUP
  - >> Sys_Standby
  - >> Ex_NVIC_Config
  - >> MY_NVIC_Init

  Dac1_Init (Thumb, 102 bytes, Stack size 0 bytes, dac.o(.text), UNUSED)

  Dac1_Set_Vol (Thumb, 76 bytes, Stack size 32 bytes, dac.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = Dac1_Set_Vol ⇒ __aeabi_ddiv
  [Calls]
  - >> __aeabi_fmul
  - >> __aeabi_ui2f
  - >> __aeabi_f2uiz
  - >> __aeabi_fdiv
  - >> __aeabi_f2d
  - >> __aeabi_ddiv
  - >> __aeabi_d2f
  [Address Reference Count : 1]
  - usmart_config.o(.data)

  IIC_Init (Thumb, 52 bytes, Stack size 0 bytes, myiic.o(.text))
  [Called By]

  - >> AT24CXX_Init

  IIC_Start (Thumb, 68 bytes, Stack size 8 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_Start
  [Calls]
  - >> delay_us
  [Called By]
  - >> AT24CXX_WriteOneByte
  - >> AT24CXX_ReadOneByte

  IIC_Stop (Thumb, 66 bytes, Stack size 8 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_Stop
  [Calls]
  - >> delay_us
  [Called By]
  - >> AT24CXX_WriteOneByte
  - >> AT24CXX_ReadOneByte
  - >> IIC_Wait_Ack

  IIC_Wait_Ack (Thumb, 82 bytes, Stack size 8 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = IIC_Wait_Ack ⇒ IIC_Stop
  [Calls]
  - >> IIC_Stop
  - >> delay_us
  [Called By]
  - >> AT24CXX_WriteOneByte
  - >> AT24CXX_ReadOneByte

  IIC_Ack (Thumb, 72 bytes, Stack size 8 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_Ack
  [Calls]
  - >> delay_us
  [Called By]
  - >> IIC_Read_Byte

  IIC_NAck (Thumb, 72 bytes, Stack size 8 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_NAck
  [Calls]
  - >> delay_us
  [Called By]
  - >> IIC_Read_Byte

  IIC_Send_Byte (Thumb, 96 bytes, Stack size 16 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = IIC_Send_Byte
  [Calls]
  - >> delay_us
  [Called By]
  - >> AT24CXX_WriteOneByte
  - >> AT24CXX_ReadOneByte

  IIC_Read_Byte (Thumb, 98 bytes, Stack size 16 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = IIC_Read_Byte ⇒ IIC_NAck
  [Calls]
  - >> IIC_NAck
  - >> IIC_Ack
  - >> delay_us
  [Called By]
  - >> AT24CXX_ReadOneByte

  AT24CXX_Init (Thumb, 8 bytes, Stack size 8 bytes, 24cxx.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = AT24CXX_Init
  [Calls]
  - >> IIC_Init
  [Called By]
  - >> TP_Init

  AT24CXX_ReadOneByte (Thumb, 88 bytes, Stack size 16 bytes, 24cxx.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = AT24CXX_ReadOneByte ⇒ IIC_Read_Byte ⇒ IIC_NAck
  [Calls]
  - >> IIC_Read_Byte
  - >> IIC_Send_Byte
  - >> IIC_Wait_Ack
  - >> IIC_Stop
  - >> IIC_Start
  [Called By]
  - >> TP_Get_Adjdata
  - >> AT24CXX_Read
  - >> AT24CXX_Check
  - >> AT24CXX_ReadLenByte
  [Address Reference Count : 1]
  - usmart_config.o(.data)

  AT24CXX_WriteOneByte (Thumb, 80 bytes, Stack size 16 bytes, 24cxx.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = AT24CXX_WriteOneByte ⇒ IIC_Send_Byte
  [Calls]
  - >> IIC_Send_Byte
  - >> IIC_Wait_Ack
  - >> IIC_Stop
  - >> IIC_Start
  - >> delay_ms
  [Called By]
  - >> AT24CXX_Write
  - >> AT24CXX_Check
  - >> AT24CXX_WriteLenByte
  - >> TP_Save_Adjdata
  [Address Reference Count : 1]
  - usmart_config.o(.data)

  AT24CXX_WriteLenByte (Thumb, 42 bytes, Stack size 24 bytes, 24cxx.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = AT24CXX_WriteLenByte ⇒ AT24CXX_WriteOneByte ⇒ IIC_Send_Byte
  [Calls]
  - >> AT24CXX_WriteOneByte
  [Called By]
  - >> TP_Save_Adjdata

  AT24CXX_ReadLenByte (Thumb, 44 bytes, Stack size 24 bytes, 24cxx.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = AT24CXX_ReadLenByte ⇒ AT24CXX_ReadOneByte ⇒ IIC_Read_Byte ⇒ IIC_NAck
  [Calls]
  - >> AT24CXX_ReadOneByte
  [Called By]
  - >> TP_Get_Adjdata

  AT24CXX_Check (Thumb, 46 bytes, Stack size 8 bytes, 24cxx.o(.text), UNUSED)
  [Calls]

  - >> AT24CXX_WriteOneByte
  - >> AT24CXX_ReadOneByte

  AT24CXX_Read (Thumb, 34 bytes, Stack size 16 bytes, 24cxx.o(.text), UNUSED)
  [Calls]

  - >> AT24CXX_ReadOneByte

  AT24CXX_Write (Thumb, 36 bytes, Stack size 16 bytes, 24cxx.o(.text), UNUSED)
  [Calls]

  - >> AT24CXX_WriteOneByte

  USART2_IRQHandler (Thumb, 46 bytes, Stack size 0 bytes, rs485.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RS485_Init (Thumb, 254 bytes, Stack size 40 bytes, rs485.o(.text), UNUSED)
  [Calls]

  - >> MY_NVIC_Init
  - >> __aeabi_fmul
  - >> __aeabi_ui2f
  - >> __aeabi_f2uiz
  - >> __aeabi_fdiv
  - >> __aeabi_frsub

  RS485_Send_Data (Thumb, 68 bytes, Stack size 8 bytes, rs485.o(.text), UNUSED)

  RS485_Receive_Data (Thumb, 68 bytes, Stack size 24 bytes, rs485.o(.text), UNUSED)
  [Calls]

  - >> delay_ms

  TP_Write_Byte (Thumb, 64 bytes, Stack size 0 bytes, touch.o(.text))
  [Called By]

  - >> TP_Read_AD

  TP_Read_AD (Thumb, 124 bytes, Stack size 16 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = TP_Read_AD
  [Calls]
  - >> TP_Write_Byte
  - >> delay_us
  [Called By]
  - >> TP_Read_XOY

  TP_Read_XOY (Thumb, 120 bytes, Stack size 40 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = TP_Read_XOY ⇒ TP_Read_AD
  [Calls]
  - >> TP_Read_AD
  [Called By]
  - >> TP_Read_XY

  TP_Read_XY (Thumb, 38 bytes, Stack size 24 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = TP_Read_XY ⇒ TP_Read_XOY ⇒ TP_Read_AD
  [Calls]
  - >> TP_Read_XOY
  [Called By]
  - >> TP_Init
  - >> TP_Read_XY2

  TP_Read_XY2 (Thumb, 192 bytes, Stack size 32 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = TP_Read_XY2 ⇒ TP_Read_XY ⇒ TP_Read_XOY ⇒ TP_Read_AD
  [Calls]
  - >> TP_Read_XY
  [Called By]
  - >> TP_Scan

  TP_Drow_Touch_Point (Thumb, 108 bytes, Stack size 16 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = TP_Drow_Touch_Point ⇒ LCD_DrawLine ⇒ LCD_DrawPoint ⇒ LCD_SetCursor
  [Calls]
  - >> Draw_Circle
  - >> LCD_DrawLine
  - >> LCD_DrawPoint
  [Called By]
  - >> TP_Adjust

  TP_Draw_Big_Point (Thumb, 54 bytes, Stack size 16 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = TP_Draw_Big_Point ⇒ LCD_DrawPoint ⇒ LCD_SetCursor
  [Calls]
  - >> LCD_DrawPoint
  [Called By]
  - >> main

  TP_Scan (Thumb, 244 bytes, Stack size 24 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = TP_Scan ⇒ TP_Read_XY2 ⇒ TP_Read_XY ⇒ TP_Read_XOY ⇒ TP_Read_AD
  [Calls]
  - >> TP_Read_XY2
  - >> __aeabi_fmul
  - >> __aeabi_ui2f
  - >> __aeabi_i2f
  - >> __aeabi_f2uiz
  - >> __aeabi_fadd
  [Address Reference Count : 1]
  - touch.o(.data)

  TP_Save_Adjdata (Thumb, 168 bytes, Stack size 16 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = TP_Save_Adjdata ⇒ AT24CXX_WriteLenByte ⇒ AT24CXX_WriteOneByte ⇒ IIC_Send_Byte
  [Calls]
  - >> AT24CXX_WriteLenByte
  - >> AT24CXX_WriteOneByte
  - >> __aeabi_fmul
  - >> __aeabi_f2iz
  [Called By]
  - >> TP_Init
  - >> TP_Adjust
  - >> main

  TP_Get_Adjdata (Thumb, 152 bytes, Stack size 16 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = TP_Get_Adjdata ⇒ AT24CXX_ReadLenByte ⇒ AT24CXX_ReadOneByte ⇒ IIC_Read_Byte ⇒ IIC_NAck
  [Calls]
  - >> AT24CXX_ReadLenByte
  - >> AT24CXX_ReadOneByte
  - >> __aeabi_i2f
  - >> __aeabi_fdiv
  [Called By]
  - >> TP_Init
  - >> TP_Adjust

  TP_Adj_Info_Show (Thumb, 376 bytes, Stack size 48 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 164
  - Call Chain = TP_Adj_Info_Show ⇒ LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor
  [Calls]
  - >> LCD_ShowNum
  - >> LCD_ShowString
  [Called By]
  - >> TP_Adjust

  TP_Adjust (Thumb, 2082 bytes, Stack size 88 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 252
  - Call Chain = TP_Adjust ⇒ TP_Adj_Info_Show ⇒ LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor
  [Calls]
  - >> TP_Adj_Info_Show
  - >> TP_Get_Adjdata
  - >> TP_Drow_Touch_Point
  - >> delay_ms
  - >> TP_Save_Adjdata
  - >> LCD_ShowString
  - >> LCD_Clear
  - >> sqrt
  - >> __aeabi_fmul
  - >> __aeabi_ui2f
  - >> __aeabi_i2f
  - >> __aeabi_f2uiz
  - >> __aeabi_f2iz
  - >> __aeabi_fdiv
  - >> __aeabi_fsub
  - >> __aeabi_f2d
  - >> __aeabi_cdrcmple
  - >> __aeabi_cdcmple
  - >> __aeabi_ui2d
  - >> __aeabi_d2uiz
  [Called By]
  - >> TP_Init
  - >> main
  [Address Reference Count : 1]
  - touch.o(.data)

  TP_Init (Thumb, 152 bytes, Stack size 8 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 260
  - Call Chain = TP_Init ⇒ TP_Adjust ⇒ TP_Adj_Info_Show ⇒ LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor
  [Calls]
  - >> TP_Get_Adjdata
  - >> TP_Read_XY
  - >> AT24CXX_Init
  - >> TP_Save_Adjdata
  - >> TP_Adjust
  - >> LCD_Clear
  [Address Reference Count : 1]
  - touch.o(.data)

  usmart_sys_cmd_exe (Thumb, 1570 bytes, Stack size 56 bytes, usmart.o(.text))
  [Stack]

  - Max Depth = 200 + Unknown Stack Size
  - Call Chain = usmart_sys_cmd_exe ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> usmart_strcmp
  - >> usmart_str2num
  - >> usmart_get_fname
  - >> usmart_get_cmdname
  - >> usmart_get_aparm
  - >> __2printf
  [Called By]
  - >> usmart_scan

  TIM2_IRQHandler (Thumb, 38 bytes, Stack size 8 bytes, usmart.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  Timer2_Init (Thumb, 68 bytes, Stack size 16 bytes, usmart.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = Timer2_Init ⇒ MY_NVIC_Init
  [Calls]
  - >> MY_NVIC_Init
  [Called By]
  - >> usmart_init

  usmart_init (Thumb, 36 bytes, Stack size 8 bytes, usmart.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = usmart_init ⇒ Timer2_Init ⇒ MY_NVIC_Init
  [Calls]
  - >> Timer2_Init
  [Address Reference Count : 1]
  - usmart_config.o(.data)

  usmart_cmd_rec (Thumb, 170 bytes, Stack size 96 bytes, usmart.o(.text))
  [Stack]

  - Max Depth = 372
  - Call Chain = usmart_cmd_rec ⇒ usmart_get_fparam ⇒ usmart_str2num ⇒ usmart_pow
  [Calls]
  - >> usmart_strcmp
  - >> usmart_get_fparam
  - >> usmart_get_fname
  [Address Reference Count : 1]
  - usmart_config.o(.data)

  usmart_exe (Thumb, 712 bytes, Stack size 128 bytes, usmart.o(.text))
  [Stack]

  - Max Depth = 272 + Unknown Stack Size
  - Call Chain = usmart_exe ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> usmart_get_parmpos
  - >> usmart_get_fname
  - >> __2printf
  [Address Reference Count : 1]
  - usmart_config.o(.data)

  usmart_scan (Thumb, 118 bytes, Stack size 16 bytes, usmart.o(.text))
  [Stack]

  - Max Depth = 216 + Unknown Stack Size
  - Call Chain = usmart_scan ⇒ usmart_sys_cmd_exe ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> usmart_sys_cmd_exe
  - >> __2printf
  [Address Reference Count : 1]
  - usmart_config.o(.data)

  read_addr (Thumb, 6 bytes, Stack size 0 bytes, usmart.o(.text))
  [Address Reference Count : 1]

  - usmart_config.o(.data)

  write_addr (Thumb, 4 bytes, Stack size 0 bytes, usmart.o(.text))
  [Address Reference Count : 1]

  - usmart_config.o(.data)

  usmart_strcmp (Thumb, 34 bytes, Stack size 0 bytes, usmart_str.o(.text))
  [Called By]

  - >> usmart_get_fname
  - >> usmart_cmd_rec
  - >> usmart_sys_cmd_exe

  usmart_strcopy (Thumb, 22 bytes, Stack size 0 bytes, usmart_str.o(.text))
  [Called By]

  - >> usmart_get_fparam

  usmart_strlen (Thumb, 24 bytes, Stack size 0 bytes, usmart_str.o(.text))
  [Called By]

  - >> usmart_get_fparam

  usmart_pow (Thumb, 22 bytes, Stack size 8 bytes, usmart_str.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = usmart_pow
  [Called By]
  - >> usmart_str2num

  usmart_str2num (Thumb, 202 bytes, Stack size 28 bytes, usmart_str.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = usmart_str2num ⇒ usmart_pow
  [Calls]
  - >> usmart_pow
  [Called By]
  - >> usmart_get_fparam
  - >> usmart_sys_cmd_exe

  usmart_get_cmdname (Thumb, 54 bytes, Stack size 8 bytes, usmart_str.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = usmart_get_cmdname
  [Called By]
  - >> usmart_sys_cmd_exe

  usmart_search_nextc (Thumb, 22 bytes, Stack size 0 bytes, usmart_str.o(.text))
  [Called By]

  - >> usmart_get_fname

  usmart_get_fname (Thumb, 440 bytes, Stack size 72 bytes, usmart_str.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = usmart_get_fname
  [Calls]
  - >> usmart_strcmp
  - >> usmart_search_nextc
  [Called By]
  - >> usmart_exe
  - >> usmart_cmd_rec
  - >> usmart_sys_cmd_exe

  usmart_get_aparm (Thumb, 188 bytes, Stack size 20 bytes, usmart_str.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = usmart_get_aparm
  [Called By]
  - >> usmart_get_fparam
  - >> usmart_sys_cmd_exe

  usmart_get_parmpos (Thumb, 26 bytes, Stack size 0 bytes, usmart_str.o(.text))
  [Called By]

  - >> usmart_get_fparam
  - >> usmart_exe

  usmart_get_fparam (Thumb, 262 bytes, Stack size 240 bytes, usmart_str.o(.text))
  [Stack]

  - Max Depth = 276
  - Call Chain = usmart_get_fparam ⇒ usmart_str2num ⇒ usmart_pow
  [Calls]
  - >> usmart_str2num
  - >> usmart_get_parmpos
  - >> usmart_get_aparm
  - >> usmart_strlen
  - >> usmart_strcopy
  [Called By]
  - >> usmart_cmd_rec

  __use_no_semihosting (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi_2.o(.text), UNUSED)

  __2printf (Thumb, 20 bytes, Stack size 24 bytes, noretval__2printf.o(.text))
  [Stack]

  - Max Depth = 144 + Unknown Stack Size
  - Call Chain = __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> _printf_char_file
  [Called By]
  - >> usmart_scan
  - >> usmart_exe
  - >> usmart_sys_cmd_exe
  - >> RTC_Init
  - >> LCD_Init

  _printf_pre_padding (Thumb, 46 bytes, Stack size 16 bytes, _printf_pad.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = _printf_pre_padding
  [Called By]
  - >> _printf_int_common
  - >> _printf_str

  _printf_post_padding (Thumb, 36 bytes, Stack size 16 bytes, _printf_pad.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = _printf_post_padding
  [Called By]
  - >> _printf_int_common
  - >> _printf_str

  _printf_str (Thumb, 82 bytes, Stack size 16 bytes, _printf_str.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_post_padding
  - >> _printf_pre_padding
  [Called By]
  - >> _printf_cs_common

  _printf_int_dec (Thumb, 102 bytes, Stack size 24 bytes, _printf_dec.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = _printf_int_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_common
  [Called By]
  - >> _printf_u
  - >> _printf_d

  _printf_int_hex (Thumb, 88 bytes, Stack size 16 bytes, _printf_hex_int.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = _printf_int_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_common
  [Called By]
  - >> _printf_x

  _printf_longlong_hex (Thumb, 0 bytes, Stack size 16 bytes, _printf_hex_int.o(.text), UNUSED)

  __printf (Thumb, 390 bytes, Stack size 40 bytes, __printf_flags_ss_wp.o(.text))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = __printf
  [Calls]
  - >> _printf_percent
  - >> _is_digit
  [Called By]
  - >> _printf_char_common

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __read_errno (Thumb, 10 bytes, Stack size 8 bytes, _rserrno.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_errno_addr

  __set_errno (Thumb, 12 bytes, Stack size 8 bytes, _rserrno.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __set_errno
  [Calls]
  - >> __aeabi_errno_addr
  [Called By]
  - >> sqrt

  _printf_int_common (Thumb, 184 bytes, Stack size 32 bytes, _printf_intcommon.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_post_padding
  - >> _printf_pre_padding
  [Called By]
  - >> _printf_int_hex
  - >> _printf_int_dec

  _printf_cs_common (Thumb, 20 bytes, Stack size 8 bytes, _printf_char.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _printf_cs_common ⇒ _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_str
  [Called By]
  - >> _printf_string
  - >> _printf_char

  _printf_char (Thumb, 16 bytes, Stack size 0 bytes, _printf_char.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _printf_char ⇒ _printf_cs_common ⇒ _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_cs_common
  [Called By]
  - >> _printf_c

  _printf_string (Thumb, 8 bytes, Stack size 0 bytes, _printf_char.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _printf_string ⇒ _printf_cs_common ⇒ _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_cs_common
  [Called By]
  - >> _printf_s

  _printf_char_file (Thumb, 32 bytes, Stack size 16 bytes, _printf_char_file.o(.text))
  [Stack]

  - Max Depth = 120 + Unknown Stack Size
  - Call Chain = _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> ferror
  - >> _printf_char_common
  [Called By]
  - >> __2printf

  __aeabi_errno_addr (Thumb, 8 bytes, Stack size 0 bytes, rt_errno_addr_intlibspace.o(.text))
  [Called By]

  - >> __set_errno
  - >> __read_errno

  __errno$intlibspace (Thumb, 0 bytes, Stack size 0 bytes, rt_errno_addr_intlibspace.o(.text), UNUSED)

  __rt_errno_addr$intlibspace (Thumb, 0 bytes, Stack size 0 bytes, rt_errno_addr_intlibspace.o(.text), UNUSED)

  _printf_char_common (Thumb, 32 bytes, Stack size 64 bytes, _printf_char_common.o(.text))
  [Stack]

  - Max Depth = 104 + Unknown Stack Size
  - Call Chain = _printf_char_common ⇒ __printf
  [Calls]
  - >> __printf
  [Called By]
  - >> _printf_char_file

  ferror (Thumb, 8 bytes, Stack size 0 bytes, ferror.o(.text))
  [Called By]

  - >> _printf_char_file

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 12 bytes, Stack size 0 bytes, exit.o(.text))
  [Calls]

  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  _is_digit (Thumb, 14 bytes, Stack size 0 bytes, __printf_wp.o(i._is_digit))
  [Called By]

  - >> __printf

  sqrt (Thumb, 78 bytes, Stack size 24 bytes, sqrt.o(i.sqrt))
  [Stack]

  - Max Depth = 64
  - Call Chain = sqrt ⇒ _dsqrt ⇒ __fpl_dnaninf
  [Calls]
  - >> _dsqrt
  - >> __set_errno
  [Called By]
  - >> TP_Adjust

  __aeabi_d2f (Thumb, 0 bytes, Stack size 32 bytes, d2f.o(x$fpl$d2f))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_d2f
  [Called By]
  - >> Dac1_Set_Vol

  _d2f (Thumb, 98 bytes, Stack size 32 bytes, d2f.o(x$fpl$d2f), UNUSED)
  [Calls]

  - >> __fpl_fretinf
  - >> __fpl_dnaninf

  __fpl_dcmp_Inf (Thumb, 24 bytes, Stack size 0 bytes, dcmpi.o(x$fpl$dcmpinf), UNUSED)
  [Called By]

  - >> _dcmple

  __aeabi_ddiv (Thumb, 0 bytes, Stack size 32 bytes, ddiv.o(x$fpl$ddiv))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_ddiv
  [Called By]
  - >> Dac1_Set_Vol

  _ddiv (Thumb, 552 bytes, Stack size 32 bytes, ddiv.o(x$fpl$ddiv), UNUSED)
  [Calls]

  - >> __fpl_dretinf
  - >> __fpl_dnaninf

  __aeabi_d2uiz (Thumb, 0 bytes, Stack size 32 bytes, dfixu.o(x$fpl$dfixu))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_d2uiz
  [Called By]
  - >> TP_Adjust

  _dfixu (Thumb, 90 bytes, Stack size 32 bytes, dfixu.o(x$fpl$dfixu), UNUSED)
  [Calls]

  - >> __fpl_dnaninf

  __aeabi_ui2d (Thumb, 0 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dfltu))
  [Called By]

  - >> TP_Adjust

  _dfltu (Thumb, 38 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dfltu), UNUSED)

  __aeabi_cdcmple (Thumb, 0 bytes, Stack size 32 bytes, dleqf.o(x$fpl$dleqf))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_cdcmple
  [Called By]
  - >> TP_Adjust

  _dcmple (Thumb, 120 bytes, Stack size 32 bytes, dleqf.o(x$fpl$dleqf), UNUSED)
  [Calls]

  - >> __fpl_dnaninf
  - >> __fpl_dcmp_Inf

  __fpl_dcmple_InfNaN (Thumb, 0 bytes, Stack size unknown bytes, dleqf.o(x$fpl$dleqf), UNUSED)
  [Called By]

  - >> _drcmple

  __fpl_dnaninf (Thumb, 156 bytes, Stack size 16 bytes, dnaninf.o(x$fpl$dnaninf))
  [Stack]

  - Max Depth = 16
  - Call Chain = __fpl_dnaninf
  [Called By]
  - >> _dsqrt
  - >> _dcmple
  - >> _dfixu
  - >> _ddiv
  - >> _d2f

  __fpl_dretinf (Thumb, 12 bytes, Stack size 0 bytes, dretinf.o(x$fpl$dretinf), UNUSED)
  [Called By]

  - >> _f2d
  - >> _ddiv

  __aeabi_cdrcmple (Thumb, 0 bytes, Stack size 16 bytes, drleqf.o(x$fpl$drleqf))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_cdrcmple
  [Called By]
  - >> TP_Adjust

  _drcmple (Thumb, 108 bytes, Stack size 16 bytes, drleqf.o(x$fpl$drleqf), UNUSED)
  [Calls]

  - >> __fpl_dcmple_InfNaN

  _dsqrt (Thumb, 456 bytes, Stack size 24 bytes, dsqrt_noumaal.o(x$fpl$dsqrt))
  [Stack]

  - Max Depth = 40
  - Call Chain = _dsqrt ⇒ __fpl_dnaninf
  [Calls]
  - >> __fpl_dnaninf
  [Called By]
  - >> sqrt

  __aeabi_f2d (Thumb, 0 bytes, Stack size 16 bytes, f2d.o(x$fpl$f2d))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_f2d
  [Called By]
  - >> Dac1_Set_Vol
  - >> TP_Adjust

  _f2d (Thumb, 86 bytes, Stack size 16 bytes, f2d.o(x$fpl$f2d), UNUSED)
  [Calls]

  - >> __fpl_fnaninf
  - >> __fpl_dretinf

  __aeabi_fadd (Thumb, 0 bytes, Stack size 16 bytes, faddsub_clz.o(x$fpl$fadd))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_fadd
  [Called By]
  - >> TP_Scan

  _fadd (Thumb, 196 bytes, Stack size 16 bytes, faddsub_clz.o(x$fpl$fadd), UNUSED)
  [Calls]

  - >> __fpl_fretinf
  - >> __fpl_fnaninf
  - >> _fsub1

  __aeabi_fdiv (Thumb, 0 bytes, Stack size 16 bytes, fdiv.o(x$fpl$fdiv))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_fdiv
  [Called By]
  - >> TP_Get_Adjdata
  - >> RS485_Init
  - >> Dac1_Set_Vol
  - >> uart_init
  - >> TP_Adjust

  _fdiv (Thumb, 384 bytes, Stack size 16 bytes, fdiv.o(x$fpl$fdiv), UNUSED)
  [Calls]

  - >> __fpl_fretinf
  - >> __fpl_fnaninf

  __aeabi_f2iz (Thumb, 0 bytes, Stack size 16 bytes, ffix.o(x$fpl$ffix))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_f2iz
  [Called By]
  - >> TP_Save_Adjdata
  - >> TP_Adjust

  _ffix (Thumb, 54 bytes, Stack size 16 bytes, ffix.o(x$fpl$ffix), UNUSED)
  [Calls]

  - >> __fpl_fnaninf

  __aeabi_f2uiz (Thumb, 0 bytes, Stack size 16 bytes, ffixu.o(x$fpl$ffixu))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_f2uiz
  [Called By]
  - >> TP_Scan
  - >> RS485_Init
  - >> Dac1_Set_Vol
  - >> uart_init
  - >> TP_Adjust

  _ffixu (Thumb, 62 bytes, Stack size 16 bytes, ffixu.o(x$fpl$ffixu), UNUSED)
  [Calls]

  - >> __fpl_fnaninf

  __aeabi_i2f (Thumb, 0 bytes, Stack size 0 bytes, fflt_clz.o(x$fpl$fflt))
  [Called By]

  - >> TP_Get_Adjdata
  - >> TP_Scan
  - >> TP_Adjust

  _fflt (Thumb, 48 bytes, Stack size 0 bytes, fflt_clz.o(x$fpl$fflt), UNUSED)

  __aeabi_ui2f (Thumb, 0 bytes, Stack size 0 bytes, fflt_clz.o(x$fpl$ffltu))
  [Called By]

  - >> TP_Scan
  - >> RS485_Init
  - >> Dac1_Set_Vol
  - >> uart_init
  - >> TP_Adjust

  _ffltu (Thumb, 38 bytes, Stack size 0 bytes, fflt_clz.o(x$fpl$ffltu), UNUSED)

  __aeabi_fmul (Thumb, 0 bytes, Stack size 16 bytes, fmul.o(x$fpl$fmul))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_fmul
  [Called By]
  - >> TP_Scan
  - >> RS485_Init
  - >> Dac1_Set_Vol
  - >> uart_init
  - >> TP_Save_Adjdata
  - >> TP_Adjust

  _fmul (Thumb, 258 bytes, Stack size 16 bytes, fmul.o(x$fpl$fmul), UNUSED)
  [Calls]

  - >> __fpl_fretinf
  - >> __fpl_fnaninf

  __fpl_fnaninf (Thumb, 140 bytes, Stack size 8 bytes, fnaninf.o(x$fpl$fnaninf), UNUSED)
  [Called By]

  - >> _fmul
  - >> _ffixu
  - >> _ffix
  - >> _fdiv
  - >> _fsub
  - >> _fadd
  - >> _f2d

  __fpl_fretinf (Thumb, 10 bytes, Stack size 0 bytes, fretinf.o(x$fpl$fretinf), UNUSED)
  [Called By]

  - >> _fmul
  - >> _fdiv
  - >> _fadd
  - >> _d2f

  __aeabi_frsub (Thumb, 0 bytes, Stack size 0 bytes, faddsub_clz.o(x$fpl$frsb))
  [Called By]

  - >> RS485_Init
  - >> uart_init

  _frsb (Thumb, 20 bytes, Stack size 0 bytes, faddsub_clz.o(x$fpl$frsb), UNUSED)
  [Calls]

  - >> _fsub1
  - >> _fadd1

  __aeabi_fsub (Thumb, 0 bytes, Stack size 16 bytes, faddsub_clz.o(x$fpl$fsub))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_fsub
  [Called By]
  - >> TP_Adjust

  _fsub (Thumb, 234 bytes, Stack size 16 bytes, faddsub_clz.o(x$fpl$fsub), UNUSED)
  [Calls]

  - >> __fpl_fnaninf
  - >> _fadd1

  ### Local Symbols

  _fadd1 (Thumb, 0 bytes, Stack size unknown bytes, faddsub_clz.o(x$fpl$fadd), UNUSED)
  [Called By]

  - >> _fsub
  - >> _frsb

  _fsub1 (Thumb, 0 bytes, Stack size unknown bytes, faddsub_clz.o(x$fpl$fsub), UNUSED)
  [Called By]

  - >> _frsb
  - >> _fadd

  _printf_input_char (Thumb, 10 bytes, Stack size 0 bytes, _printf_char_common.o(.text))
  [Address Reference Count : 1]

  - _printf_char_common.o(.text)

  ### Undefined Global Symbols