#

##

##

##

    礦ision Build Log
    Tool Versions:
    IDE-Version: μVision V5.17.0.0
    Copyright (C) 2015 ARM Ltd and ARM Germany GmbH. All rights reserved.
    License Information: X XT, Fly, LIC=21NPC-7EQ48-6B7EJ-U9LGF-6DJAV-RDK1B

    Tool Versions:
    Toolchain:       PK51 Prof. Developers Kit  Version: 9.54
    Toolchain Path:  C:\Keil_v5\C51\BIN
    C Compiler:      C51.exe V9.54
    Assembler:       A51.exe V8.02c
    Linker/Locator:  BL51.exe V6.22
    Library Manager: LIB51.exe V4.30.1.0
    Hex Converter:   OH51.exe V2.7.0.0
    CPU DLL:         S8051.DLL V3.100.0.0
    Dialog DLL:      DP51.DLL V2.62.0.1
    Project:
    F:\01-核心结构\04-信息架构\02-产品信息\01-开发板类\NO.1011710-STC15W408AS Micro Board\01-资料整理\STC15W408AS最小系统板资料v1.0\03-例程\中断测试\Interrupt Test.uvproj
    Project File Date:  04/18/2017

    Output:
    Rebuild target 'STC89C52'
    assembling STARTUP.A51...
    compiling main.c...
    linking...
    Program Size: data=9.0 xdata=0 code=33
    creating hex file from "Interrupt Test"...
    "Interrupt Test" - 0 Error(s), 0 Warning(s).
    Build Time Elapsed:  00:00:01