#

##

##

##

    礦ision Build Log
    Tool Versions:
    IDE-Version: μVision V5.12.0.0
    Copyright (C) 2014 ARM Ltd and ARM Germany GmbH. All rights reserved.
    License Information: wang 微软用户, 微软中国, LIC=21NGK-ZCD15-YFLI4-FI5FA-I9FMM-NUG9C

    Tool Versions:
    Toolchain:       PK51 Prof. Developers Kit  Version: 9.52.0.0
    Toolchain Path:  D:\Keil_v5\C51\BIN
    C Compiler:      C51.exe V9.52.0.0
    Assembler:       A51.exe V8.02b
    Linker/Locator:  BL51.exe V6.22
    Library Manager: LIB51.exe V4.29
    Hex Converter:   OH51.exe V2.7.0.0
    CPU DLL:         S8051.DLL V3.91.0.0
    Dialog DLL:      DP51.DLL V2.62.0.1
        Target DLL: NULink\Nu_Link_51.dll
    Dialog DLL:      TP51.DLL V2.58

    Project:
    E:\360云盘\项目\RC522模块 SPI(0001)\RC522 SPI程序\51读写卡参考例程\RC522 SPI\TEST522.uvproj
    Project File Date:  02/17/2014

    Output:
    Rebuild target '射频读写卡器'
    compiling MAIN.C...
    compiling RC522.C...
    linking...
    *** WARNING L16: UNCALLED SEGMENT, IGNORED FOR OVERLAY PROCESS
        SEGMENT: ?PR?_PCDWRITE?RC522
    *** WARNING L16: UNCALLED SEGMENT, IGNORED FOR OVERLAY PROCESS
        SEGMENT: ?PR?PCDHALT?RC522
    *** WARNING L16: UNCALLED SEGMENT, IGNORED FOR OVERLAY PROCESS
        SEGMENT: ?PR?_M500PCDCONFIGISOTYPE?RC522
    Program Size: data=122.0 xdata=0 code=1964
    creating hex file from "TEST522"...
    "TEST522" - 0 Error(s), 3 Warning(s).