Static Call Graph - [.\STM32100E-EVAL\STM32100E-EVAL.axf]

# Static Call Graph for image .\STM32100E-EVAL\STM32100E-EVAL.axf

#<CALLGRAPH># ARM Linker, 5050041: Last Updated: Sun Dec 07 15:59:51 2014

### Maximum Stack Usage = 192 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ WaitCardOff ⇒ PcdRequest ⇒ PcdComMF522 ⇒ SetBitMask ⇒ WriteRawRC

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler
- BusFault_Handler ⇒ BusFault_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- UsageFault_Handler ⇒ UsageFault_Handler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - BusFault_Handler from stm32f10x_it.o(i.BusFault_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DebugMon_Handler from stm32f10x_it.o(i.DebugMon_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - FLASH_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - HardFault_Handler from stm32f10x_it.o(i.HardFault_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - MemManage_Handler from stm32f10x_it.o(i.MemManage_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - NMI_Handler from stm32f10x_it.o(i.NMI_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - PVD_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - PendSV_Handler from stm32f10x_it.o(i.PendSV_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - RCC_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - RTCAlarm_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - RTC_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - Reset_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - SPI1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - SPI2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - SVC_Handler from stm32f10x_it.o(i.SVC_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - SysTick_Handler from stm32f10x_it.o(i.SysTick_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - SystemInit from system_stm32f10x.o(i.SystemInit) referenced from startup_stm32f10x_md.o(.text)
  - TAMPER_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM3_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM4_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USART1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USART2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USART3_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - UsageFault_Handler from stm32f10x_it.o(i.UsageFault_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - WWDG_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f10x_md.o(.text)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.BusFault_Handler))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  CalulateCRC (Thumb, 102 bytes, Stack size 24 bytes, rc522.o(i.CalulateCRC))
  [Stack]

  - Max Depth = 80
  - Call Chain = CalulateCRC ⇒ SetBitMask ⇒ WriteRawRC
  [Calls]
  - >> WriteRawRC
  - >> SetBitMask
  - >> ReadRawRC
  - >> ClearBitMask
  [Called By]
  - >> PcdSelect
  - >> PcdRead

  ClearBitMask (Thumb, 24 bytes, Stack size 16 bytes, rc522.o(i.ClearBitMask))
  [Stack]

  - Max Depth = 56
  - Call Chain = ClearBitMask ⇒ WriteRawRC
  [Calls]
  - >> WriteRawRC
  - >> ReadRawRC
  [Called By]
  - >> PcdSelect
  - >> PcdRequest
  - >> PcdComMF522
  - >> PcdAnticoll
  - >> PcdAntennaOff
  - >> M500PcdConfigISOType
  - >> CalulateCRC

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  GPIO_Init (Thumb, 162 bytes, Stack size 20 bytes, stm32f10x_gpio.o(i.GPIO_Init))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> GPIO_ini

  GPIO_ReadInputDataBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_ReadInputDataBit))
  [Called By]

  - >> ReadRawRC

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_ResetBits))
  [Called By]

  - >> main
  - >> InitializeSystem
  - >> WriteRawRC
  - >> ReadRawRC
  - >> PcdReset

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_SetBits))
  [Called By]

  - >> main
  - >> InitializeSystem
  - >> WriteRawRC
  - >> ReadRawRC
  - >> PcdReset

  GPIO_ini (Thumb, 194 bytes, Stack size 24 bytes, main.o(i.GPIO_ini))
  [Stack]

  - Max Depth = 44
  - Call Chain = GPIO_ini ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> main

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.HardFault_Handler))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  InitializeSystem (Thumb, 90 bytes, Stack size 8 bytes, main.o(i.InitializeSystem))
  [Stack]

  - Max Depth = 80
  - Call Chain = InitializeSystem ⇒ M500PcdConfigISOType ⇒ PcdAntennaOn ⇒ SetBitMask ⇒ WriteRawRC
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> delay_10ms
  - >> PcdReset
  - >> PcdAntennaOn
  - >> PcdAntennaOff
  - >> M500PcdConfigISOType
  [Called By]
  - >> main

  M500PcdConfigISOType (Thumb, 88 bytes, Stack size 8 bytes, rc522.o(i.M500PcdConfigISOType))
  [Stack]

  - Max Depth = 72
  - Call Chain = M500PcdConfigISOType ⇒ PcdAntennaOn ⇒ SetBitMask ⇒ WriteRawRC
  [Calls]
  - >> delay_10ms
  - >> WriteRawRC
  - >> PcdAntennaOn
  - >> ClearBitMask
  [Called By]
  - >> InitializeSystem

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.MemManage_Handler))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  PcdAntennaOff (Thumb, 8 bytes, Stack size 0 bytes, rc522.o(i.PcdAntennaOff))
  [Stack]

  - Max Depth = 56
  - Call Chain = PcdAntennaOff ⇒ ClearBitMask ⇒ WriteRawRC
  [Calls]
  - >> ClearBitMask
  [Called By]
  - >> InitializeSystem

  PcdAntennaOn (Thumb, 26 bytes, Stack size 8 bytes, rc522.o(i.PcdAntennaOn))
  [Stack]

  - Max Depth = 64
  - Call Chain = PcdAntennaOn ⇒ SetBitMask ⇒ WriteRawRC
  [Calls]
  - >> SetBitMask
  - >> ReadRawRC
  [Called By]
  - >> InitializeSystem
  - >> M500PcdConfigISOType

  PcdAnticoll (Thumb, 106 bytes, Stack size 48 bytes, rc522.o(i.PcdAnticoll))
  [Stack]

  - Max Depth = 160
  - Call Chain = PcdAnticoll ⇒ PcdComMF522 ⇒ SetBitMask ⇒ WriteRawRC
  [Calls]
  - >> WriteRawRC
  - >> SetBitMask
  - >> PcdComMF522
  - >> ClearBitMask
  [Called By]
  - >> main

  PcdAuthState (Thumb, 82 bytes, Stack size 40 bytes, rc522.o(i.PcdAuthState))
  [Stack]

  - Max Depth = 152
  - Call Chain = PcdAuthState ⇒ PcdComMF522 ⇒ SetBitMask ⇒ WriteRawRC
  [Calls]
  - >> ReadRawRC
  - >> PcdComMF522
  [Called By]
  - >> main

  PcdComMF522 (Thumb, 278 bytes, Stack size 56 bytes, rc522.o(i.PcdComMF522))
  [Stack]

  - Max Depth = 112
  - Call Chain = PcdComMF522 ⇒ SetBitMask ⇒ WriteRawRC
  [Calls]
  - >> WriteRawRC
  - >> SetBitMask
  - >> ReadRawRC
  - >> ClearBitMask
  [Called By]
  - >> PcdSelect
  - >> PcdRequest
  - >> PcdRead
  - >> PcdAuthState
  - >> PcdAnticoll

  PcdRead (Thumb, 74 bytes, Stack size 40 bytes, rc522.o(i.PcdRead))
  [Stack]

  - Max Depth = 152
  - Call Chain = PcdRead ⇒ PcdComMF522 ⇒ SetBitMask ⇒ WriteRawRC
  [Calls]
  - >> PcdComMF522
  - >> CalulateCRC
  [Called By]
  - >> main

  PcdRequest (Thumb, 80 bytes, Stack size 40 bytes, rc522.o(i.PcdRequest))
  [Stack]

  - Max Depth = 152
  - Call Chain = PcdRequest ⇒ PcdComMF522 ⇒ SetBitMask ⇒ WriteRawRC
  [Calls]
  - >> WriteRawRC
  - >> SetBitMask
  - >> PcdComMF522
  - >> ClearBitMask
  [Called By]
  - >> main
  - >> WaitCardOff

  PcdReset (Thumb, 178 bytes, Stack size 16 bytes, rc522.o(i.PcdReset))
  [Stack]

  - Max Depth = 56
  - Call Chain = PcdReset ⇒ WriteRawRC
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> delay_10ms
  - >> WriteRawRC
  - >> ReadRawRC
  [Called By]
  - >> InitializeSystem

  PcdSelect (Thumb, 98 bytes, Stack size 40 bytes, rc522.o(i.PcdSelect))
  [Stack]

  - Max Depth = 152
  - Call Chain = PcdSelect ⇒ PcdComMF522 ⇒ SetBitMask ⇒ WriteRawRC
  [Calls]
  - >> PcdComMF522
  - >> ClearBitMask
  - >> CalulateCRC
  [Called By]
  - >> main

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  RCC_APB2PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB2PeriphClockCmd))
  [Called By]

  - >> GPIO_ini

  ReadRawRC (Thumb, 174 bytes, Stack size 40 bytes, rc522.o(i.ReadRawRC))
  [Stack]

  - Max Depth = 40
  - Call Chain = ReadRawRC
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> GPIO_ReadInputDataBit
  [Called By]
  - >> SetBitMask
  - >> PcdReset
  - >> PcdComMF522
  - >> PcdAuthState
  - >> PcdAntennaOn
  - >> ClearBitMask
  - >> CalulateCRC

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  SetBitMask (Thumb, 24 bytes, Stack size 16 bytes, rc522.o(i.SetBitMask))
  [Stack]

  - Max Depth = 56
  - Call Chain = SetBitMask ⇒ WriteRawRC
  [Calls]
  - >> WriteRawRC
  - >> ReadRawRC
  [Called By]
  - >> PcdRequest
  - >> PcdComMF522
  - >> PcdAnticoll
  - >> PcdAntennaOn
  - >> CalulateCRC

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SysTick_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  SystemInit (Thumb, 68 bytes, Stack size 8 bytes, system_stm32f10x.o(i.SystemInit))
  [Stack]

  - Max Depth = 20
  - Call Chain = SystemInit ⇒ SetSysClockTo24
  [Calls]
  - >> SetSysClockTo24
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(.text)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.UsageFault_Handler))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  WaitCardOff (Thumb, 44 bytes, Stack size 8 bytes, rc522.o(i.WaitCardOff))
  [Stack]

  - Max Depth = 160
  - Call Chain = WaitCardOff ⇒ PcdRequest ⇒ PcdComMF522 ⇒ SetBitMask ⇒ WriteRawRC
  [Calls]
  - >> delay_10ms
  - >> PcdRequest
  [Called By]
  - >> main

  WriteRawRC (Thumb, 166 bytes, Stack size 40 bytes, rc522.o(i.WriteRawRC))
  [Stack]

  - Max Depth = 40
  - Call Chain = WriteRawRC
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  [Called By]
  - >> SetBitMask
  - >> PcdReset
  - >> PcdRequest
  - >> PcdComMF522
  - >> PcdAnticoll
  - >> M500PcdConfigISOType
  - >> ClearBitMask
  - >> CalulateCRC

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  delay_10ms (Thumb, 28 bytes, Stack size 8 bytes, rc522.o(i.delay_10ms))
  [Stack]

  - Max Depth = 8
  - Call Chain = delay_10ms
  [Called By]
  - >> InitializeSystem
  - >> WaitCardOff
  - >> PcdReset
  - >> M500PcdConfigISOType

  main (Thumb, 94 bytes, Stack size 32 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 192
  - Call Chain = main ⇒ WaitCardOff ⇒ PcdRequest ⇒ PcdComMF522 ⇒ SetBitMask ⇒ WriteRawRC
  [Calls]
  - >> InitializeSystem
  - >> GPIO_ini
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> WaitCardOff
  - >> PcdSelect
  - >> PcdRequest
  - >> PcdRead
  - >> PcdAuthState
  - >> PcdAnticoll
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  ### Local Symbols

  SetSysClockTo24 (Thumb, 130 bytes, Stack size 12 bytes, system_stm32f10x.o(i.SetSysClockTo24))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClockTo24
  [Called By]
  - >> SystemInit

  ### Undefined Global Symbols