#

##

##

    礦ision Build Log
    Project:
    E:\完成设计的产品\(MCUDEV)-STM32开发板系列\(MCUDEV)STM32_F4VE\STM32F407VET6资料\STM32F407VET6最小系统板--资料\7、出厂测试例程例程\USER\SD.uvproj
    Project File Date:  10/14/2015

    Output:
    Rebuild target 'SD'
    compiling main.c...
    ..\USER\stm32f4xx.h(89): warning:  #47-D: incompatible redefinition of macro "STM32F40_41xxx"
    compiling stm32f4xx_it.c...
    stm32f4xx.h(89): warning:  #47-D: incompatible redefinition of macro "STM32F40_41xxx"
    compiling system_stm32f4xx.c...
    stm32f4xx.h(89): warning:  #47-D: incompatible redefinition of macro "STM32F40_41xxx"
    compiling led.c...
    ..\USER\stm32f4xx.h(89): warning:  #47-D: incompatible redefinition of macro "STM32F40_41xxx"
    compiling lcd.c...
    ..\USER\stm32f4xx.h(89): warning:  #47-D: incompatible redefinition of macro "STM32F40_41xxx"
    compiling key.c...
    ..\USER\stm32f4xx.h(89): warning:  #47-D: incompatible redefinition of macro "STM32F40_41xxx"
    compiling sdio_sdcard.c...
    ..\USER\stm32f4xx.h(89): warning:  #47-D: incompatible redefinition of macro "STM32F40_41xxx"
    compiling w25qxx.c...
    ..\USER\stm32f4xx.h(89): warning:  #47-D: incompatible redefinition of macro "STM32F40_41xxx"
    compiling spi.c...
    ..\USER\stm32f4xx.h(89): warning:  #47-D: incompatible redefinition of macro "STM32F40_41xxx"
    compiling delay.c...
    ..\USER\stm32f4xx.h(89): warning:  #47-D: incompatible redefinition of macro "STM32F40_41xxx"
    compiling sys.c...
    ..\USER\stm32f4xx.h(89): warning:  #47-D: incompatible redefinition of macro "STM32F40_41xxx"
    compiling usart.c...
    ..\USER\stm32f4xx.h(89): warning:  #47-D: incompatible redefinition of macro "STM32F40_41xxx"
    assembling startup_stm32f40_41xxx.s...
    compiling misc.c...
    ..\USER\stm32f4xx.h(89): warning:  #47-D: incompatible redefinition of macro "STM32F40_41xxx"
    compiling stm32f4xx_fsmc.c...
    ..\USER\stm32f4xx.h(89): warning:  #47-D: incompatible redefinition of macro "STM32F40_41xxx"
    compiling stm32f4xx_gpio.c...
    ..\USER\stm32f4xx.h(89): warning:  #47-D: incompatible redefinition of macro "STM32F40_41xxx"
    compiling stm32f4xx_rcc.c...
    ..\USER\stm32f4xx.h(89): warning:  #47-D: incompatible redefinition of macro "STM32F40_41xxx"
    compiling stm32f4xx_sdio.c...
    ..\USER\stm32f4xx.h(89): warning:  #47-D: incompatible redefinition of macro "STM32F40_41xxx"
    compiling stm32f4xx_syscfg.c...
    ..\USER\stm32f4xx.h(89): warning:  #47-D: incompatible redefinition of macro "STM32F40_41xxx"
    compiling stm32f4xx_usart.c...
    ..\USER\stm32f4xx.h(89): warning:  #47-D: incompatible redefinition of macro "STM32F40_41xxx"
    compiling stm32f4xx_dma.c...
    ..\USER\stm32f4xx.h(89): warning:  #47-D: incompatible redefinition of macro "STM32F40_41xxx"
    compiling stm32f4xx_spi.c...
    ..\USER\stm32f4xx.h(89): warning:  #47-D: incompatible redefinition of macro "STM32F40_41xxx"
    compiling malloc.c...
    ..\USER\stm32f4xx.h(89): warning:  #47-D: incompatible redefinition of macro "STM32F40_41xxx"
    linking...
    Program Size: Code=39314 RO-data=6610 RW-data=116 ZI-data=1225228
    FromELF: creating hex file...
    "..\OBJ\SD.axf" - 0 Errors, 22 Warning(s).
    Load "..\\OBJ\\SD.axf"
    Full Chip Erase Done.
    Programming Done.
    Verify OK.
    Load "..\\OBJ\\SD.axf"
    Load "..\\OBJ\\SD.axf"
    Full Chip Erase Done.
    Programming Done.
    Verify OK.