Static Call Graph - [..\OBJ\SD.axf]

# Static Call Graph for image ..\OBJ\SD.axf

#<CALLGRAPH># ARM Linker, 5.03 [Build 76]: Last Updated: Sat Oct 17 21:52:34 2015

### Maximum Stack Usage = 280 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ LCD_Init ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - BusFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN1_RX0_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN1_TX_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN2_RX0_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN2_RX1_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN2_SCE_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN2_TX_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CRYP_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DCMI_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DebugMon_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - ETH_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - ETH_WKUP_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - FLASH_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - FPU_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - FSMC_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - HASH_RNG_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - HardFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - MemManage_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - NMI_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - OTG_HS_EP1_IN_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - OTG_HS_EP1_OUT_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - OTG_HS_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - OTG_HS_WKUP_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - PVD_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - PendSV_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - RCC_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - Reset_Handler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SDIO_IRQHandler from sdio_sdcard.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SPI1_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SPI2_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SPI3_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SVC_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SysTick_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SystemInit from system_stm32f4xx.o(.text) referenced from startup_stm32f40_41xxx.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM2_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM3_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM4_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM5_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM7_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM8_BRK_TIM12_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM8_TRG_COM_TIM14_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM8_UP_TIM13_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - UART4_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - UART5_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - USART1_IRQHandler from usart.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - USART2_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - USART3_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - USART6_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - UsageFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - WWDG_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32f40_41xxx.o(.text)
  - _printf_input_char from _printf_char_common.o(.text) referenced from _printf_char_common.o(.text)
  - fputc from usart.o(.text) referenced from _printf_char_file.o(.text)
  - my_mem_init from malloc.o(.text) referenced from malloc.o(.data)
  - my_mem_perused from malloc.o(.text) referenced from malloc.o(.data)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __rt_entry
  - >> __scatterload

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  _printf_d (Thumb, 0 bytes, Stack size unknown bytes, _printf_d.o(.ARM.Collect$$_printf_percent$$00000009))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = _printf_d ⇒ _printf_int_dec ⇒ _printf_int_common
  [Calls]
  - >> _printf_int_dec

  _printf_percent (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent.o(.ARM.Collect$$_printf_percent$$00000000))
  [Called By]

  - >> __printf

  _printf_x (Thumb, 0 bytes, Stack size unknown bytes, _printf_x.o(.ARM.Collect$$_printf_percent$$0000000C))
  [Stack]

  - Max Depth = 48 + Unknown Stack Size
  - Call Chain = _printf_x ⇒ _printf_int_hex ⇒ _printf_int_common
  [Calls]
  - >> _printf_int_hex

  _printf_percent_end (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent_end.o(.ARM.Collect$$_printf_percent$$00000017))

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000001))
  [Calls]

  - >> _fp_init

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002A))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000008))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000F))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000031))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000006))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000009))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000003))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000B))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __main
  - >> __scatterload_rt2

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 280 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ LCD_Init ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  WFI_SET (Thumb, 2 bytes, Stack size 0 bytes, sys.o(.emb_text), UNUSED)

  INTX_DISABLE (Thumb, 4 bytes, Stack size 0 bytes, sys.o(.emb_text))
  [Called By]

  - >> SD_WriteMultiBlocks
  - >> SD_WriteBlock
  - >> SD_ReadMultiBlocks
  - >> SD_ReadBlock

  INTX_ENABLE (Thumb, 4 bytes, Stack size 0 bytes, sys.o(.emb_text))
  [Called By]

  - >> SD_WriteMultiBlocks
  - >> SD_WriteBlock
  - >> SD_ReadMultiBlocks
  - >> SD_ReadBlock

  MSR_MSP (Thumb, 6 bytes, Stack size 0 bytes, sys.o(.emb_text), UNUSED)

  show_sdcard_info (Thumb, 112 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 136 + Unknown Stack Size
  - Call Chain = show_sdcard_info ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2printf
  [Called By]
  - >> main

  main (Thumb, 622 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 280 + Unknown Stack Size
  - Call Chain = main ⇒ LCD_Init ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> uart_init
  - >> mymalloc
  - >> myfree
  - >> my_mem_init
  - >> delay_ms
  - >> delay_init
  - >> W25QXX_ReadID
  - >> W25QXX_Init
  - >> SD_ReadDisk
  - >> SD_Init
  - >> NVIC_PriorityGroupConfig
  - >> LED_Init
  - >> LCD_ShowString
  - >> LCD_ShowNum
  - >> LCD_Init
  - >> KEY_Scan
  - >> KEY_Init
  - >> show_sdcard_info
  - >> __2printf
  [Called By]
  - >> __rt_entry_main

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  SystemInit (Thumb, 88 bytes, Stack size 8 bytes, system_stm32f4xx.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = SystemInit ⇒ SetSysClock
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_stm32f40_41xxx.o(.text)

  SystemCoreClockUpdate (Thumb, 174 bytes, Stack size 16 bytes, system_stm32f4xx.o(.text), UNUSED)

  LED_Init (Thumb, 56 bytes, Stack size 16 bytes, led.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = LED_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  [Called By]
  - >> main

  LCD_WR_REG (Thumb, 18 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_WR_REG
  [Called By]
  - >> LCD_Set_Window
  - >> LCD_Fast_DrawPoint
  - >> LCD_Scan_Dir
  - >> LCD_DisplayOff
  - >> LCD_DisplayOn
  - >> LCD_ReadPoint
  - >> LCD_SetCursor
  - >> LCD_ReadReg
  - >> LCD_Init

  LCD_WR_DATA (Thumb, 20 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_WR_DATA
  [Called By]
  - >> LCD_Set_Window
  - >> LCD_Fast_DrawPoint
  - >> LCD_Scan_Dir
  - >> LCD_SetCursor
  - >> LCD_Init

  LCD_RD_DATA (Thumb, 16 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_RD_DATA
  [Called By]
  - >> LCD_ReadPoint
  - >> LCD_ReadReg
  - >> LCD_Init

  LCD_WriteReg (Thumb, 20 bytes, Stack size 12 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = LCD_WriteReg
  [Called By]
  - >> LCD_Set_Window
  - >> LCD_Fast_DrawPoint
  - >> LCD_Scan_Dir
  - >> LCD_DisplayOff
  - >> LCD_DisplayOn
  - >> LCD_SetCursor
  - >> LCD_Init

  LCD_ReadReg (Thumb, 22 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_ReadReg ⇒ LCD_RD_DATA
  [Calls]
  - >> delay_us
  - >> LCD_RD_DATA
  - >> LCD_WR_REG
  [Called By]
  - >> LCD_Init

  LCD_WriteRAM_Prepare (Thumb, 10 bytes, Stack size 0 bytes, lcd.o(.text))
  [Called By]

  - >> LCD_Color_Fill
  - >> LCD_Fill
  - >> LCD_Clear
  - >> LCD_DrawPoint

  LCD_WriteRAM (Thumb, 8 bytes, Stack size 0 bytes, lcd.o(.text), UNUSED)

  LCD_BGR2RGB (Thumb, 26 bytes, Stack size 12 bytes, lcd.o(.text), UNUSED)
  [Called By]

  - >> LCD_ReadPoint

  opt_delay (Thumb, 14 bytes, Stack size 0 bytes, lcd.o(.text), UNUSED)
  [Called By]

  - >> LCD_ReadPoint

  LCD_SetCursor (Thumb, 262 bytes, Stack size 12 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = LCD_SetCursor ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_WriteReg
  - >> LCD_WR_DATA
  - >> LCD_WR_REG
  [Called By]
  - >> LCD_Color_Fill
  - >> LCD_Fill
  - >> LCD_Clear
  - >> LCD_Set_Window
  - >> LCD_DrawPoint
  - >> LCD_ReadPoint

  LCD_ReadPoint (Thumb, 358 bytes, Stack size 24 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_SetCursor
  - >> opt_delay
  - >> LCD_BGR2RGB
  - >> LCD_RD_DATA
  - >> LCD_WR_REG

  LCD_DisplayOn (Thumb, 80 bytes, Stack size 4 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_WriteReg
  - >> LCD_WR_REG

  LCD_DisplayOff (Thumb, 78 bytes, Stack size 4 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_WriteReg
  - >> LCD_WR_REG

  LCD_Scan_Dir (Thumb, 736 bytes, Stack size 28 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = LCD_Scan_Dir ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_WriteReg
  - >> LCD_WR_DATA
  - >> LCD_WR_REG
  [Called By]
  - >> LCD_Display_Dir

  LCD_DrawPoint (Thumb, 28 bytes, Stack size 12 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_SetCursor
  - >> LCD_WriteRAM_Prepare
  [Called By]
  - >> LCD_Draw_Circle
  - >> LCD_DrawLine

  LCD_Fast_DrawPoint (Thumb, 278 bytes, Stack size 16 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = LCD_Fast_DrawPoint ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_WriteReg
  - >> LCD_WR_DATA
  - >> LCD_WR_REG
  [Called By]
  - >> LCD_ShowChar

  LCD_Display_Dir (Thumb, 378 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = LCD_Display_Dir ⇒ LCD_Scan_Dir ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_Scan_Dir
  [Called By]
  - >> LCD_Init

  LCD_Set_Window (Thumb, 382 bytes, Stack size 52 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_SetCursor
  - >> LCD_WriteReg
  - >> LCD_WR_DATA
  - >> LCD_WR_REG

  LCD_Clear (Thumb, 100 bytes, Stack size 16 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = LCD_Clear ⇒ LCD_SetCursor ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_SetCursor
  - >> LCD_WriteRAM_Prepare
  [Called By]
  - >> LCD_Init

  LCD_Init (Thumb, 14124 bytes, Stack size 136 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 264 + Unknown Stack Size
  - Call Chain = LCD_Init ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> delay_us
  - >> RCC_AHB3PeriphClockCmd
  - >> GPIO_PinAFConfig
  - >> FSMC_NORSRAMInit
  - >> FSMC_NORSRAMCmd
  - >> LCD_Clear
  - >> LCD_Display_Dir
  - >> LCD_ReadReg
  - >> LCD_WriteReg
  - >> LCD_RD_DATA
  - >> LCD_WR_DATA
  - >> LCD_WR_REG
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  - >> delay_ms
  - >> __2printf
  [Called By]
  - >> main

  LCD_Fill (Thumb, 178 bytes, Stack size 44 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_Fill
  - >> LCD_SetCursor
  - >> LCD_WriteRAM_Prepare
  [Called By]
  - >> LCD_Fill

  LCD_Color_Fill (Thumb, 92 bytes, Stack size 40 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_SetCursor
  - >> LCD_WriteRAM_Prepare

  LCD_DrawLine (Thumb, 176 bytes, Stack size 68 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_DrawPoint
  [Called By]
  - >> LCD_DrawRectangle

  LCD_DrawRectangle (Thumb, 60 bytes, Stack size 20 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_DrawLine

  LCD_Draw_Circle (Thumb, 166 bytes, Stack size 28 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_DrawPoint

  LCD_ShowChar (Thumb, 268 bytes, Stack size 40 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = LCD_ShowChar ⇒ LCD_Fast_DrawPoint ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_Fast_DrawPoint
  [Called By]
  - >> LCD_ShowxNum
  - >> LCD_ShowString
  - >> LCD_ShowNum

  LCD_Pow (Thumb, 22 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_Pow
  [Called By]
  - >> LCD_ShowxNum
  - >> LCD_ShowNum

  LCD_ShowNum (Thumb, 148 bytes, Stack size 56 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 124
  - Call Chain = LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_Fast_DrawPoint ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_Pow
  - >> LCD_ShowChar
  [Called By]
  - >> main

  LCD_ShowxNum (Thumb, 190 bytes, Stack size 60 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_Pow
  - >> LCD_ShowChar

  LCD_ShowString (Thumb, 102 bytes, Stack size 36 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = LCD_ShowString ⇒ LCD_ShowChar ⇒ LCD_Fast_DrawPoint ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_ShowChar
  [Called By]
  - >> main

  KEY_Init (Thumb, 60 bytes, Stack size 16 bytes, key.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = KEY_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> main

  KEY_Scan (Thumb, 150 bytes, Stack size 8 bytes, key.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = KEY_Scan ⇒ delay_ms
  [Calls]
  - >> GPIO_ReadInputDataBit
  - >> delay_ms
  [Called By]
  - >> main

  SDIO_Register_Deinit (Thumb, 48 bytes, Stack size 0 bytes, sdio_sdcard.o(.text))
  [Called By]

  - >> SD_Init

  SD_SetDeviceMode (Thumb, 20 bytes, Stack size 0 bytes, sdio_sdcard.o(.text))
  [Called By]

  - >> SD_Init

  SDIO_Clock_Set (Thumb, 18 bytes, Stack size 0 bytes, sdio_sdcard.o(.text))
  [Called By]

  - >> SD_Init

  CmdResp1Error (Thumb, 96 bytes, Stack size 16 bytes, sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CmdResp1Error
  [Calls]
  - >> SDIO_GetFlagStatus
  - >> SDIO_ClearFlag
  [Called By]
  - >> SD_SendStatus
  - >> SD_ProcessIRQSrc
  - >> SD_WriteMultiBlocks
  - >> SD_WriteBlock
  - >> SD_ReadMultiBlocks
  - >> SD_ReadBlock
  - >> SD_PowerON
  - >> SD_SelectDeselect
  - >> SDEnWideBus
  - >> FindSCR

  FindSCR (Thumb, 388 bytes, Stack size 32 bytes, sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = FindSCR ⇒ CmdResp1Error
  [Calls]
  - >> SDIO_SendCommand
  - >> SDIO_GetFlagStatus
  - >> SDIO_DataConfig
  - >> SDIO_ClearFlag
  - >> CmdResp1Error
  [Called By]
  - >> SDEnWideBus

  SDEnWideBus (Thumb, 160 bytes, Stack size 24 bytes, sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = SDEnWideBus ⇒ FindSCR ⇒ CmdResp1Error
  [Calls]
  - >> SDIO_SendCommand
  - >> FindSCR
  - >> CmdResp1Error
  [Called By]
  - >> SD_EnableWideBusOperation

  SD_EnableWideBusOperation (Thumb, 98 bytes, Stack size 16 bytes, sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = SD_EnableWideBusOperation ⇒ SDEnWideBus ⇒ FindSCR ⇒ CmdResp1Error
  [Calls]
  - >> SDEnWideBus
  [Called By]
  - >> SD_Init

  SD_SelectDeselect (Thumb, 42 bytes, Stack size 8 bytes, sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = SD_SelectDeselect ⇒ CmdResp1Error
  [Calls]
  - >> SDIO_SendCommand
  - >> CmdResp1Error
  [Called By]
  - >> SD_Init

  SD_GetCardInfo (Thumb, 848 bytes, Stack size 20 bytes, sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = SD_GetCardInfo
  [Called By]
  - >> SD_Init

  CmdResp2Error (Thumb, 80 bytes, Stack size 16 bytes, sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CmdResp2Error
  [Calls]
  - >> SDIO_GetFlagStatus
  - >> SDIO_ClearFlag
  [Called By]
  - >> SD_InitializeCards

  CmdResp6Error (Thumb, 144 bytes, Stack size 24 bytes, sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = CmdResp6Error
  [Calls]
  - >> SDIO_GetFlagStatus
  - >> SDIO_ClearFlag
  [Called By]
  - >> SD_InitializeCards

  SD_InitializeCards (Thumb, 354 bytes, Stack size 16 bytes, sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = SD_InitializeCards ⇒ CmdResp6Error
  [Calls]
  - >> SDIO_SendCommand
  - >> SDIO_GetPowerState
  - >> CmdResp6Error
  - >> CmdResp2Error
  [Called By]
  - >> SD_Init

  CmdResp3Error (Thumb, 52 bytes, Stack size 8 bytes, sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = CmdResp3Error
  [Calls]
  - >> SDIO_GetFlagStatus
  - >> SDIO_ClearFlag
  [Called By]
  - >> SD_PowerON

  CmdResp7Error (Thumb, 72 bytes, Stack size 16 bytes, sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CmdResp7Error
  [Calls]
  - >> SDIO_ClearFlag
  [Called By]
  - >> SD_PowerON

  CmdError (Thumb, 48 bytes, Stack size 16 bytes, sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CmdError
  [Calls]
  - >> SDIO_GetFlagStatus
  - >> SDIO_ClearFlag
  [Called By]
  - >> SD_PowerON

  SD_PowerON (Thumb, 460 bytes, Stack size 32 bytes, sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = SD_PowerON ⇒ CmdError
  [Calls]
  - >> SDIO_SetPowerState
  - >> SDIO_SendCommand
  - >> SDIO_Init
  - >> CmdError
  - >> CmdResp7Error
  - >> CmdResp3Error
  - >> CmdResp1Error
  [Called By]
  - >> SD_Init

  SD_Init (Thumb, 304 bytes, Stack size 24 bytes, sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = SD_Init ⇒ SD_EnableWideBusOperation ⇒ SDEnWideBus ⇒ FindSCR ⇒ CmdResp1Error
  [Calls]
  - >> RCC_APB2PeriphResetCmd
  - >> RCC_APB2PeriphClockCmd
  - >> NVIC_Init
  - >> SD_PowerON
  - >> SD_InitializeCards
  - >> SD_GetCardInfo
  - >> SD_SelectDeselect
  - >> SD_EnableWideBusOperation
  - >> SDIO_Clock_Set
  - >> SD_SetDeviceMode
  - >> SDIO_Register_Deinit
  - >> GPIO_PinAFConfig
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> SD_WriteMultiBlocks
  - >> SD_WriteBlock
  - >> main

  SD_PowerOFF (Thumb, 12 bytes, Stack size 8 bytes, sdio_sdcard.o(.text), UNUSED)
  [Calls]

  - >> SDIO_SetPowerState

  SD_DMA_Config (Thumb, 118 bytes, Stack size 80 bytes, sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = SD_DMA_Config ⇒ DMA_Init
  [Calls]
  - >> DMA_Init
  - >> DMA_GetCmdStatus
  - >> DMA_FlowControllerConfig
  - >> DMA_DeInit
  - >> DMA_Cmd
  [Called By]
  - >> SD_WriteMultiBlocks
  - >> SD_WriteBlock
  - >> SD_ReadMultiBlocks
  - >> SD_ReadBlock

  convert_from_bytes_to_power_of_two (Thumb, 18 bytes, Stack size 0 bytes, sdio_sdcard.o(.text))
  [Called By]

  - >> SD_WriteMultiBlocks
  - >> SD_WriteBlock
  - >> SD_ReadMultiBlocks
  - >> SD_ReadBlock

  SD_ReadBlock (Thumb, 576 bytes, Stack size 40 bytes, sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = SD_ReadBlock ⇒ SD_DMA_Config ⇒ DMA_Init
  [Calls]
  - >> SDIO_SendCommand
  - >> SDIO_GetFlagStatus
  - >> SDIO_DataConfig
  - >> SDIO_ClearFlag
  - >> INTX_ENABLE
  - >> INTX_DISABLE
  - >> convert_from_bytes_to_power_of_two
  - >> SD_DMA_Config
  - >> CmdResp1Error
  [Called By]
  - >> SD_ReadDisk

  SD_ReadMultiBlocks (Thumb, 764 bytes, Stack size 56 bytes, sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 144
  - Call Chain = SD_ReadMultiBlocks ⇒ SD_DMA_Config ⇒ DMA_Init
  [Calls]
  - >> SDIO_SendCommand
  - >> SDIO_GetFlagStatus
  - >> SDIO_DataConfig
  - >> SDIO_ClearFlag
  - >> INTX_ENABLE
  - >> INTX_DISABLE
  - >> convert_from_bytes_to_power_of_two
  - >> SD_DMA_Config
  - >> CmdResp1Error
  [Called By]
  - >> SD_ReadDisk

  IsCardProgramming (Thumb, 148 bytes, Stack size 16 bytes, sdio_sdcard.o(.text), UNUSED)
  [Calls]

  - >> SDIO_SendCommand
  - >> SDIO_GetFlagStatus
  - >> SDIO_ClearFlag
  [Called By]
  - >> SD_WriteMultiBlocks
  - >> SD_WriteBlock

  SD_WriteBlock (Thumb, 912 bytes, Stack size 80 bytes, sdio_sdcard.o(.text), UNUSED)
  [Calls]

  - >> SDIO_SendCommand
  - >> SDIO_GetFlagStatus
  - >> SDIO_DataConfig
  - >> SDIO_ClearFlag
  - >> INTX_ENABLE
  - >> INTX_DISABLE
  - >> IsCardProgramming
  - >> convert_from_bytes_to_power_of_two
  - >> SD_DMA_Config
  - >> CmdResp1Error
  - >> SD_Init
  [Called By]
  - >> SD_WriteDisk

  SD_WriteMultiBlocks (Thumb, 974 bytes, Stack size 72 bytes, sdio_sdcard.o(.text), UNUSED)
  [Calls]

  - >> SDIO_SendCommand
  - >> SDIO_GetFlagStatus
  - >> SDIO_DataConfig
  - >> SDIO_ClearFlag
  - >> INTX_ENABLE
  - >> INTX_DISABLE
  - >> IsCardProgramming
  - >> convert_from_bytes_to_power_of_two
  - >> SD_DMA_Config
  - >> CmdResp1Error
  - >> SD_Init
  [Called By]
  - >> SD_WriteDisk

  SD_ProcessIRQSrc (Thumb, 322 bytes, Stack size 8 bytes, sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = SD_ProcessIRQSrc ⇒ CmdResp1Error
  [Calls]
  - >> SDIO_SendCommand
  - >> SDIO_GetFlagStatus
  - >> SDIO_ClearFlag
  - >> CmdResp1Error
  [Called By]
  - >> SDIO_IRQHandler

  SDIO_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = SDIO_IRQHandler ⇒ SD_ProcessIRQSrc ⇒ CmdResp1Error
  [Calls]
  - >> SD_ProcessIRQSrc
  [Address Reference Count : 1]
  - startup_stm32f40_41xxx.o(RESET)

  SD_SendStatus (Thumb, 74 bytes, Stack size 16 bytes, sdio_sdcard.o(.text), UNUSED)
  [Calls]

  - >> SDIO_SendCommand
  - >> CmdResp1Error
  [Called By]
  - >> SD_GetState

  SD_GetState (Thumb, 26 bytes, Stack size 8 bytes, sdio_sdcard.o(.text), UNUSED)
  [Calls]

  - >> SD_SendStatus

  SD_ReadDisk (Thumb, 192 bytes, Stack size 48 bytes, sdio_sdcard.o(.text))
  [Stack]

  - Max Depth = 192
  - Call Chain = SD_ReadDisk ⇒ SD_ReadMultiBlocks ⇒ SD_DMA_Config ⇒ DMA_Init
  [Calls]
  - >> SD_ReadMultiBlocks
  - >> SD_ReadBlock
  - >> __aeabi_memcpy
  [Called By]
  - >> main

  SD_WriteDisk (Thumb, 152 bytes, Stack size 48 bytes, sdio_sdcard.o(.text), UNUSED)
  [Calls]

  - >> SD_WriteMultiBlocks
  - >> SD_WriteBlock
  - >> __aeabi_memcpy

  W25QXX_ReadID (Thumb, 66 bytes, Stack size 8 bytes, w25qxx.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = W25QXX_ReadID ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SPI1_ReadWriteByte
  [Called By]
  - >> W25QXX_Init
  - >> main

  W25QXX_Init (Thumb, 70 bytes, Stack size 16 bytes, w25qxx.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = W25QXX_Init ⇒ SPI1_Init ⇒ GPIO_PinAFConfig
  [Calls]
  - >> SPI1_SetSpeed
  - >> SPI1_Init
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  - >> W25QXX_ReadID
  [Called By]
  - >> main

  W25QXX_ReadSR (Thumb, 38 bytes, Stack size 8 bytes, w25qxx.o(.text), UNUSED)
  [Calls]

  - >> SPI1_ReadWriteByte
  [Called By]
  - >> W25QXX_Wait_Busy

  W25QXX_Write_SR (Thumb, 34 bytes, Stack size 8 bytes, w25qxx.o(.text), UNUSED)
  [Calls]

  - >> SPI1_ReadWriteByte

  W25QXX_Write_Enable (Thumb, 26 bytes, Stack size 8 bytes, w25qxx.o(.text), UNUSED)
  [Calls]

  - >> SPI1_ReadWriteByte
  [Called By]
  - >> W25QXX_Erase_Chip
  - >> W25QXX_Erase_Sector
  - >> W25QXX_Write_Page

  W25QXX_Write_Disable (Thumb, 26 bytes, Stack size 8 bytes, w25qxx.o(.text), UNUSED)
  [Calls]

  - >> SPI1_ReadWriteByte

  W25QXX_Read (Thumb, 76 bytes, Stack size 24 bytes, w25qxx.o(.text), UNUSED)
  [Calls]

  - >> SPI1_ReadWriteByte
  [Called By]
  - >> W25QXX_Write

  W25QXX_Wait_Busy (Thumb, 16 bytes, Stack size 8 bytes, w25qxx.o(.text), UNUSED)
  [Calls]

  - >> W25QXX_ReadSR
  [Called By]
  - >> W25QXX_Erase_Chip
  - >> W25QXX_Erase_Sector
  - >> W25QXX_Write_Page

  W25QXX_Write_Page (Thumb, 82 bytes, Stack size 24 bytes, w25qxx.o(.text), UNUSED)
  [Calls]

  - >> SPI1_ReadWriteByte
  - >> W25QXX_Wait_Busy
  - >> W25QXX_Write_Enable
  [Called By]
  - >> W25QXX_Write_NoCheck

  W25QXX_Write_NoCheck (Thumb, 70 bytes, Stack size 24 bytes, w25qxx.o(.text), UNUSED)
  [Calls]

  - >> W25QXX_Write_Page
  [Called By]
  - >> W25QXX_Write

  W25QXX_Erase_Sector (Thumb, 72 bytes, Stack size 8 bytes, w25qxx.o(.text), UNUSED)
  [Calls]

  - >> SPI1_ReadWriteByte
  - >> W25QXX_Wait_Busy
  - >> W25QXX_Write_Enable
  - >> __2printf
  [Called By]
  - >> W25QXX_Write

  W25QXX_Write (Thumb, 180 bytes, Stack size 40 bytes, w25qxx.o(.text), UNUSED)
  [Calls]

  - >> W25QXX_Erase_Sector
  - >> W25QXX_Write_NoCheck
  - >> W25QXX_Read

  W25QXX_Erase_Chip (Thumb, 38 bytes, Stack size 8 bytes, w25qxx.o(.text), UNUSED)
  [Calls]

  - >> SPI1_ReadWriteByte
  - >> W25QXX_Wait_Busy
  - >> W25QXX_Write_Enable

  W25QXX_PowerDown (Thumb, 32 bytes, Stack size 8 bytes, w25qxx.o(.text), UNUSED)
  [Calls]

  - >> SPI1_ReadWriteByte
  - >> delay_us

  W25QXX_WAKEUP (Thumb, 32 bytes, Stack size 8 bytes, w25qxx.o(.text), UNUSED)
  [Calls]

  - >> SPI1_ReadWriteByte
  - >> delay_us

  SPI1_ReadWriteByte (Thumb, 50 bytes, Stack size 8 bytes, spi.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SPI1_ReadWriteByte
  [Calls]
  - >> SPI_I2S_SendData
  - >> SPI_I2S_ReceiveData
  - >> SPI_I2S_GetFlagStatus
  [Called By]
  - >> SPI1_Init
  - >> W25QXX_WAKEUP
  - >> W25QXX_PowerDown
  - >> W25QXX_Erase_Chip
  - >> W25QXX_Erase_Sector
  - >> W25QXX_Write_Page
  - >> W25QXX_Read
  - >> W25QXX_Write_Disable
  - >> W25QXX_Write_Enable
  - >> W25QXX_Write_SR
  - >> W25QXX_ReadSR
  - >> W25QXX_ReadID

  SPI1_Init (Thumb, 186 bytes, Stack size 32 bytes, spi.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = SPI1_Init ⇒ GPIO_PinAFConfig
  [Calls]
  - >> SPI_Init
  - >> SPI_Cmd
  - >> SPI1_ReadWriteByte
  - >> RCC_APB2PeriphResetCmd
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_PinAFConfig
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> W25QXX_Init

  SPI1_SetSpeed (Thumb, 36 bytes, Stack size 8 bytes, spi.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SPI1_SetSpeed
  [Calls]
  - >> SPI_Cmd
  [Called By]
  - >> W25QXX_Init

  delay_init (Thumb, 52 bytes, Stack size 8 bytes, delay.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = delay_init
  [Calls]
  - >> SysTick_CLKSourceConfig
  [Called By]
  - >> main

  delay_us (Thumb, 70 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> W25QXX_WAKEUP
  - >> W25QXX_PowerDown
  - >> LCD_ReadReg
  - >> LCD_Init

  delay_xms (Thumb, 70 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> delay_ms

  delay_ms (Thumb, 56 bytes, Stack size 16 bytes, delay.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = delay_ms
  [Calls]
  - >> delay_xms
  [Called By]
  - >> LCD_Init
  - >> KEY_Scan
  - >> main

  _sys_exit (Thumb, 6 bytes, Stack size 0 bytes, usart.o(.text))
  [Called By]

  - >> __rt_exit_exit

  fputc (Thumb, 20 bytes, Stack size 0 bytes, usart.o(.text))
  [Address Reference Count : 1]

  - _printf_char_file.o(.text)

  uart_init (Thumb, 172 bytes, Stack size 40 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 108
  - Call Chain = uart_init ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> USART_Init
  - >> USART_ITConfig
  - >> USART_Cmd
  - >> USART_ClearFlag
  - >> RCC_APB2PeriphClockCmd
  - >> NVIC_Init
  - >> GPIO_PinAFConfig
  - >> RCC_AHB1PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> main

  USART1_IRQHandler (Thumb, 122 bytes, Stack size 8 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = USART1_IRQHandler ⇒ USART_GetITStatus
  [Calls]
  - >> USART_ReceiveData
  - >> USART_GetITStatus
  [Address Reference Count : 1]
  - startup_stm32f40_41xxx.o(RESET)

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f40_41xxx.o(RESET)

  CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN2_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN2_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN2_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN2_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CRYP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DCMI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  HASH_RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  OTG_HS_EP1_IN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  OTG_HS_EP1_OUT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  OTG_HS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  OTG_HS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM8_BRK_TIM12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM8_TRG_COM_TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM8_UP_TIM13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f40_41xxx.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> main

  NVIC_Init (Thumb, 108 bytes, Stack size 16 bytes, misc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = NVIC_Init
  [Called By]
  - >> uart_init
  - >> SD_Init

  NVIC_SetVectorTable (Thumb, 14 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  NVIC_SystemLPConfig (Thumb, 34 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  SysTick_CLKSourceConfig (Thumb, 40 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> delay_init

  FSMC_NORSRAMDeInit (Thumb, 56 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_NORSRAMInit (Thumb, 224 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text))
  [Called By]

  - >> LCD_Init

  FSMC_NORSRAMStructInit (Thumb, 48 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_NORSRAMCmd (Thumb, 46 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text))
  [Called By]

  - >> LCD_Init

  FSMC_NANDDeInit (Thumb, 62 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_NANDInit (Thumb, 130 bytes, Stack size 12 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_NANDStructInit (Thumb, 54 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_NANDCmd (Thumb, 86 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_NANDECCCmd (Thumb, 86 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_GetECC (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_PCCARDDeInit (Thumb, 40 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_PCCARDInit (Thumb, 124 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_PCCARDStructInit (Thumb, 60 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_PCCARDCmd (Thumb, 40 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_ITConfig (Thumb, 128 bytes, Stack size 8 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_GetFlagStatus (Thumb, 48 bytes, Stack size 8 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_ClearFlag (Thumb, 114 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_GetITStatus (Thumb, 60 bytes, Stack size 16 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  FSMC_ClearITPendingBit (Thumb, 64 bytes, Stack size 0 bytes, stm32f4xx_fsmc.o(.text), UNUSED)

  GPIO_DeInit (Thumb, 268 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_AHB1PeriphResetCmd

  GPIO_Init (Thumb, 144 bytes, Stack size 20 bytes, stm32f4xx_gpio.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> SPI1_Init
  - >> uart_init
  - >> W25QXX_Init
  - >> SD_Init
  - >> LED_Init
  - >> LCD_Init
  - >> KEY_Init

  GPIO_StructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_PinLockConfig (Thumb, 34 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text))
  [Called By]

  - >> KEY_Scan

  GPIO_ReadInputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text))
  [Called By]

  - >> LED_Init

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ToggleBits (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_PinAFConfig (Thumb, 70 bytes, Stack size 20 bytes, stm32f4xx_gpio.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_PinAFConfig
  [Called By]
  - >> SPI1_Init
  - >> uart_init
  - >> SD_Init
  - >> LCD_Init

  RCC_DeInit (Thumb, 82 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HSEConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetFlagStatus (Thumb, 60 bytes, Stack size 8 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_WaitForHSEStartUp

  RCC_WaitForHSEStartUp (Thumb, 56 bytes, Stack size 16 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus

  RCC_AdjustHSICalibrationValue (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LSEConfig (Thumb, 46 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLConfig (Thumb, 32 bytes, Stack size 16 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLI2SConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLI2SCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLSAIConfig (Thumb, 20 bytes, Stack size 8 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLSAICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_MCO1Config (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_MCO2Config (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SYSCLKConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetSYSCLKSource (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HCLKConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PCLK1Config (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PCLK2Config (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 222 bytes, Stack size 20 bytes, stm32f4xx_rcc.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> USART_Init

  RCC_RTCCLKConfig (Thumb, 54 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_RTCCLKCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_BackupResetCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_I2SCLKConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SAIPLLI2SClkDivConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SAIPLLSAIClkDivConfig (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SAIBlockACLKConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SAIBlockBCLKConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LTDCCLKDivConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_TIMCLKPresConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB1PeriphClockCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> SPI1_Init
  - >> uart_init
  - >> W25QXX_Init
  - >> SD_Init
  - >> LED_Init
  - >> LCD_Init
  - >> KEY_Init

  RCC_AHB2PeriphClockCmd (Thumb, 78 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB3PeriphClockCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> LCD_Init

  RCC_APB1PeriphClockCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB2PeriphClockCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> SPI1_Init
  - >> uart_init
  - >> SD_Init

  RCC_AHB1PeriphResetCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> GPIO_DeInit

  RCC_AHB2PeriphResetCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB3PeriphResetCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphResetCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> SPI_I2S_DeInit
  - >> USART_DeInit

  RCC_APB2PeriphResetCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> SPI1_Init
  - >> SD_Init
  - >> SPI_I2S_DeInit
  - >> USART_DeInit
  - >> SDIO_DeInit

  RCC_AHB1PeriphClockLPModeCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB2PeriphClockLPModeCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB3PeriphClockLPModeCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphClockLPModeCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB2PeriphClockLPModeCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LSEModeConfig (Thumb, 40 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ITConfig (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  SDIO_DeInit (Thumb, 22 bytes, Stack size 8 bytes, stm32f4xx_sdio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  SDIO_Init (Thumb, 42 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text))
  [Called By]

  - >> SD_PowerON

  SDIO_StructInit (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_ClockCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_SetPowerState (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text))
  [Called By]

  - >> SD_PowerOFF
  - >> SD_PowerON

  SDIO_GetPowerState (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text))
  [Called By]

  - >> SD_InitializeCards

  SDIO_SendCommand (Thumb, 42 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text))
  [Called By]

  - >> SD_SendStatus
  - >> SD_ProcessIRQSrc
  - >> SD_WriteMultiBlocks
  - >> SD_WriteBlock
  - >> IsCardProgramming
  - >> SD_ReadMultiBlocks
  - >> SD_ReadBlock
  - >> SD_PowerON
  - >> SD_InitializeCards
  - >> SD_SelectDeselect
  - >> SDEnWideBus
  - >> FindSCR

  SDIO_CmdStructInit (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_GetCommandResponse (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_GetResponse (Thumb, 22 bytes, Stack size 8 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_DataConfig (Thumb, 48 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text))
  [Called By]

  - >> SD_WriteMultiBlocks
  - >> SD_WriteBlock
  - >> SD_ReadMultiBlocks
  - >> SD_ReadBlock
  - >> FindSCR

  SDIO_DataStructInit (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_GetDataCounter (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_ReadData (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_WriteData (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_GetFIFOCount (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_StartSDIOReadWait (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_StopSDIOReadWait (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_SetSDIOReadWaitMode (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_SetSDIOOperation (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_SendSDIOSuspendCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_CommandCompletionCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_CEATAITCmd (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_SendCEATACmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_DMACmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_ITConfig (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_GetFlagStatus (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text))
  [Called By]

  - >> SD_ProcessIRQSrc
  - >> SD_WriteMultiBlocks
  - >> SD_WriteBlock
  - >> IsCardProgramming
  - >> SD_ReadMultiBlocks
  - >> SD_ReadBlock
  - >> CmdError
  - >> CmdResp3Error
  - >> CmdResp6Error
  - >> CmdResp2Error
  - >> FindSCR
  - >> CmdResp1Error

  SDIO_ClearFlag (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text))
  [Called By]

  - >> SD_ProcessIRQSrc
  - >> SD_WriteMultiBlocks
  - >> SD_WriteBlock
  - >> IsCardProgramming
  - >> SD_ReadMultiBlocks
  - >> SD_ReadBlock
  - >> CmdError
  - >> CmdResp7Error
  - >> CmdResp3Error
  - >> CmdResp6Error
  - >> CmdResp2Error
  - >> FindSCR
  - >> CmdResp1Error

  SDIO_GetITStatus (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  SDIO_ClearITPendingBit (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_sdio.o(.text), UNUSED)

  USART_DeInit (Thumb, 206 bytes, Stack size 8 bytes, stm32f4xx_usart.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd
  - >> RCC_APB1PeriphResetCmd

  USART_Init (Thumb, 204 bytes, Stack size 48 bytes, stm32f4xx_usart.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> uart_init

  USART_StructInit (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_ClockInit (Thumb, 32 bytes, Stack size 8 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_ClockStructInit (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text))
  [Called By]

  - >> uart_init

  USART_SetPrescaler (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_OverSampling8Cmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_OneBitMethodCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_ReceiveData (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text))
  [Called By]

  - >> USART1_IRQHandler

  USART_SetAddress (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_ReceiverWakeUpCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_WakeUpConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_LINBreakDetectLengthConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_LINCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_SendBreak (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_HalfDuplexCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_SetGuardTime (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_SmartCardCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_SmartCardNACKCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_IrDAConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_IrDACmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_DMACmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_ITConfig (Thumb, 74 bytes, Stack size 20 bytes, stm32f4xx_usart.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = USART_ITConfig
  [Called By]
  - >> uart_init

  USART_GetFlagStatus (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text), UNUSED)

  USART_ClearFlag (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_usart.o(.text))
  [Called By]

  - >> uart_init

  USART_GetITStatus (Thumb, 118 bytes, Stack size 16 bytes, stm32f4xx_usart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USART_GetITStatus
  [Called By]
  - >> USART1_IRQHandler

  USART_ClearITPendingBit (Thumb, 30 bytes, Stack size 8 bytes, stm32f4xx_usart.o(.text), UNUSED)

  DMA_DeInit (Thumb, 324 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text))
  [Called By]

  - >> SD_DMA_Config

  DMA_Init (Thumb, 82 bytes, Stack size 8 bytes, stm32f4xx_dma.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = DMA_Init
  [Called By]
  - >> SD_DMA_Config

  DMA_StructInit (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_Cmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text))
  [Called By]

  - >> SD_DMA_Config

  DMA_PeriphIncOffsetSizeConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_FlowControllerConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text))
  [Called By]

  - >> SD_DMA_Config

  DMA_SetCurrDataCounter (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_GetCurrDataCounter (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_DoubleBufferModeConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_DoubleBufferModeCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_MemoryTargetConfig (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_GetCurrentMemoryTarget (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_GetCmdStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text))
  [Called By]

  - >> SD_DMA_Config

  DMA_GetFIFOStatus (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_GetFlagStatus (Thumb, 54 bytes, Stack size 12 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_ClearFlag (Thumb, 40 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_ITConfig (Thumb, 58 bytes, Stack size 8 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_GetITStatus (Thumb, 82 bytes, Stack size 16 bytes, stm32f4xx_dma.o(.text), UNUSED)

  DMA_ClearITPendingBit (Thumb, 40 bytes, Stack size 0 bytes, stm32f4xx_dma.o(.text), UNUSED)

  SPI_I2S_DeInit (Thumb, 152 bytes, Stack size 8 bytes, stm32f4xx_spi.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd
  - >> RCC_APB1PeriphResetCmd

  SPI_Init (Thumb, 60 bytes, Stack size 8 bytes, stm32f4xx_spi.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SPI_Init
  [Called By]
  - >> SPI1_Init

  I2S_Init (Thumb, 392 bytes, Stack size 36 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_StructInit (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  I2S_StructInit (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text))
  [Called By]

  - >> SPI1_SetSpeed
  - >> SPI1_Init

  I2S_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_DataSizeConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_BiDirectionalLineConfig (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_NSSInternalSoftwareConfig (Thumb, 30 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_SSOutputCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_TIModeCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  I2S_FullDuplexConfig (Thumb, 80 bytes, Stack size 12 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_ReceiveData (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text))
  [Called By]

  - >> SPI1_ReadWriteByte

  SPI_I2S_SendData (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text))
  [Called By]

  - >> SPI1_ReadWriteByte

  SPI_CalculateCRC (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_TransmitCRC (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_GetCRC (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_GetCRCPolynomial (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_DMACmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_ITConfig (Thumb, 68 bytes, Stack size 12 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_GetFlagStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text))
  [Called By]

  - >> SPI1_ReadWriteByte

  SPI_I2S_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_GetITStatus (Thumb, 52 bytes, Stack size 20 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_ClearITPendingBit (Thumb, 20 bytes, Stack size 8 bytes, stm32f4xx_spi.o(.text), UNUSED)

  mymemcpy (Thumb, 26 bytes, Stack size 16 bytes, malloc.o(.text), UNUSED)
  [Called By]

  - >> myrealloc

  mymemset (Thumb, 20 bytes, Stack size 12 bytes, malloc.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = mymemset
  [Called By]
  - >> my_mem_init

  my_mem_init (Thumb, 54 bytes, Stack size 8 bytes, malloc.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = my_mem_init ⇒ mymemset
  [Calls]
  - >> mymemset
  [Called By]
  - >> main
  [Address Reference Count : 1]
  - malloc.o(.data)

  my_mem_perused (Thumb, 54 bytes, Stack size 8 bytes, malloc.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = my_mem_perused
  [Address Reference Count : 1]
  - malloc.o(.data)

  my_mem_malloc (Thumb, 154 bytes, Stack size 32 bytes, malloc.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = my_mem_malloc
  [Called By]
  - >> mymalloc
  - >> myrealloc

  my_mem_free (Thumb, 94 bytes, Stack size 24 bytes, malloc.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = my_mem_free
  [Called By]
  - >> myfree

  myfree (Thumb, 32 bytes, Stack size 16 bytes, malloc.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = myfree ⇒ my_mem_free
  [Calls]
  - >> my_mem_free
  [Called By]
  - >> main
  - >> myrealloc

  mymalloc (Thumb, 34 bytes, Stack size 16 bytes, malloc.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = mymalloc ⇒ my_mem_malloc
  [Calls]
  - >> my_mem_malloc
  [Called By]
  - >> main

  myrealloc (Thumb, 66 bytes, Stack size 24 bytes, malloc.o(.text), UNUSED)
  [Calls]

  - >> myfree
  - >> my_mem_malloc
  - >> mymemcpy

  __use_no_semihosting (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi_2.o(.text), UNUSED)

  __2printf (Thumb, 20 bytes, Stack size 24 bytes, noretval__2printf.o(.text))
  [Stack]

  - Max Depth = 128 + Unknown Stack Size
  - Call Chain = __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> _printf_char_file
  [Called By]
  - >> W25QXX_Erase_Sector
  - >> LCD_Init
  - >> main
  - >> show_sdcard_info

  __printf (Thumb, 104 bytes, Stack size 24 bytes, __printf.o(.text))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = __printf
  [Calls]
  - >> _printf_percent
  [Called By]
  - >> _printf_char_common

  _printf_int_dec (Thumb, 102 bytes, Stack size 24 bytes, _printf_dec.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = _printf_int_dec ⇒ _printf_int_common
  [Calls]
  - >> _printf_int_common
  [Called By]
  - >> _printf_d

  _printf_int_hex (Thumb, 88 bytes, Stack size 16 bytes, _printf_hex_int.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = _printf_int_hex ⇒ _printf_int_common
  [Calls]
  - >> _printf_int_common
  [Called By]
  - >> _printf_x

  _printf_longlong_hex (Thumb, 0 bytes, Stack size 16 bytes, _printf_hex_int.o(.text), UNUSED)

  __aeabi_memcpy (Thumb, 0 bytes, Stack size 0 bytes, rt_memcpy_v6.o(.text))
  [Called By]

  - >> SD_WriteDisk
  - >> SD_ReadDisk

  __rt_memcpy (Thumb, 138 bytes, Stack size 0 bytes, rt_memcpy_v6.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memcpy4

  _memcpy_lastbytes (Thumb, 0 bytes, Stack size unknown bytes, rt_memcpy_v6.o(.text), UNUSED)

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  _printf_int_common (Thumb, 184 bytes, Stack size 32 bytes, _printf_intcommon.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = _printf_int_common
  [Called By]
  - >> _printf_int_hex
  - >> _printf_int_dec

  _printf_char_file (Thumb, 32 bytes, Stack size 16 bytes, _printf_char_file.o(.text))
  [Stack]

  - Max Depth = 104 + Unknown Stack Size
  - Call Chain = _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> ferror
  - >> _printf_char_common
  [Called By]
  - >> __2printf

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 8 bytes, rt_memcpy_w.o(.text), UNUSED)
  [Called By]

  - >> __rt_memcpy

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 8 bytes, rt_memcpy_w.o(.text), UNUSED)

  __rt_memcpy_w (Thumb, 100 bytes, Stack size 8 bytes, rt_memcpy_w.o(.text), UNUSED)

  _memcpy_lastbytes_aligned (Thumb, 0 bytes, Stack size unknown bytes, rt_memcpy_w.o(.text), UNUSED)

  _printf_char_common (Thumb, 32 bytes, Stack size 64 bytes, _printf_char_common.o(.text))
  [Stack]

  - Max Depth = 88 + Unknown Stack Size
  - Call Chain = _printf_char_common ⇒ __printf
  [Calls]
  - >> __printf
  [Called By]
  - >> _printf_char_file

  ferror (Thumb, 8 bytes, Stack size 0 bytes, ferror.o(.text))
  [Called By]

  - >> _printf_char_file

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 12 bytes, Stack size 0 bytes, exit.o(.text))
  [Calls]

  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  _fp_init (Thumb, 10 bytes, Stack size 0 bytes, fpinit.o(x$fpl$fpinit))
  [Called By]

  - >> __rt_lib_init_fp_1

  __fplib_config_fpu_vfp (Thumb, 0 bytes, Stack size unknown bytes, fpinit.o(x$fpl$fpinit), UNUSED)

  __fplib_config_pureend_doubles (Thumb, 0 bytes, Stack size unknown bytes, fpinit.o(x$fpl$fpinit), UNUSED)

  ### Local Symbols

  SetSysClock (Thumb, 218 bytes, Stack size 12 bytes, system_stm32f4xx.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClock
  [Called By]
  - >> SystemInit

  _printf_input_char (Thumb, 10 bytes, Stack size 0 bytes, _printf_char_common.o(.text))
  [Address Reference Count : 1]

  - _printf_char_common.o(.text)

  ### Undefined Global Symbols