Component: ARM Compiler 5.06 update 3 (build 300) Tool: armlink [4d35c9]

==============================================================================

Section Cross References

    startup_stm32f767xx.o(RESET) refers to startup_stm32f767xx.o(STACK) for __initial_sp
    startup_stm32f767xx.o(RESET) refers to startup_stm32f767xx.o(.text) for Reset_Handler
    startup_stm32f767xx.o(RESET) refers to stm32f7xx_it.o(i.NMI_Handler) for NMI_Handler
    startup_stm32f767xx.o(RESET) refers to stm32f7xx_it.o(i.HardFault_Handler) for HardFault_Handler
    startup_stm32f767xx.o(RESET) refers to stm32f7xx_it.o(i.MemManage_Handler) for MemManage_Handler
    startup_stm32f767xx.o(RESET) refers to stm32f7xx_it.o(i.BusFault_Handler) for BusFault_Handler
    startup_stm32f767xx.o(RESET) refers to stm32f7xx_it.o(i.UsageFault_Handler) for UsageFault_Handler
    startup_stm32f767xx.o(RESET) refers to stm32f7xx_it.o(i.SVC_Handler) for SVC_Handler
    startup_stm32f767xx.o(RESET) refers to stm32f7xx_it.o(i.DebugMon_Handler) for DebugMon_Handler
    startup_stm32f767xx.o(RESET) refers to stm32f7xx_it.o(i.PendSV_Handler) for PendSV_Handler
    startup_stm32f767xx.o(RESET) refers to stm32f7xx_it.o(i.SysTick_Handler) for SysTick_Handler
    startup_stm32f767xx.o(.text) refers to system_stm32f7xx.o(i.SystemInit) for SystemInit
    startup_stm32f767xx.o(.text) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    system_stm32f7xx.o(i.SystemCoreClockUpdate) refers to system_stm32f7xx.o(.data) for .data
    system_stm32f7xx.o(i.SystemCoreClockUpdate) refers to system_stm32f7xx.o(.constdata) for .constdata
    stm32f7xx_hal.o(i.HAL_DeInit) refers to stm32f7xx_hal_msp_template.o(i.HAL_MspDeInit) for HAL_MspDeInit
    stm32f7xx_hal.o(i.HAL_Delay) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal.o(i.HAL_GetTick) refers to stm32f7xx_hal.o(.data) for .data
    stm32f7xx_hal.o(i.HAL_IncTick) refers to stm32f7xx_hal.o(.data) for .data
    stm32f7xx_hal.o(i.HAL_Init) refers to stm32f7xx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping) for HAL_NVIC_SetPriorityGrouping
    stm32f7xx_hal.o(i.HAL_Init) refers to stm32f7xx_hal.o(i.HAL_InitTick) for HAL_InitTick
    stm32f7xx_hal.o(i.HAL_Init) refers to stm32f7xx_hal_msp_template.o(i.HAL_MspInit) for HAL_MspInit
    stm32f7xx_hal.o(i.HAL_InitTick) refers to stm32f7xx_hal_cortex.o(i.HAL_SYSTICK_Config) for HAL_SYSTICK_Config
    stm32f7xx_hal.o(i.HAL_InitTick) refers to stm32f7xx_hal_cortex.o(i.HAL_NVIC_SetPriority) for HAL_NVIC_SetPriority
    stm32f7xx_hal.o(i.HAL_InitTick) refers to system_stm32f7xx.o(.data) for SystemCoreClock
    stm32f7xx_hal_adc.o(i.ADC_DMAConvCplt) refers to stm32f7xx_hal_adc.o(i.HAL_ADC_ConvCpltCallback) for HAL_ADC_ConvCpltCallback
    stm32f7xx_hal_adc.o(i.ADC_DMAError) refers to stm32f7xx_hal_adc.o(i.HAL_ADC_ErrorCallback) for HAL_ADC_ErrorCallback
    stm32f7xx_hal_adc.o(i.ADC_DMAHalfConvCplt) refers to stm32f7xx_hal_adc.o(i.HAL_ADC_ConvHalfCpltCallback) for HAL_ADC_ConvHalfCpltCallback
    stm32f7xx_hal_adc.o(i.HAL_ADC_ConfigChannel) refers to system_stm32f7xx.o(.data) for SystemCoreClock
    stm32f7xx_hal_adc.o(i.HAL_ADC_DeInit) refers to stm32f7xx_hal_adc.o(i.HAL_ADC_MspDeInit) for HAL_ADC_MspDeInit
    stm32f7xx_hal_adc.o(i.HAL_ADC_IRQHandler) refers to stm32f7xx_hal_adc.o(i.HAL_ADC_ConvCpltCallback) for HAL_ADC_ConvCpltCallback
    stm32f7xx_hal_adc.o(i.HAL_ADC_IRQHandler) refers to stm32f7xx_hal_adc_ex.o(i.HAL_ADCEx_InjectedConvCpltCallback) for HAL_ADCEx_InjectedConvCpltCallback
    stm32f7xx_hal_adc.o(i.HAL_ADC_IRQHandler) refers to stm32f7xx_hal_adc.o(i.HAL_ADC_LevelOutOfWindowCallback) for HAL_ADC_LevelOutOfWindowCallback
    stm32f7xx_hal_adc.o(i.HAL_ADC_IRQHandler) refers to stm32f7xx_hal_adc.o(i.HAL_ADC_ErrorCallback) for HAL_ADC_ErrorCallback
    stm32f7xx_hal_adc.o(i.HAL_ADC_Init) refers to stm32f7xx_hal_adc.o(i.HAL_ADC_MspInit) for HAL_ADC_MspInit
    stm32f7xx_hal_adc.o(i.HAL_ADC_Init) refers to stm32f7xx_hal_adc.o(i.ADC_Init) for ADC_Init
    stm32f7xx_hal_adc.o(i.HAL_ADC_PollForConversion) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_adc.o(i.HAL_ADC_PollForEvent) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_adc.o(i.HAL_ADC_Start) refers to system_stm32f7xx.o(.data) for SystemCoreClock
    stm32f7xx_hal_adc.o(i.HAL_ADC_Start_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_adc.o(i.HAL_ADC_Start_DMA) refers to system_stm32f7xx.o(.data) for SystemCoreClock
    stm32f7xx_hal_adc.o(i.HAL_ADC_Start_DMA) refers to stm32f7xx_hal_adc.o(i.ADC_DMAConvCplt) for ADC_DMAConvCplt
    stm32f7xx_hal_adc.o(i.HAL_ADC_Start_DMA) refers to stm32f7xx_hal_adc.o(i.ADC_DMAHalfConvCplt) for ADC_DMAHalfConvCplt
    stm32f7xx_hal_adc.o(i.HAL_ADC_Start_DMA) refers to stm32f7xx_hal_adc.o(i.ADC_DMAError) for ADC_DMAError
    stm32f7xx_hal_adc.o(i.HAL_ADC_Start_IT) refers to system_stm32f7xx.o(.data) for SystemCoreClock
    stm32f7xx_hal_adc.o(i.HAL_ADC_Stop_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f7xx_hal_adc_ex.o(i.ADC_MultiModeDMAConvCplt) refers to stm32f7xx_hal_adc.o(i.HAL_ADC_ConvCpltCallback) for HAL_ADC_ConvCpltCallback
    stm32f7xx_hal_adc_ex.o(i.ADC_MultiModeDMAError) refers to stm32f7xx_hal_adc.o(i.HAL_ADC_ErrorCallback) for HAL_ADC_ErrorCallback
    stm32f7xx_hal_adc_ex.o(i.ADC_MultiModeDMAHalfConvCplt) refers to stm32f7xx_hal_adc.o(i.HAL_ADC_ConvHalfCpltCallback) for HAL_ADC_ConvHalfCpltCallback
    stm32f7xx_hal_adc_ex.o(i.HAL_ADCEx_InjectedPollForConversion) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_adc_ex.o(i.HAL_ADCEx_InjectedStart) refers to system_stm32f7xx.o(.data) for SystemCoreClock
    stm32f7xx_hal_adc_ex.o(i.HAL_ADCEx_InjectedStart_IT) refers to system_stm32f7xx.o(.data) for SystemCoreClock
    stm32f7xx_hal_adc_ex.o(i.HAL_ADCEx_MultiModeStart_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_adc_ex.o(i.HAL_ADCEx_MultiModeStart_DMA) refers to system_stm32f7xx.o(.data) for SystemCoreClock
    stm32f7xx_hal_adc_ex.o(i.HAL_ADCEx_MultiModeStart_DMA) refers to stm32f7xx_hal_adc_ex.o(i.ADC_MultiModeDMAConvCplt) for ADC_MultiModeDMAConvCplt
    stm32f7xx_hal_adc_ex.o(i.HAL_ADCEx_MultiModeStart_DMA) refers to stm32f7xx_hal_adc_ex.o(i.ADC_MultiModeDMAHalfConvCplt) for ADC_MultiModeDMAHalfConvCplt
    stm32f7xx_hal_adc_ex.o(i.HAL_ADCEx_MultiModeStart_DMA) refers to stm32f7xx_hal_adc_ex.o(i.ADC_MultiModeDMAError) for ADC_MultiModeDMAError
    stm32f7xx_hal_adc_ex.o(i.HAL_ADCEx_MultiModeStop_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f7xx_hal_can.o(i.CAN_Receive_IT) refers to stm32f7xx_hal_can.o(i.HAL_CAN_RxCpltCallback) for HAL_CAN_RxCpltCallback
    stm32f7xx_hal_can.o(i.CAN_Transmit_IT) refers to stm32f7xx_hal_can.o(i.HAL_CAN_TxCpltCallback) for HAL_CAN_TxCpltCallback
    stm32f7xx_hal_can.o(i.HAL_CAN_DeInit) refers to stm32f7xx_hal_can.o(i.HAL_CAN_MspDeInit) for HAL_CAN_MspDeInit
    stm32f7xx_hal_can.o(i.HAL_CAN_IRQHandler) refers to stm32f7xx_hal_can.o(i.CAN_Transmit_IT) for CAN_Transmit_IT
    stm32f7xx_hal_can.o(i.HAL_CAN_IRQHandler) refers to stm32f7xx_hal_can.o(i.CAN_Receive_IT) for CAN_Receive_IT
    stm32f7xx_hal_can.o(i.HAL_CAN_IRQHandler) refers to stm32f7xx_hal_can.o(i.HAL_CAN_ErrorCallback) for HAL_CAN_ErrorCallback
    stm32f7xx_hal_can.o(i.HAL_CAN_Init) refers to stm32f7xx_hal_can.o(i.HAL_CAN_MspInit) for HAL_CAN_MspInit
    stm32f7xx_hal_can.o(i.HAL_CAN_Init) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_can.o(i.HAL_CAN_Receive) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_can.o(i.HAL_CAN_Sleep) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_can.o(i.HAL_CAN_Transmit) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_can.o(i.HAL_CAN_WakeUp) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_cec.o(i.HAL_CEC_DeInit) refers to stm32f7xx_hal_cec.o(i.HAL_CEC_MspDeInit) for HAL_CEC_MspDeInit
    stm32f7xx_hal_cec.o(i.HAL_CEC_IRQHandler) refers to stm32f7xx_hal_cec.o(i.HAL_CEC_RxCpltCallback) for HAL_CEC_RxCpltCallback
    stm32f7xx_hal_cec.o(i.HAL_CEC_IRQHandler) refers to stm32f7xx_hal_cec.o(i.HAL_CEC_TxCpltCallback) for HAL_CEC_TxCpltCallback
    stm32f7xx_hal_cec.o(i.HAL_CEC_IRQHandler) refers to stm32f7xx_hal_cec.o(i.HAL_CEC_ErrorCallback) for HAL_CEC_ErrorCallback
    stm32f7xx_hal_cec.o(i.HAL_CEC_Init) refers to stm32f7xx_hal_cec.o(i.HAL_CEC_MspInit) for HAL_CEC_MspInit
    stm32f7xx_hal_cortex.o(i.HAL_NVIC_SetPriority) refers to stm32f7xx_hal_cortex.o(i.NVIC_SetPriority) for NVIC_SetPriority
    stm32f7xx_hal_cortex.o(i.HAL_SYSTICK_Config) refers to stm32f7xx_hal_cortex.o(i.NVIC_SetPriority) for NVIC_SetPriority
    stm32f7xx_hal_cortex.o(i.HAL_SYSTICK_IRQHandler) refers to stm32f7xx_hal_cortex.o(i.HAL_SYSTICK_Callback) for HAL_SYSTICK_Callback
    stm32f7xx_hal_crc.o(i.HAL_CRC_Accumulate) refers to stm32f7xx_hal_crc.o(i.CRC_Handle_8) for CRC_Handle_8
    stm32f7xx_hal_crc.o(i.HAL_CRC_Accumulate) refers to stm32f7xx_hal_crc.o(i.CRC_Handle_16) for CRC_Handle_16
    stm32f7xx_hal_crc.o(i.HAL_CRC_Calculate) refers to stm32f7xx_hal_crc.o(i.CRC_Handle_8) for CRC_Handle_8
    stm32f7xx_hal_crc.o(i.HAL_CRC_Calculate) refers to stm32f7xx_hal_crc.o(i.CRC_Handle_16) for CRC_Handle_16
    stm32f7xx_hal_crc.o(i.HAL_CRC_DeInit) refers to stm32f7xx_hal_crc.o(i.HAL_CRC_MspDeInit) for HAL_CRC_MspDeInit
    stm32f7xx_hal_crc.o(i.HAL_CRC_Init) refers to stm32f7xx_hal_crc.o(i.HAL_CRC_MspInit) for HAL_CRC_MspInit
    stm32f7xx_hal_crc.o(i.HAL_CRC_Init) refers to stm32f7xx_hal_crc_ex.o(i.HAL_CRCEx_Polynomial_Set) for HAL_CRCEx_Polynomial_Set
    stm32f7xx_hal_dac.o(i.DAC_DMAConvCpltCh1) refers to stm32f7xx_hal_dac.o(i.HAL_DAC_ConvCpltCallbackCh1) for HAL_DAC_ConvCpltCallbackCh1
    stm32f7xx_hal_dac.o(i.DAC_DMAErrorCh1) refers to stm32f7xx_hal_dac.o(i.HAL_DAC_ErrorCallbackCh1) for HAL_DAC_ErrorCallbackCh1
    stm32f7xx_hal_dac.o(i.DAC_DMAHalfConvCpltCh1) refers to stm32f7xx_hal_dac.o(i.HAL_DAC_ConvHalfCpltCallbackCh1) for HAL_DAC_ConvHalfCpltCallbackCh1
    stm32f7xx_hal_dac.o(i.HAL_DAC_DeInit) refers to stm32f7xx_hal_dac.o(i.HAL_DAC_MspDeInit) for HAL_DAC_MspDeInit
    stm32f7xx_hal_dac.o(i.HAL_DAC_IRQHandler) refers to stm32f7xx_hal_dac.o(i.HAL_DAC_DMAUnderrunCallbackCh1) for HAL_DAC_DMAUnderrunCallbackCh1
    stm32f7xx_hal_dac.o(i.HAL_DAC_IRQHandler) refers to stm32f7xx_hal_dac_ex.o(i.HAL_DACEx_DMAUnderrunCallbackCh2) for HAL_DACEx_DMAUnderrunCallbackCh2
    stm32f7xx_hal_dac.o(i.HAL_DAC_Init) refers to stm32f7xx_hal_dac.o(i.HAL_DAC_MspInit) for HAL_DAC_MspInit
    stm32f7xx_hal_dac.o(i.HAL_DAC_Start_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_dac.o(i.HAL_DAC_Start_DMA) refers to stm32f7xx_hal_dac_ex.o(i.DAC_DMAConvCpltCh2) for DAC_DMAConvCpltCh2
    stm32f7xx_hal_dac.o(i.HAL_DAC_Start_DMA) refers to stm32f7xx_hal_dac_ex.o(i.DAC_DMAHalfConvCpltCh2) for DAC_DMAHalfConvCpltCh2
    stm32f7xx_hal_dac.o(i.HAL_DAC_Start_DMA) refers to stm32f7xx_hal_dac_ex.o(i.DAC_DMAErrorCh2) for DAC_DMAErrorCh2
    stm32f7xx_hal_dac.o(i.HAL_DAC_Start_DMA) refers to stm32f7xx_hal_dac.o(i.DAC_DMAConvCpltCh1) for DAC_DMAConvCpltCh1
    stm32f7xx_hal_dac.o(i.HAL_DAC_Start_DMA) refers to stm32f7xx_hal_dac.o(i.DAC_DMAHalfConvCpltCh1) for DAC_DMAHalfConvCpltCh1
    stm32f7xx_hal_dac.o(i.HAL_DAC_Start_DMA) refers to stm32f7xx_hal_dac.o(i.DAC_DMAErrorCh1) for DAC_DMAErrorCh1
    stm32f7xx_hal_dac.o(i.HAL_DAC_Stop_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f7xx_hal_dac_ex.o(i.DAC_DMAConvCpltCh2) refers to stm32f7xx_hal_dac_ex.o(i.HAL_DACEx_ConvCpltCallbackCh2) for HAL_DACEx_ConvCpltCallbackCh2
    stm32f7xx_hal_dac_ex.o(i.DAC_DMAErrorCh2) refers to stm32f7xx_hal_dac_ex.o(i.HAL_DACEx_ErrorCallbackCh2) for HAL_DACEx_ErrorCallbackCh2
    stm32f7xx_hal_dac_ex.o(i.DAC_DMAHalfConvCpltCh2) refers to stm32f7xx_hal_dac_ex.o(i.HAL_DACEx_ConvHalfCpltCallbackCh2) for HAL_DACEx_ConvHalfCpltCallbackCh2
    stm32f7xx_hal_dcmi.o(i.DCMI_DMAError) refers to stm32f7xx_hal_dcmi.o(i.HAL_DCMI_ErrorCallback) for HAL_DCMI_ErrorCallback
    stm32f7xx_hal_dcmi.o(i.DCMI_DMAXferCplt) refers to stm32f7xx_hal_dma_ex.o(i.HAL_DMAEx_ChangeMemory) for HAL_DMAEx_ChangeMemory
    stm32f7xx_hal_dcmi.o(i.HAL_DCMI_DeInit) refers to stm32f7xx_hal_dcmi.o(i.HAL_DCMI_MspDeInit) for HAL_DCMI_MspDeInit
    stm32f7xx_hal_dcmi.o(i.HAL_DCMI_IRQHandler) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32f7xx_hal_dcmi.o(i.HAL_DCMI_IRQHandler) refers to stm32f7xx_hal_dcmi.o(i.HAL_DCMI_LineEventCallback) for HAL_DCMI_LineEventCallback
    stm32f7xx_hal_dcmi.o(i.HAL_DCMI_IRQHandler) refers to stm32f7xx_hal_dcmi.o(i.HAL_DCMI_VsyncEventCallback) for HAL_DCMI_VsyncEventCallback
    stm32f7xx_hal_dcmi.o(i.HAL_DCMI_IRQHandler) refers to stm32f7xx_hal_dcmi.o(i.HAL_DCMI_FrameEventCallback) for HAL_DCMI_FrameEventCallback
    stm32f7xx_hal_dcmi.o(i.HAL_DCMI_IRQHandler) refers to stm32f7xx_hal_dcmi.o(i.DCMI_DMAError) for DCMI_DMAError
    stm32f7xx_hal_dcmi.o(i.HAL_DCMI_Init) refers to stm32f7xx_hal_dcmi.o(i.HAL_DCMI_MspInit) for HAL_DCMI_MspInit
    stm32f7xx_hal_dcmi.o(i.HAL_DCMI_Start_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_dcmi.o(i.HAL_DCMI_Start_DMA) refers to stm32f7xx_hal_dma_ex.o(i.HAL_DMAEx_MultiBufferStart_IT) for HAL_DMAEx_MultiBufferStart_IT
    stm32f7xx_hal_dcmi.o(i.HAL_DCMI_Start_DMA) refers to stm32f7xx_hal_dcmi.o(i.DCMI_DMAXferCplt) for DCMI_DMAXferCplt
    stm32f7xx_hal_dcmi.o(i.HAL_DCMI_Start_DMA) refers to stm32f7xx_hal_dcmi.o(i.DCMI_DMAError) for DCMI_DMAError
    stm32f7xx_hal_dcmi.o(i.HAL_DCMI_Stop) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f7xx_hal_dcmi.o(i.HAL_DCMI_Stop) refers to system_stm32f7xx.o(.data) for SystemCoreClock
    stm32f7xx_hal_dcmi.o(i.HAL_DCMI_Suspend) refers to system_stm32f7xx.o(.data) for SystemCoreClock
    stm32f7xx_hal_dma.o(i.DMA_CalcBaseAndBitshift) refers to stm32f7xx_hal_dma.o(.constdata) for .constdata
    stm32f7xx_hal_dma.o(i.HAL_DMA_Abort) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_dma.o(i.HAL_DMA_DeInit) refers to stm32f7xx_hal_dma.o(i.DMA_CalcBaseAndBitshift) for DMA_CalcBaseAndBitshift
    stm32f7xx_hal_dma.o(i.HAL_DMA_IRQHandler) refers to system_stm32f7xx.o(.data) for SystemCoreClock
    stm32f7xx_hal_dma.o(i.HAL_DMA_Init) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_dma.o(i.HAL_DMA_Init) refers to stm32f7xx_hal_dma.o(i.DMA_CheckFifoParam) for DMA_CheckFifoParam
    stm32f7xx_hal_dma.o(i.HAL_DMA_Init) refers to stm32f7xx_hal_dma.o(i.DMA_CalcBaseAndBitshift) for DMA_CalcBaseAndBitshift
    stm32f7xx_hal_dma.o(i.HAL_DMA_PollForTransfer) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_dma.o(i.HAL_DMA_PollForTransfer) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f7xx_hal_dma.o(i.HAL_DMA_Start) refers to stm32f7xx_hal_dma.o(i.DMA_SetConfig) for DMA_SetConfig
    stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) refers to stm32f7xx_hal_dma.o(i.DMA_SetConfig) for DMA_SetConfig
    stm32f7xx_hal_dma_ex.o(i.HAL_DMAEx_MultiBufferStart) refers to stm32f7xx_hal_dma_ex.o(i.DMA_MultiBufferSetConfig) for DMA_MultiBufferSetConfig
    stm32f7xx_hal_dma_ex.o(i.HAL_DMAEx_MultiBufferStart_IT) refers to stm32f7xx_hal_dma_ex.o(i.DMA_MultiBufferSetConfig) for DMA_MultiBufferSetConfig
    stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_Abort) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_BlendingStart) refers to stm32f7xx_hal_dma2d.o(i.DMA2D_SetConfig) for DMA2D_SetConfig
    stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_BlendingStart_IT) refers to stm32f7xx_hal_dma2d.o(i.DMA2D_SetConfig) for DMA2D_SetConfig
    stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_CLUTLoading_Abort) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_CLUTLoading_Suspend) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_DeInit) refers to stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_Abort) for HAL_DMA2D_Abort
    stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_DeInit) refers to stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_CLUTLoading_Abort) for HAL_DMA2D_CLUTLoading_Abort
    stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_DeInit) refers to stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_MspDeInit) for HAL_DMA2D_MspDeInit
    stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_IRQHandler) refers to stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_LineEventCallback) for HAL_DMA2D_LineEventCallback
    stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_IRQHandler) refers to stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_CLUTLoadingCpltCallback) for HAL_DMA2D_CLUTLoadingCpltCallback
    stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_Init) refers to stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_MspInit) for HAL_DMA2D_MspInit
    stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_PollForTransfer) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_Start) refers to stm32f7xx_hal_dma2d.o(i.DMA2D_SetConfig) for DMA2D_SetConfig
    stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_Start_IT) refers to stm32f7xx_hal_dma2d.o(i.DMA2D_SetConfig) for DMA2D_SetConfig
    stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_Suspend) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_eth.o(i.ETH_FlushTransmitFIFO) refers to stm32f7xx_hal.o(i.HAL_Delay) for HAL_Delay
    stm32f7xx_hal_eth.o(i.ETH_MACDMAConfig) refers to stm32f7xx_hal.o(i.HAL_Delay) for HAL_Delay
    stm32f7xx_hal_eth.o(i.ETH_MACDMAConfig) refers to stm32f7xx_hal_eth.o(i.ETH_MACAddressConfig) for ETH_MACAddressConfig
    stm32f7xx_hal_eth.o(i.ETH_MACReceptionDisable) refers to stm32f7xx_hal.o(i.HAL_Delay) for HAL_Delay
    stm32f7xx_hal_eth.o(i.ETH_MACReceptionEnable) refers to stm32f7xx_hal.o(i.HAL_Delay) for HAL_Delay
    stm32f7xx_hal_eth.o(i.ETH_MACTransmissionDisable) refers to stm32f7xx_hal.o(i.HAL_Delay) for HAL_Delay
    stm32f7xx_hal_eth.o(i.ETH_MACTransmissionEnable) refers to stm32f7xx_hal.o(i.HAL_Delay) for HAL_Delay
    stm32f7xx_hal_eth.o(i.HAL_ETH_ConfigDMA) refers to stm32f7xx_hal.o(i.HAL_Delay) for HAL_Delay
    stm32f7xx_hal_eth.o(i.HAL_ETH_ConfigMAC) refers to stm32f7xx_hal.o(i.HAL_Delay) for HAL_Delay
    stm32f7xx_hal_eth.o(i.HAL_ETH_DeInit) refers to stm32f7xx_hal_eth.o(i.HAL_ETH_MspDeInit) for HAL_ETH_MspDeInit
    stm32f7xx_hal_eth.o(i.HAL_ETH_IRQHandler) refers to stm32f7xx_hal_eth.o(i.HAL_ETH_RxCpltCallback) for HAL_ETH_RxCpltCallback
    stm32f7xx_hal_eth.o(i.HAL_ETH_IRQHandler) refers to stm32f7xx_hal_eth.o(i.HAL_ETH_TxCpltCallback) for HAL_ETH_TxCpltCallback
    stm32f7xx_hal_eth.o(i.HAL_ETH_IRQHandler) refers to stm32f7xx_hal_eth.o(i.HAL_ETH_ErrorCallback) for HAL_ETH_ErrorCallback
    stm32f7xx_hal_eth.o(i.HAL_ETH_Init) refers to stm32f7xx_hal_eth.o(i.HAL_ETH_MspInit) for HAL_ETH_MspInit
    stm32f7xx_hal_eth.o(i.HAL_ETH_Init) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_eth.o(i.HAL_ETH_Init) refers to stm32f7xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq) for HAL_RCC_GetHCLKFreq
    stm32f7xx_hal_eth.o(i.HAL_ETH_Init) refers to stm32f7xx_hal_eth.o(i.HAL_ETH_WritePHYRegister) for HAL_ETH_WritePHYRegister
    stm32f7xx_hal_eth.o(i.HAL_ETH_Init) refers to stm32f7xx_hal_eth.o(i.ETH_MACDMAConfig) for ETH_MACDMAConfig
    stm32f7xx_hal_eth.o(i.HAL_ETH_Init) refers to stm32f7xx_hal.o(i.HAL_Delay) for HAL_Delay
    stm32f7xx_hal_eth.o(i.HAL_ETH_Init) refers to stm32f7xx_hal_eth.o(i.HAL_ETH_ReadPHYRegister) for HAL_ETH_ReadPHYRegister
    stm32f7xx_hal_eth.o(i.HAL_ETH_ReadPHYRegister) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_eth.o(i.HAL_ETH_Start) refers to stm32f7xx_hal_eth.o(i.ETH_MACTransmissionEnable) for ETH_MACTransmissionEnable
    stm32f7xx_hal_eth.o(i.HAL_ETH_Start) refers to stm32f7xx_hal_eth.o(i.ETH_MACReceptionEnable) for ETH_MACReceptionEnable
    stm32f7xx_hal_eth.o(i.HAL_ETH_Start) refers to stm32f7xx_hal_eth.o(i.ETH_FlushTransmitFIFO) for ETH_FlushTransmitFIFO
    stm32f7xx_hal_eth.o(i.HAL_ETH_Start) refers to stm32f7xx_hal_eth.o(i.ETH_DMATransmissionEnable) for ETH_DMATransmissionEnable
    stm32f7xx_hal_eth.o(i.HAL_ETH_Start) refers to stm32f7xx_hal_eth.o(i.ETH_DMAReceptionEnable) for ETH_DMAReceptionEnable
    stm32f7xx_hal_eth.o(i.HAL_ETH_Stop) refers to stm32f7xx_hal_eth.o(i.ETH_DMATransmissionDisable) for ETH_DMATransmissionDisable
    stm32f7xx_hal_eth.o(i.HAL_ETH_Stop) refers to stm32f7xx_hal_eth.o(i.ETH_DMAReceptionDisable) for ETH_DMAReceptionDisable
    stm32f7xx_hal_eth.o(i.HAL_ETH_Stop) refers to stm32f7xx_hal_eth.o(i.ETH_MACReceptionDisable) for ETH_MACReceptionDisable
    stm32f7xx_hal_eth.o(i.HAL_ETH_Stop) refers to stm32f7xx_hal_eth.o(i.ETH_FlushTransmitFIFO) for ETH_FlushTransmitFIFO
    stm32f7xx_hal_eth.o(i.HAL_ETH_Stop) refers to stm32f7xx_hal_eth.o(i.ETH_MACTransmissionDisable) for ETH_MACTransmissionDisable
    stm32f7xx_hal_eth.o(i.HAL_ETH_WritePHYRegister) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_flash.o(i.FLASH_SetErrorCode) refers to stm32f7xx_hal_flash.o(.bss) for .bss
    stm32f7xx_hal_flash.o(i.FLASH_WaitForLastOperation) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_flash.o(i.FLASH_WaitForLastOperation) refers to stm32f7xx_hal_flash.o(i.FLASH_SetErrorCode) for FLASH_SetErrorCode
    stm32f7xx_hal_flash.o(i.FLASH_WaitForLastOperation) refers to stm32f7xx_hal_flash.o(.bss) for .bss
    stm32f7xx_hal_flash.o(i.HAL_FLASH_GetError) refers to stm32f7xx_hal_flash.o(.bss) for .bss
    stm32f7xx_hal_flash.o(i.HAL_FLASH_IRQHandler) refers to stm32f7xx_hal_flash.o(i.HAL_FLASH_EndOfOperationCallback) for HAL_FLASH_EndOfOperationCallback
    stm32f7xx_hal_flash.o(i.HAL_FLASH_IRQHandler) refers to stm32f7xx_hal_flash_ex.o(i.FLASH_Erase_Sector) for FLASH_Erase_Sector
    stm32f7xx_hal_flash.o(i.HAL_FLASH_IRQHandler) refers to stm32f7xx_hal_flash.o(i.FLASH_SetErrorCode) for FLASH_SetErrorCode
    stm32f7xx_hal_flash.o(i.HAL_FLASH_IRQHandler) refers to stm32f7xx_hal_flash.o(i.HAL_FLASH_OperationErrorCallback) for HAL_FLASH_OperationErrorCallback
    stm32f7xx_hal_flash.o(i.HAL_FLASH_IRQHandler) refers to stm32f7xx_hal_flash.o(.bss) for .bss
    stm32f7xx_hal_flash.o(i.HAL_FLASH_OB_Launch) refers to stm32f7xx_hal_flash.o(i.FLASH_WaitForLastOperation) for FLASH_WaitForLastOperation
    stm32f7xx_hal_flash.o(i.HAL_FLASH_Program) refers to stm32f7xx_hal_flash.o(i.FLASH_WaitForLastOperation) for FLASH_WaitForLastOperation
    stm32f7xx_hal_flash.o(i.HAL_FLASH_Program) refers to stm32f7xx_hal_flash.o(i.FLASH_Program_Byte) for FLASH_Program_Byte
    stm32f7xx_hal_flash.o(i.HAL_FLASH_Program) refers to stm32f7xx_hal_flash.o(i.FLASH_Program_HalfWord) for FLASH_Program_HalfWord
    stm32f7xx_hal_flash.o(i.HAL_FLASH_Program) refers to stm32f7xx_hal_flash.o(i.FLASH_Program_Word) for FLASH_Program_Word
    stm32f7xx_hal_flash.o(i.HAL_FLASH_Program) refers to stm32f7xx_hal_flash.o(i.FLASH_Program_DoubleWord) for FLASH_Program_DoubleWord
    stm32f7xx_hal_flash.o(i.HAL_FLASH_Program) refers to stm32f7xx_hal_flash.o(.bss) for .bss
    stm32f7xx_hal_flash.o(i.HAL_FLASH_Program_IT) refers to stm32f7xx_hal_flash.o(i.FLASH_Program_Byte) for FLASH_Program_Byte
    stm32f7xx_hal_flash.o(i.HAL_FLASH_Program_IT) refers to stm32f7xx_hal_flash.o(i.FLASH_Program_HalfWord) for FLASH_Program_HalfWord
    stm32f7xx_hal_flash.o(i.HAL_FLASH_Program_IT) refers to stm32f7xx_hal_flash.o(i.FLASH_Program_Word) for FLASH_Program_Word
    stm32f7xx_hal_flash.o(i.HAL_FLASH_Program_IT) refers to stm32f7xx_hal_flash.o(i.FLASH_Program_DoubleWord) for FLASH_Program_DoubleWord
    stm32f7xx_hal_flash.o(i.HAL_FLASH_Program_IT) refers to stm32f7xx_hal_flash.o(.bss) for .bss
    stm32f7xx_hal_flash_ex.o(i.FLASH_OB_BootAddressConfig) refers to stm32f7xx_hal_flash.o(i.FLASH_WaitForLastOperation) for FLASH_WaitForLastOperation
    stm32f7xx_hal_flash_ex.o(i.FLASH_OB_DisableWRP) refers to stm32f7xx_hal_flash.o(i.FLASH_WaitForLastOperation) for FLASH_WaitForLastOperation
    stm32f7xx_hal_flash_ex.o(i.FLASH_OB_EnableWRP) refers to stm32f7xx_hal_flash.o(i.FLASH_WaitForLastOperation) for FLASH_WaitForLastOperation
    stm32f7xx_hal_flash_ex.o(i.FLASH_OB_RDP_LevelConfig) refers to stm32f7xx_hal_flash.o(i.FLASH_WaitForLastOperation) for FLASH_WaitForLastOperation
    stm32f7xx_hal_flash_ex.o(i.FLASH_OB_UserConfig) refers to stm32f7xx_hal_flash.o(i.FLASH_WaitForLastOperation) for FLASH_WaitForLastOperation
    stm32f7xx_hal_flash_ex.o(i.HAL_FLASHEx_Erase) refers to stm32f7xx_hal_flash.o(i.FLASH_WaitForLastOperation) for FLASH_WaitForLastOperation
    stm32f7xx_hal_flash_ex.o(i.HAL_FLASHEx_Erase) refers to stm32f7xx_hal_flash_ex.o(i.FLASH_MassErase) for FLASH_MassErase
    stm32f7xx_hal_flash_ex.o(i.HAL_FLASHEx_Erase) refers to stm32f7xx_hal_flash_ex.o(i.FLASH_Erase_Sector) for FLASH_Erase_Sector
    stm32f7xx_hal_flash_ex.o(i.HAL_FLASHEx_Erase) refers to stm32f7xx_hal_flash.o(.bss) for pFlash
    stm32f7xx_hal_flash_ex.o(i.HAL_FLASHEx_Erase_IT) refers to stm32f7xx_hal_flash_ex.o(i.FLASH_Erase_Sector) for FLASH_Erase_Sector
    stm32f7xx_hal_flash_ex.o(i.HAL_FLASHEx_Erase_IT) refers to stm32f7xx_hal_flash_ex.o(i.FLASH_MassErase) for FLASH_MassErase
    stm32f7xx_hal_flash_ex.o(i.HAL_FLASHEx_Erase_IT) refers to stm32f7xx_hal_flash.o(.bss) for pFlash
    stm32f7xx_hal_flash_ex.o(i.HAL_FLASHEx_OBGetConfig) refers to stm32f7xx_hal_flash_ex.o(i.FLASH_OB_GetWRP) for FLASH_OB_GetWRP
    stm32f7xx_hal_flash_ex.o(i.HAL_FLASHEx_OBGetConfig) refers to stm32f7xx_hal_flash_ex.o(i.FLASH_OB_GetRDP) for FLASH_OB_GetRDP
    stm32f7xx_hal_flash_ex.o(i.HAL_FLASHEx_OBGetConfig) refers to stm32f7xx_hal_flash_ex.o(i.FLASH_OB_GetUser) for FLASH_OB_GetUser
    stm32f7xx_hal_flash_ex.o(i.HAL_FLASHEx_OBGetConfig) refers to stm32f7xx_hal_flash_ex.o(i.FLASH_OB_GetBOR) for FLASH_OB_GetBOR
    stm32f7xx_hal_flash_ex.o(i.HAL_FLASHEx_OBGetConfig) refers to stm32f7xx_hal_flash_ex.o(i.FLASH_OB_GetBootAddress) for FLASH_OB_GetBootAddress
    stm32f7xx_hal_flash_ex.o(i.HAL_FLASHEx_OBProgram) refers to stm32f7xx_hal_flash_ex.o(i.FLASH_OB_DisableWRP) for FLASH_OB_DisableWRP
    stm32f7xx_hal_flash_ex.o(i.HAL_FLASHEx_OBProgram) refers to stm32f7xx_hal_flash_ex.o(i.FLASH_OB_RDP_LevelConfig) for FLASH_OB_RDP_LevelConfig
    stm32f7xx_hal_flash_ex.o(i.HAL_FLASHEx_OBProgram) refers to stm32f7xx_hal_flash_ex.o(i.FLASH_OB_UserConfig) for FLASH_OB_UserConfig
    stm32f7xx_hal_flash_ex.o(i.HAL_FLASHEx_OBProgram) refers to stm32f7xx_hal_flash_ex.o(i.FLASH_OB_BOR_LevelConfig) for FLASH_OB_BOR_LevelConfig
    stm32f7xx_hal_flash_ex.o(i.HAL_FLASHEx_OBProgram) refers to stm32f7xx_hal_flash_ex.o(i.FLASH_OB_BootAddressConfig) for FLASH_OB_BootAddressConfig
    stm32f7xx_hal_flash_ex.o(i.HAL_FLASHEx_OBProgram) refers to stm32f7xx_hal_flash_ex.o(i.FLASH_OB_EnableWRP) for FLASH_OB_EnableWRP
    stm32f7xx_hal_flash_ex.o(i.HAL_FLASHEx_OBProgram) refers to stm32f7xx_hal_flash.o(.bss) for pFlash
    stm32f7xx_hal_gpio.o(i.HAL_GPIO_EXTI_IRQHandler) refers to stm32f7xx_hal_gpio.o(i.HAL_GPIO_EXTI_Callback) for HAL_GPIO_EXTI_Callback
    stm32f7xx_hal_hcd.o(i.HAL_HCD_DeInit) refers to stm32f7xx_hal_hcd.o(i.HAL_HCD_MspDeInit) for HAL_HCD_MspDeInit
    stm32f7xx_hal_hcd.o(i.HAL_HCD_DeInit) refers to stm32f7xx_ll_usb.o(i.USB_DisableGlobalInt) for USB_DisableGlobalInt
    stm32f7xx_hal_hcd.o(i.HAL_HCD_GetCurrentFrame) refers to stm32f7xx_ll_usb.o(i.USB_GetCurrentFrame) for USB_GetCurrentFrame
    stm32f7xx_hal_hcd.o(i.HAL_HCD_GetCurrentSpeed) refers to stm32f7xx_ll_usb.o(i.USB_GetHostSpeed) for USB_GetHostSpeed
    stm32f7xx_hal_hcd.o(i.HAL_HCD_HC_Halt) refers to stm32f7xx_ll_usb.o(i.USB_HC_Halt) for USB_HC_Halt
    stm32f7xx_hal_hcd.o(i.HAL_HCD_HC_Init) refers to stm32f7xx_ll_usb.o(i.USB_HC_Init) for USB_HC_Init
    stm32f7xx_hal_hcd.o(i.HAL_HCD_HC_SubmitRequest) refers to stm32f7xx_ll_usb.o(i.USB_HC_StartXfer) for USB_HC_StartXfer
    stm32f7xx_hal_hcd.o(i.HAL_HCD_IRQHandler) refers to stm32f7xx_ll_usb.o(i.USB_GetMode) for USB_GetMode
    stm32f7xx_hal_hcd.o(i.HAL_HCD_IRQHandler) refers to stm32f7xx_ll_usb.o(i.USB_ReadInterrupts) for USB_ReadInterrupts
    stm32f7xx_hal_hcd.o(i.HAL_HCD_IRQHandler) refers to stm32f7xx_hal_hcd.o(i.HAL_HCD_Disconnect_Callback) for HAL_HCD_Disconnect_Callback
    stm32f7xx_hal_hcd.o(i.HAL_HCD_IRQHandler) refers to stm32f7xx_ll_usb.o(i.USB_InitFSLSPClkSel) for USB_InitFSLSPClkSel
    stm32f7xx_hal_hcd.o(i.HAL_HCD_IRQHandler) refers to stm32f7xx_hal_hcd.o(i.HCD_Port_IRQHandler) for HCD_Port_IRQHandler
    stm32f7xx_hal_hcd.o(i.HAL_HCD_IRQHandler) refers to stm32f7xx_hal_hcd.o(i.HAL_HCD_SOF_Callback) for HAL_HCD_SOF_Callback
    stm32f7xx_hal_hcd.o(i.HAL_HCD_IRQHandler) refers to stm32f7xx_ll_usb.o(i.USB_HC_ReadInterrupt) for USB_HC_ReadInterrupt
    stm32f7xx_hal_hcd.o(i.HAL_HCD_IRQHandler) refers to stm32f7xx_hal_hcd.o(i.HCD_HC_IN_IRQHandler) for HCD_HC_IN_IRQHandler
    stm32f7xx_hal_hcd.o(i.HAL_HCD_IRQHandler) refers to stm32f7xx_hal_hcd.o(i.HCD_HC_OUT_IRQHandler) for HCD_HC_OUT_IRQHandler
    stm32f7xx_hal_hcd.o(i.HAL_HCD_IRQHandler) refers to stm32f7xx_hal_hcd.o(i.HCD_RXQLVL_IRQHandler) for HCD_RXQLVL_IRQHandler
    stm32f7xx_hal_hcd.o(i.HAL_HCD_Init) refers to stm32f7xx_hal_hcd.o(i.HAL_HCD_MspInit) for HAL_HCD_MspInit
    stm32f7xx_hal_hcd.o(i.HAL_HCD_Init) refers to stm32f7xx_ll_usb.o(i.USB_DisableGlobalInt) for USB_DisableGlobalInt
    stm32f7xx_hal_hcd.o(i.HAL_HCD_Init) refers to memcpya.o(.text) for __aeabi_memcpy4
    stm32f7xx_hal_hcd.o(i.HAL_HCD_Init) refers to stm32f7xx_ll_usb.o(i.USB_CoreInit) for USB_CoreInit
    stm32f7xx_hal_hcd.o(i.HAL_HCD_Init) refers to stm32f7xx_ll_usb.o(i.USB_SetCurrentMode) for USB_SetCurrentMode
    stm32f7xx_hal_hcd.o(i.HAL_HCD_Init) refers to stm32f7xx_ll_usb.o(i.USB_HostInit) for USB_HostInit
    stm32f7xx_hal_hcd.o(i.HAL_HCD_ResetPort) refers to stm32f7xx_ll_usb.o(i.USB_ResetPort) for USB_ResetPort
    stm32f7xx_hal_hcd.o(i.HAL_HCD_Start) refers to stm32f7xx_ll_usb.o(i.USB_EnableGlobalInt) for USB_EnableGlobalInt
    stm32f7xx_hal_hcd.o(i.HAL_HCD_Start) refers to stm32f7xx_ll_usb.o(i.USB_DriveVbus) for USB_DriveVbus
    stm32f7xx_hal_hcd.o(i.HAL_HCD_Stop) refers to stm32f7xx_ll_usb.o(i.USB_StopHost) for USB_StopHost
    stm32f7xx_hal_hcd.o(i.HCD_HC_IN_IRQHandler) refers to stm32f7xx_ll_usb.o(i.USB_HC_Halt) for USB_HC_Halt
    stm32f7xx_hal_hcd.o(i.HCD_HC_IN_IRQHandler) refers to stm32f7xx_hal_hcd.o(i.HAL_HCD_HC_NotifyURBChange_Callback) for HAL_HCD_HC_NotifyURBChange_Callback
    stm32f7xx_hal_hcd.o(i.HCD_HC_OUT_IRQHandler) refers to stm32f7xx_ll_usb.o(i.USB_HC_Halt) for USB_HC_Halt
    stm32f7xx_hal_hcd.o(i.HCD_HC_OUT_IRQHandler) refers to stm32f7xx_hal_hcd.o(i.HAL_HCD_HC_NotifyURBChange_Callback) for HAL_HCD_HC_NotifyURBChange_Callback
    stm32f7xx_hal_hcd.o(i.HCD_Port_IRQHandler) refers to stm32f7xx_hal_hcd.o(i.HAL_HCD_Connect_Callback) for HAL_HCD_Connect_Callback
    stm32f7xx_hal_hcd.o(i.HCD_Port_IRQHandler) refers to stm32f7xx_ll_usb.o(i.USB_InitFSLSPClkSel) for USB_InitFSLSPClkSel
    stm32f7xx_hal_hcd.o(i.HCD_RXQLVL_IRQHandler) refers to stm32f7xx_ll_usb.o(i.USB_ReadPacket) for USB_ReadPacket
    stm32f7xx_hal_i2c.o(i.HAL_I2C_DeInit) refers to stm32f7xx_hal_i2c.o(i.HAL_I2C_MspDeInit) for HAL_I2C_MspDeInit
    stm32f7xx_hal_i2c.o(i.HAL_I2C_DisableListen_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Disable_IRQ) for I2C_Disable_IRQ
    stm32f7xx_hal_i2c.o(i.HAL_I2C_ER_IRQHandler) refers to stm32f7xx_hal_i2c.o(i.I2C_ITError) for I2C_ITError
    stm32f7xx_hal_i2c.o(i.HAL_I2C_EnableListen_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Enable_IRQ) for I2C_Enable_IRQ
    stm32f7xx_hal_i2c.o(i.HAL_I2C_EnableListen_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Slave_ISR_IT) for I2C_Slave_ISR_IT
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Init) refers to stm32f7xx_hal_i2c.o(i.HAL_I2C_MspInit) for HAL_I2C_MspInit
    stm32f7xx_hal_i2c.o(i.HAL_I2C_IsDeviceReady) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_i2c.o(i.HAL_I2C_IsDeviceReady) refers to stm32f7xx_hal_i2c.o(i.I2C_WaitOnFlagUntilTimeout) for I2C_WaitOnFlagUntilTimeout
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Abort_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Disable_IRQ) for I2C_Disable_IRQ
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Abort_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_TransferConfig) for I2C_TransferConfig
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Abort_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Enable_IRQ) for I2C_Enable_IRQ
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Receive) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Receive) refers to stm32f7xx_hal_i2c.o(i.I2C_WaitOnFlagUntilTimeout) for I2C_WaitOnFlagUntilTimeout
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Receive) refers to stm32f7xx_hal_i2c.o(i.I2C_TransferConfig) for I2C_TransferConfig
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Receive) refers to stm32f7xx_hal_i2c.o(i.I2C_WaitOnRXNEFlagUntilTimeout) for I2C_WaitOnRXNEFlagUntilTimeout
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Receive) refers to stm32f7xx_hal_i2c.o(i.I2C_WaitOnSTOPFlagUntilTimeout) for I2C_WaitOnSTOPFlagUntilTimeout
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Receive_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Receive_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_TransferConfig) for I2C_TransferConfig
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Receive_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_Enable_IRQ) for I2C_Enable_IRQ
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Receive_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_Master_ISR_DMA) for I2C_Master_ISR_DMA
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Receive_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_DMAMasterReceiveCplt) for I2C_DMAMasterReceiveCplt
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Receive_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_DMAError) for I2C_DMAError
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Receive_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_TransferConfig) for I2C_TransferConfig
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Receive_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Enable_IRQ) for I2C_Enable_IRQ
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Receive_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Master_ISR_IT) for I2C_Master_ISR_IT
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Sequential_Receive_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_TransferConfig) for I2C_TransferConfig
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Sequential_Receive_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Enable_IRQ) for I2C_Enable_IRQ
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Sequential_Receive_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Master_ISR_IT) for I2C_Master_ISR_IT
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Sequential_Transmit_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_TransferConfig) for I2C_TransferConfig
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Sequential_Transmit_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Enable_IRQ) for I2C_Enable_IRQ
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Sequential_Transmit_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Master_ISR_IT) for I2C_Master_ISR_IT
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Transmit) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Transmit) refers to stm32f7xx_hal_i2c.o(i.I2C_WaitOnFlagUntilTimeout) for I2C_WaitOnFlagUntilTimeout
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Transmit) refers to stm32f7xx_hal_i2c.o(i.I2C_TransferConfig) for I2C_TransferConfig
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Transmit) refers to stm32f7xx_hal_i2c.o(i.I2C_WaitOnTXISFlagUntilTimeout) for I2C_WaitOnTXISFlagUntilTimeout
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Transmit) refers to stm32f7xx_hal_i2c.o(i.I2C_WaitOnSTOPFlagUntilTimeout) for I2C_WaitOnSTOPFlagUntilTimeout
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Transmit_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Transmit_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_TransferConfig) for I2C_TransferConfig
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Transmit_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_Enable_IRQ) for I2C_Enable_IRQ
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Transmit_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_Master_ISR_DMA) for I2C_Master_ISR_DMA
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Transmit_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_DMAMasterTransmitCplt) for I2C_DMAMasterTransmitCplt
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Transmit_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_DMAError) for I2C_DMAError
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Transmit_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_TransferConfig) for I2C_TransferConfig
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Transmit_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Enable_IRQ) for I2C_Enable_IRQ
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Transmit_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Master_ISR_IT) for I2C_Master_ISR_IT
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Read) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Read) refers to stm32f7xx_hal_i2c.o(i.I2C_WaitOnFlagUntilTimeout) for I2C_WaitOnFlagUntilTimeout
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Read) refers to stm32f7xx_hal_i2c.o(i.I2C_RequestMemoryRead) for I2C_RequestMemoryRead
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Read) refers to stm32f7xx_hal_i2c.o(i.I2C_TransferConfig) for I2C_TransferConfig
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Read) refers to stm32f7xx_hal_i2c.o(i.I2C_WaitOnSTOPFlagUntilTimeout) for I2C_WaitOnSTOPFlagUntilTimeout
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Read_DMA) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Read_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_RequestMemoryRead) for I2C_RequestMemoryRead
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Read_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Read_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_TransferConfig) for I2C_TransferConfig
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Read_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_Enable_IRQ) for I2C_Enable_IRQ
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Read_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_Master_ISR_DMA) for I2C_Master_ISR_DMA
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Read_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_DMAMasterReceiveCplt) for I2C_DMAMasterReceiveCplt
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Read_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_DMAError) for I2C_DMAError
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Read_IT) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Read_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_RequestMemoryRead) for I2C_RequestMemoryRead
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Read_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_TransferConfig) for I2C_TransferConfig
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Read_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Enable_IRQ) for I2C_Enable_IRQ
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Read_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Master_ISR_IT) for I2C_Master_ISR_IT
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Write) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Write) refers to stm32f7xx_hal_i2c.o(i.I2C_WaitOnFlagUntilTimeout) for I2C_WaitOnFlagUntilTimeout
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Write) refers to stm32f7xx_hal_i2c.o(i.I2C_RequestMemoryWrite) for I2C_RequestMemoryWrite
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Write) refers to stm32f7xx_hal_i2c.o(i.I2C_TransferConfig) for I2C_TransferConfig
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Write) refers to stm32f7xx_hal_i2c.o(i.I2C_WaitOnTXISFlagUntilTimeout) for I2C_WaitOnTXISFlagUntilTimeout
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Write) refers to stm32f7xx_hal_i2c.o(i.I2C_WaitOnSTOPFlagUntilTimeout) for I2C_WaitOnSTOPFlagUntilTimeout
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Write_DMA) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Write_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_RequestMemoryWrite) for I2C_RequestMemoryWrite
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Write_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Write_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_TransferConfig) for I2C_TransferConfig
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Write_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_Enable_IRQ) for I2C_Enable_IRQ
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Write_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_Master_ISR_DMA) for I2C_Master_ISR_DMA
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Write_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_DMAMasterTransmitCplt) for I2C_DMAMasterTransmitCplt
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Write_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_DMAError) for I2C_DMAError
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Write_IT) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Write_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_RequestMemoryWrite) for I2C_RequestMemoryWrite
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Write_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_TransferConfig) for I2C_TransferConfig
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Write_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Enable_IRQ) for I2C_Enable_IRQ
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Write_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Master_ISR_IT) for I2C_Master_ISR_IT
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Receive) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Receive) refers to stm32f7xx_hal_i2c.o(i.I2C_WaitOnFlagUntilTimeout) for I2C_WaitOnFlagUntilTimeout
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Receive) refers to stm32f7xx_hal_i2c.o(i.I2C_WaitOnRXNEFlagUntilTimeout) for I2C_WaitOnRXNEFlagUntilTimeout
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Receive) refers to stm32f7xx_hal_i2c.o(i.I2C_WaitOnSTOPFlagUntilTimeout) for I2C_WaitOnSTOPFlagUntilTimeout
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Receive_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Receive_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_Enable_IRQ) for I2C_Enable_IRQ
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Receive_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_Slave_ISR_DMA) for I2C_Slave_ISR_DMA
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Receive_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_DMASlaveReceiveCplt) for I2C_DMASlaveReceiveCplt
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Receive_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_DMAError) for I2C_DMAError
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Receive_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Enable_IRQ) for I2C_Enable_IRQ
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Receive_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Slave_ISR_IT) for I2C_Slave_ISR_IT
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Sequential_Receive_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Disable_IRQ) for I2C_Disable_IRQ
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Sequential_Receive_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Enable_IRQ) for I2C_Enable_IRQ
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Sequential_Receive_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Slave_ISR_IT) for I2C_Slave_ISR_IT
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Sequential_Transmit_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Disable_IRQ) for I2C_Disable_IRQ
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Sequential_Transmit_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Enable_IRQ) for I2C_Enable_IRQ
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Sequential_Transmit_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Slave_ISR_IT) for I2C_Slave_ISR_IT
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Transmit) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Transmit) refers to stm32f7xx_hal_i2c.o(i.I2C_WaitOnFlagUntilTimeout) for I2C_WaitOnFlagUntilTimeout
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Transmit) refers to stm32f7xx_hal_i2c.o(i.I2C_WaitOnTXISFlagUntilTimeout) for I2C_WaitOnTXISFlagUntilTimeout
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Transmit) refers to stm32f7xx_hal_i2c.o(i.I2C_WaitOnSTOPFlagUntilTimeout) for I2C_WaitOnSTOPFlagUntilTimeout
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Transmit_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Transmit_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_Enable_IRQ) for I2C_Enable_IRQ
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Transmit_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_Slave_ISR_DMA) for I2C_Slave_ISR_DMA
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Transmit_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_DMASlaveTransmitCplt) for I2C_DMASlaveTransmitCplt
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Transmit_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_DMAError) for I2C_DMAError
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Transmit_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Enable_IRQ) for I2C_Enable_IRQ
    stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Transmit_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Slave_ISR_IT) for I2C_Slave_ISR_IT
    stm32f7xx_hal_i2c.o(i.I2C_DMAAbort) refers to stm32f7xx_hal_i2c.o(i.HAL_I2C_ErrorCallback) for HAL_I2C_ErrorCallback
    stm32f7xx_hal_i2c.o(i.I2C_DMAAbort) refers to stm32f7xx_hal_i2c.o(i.HAL_I2C_AbortCpltCallback) for HAL_I2C_AbortCpltCallback
    stm32f7xx_hal_i2c.o(i.I2C_DMAError) refers to stm32f7xx_hal_i2c.o(i.I2C_ITError) for I2C_ITError
    stm32f7xx_hal_i2c.o(i.I2C_DMAMasterReceiveCplt) refers to stm32f7xx_hal_i2c.o(i.I2C_Enable_IRQ) for I2C_Enable_IRQ
    stm32f7xx_hal_i2c.o(i.I2C_DMAMasterReceiveCplt) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_i2c.o(i.I2C_DMAMasterTransmitCplt) refers to stm32f7xx_hal_i2c.o(i.I2C_Enable_IRQ) for I2C_Enable_IRQ
    stm32f7xx_hal_i2c.o(i.I2C_DMAMasterTransmitCplt) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_i2c.o(i.I2C_Enable_IRQ) refers to stm32f7xx_hal_i2c.o(i.I2C_Master_ISR_DMA) for I2C_Master_ISR_DMA
    stm32f7xx_hal_i2c.o(i.I2C_Enable_IRQ) refers to stm32f7xx_hal_i2c.o(i.I2C_Slave_ISR_DMA) for I2C_Slave_ISR_DMA
    stm32f7xx_hal_i2c.o(i.I2C_ITAddrCplt) refers to stm32f7xx_hal_i2c.o(i.I2C_Disable_IRQ) for I2C_Disable_IRQ
    stm32f7xx_hal_i2c.o(i.I2C_ITAddrCplt) refers to stm32f7xx_hal_i2c.o(i.HAL_I2C_AddrCallback) for HAL_I2C_AddrCallback
    stm32f7xx_hal_i2c.o(i.I2C_ITError) refers to stm32f7xx_hal_i2c.o(i.I2C_Disable_IRQ) for I2C_Disable_IRQ
    stm32f7xx_hal_i2c.o(i.I2C_ITError) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32f7xx_hal_i2c.o(i.I2C_ITError) refers to stm32f7xx_hal_i2c.o(i.HAL_I2C_ErrorCallback) for HAL_I2C_ErrorCallback
    stm32f7xx_hal_i2c.o(i.I2C_ITError) refers to stm32f7xx_hal_i2c.o(i.HAL_I2C_AbortCpltCallback) for HAL_I2C_AbortCpltCallback
    stm32f7xx_hal_i2c.o(i.I2C_ITError) refers to stm32f7xx_hal_i2c.o(i.I2C_DMAAbort) for I2C_DMAAbort
    stm32f7xx_hal_i2c.o(i.I2C_ITError) refers to stm32f7xx_hal_i2c.o(i.I2C_Slave_ISR_IT) for I2C_Slave_ISR_IT
    stm32f7xx_hal_i2c.o(i.I2C_ITListenCplt) refers to stm32f7xx_hal_i2c.o(i.I2C_Disable_IRQ) for I2C_Disable_IRQ
    stm32f7xx_hal_i2c.o(i.I2C_ITListenCplt) refers to stm32f7xx_hal_i2c.o(i.HAL_I2C_ListenCpltCallback) for HAL_I2C_ListenCpltCallback
    stm32f7xx_hal_i2c.o(i.I2C_ITMasterCplt) refers to stm32f7xx_hal_i2c.o(i.I2C_Flush_TXDR) for I2C_Flush_TXDR
    stm32f7xx_hal_i2c.o(i.I2C_ITMasterCplt) refers to stm32f7xx_hal_i2c.o(i.I2C_Disable_IRQ) for I2C_Disable_IRQ
    stm32f7xx_hal_i2c.o(i.I2C_ITMasterCplt) refers to stm32f7xx_hal_i2c.o(i.I2C_ITError) for I2C_ITError
    stm32f7xx_hal_i2c.o(i.I2C_ITMasterCplt) refers to stm32f7xx_hal_i2c.o(i.HAL_I2C_MasterRxCpltCallback) for HAL_I2C_MasterRxCpltCallback
    stm32f7xx_hal_i2c.o(i.I2C_ITMasterCplt) refers to stm32f7xx_hal_i2c.o(i.HAL_I2C_MasterTxCpltCallback) for HAL_I2C_MasterTxCpltCallback
    stm32f7xx_hal_i2c.o(i.I2C_ITMasterCplt) refers to stm32f7xx_hal_i2c.o(i.HAL_I2C_MemTxCpltCallback) for HAL_I2C_MemTxCpltCallback
    stm32f7xx_hal_i2c.o(i.I2C_ITMasterCplt) refers to stm32f7xx_hal_i2c.o(i.HAL_I2C_MemRxCpltCallback) for HAL_I2C_MemRxCpltCallback
    stm32f7xx_hal_i2c.o(i.I2C_ITMasterSequentialCplt) refers to stm32f7xx_hal_i2c.o(i.I2C_Disable_IRQ) for I2C_Disable_IRQ
    stm32f7xx_hal_i2c.o(i.I2C_ITMasterSequentialCplt) refers to stm32f7xx_hal_i2c.o(i.HAL_I2C_MasterRxCpltCallback) for HAL_I2C_MasterRxCpltCallback
    stm32f7xx_hal_i2c.o(i.I2C_ITMasterSequentialCplt) refers to stm32f7xx_hal_i2c.o(i.HAL_I2C_MasterTxCpltCallback) for HAL_I2C_MasterTxCpltCallback
    stm32f7xx_hal_i2c.o(i.I2C_ITSlaveCplt) refers to stm32f7xx_hal_i2c.o(i.I2C_Disable_IRQ) for I2C_Disable_IRQ
    stm32f7xx_hal_i2c.o(i.I2C_ITSlaveCplt) refers to stm32f7xx_hal_i2c.o(i.I2C_Flush_TXDR) for I2C_Flush_TXDR
    stm32f7xx_hal_i2c.o(i.I2C_ITSlaveCplt) refers to stm32f7xx_hal_i2c.o(i.I2C_ITError) for I2C_ITError
    stm32f7xx_hal_i2c.o(i.I2C_ITSlaveCplt) refers to stm32f7xx_hal_i2c.o(i.HAL_I2C_ListenCpltCallback) for HAL_I2C_ListenCpltCallback
    stm32f7xx_hal_i2c.o(i.I2C_ITSlaveCplt) refers to stm32f7xx_hal_i2c.o(i.HAL_I2C_SlaveTxCpltCallback) for HAL_I2C_SlaveTxCpltCallback
    stm32f7xx_hal_i2c.o(i.I2C_ITSlaveCplt) refers to stm32f7xx_hal_i2c.o(i.HAL_I2C_SlaveRxCpltCallback) for HAL_I2C_SlaveRxCpltCallback
    stm32f7xx_hal_i2c.o(i.I2C_ITSlaveSequentialCplt) refers to stm32f7xx_hal_i2c.o(i.I2C_Disable_IRQ) for I2C_Disable_IRQ
    stm32f7xx_hal_i2c.o(i.I2C_ITSlaveSequentialCplt) refers to stm32f7xx_hal_i2c.o(i.HAL_I2C_SlaveRxCpltCallback) for HAL_I2C_SlaveRxCpltCallback
    stm32f7xx_hal_i2c.o(i.I2C_ITSlaveSequentialCplt) refers to stm32f7xx_hal_i2c.o(i.HAL_I2C_SlaveTxCpltCallback) for HAL_I2C_SlaveTxCpltCallback
    stm32f7xx_hal_i2c.o(i.I2C_IsAcknowledgeFailed) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_i2c.o(i.I2C_IsAcknowledgeFailed) refers to stm32f7xx_hal_i2c.o(i.I2C_Flush_TXDR) for I2C_Flush_TXDR
    stm32f7xx_hal_i2c.o(i.I2C_Master_ISR_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_Enable_IRQ) for I2C_Enable_IRQ
    stm32f7xx_hal_i2c.o(i.I2C_Master_ISR_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_Flush_TXDR) for I2C_Flush_TXDR
    stm32f7xx_hal_i2c.o(i.I2C_Master_ISR_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_TransferConfig) for I2C_TransferConfig
    stm32f7xx_hal_i2c.o(i.I2C_Master_ISR_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_ITError) for I2C_ITError
    stm32f7xx_hal_i2c.o(i.I2C_Master_ISR_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_ITMasterCplt) for I2C_ITMasterCplt
    stm32f7xx_hal_i2c.o(i.I2C_Master_ISR_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Flush_TXDR) for I2C_Flush_TXDR
    stm32f7xx_hal_i2c.o(i.I2C_Master_ISR_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_TransferConfig) for I2C_TransferConfig
    stm32f7xx_hal_i2c.o(i.I2C_Master_ISR_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_ITError) for I2C_ITError
    stm32f7xx_hal_i2c.o(i.I2C_Master_ISR_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_ITMasterSequentialCplt) for I2C_ITMasterSequentialCplt
    stm32f7xx_hal_i2c.o(i.I2C_Master_ISR_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_ITMasterCplt) for I2C_ITMasterCplt
    stm32f7xx_hal_i2c.o(i.I2C_RequestMemoryRead) refers to stm32f7xx_hal_i2c.o(i.I2C_TransferConfig) for I2C_TransferConfig
    stm32f7xx_hal_i2c.o(i.I2C_RequestMemoryRead) refers to stm32f7xx_hal_i2c.o(i.I2C_WaitOnTXISFlagUntilTimeout) for I2C_WaitOnTXISFlagUntilTimeout
    stm32f7xx_hal_i2c.o(i.I2C_RequestMemoryRead) refers to stm32f7xx_hal_i2c.o(i.I2C_WaitOnFlagUntilTimeout) for I2C_WaitOnFlagUntilTimeout
    stm32f7xx_hal_i2c.o(i.I2C_RequestMemoryWrite) refers to stm32f7xx_hal_i2c.o(i.I2C_TransferConfig) for I2C_TransferConfig
    stm32f7xx_hal_i2c.o(i.I2C_RequestMemoryWrite) refers to stm32f7xx_hal_i2c.o(i.I2C_WaitOnTXISFlagUntilTimeout) for I2C_WaitOnTXISFlagUntilTimeout
    stm32f7xx_hal_i2c.o(i.I2C_RequestMemoryWrite) refers to stm32f7xx_hal_i2c.o(i.I2C_WaitOnFlagUntilTimeout) for I2C_WaitOnFlagUntilTimeout
    stm32f7xx_hal_i2c.o(i.I2C_Slave_ISR_DMA) refers to stm32f7xx_hal_i2c.o(i.I2C_ITSlaveCplt) for I2C_ITSlaveCplt
    stm32f7xx_hal_i2c.o(i.I2C_Slave_ISR_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_ITListenCplt) for I2C_ITListenCplt
    stm32f7xx_hal_i2c.o(i.I2C_Slave_ISR_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_Flush_TXDR) for I2C_Flush_TXDR
    stm32f7xx_hal_i2c.o(i.I2C_Slave_ISR_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_ITSlaveSequentialCplt) for I2C_ITSlaveSequentialCplt
    stm32f7xx_hal_i2c.o(i.I2C_Slave_ISR_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_ITAddrCplt) for I2C_ITAddrCplt
    stm32f7xx_hal_i2c.o(i.I2C_Slave_ISR_IT) refers to stm32f7xx_hal_i2c.o(i.I2C_ITSlaveCplt) for I2C_ITSlaveCplt
    stm32f7xx_hal_i2c.o(i.I2C_WaitOnFlagUntilTimeout) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_i2c.o(i.I2C_WaitOnRXNEFlagUntilTimeout) refers to stm32f7xx_hal_i2c.o(i.I2C_IsAcknowledgeFailed) for I2C_IsAcknowledgeFailed
    stm32f7xx_hal_i2c.o(i.I2C_WaitOnRXNEFlagUntilTimeout) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_i2c.o(i.I2C_WaitOnSTOPFlagUntilTimeout) refers to stm32f7xx_hal_i2c.o(i.I2C_IsAcknowledgeFailed) for I2C_IsAcknowledgeFailed
    stm32f7xx_hal_i2c.o(i.I2C_WaitOnSTOPFlagUntilTimeout) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_i2c.o(i.I2C_WaitOnTXISFlagUntilTimeout) refers to stm32f7xx_hal_i2c.o(i.I2C_IsAcknowledgeFailed) for I2C_IsAcknowledgeFailed
    stm32f7xx_hal_i2c.o(i.I2C_WaitOnTXISFlagUntilTimeout) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_i2s.o(i.HAL_I2S_DMAStop) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f7xx_hal_i2s.o(i.HAL_I2S_DeInit) refers to stm32f7xx_hal_i2s.o(i.HAL_I2S_MspDeInit) for HAL_I2S_MspDeInit
    stm32f7xx_hal_i2s.o(i.HAL_I2S_IRQHandler) refers to stm32f7xx_hal_i2s.o(i.I2S_Transmit_IT) for I2S_Transmit_IT
    stm32f7xx_hal_i2s.o(i.HAL_I2S_IRQHandler) refers to stm32f7xx_hal_i2s.o(i.HAL_I2S_ErrorCallback) for HAL_I2S_ErrorCallback
    stm32f7xx_hal_i2s.o(i.HAL_I2S_IRQHandler) refers to stm32f7xx_hal_i2s.o(i.I2S_Receive_IT) for I2S_Receive_IT
    stm32f7xx_hal_i2s.o(i.HAL_I2S_Init) refers to stm32f7xx_hal_i2s.o(i.HAL_I2S_MspInit) for HAL_I2S_MspInit
    stm32f7xx_hal_i2s.o(i.HAL_I2S_Init) refers to stm32f7xx_hal_i2s.o(i.I2S_GetClockFreq) for I2S_GetClockFreq
    stm32f7xx_hal_i2s.o(i.HAL_I2S_Receive) refers to stm32f7xx_hal_i2s.o(i.I2S_WaitFlagStateUntilTimeout) for I2S_WaitFlagStateUntilTimeout
    stm32f7xx_hal_i2s.o(i.HAL_I2S_Receive) refers to stm32f7xx_hal_i2s.o(i.HAL_I2S_ErrorCallback) for HAL_I2S_ErrorCallback
    stm32f7xx_hal_i2s.o(i.HAL_I2S_Receive_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_i2s.o(i.HAL_I2S_Receive_DMA) refers to stm32f7xx_hal_i2s.o(i.I2S_DMARxHalfCplt) for I2S_DMARxHalfCplt
    stm32f7xx_hal_i2s.o(i.HAL_I2S_Receive_DMA) refers to stm32f7xx_hal_i2s.o(i.I2S_DMARxCplt) for I2S_DMARxCplt
    stm32f7xx_hal_i2s.o(i.HAL_I2S_Receive_DMA) refers to stm32f7xx_hal_i2s.o(i.I2S_DMAError) for I2S_DMAError
    stm32f7xx_hal_i2s.o(i.HAL_I2S_Transmit) refers to stm32f7xx_hal_i2s.o(i.I2S_WaitFlagStateUntilTimeout) for I2S_WaitFlagStateUntilTimeout
    stm32f7xx_hal_i2s.o(i.HAL_I2S_Transmit) refers to stm32f7xx_hal_i2s.o(i.HAL_I2S_ErrorCallback) for HAL_I2S_ErrorCallback
    stm32f7xx_hal_i2s.o(i.HAL_I2S_Transmit_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_i2s.o(i.HAL_I2S_Transmit_DMA) refers to stm32f7xx_hal_i2s.o(i.I2S_DMATxHalfCplt) for I2S_DMATxHalfCplt
    stm32f7xx_hal_i2s.o(i.HAL_I2S_Transmit_DMA) refers to stm32f7xx_hal_i2s.o(i.I2S_DMATxCplt) for I2S_DMATxCplt
    stm32f7xx_hal_i2s.o(i.HAL_I2S_Transmit_DMA) refers to stm32f7xx_hal_i2s.o(i.I2S_DMAError) for I2S_DMAError
    stm32f7xx_hal_i2s.o(i.I2S_DMAError) refers to stm32f7xx_hal_i2s.o(i.HAL_I2S_ErrorCallback) for HAL_I2S_ErrorCallback
    stm32f7xx_hal_i2s.o(i.I2S_DMARxCplt) refers to stm32f7xx_hal_i2s.o(i.HAL_I2S_RxCpltCallback) for HAL_I2S_RxCpltCallback
    stm32f7xx_hal_i2s.o(i.I2S_DMARxHalfCplt) refers to stm32f7xx_hal_i2s.o(i.HAL_I2S_RxHalfCpltCallback) for HAL_I2S_RxHalfCpltCallback
    stm32f7xx_hal_i2s.o(i.I2S_DMATxCplt) refers to stm32f7xx_hal_i2s.o(i.HAL_I2S_TxCpltCallback) for HAL_I2S_TxCpltCallback
    stm32f7xx_hal_i2s.o(i.I2S_DMATxHalfCplt) refers to stm32f7xx_hal_i2s.o(i.HAL_I2S_TxHalfCpltCallback) for HAL_I2S_TxHalfCpltCallback
    stm32f7xx_hal_i2s.o(i.I2S_Receive_IT) refers to stm32f7xx_hal_i2s.o(i.HAL_I2S_RxCpltCallback) for HAL_I2S_RxCpltCallback
    stm32f7xx_hal_i2s.o(i.I2S_Transmit_IT) refers to stm32f7xx_hal_i2s.o(i.HAL_I2S_TxCpltCallback) for HAL_I2S_TxCpltCallback
    stm32f7xx_hal_i2s.o(i.I2S_WaitFlagStateUntilTimeout) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_irda.o(i.HAL_IRDA_Abort) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f7xx_hal_irda.o(i.HAL_IRDA_AbortReceive) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f7xx_hal_irda.o(i.HAL_IRDA_AbortReceive_IT) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32f7xx_hal_irda.o(i.HAL_IRDA_AbortReceive_IT) refers to stm32f7xx_hal_irda.o(i.HAL_IRDA_AbortReceiveCpltCallback) for HAL_IRDA_AbortReceiveCpltCallback
    stm32f7xx_hal_irda.o(i.HAL_IRDA_AbortReceive_IT) refers to stm32f7xx_hal_irda.o(i.IRDA_DMARxOnlyAbortCallback) for IRDA_DMARxOnlyAbortCallback
    stm32f7xx_hal_irda.o(i.HAL_IRDA_AbortTransmit) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f7xx_hal_irda.o(i.HAL_IRDA_AbortTransmit_IT) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32f7xx_hal_irda.o(i.HAL_IRDA_AbortTransmit_IT) refers to stm32f7xx_hal_irda.o(i.HAL_IRDA_AbortTransmitCpltCallback) for HAL_IRDA_AbortTransmitCpltCallback
    stm32f7xx_hal_irda.o(i.HAL_IRDA_AbortTransmit_IT) refers to stm32f7xx_hal_irda.o(i.IRDA_DMATxOnlyAbortCallback) for IRDA_DMATxOnlyAbortCallback
    stm32f7xx_hal_irda.o(i.HAL_IRDA_Abort_IT) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32f7xx_hal_irda.o(i.HAL_IRDA_Abort_IT) refers to stm32f7xx_hal_irda.o(i.HAL_IRDA_AbortCpltCallback) for HAL_IRDA_AbortCpltCallback
    stm32f7xx_hal_irda.o(i.HAL_IRDA_Abort_IT) refers to stm32f7xx_hal_irda.o(i.IRDA_DMATxAbortCallback) for IRDA_DMATxAbortCallback
    stm32f7xx_hal_irda.o(i.HAL_IRDA_Abort_IT) refers to stm32f7xx_hal_irda.o(i.IRDA_DMARxAbortCallback) for IRDA_DMARxAbortCallback
    stm32f7xx_hal_irda.o(i.HAL_IRDA_DMAStop) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f7xx_hal_irda.o(i.HAL_IRDA_DMAStop) refers to stm32f7xx_hal_irda.o(i.IRDA_EndTxTransfer) for IRDA_EndTxTransfer
    stm32f7xx_hal_irda.o(i.HAL_IRDA_DMAStop) refers to stm32f7xx_hal_irda.o(i.IRDA_EndRxTransfer) for IRDA_EndRxTransfer
    stm32f7xx_hal_irda.o(i.HAL_IRDA_DeInit) refers to stm32f7xx_hal_irda.o(i.HAL_IRDA_MspDeInit) for HAL_IRDA_MspDeInit
    stm32f7xx_hal_irda.o(i.HAL_IRDA_IRQHandler) refers to stm32f7xx_hal_irda.o(i.IRDA_Receive_IT) for IRDA_Receive_IT
    stm32f7xx_hal_irda.o(i.HAL_IRDA_IRQHandler) refers to stm32f7xx_hal_irda.o(i.IRDA_EndRxTransfer) for IRDA_EndRxTransfer
    stm32f7xx_hal_irda.o(i.HAL_IRDA_IRQHandler) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32f7xx_hal_irda.o(i.HAL_IRDA_IRQHandler) refers to stm32f7xx_hal_irda.o(i.HAL_IRDA_ErrorCallback) for HAL_IRDA_ErrorCallback
    stm32f7xx_hal_irda.o(i.HAL_IRDA_IRQHandler) refers to stm32f7xx_hal_irda.o(i.IRDA_Transmit_IT) for IRDA_Transmit_IT
    stm32f7xx_hal_irda.o(i.HAL_IRDA_IRQHandler) refers to stm32f7xx_hal_irda.o(i.IRDA_EndTransmit_IT) for IRDA_EndTransmit_IT
    stm32f7xx_hal_irda.o(i.HAL_IRDA_IRQHandler) refers to stm32f7xx_hal_irda.o(i.IRDA_DMAAbortOnError) for IRDA_DMAAbortOnError
    stm32f7xx_hal_irda.o(i.HAL_IRDA_Init) refers to stm32f7xx_hal_irda.o(i.HAL_IRDA_MspInit) for HAL_IRDA_MspInit
    stm32f7xx_hal_irda.o(i.HAL_IRDA_Init) refers to stm32f7xx_hal_irda.o(i.IRDA_SetConfig) for IRDA_SetConfig
    stm32f7xx_hal_irda.o(i.HAL_IRDA_Init) refers to stm32f7xx_hal_irda.o(i.IRDA_CheckIdleState) for IRDA_CheckIdleState
    stm32f7xx_hal_irda.o(i.HAL_IRDA_Receive) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_irda.o(i.HAL_IRDA_Receive) refers to stm32f7xx_hal_irda.o(i.IRDA_WaitOnFlagUntilTimeout) for IRDA_WaitOnFlagUntilTimeout
    stm32f7xx_hal_irda.o(i.HAL_IRDA_Receive_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_irda.o(i.HAL_IRDA_Receive_DMA) refers to stm32f7xx_hal_irda.o(i.IRDA_DMAReceiveCplt) for IRDA_DMAReceiveCplt
    stm32f7xx_hal_irda.o(i.HAL_IRDA_Receive_DMA) refers to stm32f7xx_hal_irda.o(i.IRDA_DMAReceiveHalfCplt) for IRDA_DMAReceiveHalfCplt
    stm32f7xx_hal_irda.o(i.HAL_IRDA_Receive_DMA) refers to stm32f7xx_hal_irda.o(i.IRDA_DMAError) for IRDA_DMAError
    stm32f7xx_hal_irda.o(i.HAL_IRDA_Transmit) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_irda.o(i.HAL_IRDA_Transmit) refers to stm32f7xx_hal_irda.o(i.IRDA_WaitOnFlagUntilTimeout) for IRDA_WaitOnFlagUntilTimeout
    stm32f7xx_hal_irda.o(i.HAL_IRDA_Transmit_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_irda.o(i.HAL_IRDA_Transmit_DMA) refers to stm32f7xx_hal_irda.o(i.IRDA_DMATransmitCplt) for IRDA_DMATransmitCplt
    stm32f7xx_hal_irda.o(i.HAL_IRDA_Transmit_DMA) refers to stm32f7xx_hal_irda.o(i.IRDA_DMATransmitHalfCplt) for IRDA_DMATransmitHalfCplt
    stm32f7xx_hal_irda.o(i.HAL_IRDA_Transmit_DMA) refers to stm32f7xx_hal_irda.o(i.IRDA_DMAError) for IRDA_DMAError
    stm32f7xx_hal_irda.o(i.IRDA_CheckIdleState) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_irda.o(i.IRDA_CheckIdleState) refers to stm32f7xx_hal_irda.o(i.IRDA_WaitOnFlagUntilTimeout) for IRDA_WaitOnFlagUntilTimeout
    stm32f7xx_hal_irda.o(i.IRDA_DMAAbortOnError) refers to stm32f7xx_hal_irda.o(i.HAL_IRDA_ErrorCallback) for HAL_IRDA_ErrorCallback
    stm32f7xx_hal_irda.o(i.IRDA_DMAError) refers to stm32f7xx_hal_irda.o(i.IRDA_EndTxTransfer) for IRDA_EndTxTransfer
    stm32f7xx_hal_irda.o(i.IRDA_DMAError) refers to stm32f7xx_hal_irda.o(i.IRDA_EndRxTransfer) for IRDA_EndRxTransfer
    stm32f7xx_hal_irda.o(i.IRDA_DMAError) refers to stm32f7xx_hal_irda.o(i.HAL_IRDA_ErrorCallback) for HAL_IRDA_ErrorCallback
    stm32f7xx_hal_irda.o(i.IRDA_DMAReceiveCplt) refers to stm32f7xx_hal_irda.o(i.HAL_IRDA_RxCpltCallback) for HAL_IRDA_RxCpltCallback
    stm32f7xx_hal_irda.o(i.IRDA_DMAReceiveHalfCplt) refers to stm32f7xx_hal_irda.o(i.HAL_IRDA_RxHalfCpltCallback) for HAL_IRDA_RxHalfCpltCallback
    stm32f7xx_hal_irda.o(i.IRDA_DMARxAbortCallback) refers to stm32f7xx_hal_irda.o(i.HAL_IRDA_AbortCpltCallback) for HAL_IRDA_AbortCpltCallback
    stm32f7xx_hal_irda.o(i.IRDA_DMARxOnlyAbortCallback) refers to stm32f7xx_hal_irda.o(i.HAL_IRDA_AbortReceiveCpltCallback) for HAL_IRDA_AbortReceiveCpltCallback
    stm32f7xx_hal_irda.o(i.IRDA_DMATransmitCplt) refers to stm32f7xx_hal_irda.o(i.HAL_IRDA_TxCpltCallback) for HAL_IRDA_TxCpltCallback
    stm32f7xx_hal_irda.o(i.IRDA_DMATransmitHalfCplt) refers to stm32f7xx_hal_irda.o(i.HAL_IRDA_TxHalfCpltCallback) for HAL_IRDA_TxHalfCpltCallback
    stm32f7xx_hal_irda.o(i.IRDA_DMATxAbortCallback) refers to stm32f7xx_hal_irda.o(i.HAL_IRDA_AbortCpltCallback) for HAL_IRDA_AbortCpltCallback
    stm32f7xx_hal_irda.o(i.IRDA_DMATxOnlyAbortCallback) refers to stm32f7xx_hal_irda.o(i.HAL_IRDA_AbortTransmitCpltCallback) for HAL_IRDA_AbortTransmitCpltCallback
    stm32f7xx_hal_irda.o(i.IRDA_EndTransmit_IT) refers to stm32f7xx_hal_irda.o(i.HAL_IRDA_TxCpltCallback) for HAL_IRDA_TxCpltCallback
    stm32f7xx_hal_irda.o(i.IRDA_Receive_IT) refers to stm32f7xx_hal_irda.o(i.HAL_IRDA_RxCpltCallback) for HAL_IRDA_RxCpltCallback
    stm32f7xx_hal_irda.o(i.IRDA_SetConfig) refers to stm32f7xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq) for HAL_RCC_GetPCLK1Freq
    stm32f7xx_hal_irda.o(i.IRDA_SetConfig) refers to stm32f7xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq) for HAL_RCC_GetPCLK2Freq
    stm32f7xx_hal_irda.o(i.IRDA_SetConfig) refers to stm32f7xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq) for HAL_RCC_GetSysClockFreq
    stm32f7xx_hal_irda.o(i.IRDA_WaitOnFlagUntilTimeout) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_iwdg.o(i.HAL_IWDG_Init) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_lptim.o(i.HAL_LPTIM_DeInit) refers to stm32f7xx_hal_lptim.o(i.HAL_LPTIM_MspDeInit) for HAL_LPTIM_MspDeInit
    stm32f7xx_hal_lptim.o(i.HAL_LPTIM_IRQHandler) refers to stm32f7xx_hal_lptim.o(i.HAL_LPTIM_CompareMatchCallback) for HAL_LPTIM_CompareMatchCallback
    stm32f7xx_hal_lptim.o(i.HAL_LPTIM_IRQHandler) refers to stm32f7xx_hal_lptim.o(i.HAL_LPTIM_AutoReloadMatchCallback) for HAL_LPTIM_AutoReloadMatchCallback
    stm32f7xx_hal_lptim.o(i.HAL_LPTIM_IRQHandler) refers to stm32f7xx_hal_lptim.o(i.HAL_LPTIM_TriggerCallback) for HAL_LPTIM_TriggerCallback
    stm32f7xx_hal_lptim.o(i.HAL_LPTIM_IRQHandler) refers to stm32f7xx_hal_lptim.o(i.HAL_LPTIM_CompareWriteCallback) for HAL_LPTIM_CompareWriteCallback
    stm32f7xx_hal_lptim.o(i.HAL_LPTIM_IRQHandler) refers to stm32f7xx_hal_lptim.o(i.HAL_LPTIM_AutoReloadWriteCallback) for HAL_LPTIM_AutoReloadWriteCallback
    stm32f7xx_hal_lptim.o(i.HAL_LPTIM_IRQHandler) refers to stm32f7xx_hal_lptim.o(i.HAL_LPTIM_DirectionUpCallback) for HAL_LPTIM_DirectionUpCallback
    stm32f7xx_hal_lptim.o(i.HAL_LPTIM_IRQHandler) refers to stm32f7xx_hal_lptim.o(i.HAL_LPTIM_DirectionDownCallback) for HAL_LPTIM_DirectionDownCallback
    stm32f7xx_hal_lptim.o(i.HAL_LPTIM_Init) refers to stm32f7xx_hal_lptim.o(i.HAL_LPTIM_MspInit) for HAL_LPTIM_MspInit
    stm32f7xx_hal_ltdc.o(i.HAL_LTDC_ConfigLayer) refers to memcpya.o(.text) for __aeabi_memcpy4
    stm32f7xx_hal_ltdc.o(i.HAL_LTDC_ConfigLayer) refers to stm32f7xx_hal_ltdc.o(i.LTDC_SetConfig) for LTDC_SetConfig
    stm32f7xx_hal_ltdc.o(i.HAL_LTDC_ConfigLayer_NoReload) refers to memcpya.o(.text) for __aeabi_memcpy4
    stm32f7xx_hal_ltdc.o(i.HAL_LTDC_ConfigLayer_NoReload) refers to stm32f7xx_hal_ltdc.o(i.LTDC_SetConfig) for LTDC_SetConfig
    stm32f7xx_hal_ltdc.o(i.HAL_LTDC_DeInit) refers to stm32f7xx_hal_ltdc.o(i.HAL_LTDC_MspDeInit) for HAL_LTDC_MspDeInit
    stm32f7xx_hal_ltdc.o(i.HAL_LTDC_IRQHandler) refers to stm32f7xx_hal_ltdc.o(i.HAL_LTDC_ErrorCallback) for HAL_LTDC_ErrorCallback
    stm32f7xx_hal_ltdc.o(i.HAL_LTDC_IRQHandler) refers to stm32f7xx_hal_ltdc.o(i.HAL_LTDC_LineEventCallback) for HAL_LTDC_LineEventCallback
    stm32f7xx_hal_ltdc.o(i.HAL_LTDC_IRQHandler) refers to stm32f7xx_hal_ltdc.o(i.HAL_LTDC_ReloadEventCallback) for HAL_LTDC_ReloadEventCallback
    stm32f7xx_hal_ltdc.o(i.HAL_LTDC_Init) refers to stm32f7xx_hal_ltdc.o(i.HAL_LTDC_MspInit) for HAL_LTDC_MspInit
    stm32f7xx_hal_ltdc.o(i.HAL_LTDC_SetAddress) refers to stm32f7xx_hal_ltdc.o(i.LTDC_SetConfig) for LTDC_SetConfig
    stm32f7xx_hal_ltdc.o(i.HAL_LTDC_SetAddress_NoReload) refers to stm32f7xx_hal_ltdc.o(i.LTDC_SetConfig) for LTDC_SetConfig
    stm32f7xx_hal_ltdc.o(i.HAL_LTDC_SetAlpha) refers to stm32f7xx_hal_ltdc.o(i.LTDC_SetConfig) for LTDC_SetConfig
    stm32f7xx_hal_ltdc.o(i.HAL_LTDC_SetAlpha_NoReload) refers to stm32f7xx_hal_ltdc.o(i.LTDC_SetConfig) for LTDC_SetConfig
    stm32f7xx_hal_ltdc.o(i.HAL_LTDC_SetPixelFormat) refers to stm32f7xx_hal_ltdc.o(i.LTDC_SetConfig) for LTDC_SetConfig
    stm32f7xx_hal_ltdc.o(i.HAL_LTDC_SetPixelFormat_NoReload) refers to stm32f7xx_hal_ltdc.o(i.LTDC_SetConfig) for LTDC_SetConfig
    stm32f7xx_hal_ltdc.o(i.HAL_LTDC_SetWindowPosition) refers to stm32f7xx_hal_ltdc.o(i.LTDC_SetConfig) for LTDC_SetConfig
    stm32f7xx_hal_ltdc.o(i.HAL_LTDC_SetWindowPosition_NoReload) refers to stm32f7xx_hal_ltdc.o(i.LTDC_SetConfig) for LTDC_SetConfig
    stm32f7xx_hal_ltdc.o(i.HAL_LTDC_SetWindowSize) refers to stm32f7xx_hal_ltdc.o(i.LTDC_SetConfig) for LTDC_SetConfig
    stm32f7xx_hal_ltdc.o(i.HAL_LTDC_SetWindowSize_NoReload) refers to stm32f7xx_hal_ltdc.o(i.LTDC_SetConfig) for LTDC_SetConfig
    stm32f7xx_hal_nand.o(i.HAL_NAND_DeInit) refers to stm32f7xx_hal_nand.o(i.HAL_NAND_MspDeInit) for HAL_NAND_MspDeInit
    stm32f7xx_hal_nand.o(i.HAL_NAND_DeInit) refers to stm32f7xx_ll_fmc.o(i.FMC_NAND_DeInit) for FMC_NAND_DeInit
    stm32f7xx_hal_nand.o(i.HAL_NAND_ECC_Disable) refers to stm32f7xx_ll_fmc.o(i.FMC_NAND_ECC_Disable) for FMC_NAND_ECC_Disable
    stm32f7xx_hal_nand.o(i.HAL_NAND_ECC_Enable) refers to stm32f7xx_ll_fmc.o(i.FMC_NAND_ECC_Enable) for FMC_NAND_ECC_Enable
    stm32f7xx_hal_nand.o(i.HAL_NAND_GetECC) refers to stm32f7xx_ll_fmc.o(i.FMC_NAND_GetECC) for FMC_NAND_GetECC
    stm32f7xx_hal_nand.o(i.HAL_NAND_IRQHandler) refers to stm32f7xx_hal_nand.o(i.HAL_NAND_ITCallback) for HAL_NAND_ITCallback
    stm32f7xx_hal_nand.o(i.HAL_NAND_Init) refers to stm32f7xx_hal_nand.o(i.HAL_NAND_MspInit) for HAL_NAND_MspInit
    stm32f7xx_hal_nand.o(i.HAL_NAND_Init) refers to stm32f7xx_ll_fmc.o(i.FMC_NAND_Init) for FMC_NAND_Init
    stm32f7xx_hal_nand.o(i.HAL_NAND_Init) refers to stm32f7xx_ll_fmc.o(i.FMC_NAND_CommonSpace_Timing_Init) for FMC_NAND_CommonSpace_Timing_Init
    stm32f7xx_hal_nand.o(i.HAL_NAND_Init) refers to stm32f7xx_ll_fmc.o(i.FMC_NAND_AttributeSpace_Timing_Init) for FMC_NAND_AttributeSpace_Timing_Init
    stm32f7xx_hal_nand.o(i.HAL_NAND_Write_Page_16b) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_nand.o(i.HAL_NAND_Write_Page_16b) refers to stm32f7xx_hal_nand.o(i.HAL_NAND_Read_Status) for HAL_NAND_Read_Status
    stm32f7xx_hal_nand.o(i.HAL_NAND_Write_Page_8b) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_nand.o(i.HAL_NAND_Write_Page_8b) refers to stm32f7xx_hal_nand.o(i.HAL_NAND_Read_Status) for HAL_NAND_Read_Status
    stm32f7xx_hal_nand.o(i.HAL_NAND_Write_SpareArea_16b) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_nand.o(i.HAL_NAND_Write_SpareArea_16b) refers to stm32f7xx_hal_nand.o(i.HAL_NAND_Read_Status) for HAL_NAND_Read_Status
    stm32f7xx_hal_nand.o(i.HAL_NAND_Write_SpareArea_8b) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_nand.o(i.HAL_NAND_Write_SpareArea_8b) refers to stm32f7xx_hal_nand.o(i.HAL_NAND_Read_Status) for HAL_NAND_Read_Status
    stm32f7xx_hal_nor.o(i.HAL_NOR_DeInit) refers to stm32f7xx_hal_nor.o(i.HAL_NOR_MspDeInit) for HAL_NOR_MspDeInit
    stm32f7xx_hal_nor.o(i.HAL_NOR_DeInit) refers to stm32f7xx_ll_fmc.o(i.FMC_NORSRAM_DeInit) for FMC_NORSRAM_DeInit
    stm32f7xx_hal_nor.o(i.HAL_NOR_Erase_Block) refers to stm32f7xx_hal_nor.o(.data) for .data
    stm32f7xx_hal_nor.o(i.HAL_NOR_Erase_Chip) refers to stm32f7xx_hal_nor.o(.data) for .data
    stm32f7xx_hal_nor.o(i.HAL_NOR_GetStatus) refers to stm32f7xx_hal_nor.o(i.HAL_NOR_MspWait) for HAL_NOR_MspWait
    stm32f7xx_hal_nor.o(i.HAL_NOR_GetStatus) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_nor.o(i.HAL_NOR_Init) refers to stm32f7xx_hal_nor.o(i.HAL_NOR_MspInit) for HAL_NOR_MspInit
    stm32f7xx_hal_nor.o(i.HAL_NOR_Init) refers to stm32f7xx_ll_fmc.o(i.FMC_NORSRAM_Init) for FMC_NORSRAM_Init
    stm32f7xx_hal_nor.o(i.HAL_NOR_Init) refers to stm32f7xx_ll_fmc.o(i.FMC_NORSRAM_Timing_Init) for FMC_NORSRAM_Timing_Init
    stm32f7xx_hal_nor.o(i.HAL_NOR_Init) refers to stm32f7xx_ll_fmc.o(i.FMC_NORSRAM_Extended_Timing_Init) for FMC_NORSRAM_Extended_Timing_Init
    stm32f7xx_hal_nor.o(i.HAL_NOR_Init) refers to stm32f7xx_hal_nor.o(.data) for .data
    stm32f7xx_hal_nor.o(i.HAL_NOR_Program) refers to stm32f7xx_hal_nor.o(.data) for .data
    stm32f7xx_hal_nor.o(i.HAL_NOR_ProgramBuffer) refers to stm32f7xx_hal_nor.o(.data) for .data
    stm32f7xx_hal_nor.o(i.HAL_NOR_Read) refers to stm32f7xx_hal_nor.o(.data) for .data
    stm32f7xx_hal_nor.o(i.HAL_NOR_ReadBuffer) refers to stm32f7xx_hal_nor.o(.data) for .data
    stm32f7xx_hal_nor.o(i.HAL_NOR_Read_CFI) refers to stm32f7xx_hal_nor.o(.data) for .data
    stm32f7xx_hal_nor.o(i.HAL_NOR_Read_ID) refers to stm32f7xx_hal_nor.o(.data) for .data
    stm32f7xx_hal_nor.o(i.HAL_NOR_WriteOperation_Disable) refers to stm32f7xx_ll_fmc.o(i.FMC_NORSRAM_WriteOperation_Disable) for FMC_NORSRAM_WriteOperation_Disable
    stm32f7xx_hal_nor.o(i.HAL_NOR_WriteOperation_Enable) refers to stm32f7xx_ll_fmc.o(i.FMC_NORSRAM_WriteOperation_Enable) for FMC_NORSRAM_WriteOperation_Enable
    stm32f7xx_hal_pcd.o(i.HAL_PCD_DeInit) refers to stm32f7xx_hal_pcd.o(i.HAL_PCD_Stop) for HAL_PCD_Stop
    stm32f7xx_hal_pcd.o(i.HAL_PCD_DeInit) refers to stm32f7xx_hal_pcd.o(i.HAL_PCD_MspDeInit) for HAL_PCD_MspDeInit
    stm32f7xx_hal_pcd.o(i.HAL_PCD_DevConnect) refers to stm32f7xx_ll_usb.o(i.USB_DevConnect) for USB_DevConnect
    stm32f7xx_hal_pcd.o(i.HAL_PCD_DevDisconnect) refers to stm32f7xx_ll_usb.o(i.USB_DevDisconnect) for USB_DevDisconnect
    stm32f7xx_hal_pcd.o(i.HAL_PCD_EP_Close) refers to stm32f7xx_ll_usb.o(i.USB_DeactivateEndpoint) for USB_DeactivateEndpoint
    stm32f7xx_hal_pcd.o(i.HAL_PCD_EP_ClrStall) refers to stm32f7xx_ll_usb.o(i.USB_EPClearStall) for USB_EPClearStall
    stm32f7xx_hal_pcd.o(i.HAL_PCD_EP_Flush) refers to stm32f7xx_ll_usb.o(i.USB_FlushTxFifo) for USB_FlushTxFifo
    stm32f7xx_hal_pcd.o(i.HAL_PCD_EP_Flush) refers to stm32f7xx_ll_usb.o(i.USB_FlushRxFifo) for USB_FlushRxFifo
    stm32f7xx_hal_pcd.o(i.HAL_PCD_EP_Open) refers to stm32f7xx_ll_usb.o(i.USB_ActivateEndpoint) for USB_ActivateEndpoint
    stm32f7xx_hal_pcd.o(i.HAL_PCD_EP_Receive) refers to stm32f7xx_ll_usb.o(i.USB_EPStartXfer) for USB_EPStartXfer
    stm32f7xx_hal_pcd.o(i.HAL_PCD_EP_Receive) refers to stm32f7xx_ll_usb.o(i.USB_EP0StartXfer) for USB_EP0StartXfer
    stm32f7xx_hal_pcd.o(i.HAL_PCD_EP_SetStall) refers to stm32f7xx_ll_usb.o(i.USB_EPSetStall) for USB_EPSetStall
    stm32f7xx_hal_pcd.o(i.HAL_PCD_EP_SetStall) refers to stm32f7xx_ll_usb.o(i.USB_EP0_OutStart) for USB_EP0_OutStart
    stm32f7xx_hal_pcd.o(i.HAL_PCD_EP_Transmit) refers to stm32f7xx_ll_usb.o(i.USB_EPStartXfer) for USB_EPStartXfer
    stm32f7xx_hal_pcd.o(i.HAL_PCD_EP_Transmit) refers to stm32f7xx_ll_usb.o(i.USB_EP0StartXfer) for USB_EP0StartXfer
    stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler) refers to stm32f7xx_ll_usb.o(i.USB_GetMode) for USB_GetMode
    stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler) refers to stm32f7xx_ll_usb.o(i.USB_ReadInterrupts) for USB_ReadInterrupts
    stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler) refers to stm32f7xx_ll_usb.o(i.USB_ReadDevAllOutEpInterrupt) for USB_ReadDevAllOutEpInterrupt
    stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler) refers to stm32f7xx_ll_usb.o(i.USB_ReadDevOutEPInterrupt) for USB_ReadDevOutEPInterrupt
    stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler) refers to stm32f7xx_hal_pcd.o(i.HAL_PCD_DataOutStageCallback) for HAL_PCD_DataOutStageCallback
    stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler) refers to stm32f7xx_ll_usb.o(i.USB_EP0_OutStart) for USB_EP0_OutStart
    stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler) refers to stm32f7xx_hal_pcd.o(i.HAL_PCD_SetupStageCallback) for HAL_PCD_SetupStageCallback
    stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler) refers to stm32f7xx_ll_usb.o(i.USB_ReadDevAllInEpInterrupt) for USB_ReadDevAllInEpInterrupt
    stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler) refers to stm32f7xx_ll_usb.o(i.USB_ReadDevInEPInterrupt) for USB_ReadDevInEPInterrupt
    stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler) refers to stm32f7xx_hal_pcd.o(i.HAL_PCD_DataInStageCallback) for HAL_PCD_DataInStageCallback
    stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler) refers to stm32f7xx_hal_pcd.o(i.PCD_WriteEmptyTxFifo) for PCD_WriteEmptyTxFifo
    stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler) refers to stm32f7xx_hal_pcd.o(i.HAL_PCD_ResumeCallback) for HAL_PCD_ResumeCallback
    stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler) refers to stm32f7xx_hal_pcd.o(i.HAL_PCD_SuspendCallback) for HAL_PCD_SuspendCallback
    stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler) refers to stm32f7xx_ll_usb.o(i.USB_FlushTxFifo) for USB_FlushTxFifo
    stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler) refers to stm32f7xx_hal_pcd_ex.o(i.HAL_PCDEx_LPM_Callback) for HAL_PCDEx_LPM_Callback
    stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler) refers to stm32f7xx_ll_usb.o(i.USB_ActivateSetup) for USB_ActivateSetup
    stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler) refers to stm32f7xx_ll_usb.o(i.USB_GetDevSpeed) for USB_GetDevSpeed
    stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler) refers to stm32f7xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq) for HAL_RCC_GetHCLKFreq
    stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler) refers to stm32f7xx_hal_pcd.o(i.HAL_PCD_ResetCallback) for HAL_PCD_ResetCallback
    stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler) refers to stm32f7xx_ll_usb.o(i.USB_ReadPacket) for USB_ReadPacket
    stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler) refers to stm32f7xx_hal_pcd.o(i.HAL_PCD_SOFCallback) for HAL_PCD_SOFCallback
    stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler) refers to stm32f7xx_hal_pcd.o(i.HAL_PCD_ISOINIncompleteCallback) for HAL_PCD_ISOINIncompleteCallback
    stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler) refers to stm32f7xx_hal_pcd.o(i.HAL_PCD_ISOOUTIncompleteCallback) for HAL_PCD_ISOOUTIncompleteCallback
    stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler) refers to stm32f7xx_hal_pcd.o(i.HAL_PCD_ConnectCallback) for HAL_PCD_ConnectCallback
    stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler) refers to stm32f7xx_hal_pcd.o(i.HAL_PCD_DisconnectCallback) for HAL_PCD_DisconnectCallback
    stm32f7xx_hal_pcd.o(i.HAL_PCD_Init) refers to stm32f7xx_hal_pcd.o(i.HAL_PCD_MspInit) for HAL_PCD_MspInit
    stm32f7xx_hal_pcd.o(i.HAL_PCD_Init) refers to stm32f7xx_ll_usb.o(i.USB_DisableGlobalInt) for USB_DisableGlobalInt
    stm32f7xx_hal_pcd.o(i.HAL_PCD_Init) refers to memcpya.o(.text) for __aeabi_memcpy4
    stm32f7xx_hal_pcd.o(i.HAL_PCD_Init) refers to stm32f7xx_ll_usb.o(i.USB_CoreInit) for USB_CoreInit
    stm32f7xx_hal_pcd.o(i.HAL_PCD_Init) refers to stm32f7xx_ll_usb.o(i.USB_SetCurrentMode) for USB_SetCurrentMode
    stm32f7xx_hal_pcd.o(i.HAL_PCD_Init) refers to stm32f7xx_ll_usb.o(i.USB_DevInit) for USB_DevInit
    stm32f7xx_hal_pcd.o(i.HAL_PCD_Init) refers to stm32f7xx_hal_pcd_ex.o(i.HAL_PCDEx_ActivateLPM) for HAL_PCDEx_ActivateLPM
    stm32f7xx_hal_pcd.o(i.HAL_PCD_Init) refers to stm32f7xx_ll_usb.o(i.USB_DevDisconnect) for USB_DevDisconnect
    stm32f7xx_hal_pcd.o(i.HAL_PCD_SetAddress) refers to stm32f7xx_ll_usb.o(i.USB_SetDevAddress) for USB_SetDevAddress
    stm32f7xx_hal_pcd.o(i.HAL_PCD_Start) refers to stm32f7xx_ll_usb.o(i.USB_DevConnect) for USB_DevConnect
    stm32f7xx_hal_pcd.o(i.HAL_PCD_Start) refers to stm32f7xx_ll_usb.o(i.USB_EnableGlobalInt) for USB_EnableGlobalInt
    stm32f7xx_hal_pcd.o(i.HAL_PCD_Stop) refers to stm32f7xx_ll_usb.o(i.USB_DisableGlobalInt) for USB_DisableGlobalInt
    stm32f7xx_hal_pcd.o(i.HAL_PCD_Stop) refers to stm32f7xx_ll_usb.o(i.USB_StopDevice) for USB_StopDevice
    stm32f7xx_hal_pcd.o(i.HAL_PCD_Stop) refers to stm32f7xx_ll_usb.o(i.USB_DevDisconnect) for USB_DevDisconnect
    stm32f7xx_hal_pcd.o(i.PCD_WriteEmptyTxFifo) refers to stm32f7xx_ll_usb.o(i.USB_WritePacket) for USB_WritePacket
    stm32f7xx_hal_pwr.o(i.HAL_PWR_PVD_IRQHandler) refers to stm32f7xx_hal_pwr.o(i.HAL_PWR_PVDCallback) for HAL_PWR_PVDCallback
    stm32f7xx_hal_pwr_ex.o(i.HAL_PWREx_ControlVoltageScaling) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_pwr_ex.o(i.HAL_PWREx_DisableBkUpReg) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_pwr_ex.o(i.HAL_PWREx_DisableOverDrive) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_pwr_ex.o(i.HAL_PWREx_EnableBkUpReg) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_pwr_ex.o(i.HAL_PWREx_EnableOverDrive) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_pwr_ex.o(i.HAL_PWREx_EnterUnderDriveSTOPMode) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Abort) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Abort) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Abort) refers to stm32f7xx_hal_qspi.o(i.QSPI_WaitFlagStateUntilTimeout) for QSPI_WaitFlagStateUntilTimeout
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Abort_IT) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Abort_IT) refers to stm32f7xx_hal_qspi.o(i.QSPI_DMAAbortCplt) for QSPI_DMAAbortCplt
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_AutoPolling) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_AutoPolling) refers to stm32f7xx_hal_qspi.o(i.QSPI_WaitFlagStateUntilTimeout) for QSPI_WaitFlagStateUntilTimeout
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_AutoPolling) refers to stm32f7xx_hal_qspi.o(i.QSPI_Config) for QSPI_Config
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_AutoPolling_IT) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_AutoPolling_IT) refers to stm32f7xx_hal_qspi.o(i.QSPI_WaitFlagStateUntilTimeout) for QSPI_WaitFlagStateUntilTimeout
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_AutoPolling_IT) refers to stm32f7xx_hal_qspi.o(i.QSPI_Config) for QSPI_Config
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Command) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Command) refers to stm32f7xx_hal_qspi.o(i.QSPI_WaitFlagStateUntilTimeout) for QSPI_WaitFlagStateUntilTimeout
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Command) refers to stm32f7xx_hal_qspi.o(i.QSPI_Config) for QSPI_Config
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Command_IT) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Command_IT) refers to stm32f7xx_hal_qspi.o(i.QSPI_WaitFlagStateUntilTimeout) for QSPI_WaitFlagStateUntilTimeout
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Command_IT) refers to stm32f7xx_hal_qspi.o(i.QSPI_Config) for QSPI_Config
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_DeInit) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_MspDeInit) for HAL_QSPI_MspDeInit
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_IRQHandler) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_FifoThresholdCallback) for HAL_QSPI_FifoThresholdCallback
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_IRQHandler) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_ErrorCallback) for HAL_QSPI_ErrorCallback
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_IRQHandler) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_TxCpltCallback) for HAL_QSPI_TxCpltCallback
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_IRQHandler) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_RxCpltCallback) for HAL_QSPI_RxCpltCallback
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_IRQHandler) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_CmdCpltCallback) for HAL_QSPI_CmdCpltCallback
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_IRQHandler) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_AbortCpltCallback) for HAL_QSPI_AbortCpltCallback
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_IRQHandler) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_StatusMatchCallback) for HAL_QSPI_StatusMatchCallback
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_IRQHandler) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_IRQHandler) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_TimeOutCallback) for HAL_QSPI_TimeOutCallback
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_IRQHandler) refers to stm32f7xx_hal_qspi.o(i.QSPI_DMAAbortCplt) for QSPI_DMAAbortCplt
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Init) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Init) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_MspInit) for HAL_QSPI_MspInit
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Init) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_SetTimeout) for HAL_QSPI_SetTimeout
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Init) refers to stm32f7xx_hal_qspi.o(i.QSPI_WaitFlagStateUntilTimeout) for QSPI_WaitFlagStateUntilTimeout
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_MemoryMapped) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_MemoryMapped) refers to stm32f7xx_hal_qspi.o(i.QSPI_WaitFlagStateUntilTimeout) for QSPI_WaitFlagStateUntilTimeout
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_MemoryMapped) refers to stm32f7xx_hal_qspi.o(i.QSPI_Config) for QSPI_Config
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Receive) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Receive) refers to stm32f7xx_hal_qspi.o(i.QSPI_WaitFlagStateUntilTimeout) for QSPI_WaitFlagStateUntilTimeout
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Receive_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Receive_DMA) refers to stm32f7xx_hal_qspi.o(i.QSPI_DMARxCplt) for QSPI_DMARxCplt
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Receive_DMA) refers to stm32f7xx_hal_qspi.o(i.QSPI_DMARxHalfCplt) for QSPI_DMARxHalfCplt
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Receive_DMA) refers to stm32f7xx_hal_qspi.o(i.QSPI_DMAError) for QSPI_DMAError
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Transmit) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Transmit) refers to stm32f7xx_hal_qspi.o(i.QSPI_WaitFlagStateUntilTimeout) for QSPI_WaitFlagStateUntilTimeout
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Transmit_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Transmit_DMA) refers to stm32f7xx_hal_qspi.o(i.QSPI_DMATxCplt) for QSPI_DMATxCplt
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Transmit_DMA) refers to stm32f7xx_hal_qspi.o(i.QSPI_DMATxHalfCplt) for QSPI_DMATxHalfCplt
    stm32f7xx_hal_qspi.o(i.HAL_QSPI_Transmit_DMA) refers to stm32f7xx_hal_qspi.o(i.QSPI_DMAError) for QSPI_DMAError
    stm32f7xx_hal_qspi.o(i.QSPI_DMAAbortCplt) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_ErrorCallback) for HAL_QSPI_ErrorCallback
    stm32f7xx_hal_qspi.o(i.QSPI_DMAError) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_GetError) for HAL_DMA_GetError
    stm32f7xx_hal_qspi.o(i.QSPI_DMAError) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_Abort_IT) for HAL_QSPI_Abort_IT
    stm32f7xx_hal_qspi.o(i.QSPI_DMARxHalfCplt) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_RxHalfCpltCallback) for HAL_QSPI_RxHalfCpltCallback
    stm32f7xx_hal_qspi.o(i.QSPI_DMATxHalfCplt) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_TxHalfCpltCallback) for HAL_QSPI_TxHalfCpltCallback
    stm32f7xx_hal_qspi.o(i.QSPI_WaitFlagStateUntilTimeout) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_rcc.o(i.HAL_RCC_ClockConfig) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_rcc.o(i.HAL_RCC_ClockConfig) refers to stm32f7xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq) for HAL_RCC_GetSysClockFreq
    stm32f7xx_hal_rcc.o(i.HAL_RCC_ClockConfig) refers to stm32f7xx_hal.o(i.HAL_InitTick) for HAL_InitTick
    stm32f7xx_hal_rcc.o(i.HAL_RCC_ClockConfig) refers to system_stm32f7xx.o(.constdata) for AHBPrescTable
    stm32f7xx_hal_rcc.o(i.HAL_RCC_ClockConfig) refers to system_stm32f7xx.o(.data) for SystemCoreClock
    stm32f7xx_hal_rcc.o(i.HAL_RCC_DeInit) refers to system_stm32f7xx.o(.data) for SystemCoreClock
    stm32f7xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq) refers to system_stm32f7xx.o(.data) for SystemCoreClock
    stm32f7xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq) refers to stm32f7xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq) for HAL_RCC_GetHCLKFreq
    stm32f7xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq) refers to system_stm32f7xx.o(.constdata) for APBPrescTable
    stm32f7xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq) refers to stm32f7xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq) for HAL_RCC_GetHCLKFreq
    stm32f7xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq) refers to system_stm32f7xx.o(.constdata) for APBPrescTable
    stm32f7xx_hal_rcc.o(i.HAL_RCC_MCOConfig) refers to stm32f7xx_hal_gpio.o(i.HAL_GPIO_Init) for HAL_GPIO_Init
    stm32f7xx_hal_rcc.o(i.HAL_RCC_NMI_IRQHandler) refers to stm32f7xx_hal_rcc.o(i.HAL_RCC_CSSCallback) for HAL_RCC_CSSCallback
    stm32f7xx_hal_rcc.o(i.HAL_RCC_OscConfig) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_rng.o(i.HAL_RNG_DeInit) refers to stm32f7xx_hal_rng.o(i.HAL_RNG_MspDeInit) for HAL_RNG_MspDeInit
    stm32f7xx_hal_rng.o(i.HAL_RNG_GenerateRandomNumber) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_rng.o(i.HAL_RNG_GetRandomNumber) refers to stm32f7xx_hal_rng.o(i.HAL_RNG_GenerateRandomNumber) for HAL_RNG_GenerateRandomNumber
    stm32f7xx_hal_rng.o(i.HAL_RNG_IRQHandler) refers to stm32f7xx_hal_rng.o(i.HAL_RNG_ErrorCallback) for HAL_RNG_ErrorCallback
    stm32f7xx_hal_rng.o(i.HAL_RNG_IRQHandler) refers to stm32f7xx_hal_rng.o(i.HAL_RNG_ReadyDataCallback) for HAL_RNG_ReadyDataCallback
    stm32f7xx_hal_rng.o(i.HAL_RNG_Init) refers to stm32f7xx_hal_rng.o(i.HAL_RNG_MspInit) for HAL_RNG_MspInit
    stm32f7xx_hal_rtc.o(i.HAL_RTC_AlarmIRQHandler) refers to stm32f7xx_hal_rtc.o(i.HAL_RTC_AlarmAEventCallback) for HAL_RTC_AlarmAEventCallback
    stm32f7xx_hal_rtc.o(i.HAL_RTC_AlarmIRQHandler) refers to stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_AlarmBEventCallback) for HAL_RTCEx_AlarmBEventCallback
    stm32f7xx_hal_rtc.o(i.HAL_RTC_DeInit) refers to stm32f7xx_hal_rtc.o(i.RTC_EnterInitMode) for RTC_EnterInitMode
    stm32f7xx_hal_rtc.o(i.HAL_RTC_DeInit) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_rtc.o(i.HAL_RTC_DeInit) refers to stm32f7xx_hal_rtc.o(i.HAL_RTC_WaitForSynchro) for HAL_RTC_WaitForSynchro
    stm32f7xx_hal_rtc.o(i.HAL_RTC_DeInit) refers to stm32f7xx_hal_rtc.o(i.HAL_RTC_MspDeInit) for HAL_RTC_MspDeInit
    stm32f7xx_hal_rtc.o(i.HAL_RTC_DeactivateAlarm) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_rtc.o(i.HAL_RTC_GetAlarm) refers to stm32f7xx_hal_rtc.o(i.RTC_Bcd2ToByte) for RTC_Bcd2ToByte
    stm32f7xx_hal_rtc.o(i.HAL_RTC_GetDate) refers to stm32f7xx_hal_rtc.o(i.RTC_Bcd2ToByte) for RTC_Bcd2ToByte
    stm32f7xx_hal_rtc.o(i.HAL_RTC_GetTime) refers to stm32f7xx_hal_rtc.o(i.RTC_Bcd2ToByte) for RTC_Bcd2ToByte
    stm32f7xx_hal_rtc.o(i.HAL_RTC_Init) refers to stm32f7xx_hal_rtc.o(i.HAL_RTC_MspInit) for HAL_RTC_MspInit
    stm32f7xx_hal_rtc.o(i.HAL_RTC_Init) refers to stm32f7xx_hal_rtc.o(i.RTC_EnterInitMode) for RTC_EnterInitMode
    stm32f7xx_hal_rtc.o(i.HAL_RTC_PollForAlarmAEvent) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_rtc.o(i.HAL_RTC_SetAlarm) refers to stm32f7xx_hal_rtc.o(i.RTC_Bcd2ToByte) for RTC_Bcd2ToByte
    stm32f7xx_hal_rtc.o(i.HAL_RTC_SetAlarm) refers to stm32f7xx_hal_rtc.o(i.RTC_ByteToBcd2) for RTC_ByteToBcd2
    stm32f7xx_hal_rtc.o(i.HAL_RTC_SetAlarm) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_rtc.o(i.HAL_RTC_SetAlarm_IT) refers to stm32f7xx_hal_rtc.o(i.RTC_Bcd2ToByte) for RTC_Bcd2ToByte
    stm32f7xx_hal_rtc.o(i.HAL_RTC_SetAlarm_IT) refers to stm32f7xx_hal_rtc.o(i.RTC_ByteToBcd2) for RTC_ByteToBcd2
    stm32f7xx_hal_rtc.o(i.HAL_RTC_SetAlarm_IT) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_rtc.o(i.HAL_RTC_SetDate) refers to stm32f7xx_hal_rtc.o(i.RTC_Bcd2ToByte) for RTC_Bcd2ToByte
    stm32f7xx_hal_rtc.o(i.HAL_RTC_SetDate) refers to stm32f7xx_hal_rtc.o(i.RTC_EnterInitMode) for RTC_EnterInitMode
    stm32f7xx_hal_rtc.o(i.HAL_RTC_SetDate) refers to stm32f7xx_hal_rtc.o(i.RTC_ByteToBcd2) for RTC_ByteToBcd2
    stm32f7xx_hal_rtc.o(i.HAL_RTC_SetDate) refers to stm32f7xx_hal_rtc.o(i.HAL_RTC_WaitForSynchro) for HAL_RTC_WaitForSynchro
    stm32f7xx_hal_rtc.o(i.HAL_RTC_SetTime) refers to stm32f7xx_hal_rtc.o(i.RTC_Bcd2ToByte) for RTC_Bcd2ToByte
    stm32f7xx_hal_rtc.o(i.HAL_RTC_SetTime) refers to stm32f7xx_hal_rtc.o(i.RTC_ByteToBcd2) for RTC_ByteToBcd2
    stm32f7xx_hal_rtc.o(i.HAL_RTC_SetTime) refers to stm32f7xx_hal_rtc.o(i.RTC_EnterInitMode) for RTC_EnterInitMode
    stm32f7xx_hal_rtc.o(i.HAL_RTC_SetTime) refers to stm32f7xx_hal_rtc.o(i.HAL_RTC_WaitForSynchro) for HAL_RTC_WaitForSynchro
    stm32f7xx_hal_rtc.o(i.HAL_RTC_WaitForSynchro) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_rtc.o(i.RTC_EnterInitMode) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_DeactivateRefClock) refers to stm32f7xx_hal_rtc.o(i.RTC_EnterInitMode) for RTC_EnterInitMode
    stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_DeactivateWakeUpTimer) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_GetTimeStamp) refers to stm32f7xx_hal_rtc.o(i.RTC_Bcd2ToByte) for RTC_Bcd2ToByte
    stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_PollForAlarmBEvent) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_PollForTamper1Event) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_PollForTamper2Event) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_PollForTamper3Event) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_PollForTimeStampEvent) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_PollForWakeUpTimerEvent) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_SetRefClock) refers to stm32f7xx_hal_rtc.o(i.RTC_EnterInitMode) for RTC_EnterInitMode
    stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_SetSmoothCalib) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_SetSynchroShift) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_SetSynchroShift) refers to stm32f7xx_hal_rtc.o(i.HAL_RTC_WaitForSynchro) for HAL_RTC_WaitForSynchro
    stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_SetWakeUpTimer) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_SetWakeUpTimer_IT) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_TamperTimeStampIRQHandler) refers to stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_TimeStampEventCallback) for HAL_RTCEx_TimeStampEventCallback
    stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_TamperTimeStampIRQHandler) refers to stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_Tamper1EventCallback) for HAL_RTCEx_Tamper1EventCallback
    stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_TamperTimeStampIRQHandler) refers to stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_Tamper2EventCallback) for HAL_RTCEx_Tamper2EventCallback
    stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_TamperTimeStampIRQHandler) refers to stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_Tamper3EventCallback) for HAL_RTCEx_Tamper3EventCallback
    stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_WakeUpTimerIRQHandler) refers to stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_WakeUpTimerEventCallback) for HAL_RTCEx_WakeUpTimerEventCallback
    stm32f7xx_hal_sai.o(i.HAL_SAI_Abort) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f7xx_hal_sai.o(i.HAL_SAI_Abort) refers to stm32f7xx_hal_sai.o(i.SAI_Disable) for SAI_Disable
    stm32f7xx_hal_sai.o(i.HAL_SAI_DMAStop) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f7xx_hal_sai.o(i.HAL_SAI_DMAStop) refers to stm32f7xx_hal_sai.o(i.SAI_Disable) for SAI_Disable
    stm32f7xx_hal_sai.o(i.HAL_SAI_DeInit) refers to stm32f7xx_hal_sai.o(i.SAI_Disable) for SAI_Disable
    stm32f7xx_hal_sai.o(i.HAL_SAI_DeInit) refers to stm32f7xx_hal_sai.o(i.HAL_SAI_MspDeInit) for HAL_SAI_MspDeInit
    stm32f7xx_hal_sai.o(i.HAL_SAI_IRQHandler) refers to stm32f7xx_hal_sai.o(i.HAL_SAI_ErrorCallback) for HAL_SAI_ErrorCallback
    stm32f7xx_hal_sai.o(i.HAL_SAI_IRQHandler) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32f7xx_hal_sai.o(i.HAL_SAI_IRQHandler) refers to stm32f7xx_hal_sai.o(i.HAL_SAI_Abort) for HAL_SAI_Abort
    stm32f7xx_hal_sai.o(i.HAL_SAI_IRQHandler) refers to stm32f7xx_hal_sai.o(i.SAI_DMAAbort) for SAI_DMAAbort
    stm32f7xx_hal_sai.o(i.HAL_SAI_Init) refers to stm32f7xx_hal_sai.o(i.HAL_SAI_MspInit) for HAL_SAI_MspInit
    stm32f7xx_hal_sai.o(i.HAL_SAI_Init) refers to stm32f7xx_hal_sai.o(i.SAI_Disable) for SAI_Disable
    stm32f7xx_hal_sai.o(i.HAL_SAI_Init) refers to stm32f7xx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq) for HAL_RCCEx_GetPeriphCLKFreq
    stm32f7xx_hal_sai.o(i.HAL_SAI_InitProtocol) refers to stm32f7xx_hal_sai.o(i.SAI_InitI2S) for SAI_InitI2S
    stm32f7xx_hal_sai.o(i.HAL_SAI_InitProtocol) refers to stm32f7xx_hal_sai.o(i.SAI_InitPCM) for SAI_InitPCM
    stm32f7xx_hal_sai.o(i.HAL_SAI_InitProtocol) refers to stm32f7xx_hal_sai.o(i.HAL_SAI_Init) for HAL_SAI_Init
    stm32f7xx_hal_sai.o(i.HAL_SAI_Receive) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_sai.o(i.HAL_SAI_Receive) refers to stm32f7xx_hal_sai.o(i.SAI_Disable) for SAI_Disable
    stm32f7xx_hal_sai.o(i.HAL_SAI_Receive_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_sai.o(i.HAL_SAI_Receive_DMA) refers to stm32f7xx_hal_sai.o(i.SAI_InterruptFlag) for SAI_InterruptFlag
    stm32f7xx_hal_sai.o(i.HAL_SAI_Receive_DMA) refers to stm32f7xx_hal_sai.o(i.SAI_DMARxHalfCplt) for SAI_DMARxHalfCplt
    stm32f7xx_hal_sai.o(i.HAL_SAI_Receive_DMA) refers to stm32f7xx_hal_sai.o(i.SAI_DMARxCplt) for SAI_DMARxCplt
    stm32f7xx_hal_sai.o(i.HAL_SAI_Receive_DMA) refers to stm32f7xx_hal_sai.o(i.SAI_DMAError) for SAI_DMAError
    stm32f7xx_hal_sai.o(i.HAL_SAI_Receive_IT) refers to stm32f7xx_hal_sai.o(i.SAI_InterruptFlag) for SAI_InterruptFlag
    stm32f7xx_hal_sai.o(i.HAL_SAI_Receive_IT) refers to stm32f7xx_hal_sai.o(i.SAI_Receive_IT16Bit) for SAI_Receive_IT16Bit
    stm32f7xx_hal_sai.o(i.HAL_SAI_Receive_IT) refers to stm32f7xx_hal_sai.o(i.SAI_Receive_IT8Bit) for SAI_Receive_IT8Bit
    stm32f7xx_hal_sai.o(i.HAL_SAI_Receive_IT) refers to stm32f7xx_hal_sai.o(i.SAI_Receive_IT32Bit) for SAI_Receive_IT32Bit
    stm32f7xx_hal_sai.o(i.HAL_SAI_Transmit) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_sai.o(i.HAL_SAI_Transmit) refers to stm32f7xx_hal_sai.o(i.SAI_FillFifo) for SAI_FillFifo
    stm32f7xx_hal_sai.o(i.HAL_SAI_Transmit) refers to stm32f7xx_hal_sai.o(i.SAI_Disable) for SAI_Disable
    stm32f7xx_hal_sai.o(i.HAL_SAI_Transmit_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_sai.o(i.HAL_SAI_Transmit_DMA) refers to stm32f7xx_hal_sai.o(i.SAI_InterruptFlag) for SAI_InterruptFlag
    stm32f7xx_hal_sai.o(i.HAL_SAI_Transmit_DMA) refers to stm32f7xx_hal_sai.o(i.SAI_DMATxHalfCplt) for SAI_DMATxHalfCplt
    stm32f7xx_hal_sai.o(i.HAL_SAI_Transmit_DMA) refers to stm32f7xx_hal_sai.o(i.SAI_DMATxCplt) for SAI_DMATxCplt
    stm32f7xx_hal_sai.o(i.HAL_SAI_Transmit_DMA) refers to stm32f7xx_hal_sai.o(i.SAI_DMAError) for SAI_DMAError
    stm32f7xx_hal_sai.o(i.HAL_SAI_Transmit_IT) refers to stm32f7xx_hal_sai.o(i.SAI_FillFifo) for SAI_FillFifo
    stm32f7xx_hal_sai.o(i.HAL_SAI_Transmit_IT) refers to stm32f7xx_hal_sai.o(i.SAI_InterruptFlag) for SAI_InterruptFlag
    stm32f7xx_hal_sai.o(i.HAL_SAI_Transmit_IT) refers to stm32f7xx_hal_sai.o(i.SAI_Transmit_IT16Bit) for SAI_Transmit_IT16Bit
    stm32f7xx_hal_sai.o(i.HAL_SAI_Transmit_IT) refers to stm32f7xx_hal_sai.o(i.SAI_Transmit_IT8Bit) for SAI_Transmit_IT8Bit
    stm32f7xx_hal_sai.o(i.HAL_SAI_Transmit_IT) refers to stm32f7xx_hal_sai.o(i.SAI_Transmit_IT32Bit) for SAI_Transmit_IT32Bit
    stm32f7xx_hal_sai.o(i.SAI_DMAAbort) refers to stm32f7xx_hal_sai.o(i.SAI_Disable) for SAI_Disable
    stm32f7xx_hal_sai.o(i.SAI_DMAAbort) refers to stm32f7xx_hal_sai.o(i.HAL_SAI_ErrorCallback) for HAL_SAI_ErrorCallback
    stm32f7xx_hal_sai.o(i.SAI_DMAError) refers to stm32f7xx_hal_sai.o(i.SAI_Disable) for SAI_Disable
    stm32f7xx_hal_sai.o(i.SAI_DMAError) refers to stm32f7xx_hal_sai.o(i.HAL_SAI_ErrorCallback) for HAL_SAI_ErrorCallback
    stm32f7xx_hal_sai.o(i.SAI_DMARxCplt) refers to stm32f7xx_hal_sai.o(i.SAI_InterruptFlag) for SAI_InterruptFlag
    stm32f7xx_hal_sai.o(i.SAI_DMARxCplt) refers to stm32f7xx_hal_sai.o(i.HAL_SAI_RxCpltCallback) for HAL_SAI_RxCpltCallback
    stm32f7xx_hal_sai.o(i.SAI_DMARxHalfCplt) refers to stm32f7xx_hal_sai.o(i.HAL_SAI_RxHalfCpltCallback) for HAL_SAI_RxHalfCpltCallback
    stm32f7xx_hal_sai.o(i.SAI_DMATxCplt) refers to stm32f7xx_hal_sai.o(i.SAI_InterruptFlag) for SAI_InterruptFlag
    stm32f7xx_hal_sai.o(i.SAI_DMATxCplt) refers to stm32f7xx_hal_sai.o(i.HAL_SAI_TxCpltCallback) for HAL_SAI_TxCpltCallback
    stm32f7xx_hal_sai.o(i.SAI_DMATxHalfCplt) refers to stm32f7xx_hal_sai.o(i.HAL_SAI_TxHalfCpltCallback) for HAL_SAI_TxHalfCpltCallback
    stm32f7xx_hal_sai.o(i.SAI_Disable) refers to system_stm32f7xx.o(.data) for SystemCoreClock
    stm32f7xx_hal_sai.o(i.SAI_Receive_IT16Bit) refers to stm32f7xx_hal_sai.o(i.SAI_InterruptFlag) for SAI_InterruptFlag
    stm32f7xx_hal_sai.o(i.SAI_Receive_IT16Bit) refers to stm32f7xx_hal_sai.o(i.HAL_SAI_RxCpltCallback) for HAL_SAI_RxCpltCallback
    stm32f7xx_hal_sai.o(i.SAI_Receive_IT32Bit) refers to stm32f7xx_hal_sai.o(i.SAI_InterruptFlag) for SAI_InterruptFlag
    stm32f7xx_hal_sai.o(i.SAI_Receive_IT32Bit) refers to stm32f7xx_hal_sai.o(i.HAL_SAI_RxCpltCallback) for HAL_SAI_RxCpltCallback
    stm32f7xx_hal_sai.o(i.SAI_Receive_IT8Bit) refers to stm32f7xx_hal_sai.o(i.SAI_InterruptFlag) for SAI_InterruptFlag
    stm32f7xx_hal_sai.o(i.SAI_Receive_IT8Bit) refers to stm32f7xx_hal_sai.o(i.HAL_SAI_RxCpltCallback) for HAL_SAI_RxCpltCallback
    stm32f7xx_hal_sai.o(i.SAI_Transmit_IT16Bit) refers to stm32f7xx_hal_sai.o(i.SAI_InterruptFlag) for SAI_InterruptFlag
    stm32f7xx_hal_sai.o(i.SAI_Transmit_IT16Bit) refers to stm32f7xx_hal_sai.o(i.HAL_SAI_TxCpltCallback) for HAL_SAI_TxCpltCallback
    stm32f7xx_hal_sai.o(i.SAI_Transmit_IT32Bit) refers to stm32f7xx_hal_sai.o(i.SAI_InterruptFlag) for SAI_InterruptFlag
    stm32f7xx_hal_sai.o(i.SAI_Transmit_IT32Bit) refers to stm32f7xx_hal_sai.o(i.HAL_SAI_TxCpltCallback) for HAL_SAI_TxCpltCallback
    stm32f7xx_hal_sai.o(i.SAI_Transmit_IT8Bit) refers to stm32f7xx_hal_sai.o(i.SAI_InterruptFlag) for SAI_InterruptFlag
    stm32f7xx_hal_sai.o(i.SAI_Transmit_IT8Bit) refers to stm32f7xx_hal_sai.o(i.HAL_SAI_TxCpltCallback) for HAL_SAI_TxCpltCallback
    stm32f7xx_hal_sd.o(i.HAL_SD_CheckReadOperation) refers to stm32f7xx_hal_sd.o(i.HAL_SD_StopTransfer) for HAL_SD_StopTransfer
    stm32f7xx_hal_sd.o(i.HAL_SD_CheckWriteOperation) refers to stm32f7xx_hal_sd.o(i.HAL_SD_StopTransfer) for HAL_SD_StopTransfer
    stm32f7xx_hal_sd.o(i.HAL_SD_CheckWriteOperation) refers to stm32f7xx_hal_sd.o(i.HAL_SD_GetStatus) for HAL_SD_GetStatus
    stm32f7xx_hal_sd.o(i.HAL_SD_DeInit) refers to stm32f7xx_hal_sd.o(i.SD_PowerOFF) for SD_PowerOFF
    stm32f7xx_hal_sd.o(i.HAL_SD_DeInit) refers to stm32f7xx_hal_sd.o(i.HAL_SD_MspDeInit) for HAL_SD_MspDeInit
    stm32f7xx_hal_sd.o(i.HAL_SD_Erase) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_GetResponse) for SDMMC_GetResponse
    stm32f7xx_hal_sd.o(i.HAL_SD_Erase) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_SendCommand) for SDMMC_SendCommand
    stm32f7xx_hal_sd.o(i.HAL_SD_Erase) refers to stm32f7xx_hal_sd.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    stm32f7xx_hal_sd.o(i.HAL_SD_Erase) refers to stm32f7xx_hal_sd.o(i.SD_IsCardProgramming) for SD_IsCardProgramming
    stm32f7xx_hal_sd.o(i.HAL_SD_GetCardStatus) refers to stm32f7xx_hal_sd.o(i.HAL_SD_SendSDStatus) for HAL_SD_SendSDStatus
    stm32f7xx_hal_sd.o(i.HAL_SD_GetStatus) refers to stm32f7xx_hal_sd.o(i.SD_GetState) for SD_GetState
    stm32f7xx_hal_sd.o(i.HAL_SD_HighSpeed) refers to memseta.o(.text) for __aeabi_memclr4
    stm32f7xx_hal_sd.o(i.HAL_SD_HighSpeed) refers to stm32f7xx_hal_sd.o(i.SD_FindSCR) for SD_FindSCR
    stm32f7xx_hal_sd.o(i.HAL_SD_HighSpeed) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_SendCommand) for SDMMC_SendCommand
    stm32f7xx_hal_sd.o(i.HAL_SD_HighSpeed) refers to stm32f7xx_hal_sd.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    stm32f7xx_hal_sd.o(i.HAL_SD_HighSpeed) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_DataConfig) for SDMMC_DataConfig
    stm32f7xx_hal_sd.o(i.HAL_SD_HighSpeed) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_ReadFIFO) for SDMMC_ReadFIFO
    stm32f7xx_hal_sd.o(i.HAL_SD_IRQHandler) refers to stm32f7xx_hal_sd.o(i.HAL_SD_XferCpltCallback) for HAL_SD_XferCpltCallback
    stm32f7xx_hal_sd.o(i.HAL_SD_IRQHandler) refers to stm32f7xx_hal_sd.o(i.HAL_SD_XferErrorCallback) for HAL_SD_XferErrorCallback
    stm32f7xx_hal_sd.o(i.HAL_SD_Init) refers to stm32f7xx_hal_sd.o(i.HAL_SD_MspInit) for HAL_SD_MspInit
    stm32f7xx_hal_sd.o(i.HAL_SD_Init) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_Init) for SDMMC_Init
    stm32f7xx_hal_sd.o(i.HAL_SD_Init) refers to stm32f7xx_hal_sd.o(i.SD_PowerON) for SD_PowerON
    stm32f7xx_hal_sd.o(i.HAL_SD_Init) refers to stm32f7xx_hal_sd.o(i.SD_Initialize_Cards) for SD_Initialize_Cards
    stm32f7xx_hal_sd.o(i.HAL_SD_Init) refers to stm32f7xx_hal_sd.o(i.HAL_SD_Get_CardInfo) for HAL_SD_Get_CardInfo
    stm32f7xx_hal_sd.o(i.HAL_SD_Init) refers to stm32f7xx_hal_sd.o(i.SD_Select_Deselect) for SD_Select_Deselect
    stm32f7xx_hal_sd.o(i.HAL_SD_ReadBlocks) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_SendCommand) for SDMMC_SendCommand
    stm32f7xx_hal_sd.o(i.HAL_SD_ReadBlocks) refers to stm32f7xx_hal_sd.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    stm32f7xx_hal_sd.o(i.HAL_SD_ReadBlocks) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_DataConfig) for SDMMC_DataConfig
    stm32f7xx_hal_sd.o(i.HAL_SD_ReadBlocks) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_ReadFIFO) for SDMMC_ReadFIFO
    stm32f7xx_hal_sd.o(i.HAL_SD_ReadBlocks) refers to stm32f7xx_hal_sd.o(i.HAL_SD_StopTransfer) for HAL_SD_StopTransfer
    stm32f7xx_hal_sd.o(i.HAL_SD_ReadBlocks_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_sd.o(i.HAL_SD_ReadBlocks_DMA) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_SendCommand) for SDMMC_SendCommand
    stm32f7xx_hal_sd.o(i.HAL_SD_ReadBlocks_DMA) refers to stm32f7xx_hal_sd.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    stm32f7xx_hal_sd.o(i.HAL_SD_ReadBlocks_DMA) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_DataConfig) for SDMMC_DataConfig
    stm32f7xx_hal_sd.o(i.HAL_SD_ReadBlocks_DMA) refers to stm32f7xx_hal_sd.o(i.SD_DMA_RxCplt) for SD_DMA_RxCplt
    stm32f7xx_hal_sd.o(i.HAL_SD_ReadBlocks_DMA) refers to stm32f7xx_hal_sd.o(i.SD_DMA_RxError) for SD_DMA_RxError
    stm32f7xx_hal_sd.o(i.HAL_SD_SendSDStatus) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_GetResponse) for SDMMC_GetResponse
    stm32f7xx_hal_sd.o(i.HAL_SD_SendSDStatus) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_SendCommand) for SDMMC_SendCommand
    stm32f7xx_hal_sd.o(i.HAL_SD_SendSDStatus) refers to stm32f7xx_hal_sd.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    stm32f7xx_hal_sd.o(i.HAL_SD_SendSDStatus) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_DataConfig) for SDMMC_DataConfig
    stm32f7xx_hal_sd.o(i.HAL_SD_SendSDStatus) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_ReadFIFO) for SDMMC_ReadFIFO
    stm32f7xx_hal_sd.o(i.HAL_SD_StopTransfer) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_SendCommand) for SDMMC_SendCommand
    stm32f7xx_hal_sd.o(i.HAL_SD_StopTransfer) refers to stm32f7xx_hal_sd.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    stm32f7xx_hal_sd.o(i.HAL_SD_WideBusOperation_Config) refers to stm32f7xx_hal_sd.o(i.SD_WideBus_Enable) for SD_WideBus_Enable
    stm32f7xx_hal_sd.o(i.HAL_SD_WideBusOperation_Config) refers to stm32f7xx_hal_sd.o(i.SD_WideBus_Disable) for SD_WideBus_Disable
    stm32f7xx_hal_sd.o(i.HAL_SD_WideBusOperation_Config) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_Init) for SDMMC_Init
    stm32f7xx_hal_sd.o(i.HAL_SD_WriteBlocks) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_SendCommand) for SDMMC_SendCommand
    stm32f7xx_hal_sd.o(i.HAL_SD_WriteBlocks) refers to stm32f7xx_hal_sd.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    stm32f7xx_hal_sd.o(i.HAL_SD_WriteBlocks) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_DataConfig) for SDMMC_DataConfig
    stm32f7xx_hal_sd.o(i.HAL_SD_WriteBlocks) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_WriteFIFO) for SDMMC_WriteFIFO
    stm32f7xx_hal_sd.o(i.HAL_SD_WriteBlocks) refers to stm32f7xx_hal_sd.o(i.HAL_SD_StopTransfer) for HAL_SD_StopTransfer
    stm32f7xx_hal_sd.o(i.HAL_SD_WriteBlocks) refers to stm32f7xx_hal_sd.o(i.SD_IsCardProgramming) for SD_IsCardProgramming
    stm32f7xx_hal_sd.o(i.HAL_SD_WriteBlocks_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_sd.o(i.HAL_SD_WriteBlocks_DMA) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_SendCommand) for SDMMC_SendCommand
    stm32f7xx_hal_sd.o(i.HAL_SD_WriteBlocks_DMA) refers to stm32f7xx_hal_sd.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    stm32f7xx_hal_sd.o(i.HAL_SD_WriteBlocks_DMA) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_DataConfig) for SDMMC_DataConfig
    stm32f7xx_hal_sd.o(i.HAL_SD_WriteBlocks_DMA) refers to stm32f7xx_hal_sd.o(i.SD_DMA_TxCplt) for SD_DMA_TxCplt
    stm32f7xx_hal_sd.o(i.HAL_SD_WriteBlocks_DMA) refers to stm32f7xx_hal_sd.o(i.SD_DMA_TxError) for SD_DMA_TxError
    stm32f7xx_hal_sd.o(i.SD_CmdResp1Error) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_GetCommandResponse) for SDMMC_GetCommandResponse
    stm32f7xx_hal_sd.o(i.SD_CmdResp1Error) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_GetResponse) for SDMMC_GetResponse
    stm32f7xx_hal_sd.o(i.SD_CmdResp6Error) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_GetCommandResponse) for SDMMC_GetCommandResponse
    stm32f7xx_hal_sd.o(i.SD_CmdResp6Error) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_GetResponse) for SDMMC_GetResponse
    stm32f7xx_hal_sd.o(i.SD_DMA_RxCplt) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f7xx_hal_sd.o(i.SD_DMA_RxCplt) refers to stm32f7xx_hal_sd.o(i.HAL_SD_DMA_RxCpltCallback) for HAL_SD_DMA_RxCpltCallback
    stm32f7xx_hal_sd.o(i.SD_DMA_RxError) refers to stm32f7xx_hal_sd.o(i.HAL_SD_DMA_RxErrorCallback) for HAL_SD_DMA_RxErrorCallback
    stm32f7xx_hal_sd.o(i.SD_DMA_TxCplt) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f7xx_hal_sd.o(i.SD_DMA_TxCplt) refers to stm32f7xx_hal_sd.o(i.HAL_SD_DMA_TxCpltCallback) for HAL_SD_DMA_TxCpltCallback
    stm32f7xx_hal_sd.o(i.SD_DMA_TxError) refers to stm32f7xx_hal_sd.o(i.HAL_SD_DMA_TxErrorCallback) for HAL_SD_DMA_TxErrorCallback
    stm32f7xx_hal_sd.o(i.SD_FindSCR) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_SendCommand) for SDMMC_SendCommand
    stm32f7xx_hal_sd.o(i.SD_FindSCR) refers to stm32f7xx_hal_sd.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    stm32f7xx_hal_sd.o(i.SD_FindSCR) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_DataConfig) for SDMMC_DataConfig
    stm32f7xx_hal_sd.o(i.SD_FindSCR) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_ReadFIFO) for SDMMC_ReadFIFO
    stm32f7xx_hal_sd.o(i.SD_GetState) refers to stm32f7xx_hal_sd.o(i.SD_SendStatus) for SD_SendStatus
    stm32f7xx_hal_sd.o(i.SD_Initialize_Cards) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_GetPowerState) for SDMMC_GetPowerState
    stm32f7xx_hal_sd.o(i.SD_Initialize_Cards) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_SendCommand) for SDMMC_SendCommand
    stm32f7xx_hal_sd.o(i.SD_Initialize_Cards) refers to stm32f7xx_hal_sd.o(i.SD_CmdResp2Error) for SD_CmdResp2Error
    stm32f7xx_hal_sd.o(i.SD_Initialize_Cards) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_GetResponse) for SDMMC_GetResponse
    stm32f7xx_hal_sd.o(i.SD_Initialize_Cards) refers to stm32f7xx_hal_sd.o(i.SD_CmdResp6Error) for SD_CmdResp6Error
    stm32f7xx_hal_sd.o(i.SD_IsCardProgramming) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_SendCommand) for SDMMC_SendCommand
    stm32f7xx_hal_sd.o(i.SD_IsCardProgramming) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_GetCommandResponse) for SDMMC_GetCommandResponse
    stm32f7xx_hal_sd.o(i.SD_IsCardProgramming) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_GetResponse) for SDMMC_GetResponse
    stm32f7xx_hal_sd.o(i.SD_PowerOFF) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_PowerState_OFF) for SDMMC_PowerState_OFF
    stm32f7xx_hal_sd.o(i.SD_PowerON) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_PowerState_ON) for SDMMC_PowerState_ON
    stm32f7xx_hal_sd.o(i.SD_PowerON) refers to stm32f7xx_hal.o(i.HAL_Delay) for HAL_Delay
    stm32f7xx_hal_sd.o(i.SD_PowerON) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_SendCommand) for SDMMC_SendCommand
    stm32f7xx_hal_sd.o(i.SD_PowerON) refers to stm32f7xx_hal_sd.o(i.SD_CmdError) for SD_CmdError
    stm32f7xx_hal_sd.o(i.SD_PowerON) refers to stm32f7xx_hal_sd.o(i.SD_CmdResp7Error) for SD_CmdResp7Error
    stm32f7xx_hal_sd.o(i.SD_PowerON) refers to stm32f7xx_hal_sd.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    stm32f7xx_hal_sd.o(i.SD_PowerON) refers to stm32f7xx_hal_sd.o(i.SD_CmdResp3Error) for SD_CmdResp3Error
    stm32f7xx_hal_sd.o(i.SD_PowerON) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_GetResponse) for SDMMC_GetResponse
    stm32f7xx_hal_sd.o(i.SD_Select_Deselect) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_SendCommand) for SDMMC_SendCommand
    stm32f7xx_hal_sd.o(i.SD_Select_Deselect) refers to stm32f7xx_hal_sd.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    stm32f7xx_hal_sd.o(i.SD_SendStatus) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_SendCommand) for SDMMC_SendCommand
    stm32f7xx_hal_sd.o(i.SD_SendStatus) refers to stm32f7xx_hal_sd.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    stm32f7xx_hal_sd.o(i.SD_SendStatus) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_GetResponse) for SDMMC_GetResponse
    stm32f7xx_hal_sd.o(i.SD_WideBus_Disable) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_GetResponse) for SDMMC_GetResponse
    stm32f7xx_hal_sd.o(i.SD_WideBus_Disable) refers to stm32f7xx_hal_sd.o(i.SD_FindSCR) for SD_FindSCR
    stm32f7xx_hal_sd.o(i.SD_WideBus_Disable) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_SendCommand) for SDMMC_SendCommand
    stm32f7xx_hal_sd.o(i.SD_WideBus_Disable) refers to stm32f7xx_hal_sd.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    stm32f7xx_hal_sd.o(i.SD_WideBus_Enable) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_GetResponse) for SDMMC_GetResponse
    stm32f7xx_hal_sd.o(i.SD_WideBus_Enable) refers to stm32f7xx_hal_sd.o(i.SD_FindSCR) for SD_FindSCR
    stm32f7xx_hal_sd.o(i.SD_WideBus_Enable) refers to stm32f7xx_ll_sdmmc.o(i.SDMMC_SendCommand) for SDMMC_SendCommand
    stm32f7xx_hal_sd.o(i.SD_WideBus_Enable) refers to stm32f7xx_hal_sd.o(i.SD_CmdResp1Error) for SD_CmdResp1Error
    stm32f7xx_hal_sdram.o(i.HAL_SDRAM_DeInit) refers to stm32f7xx_hal_sdram.o(i.HAL_SDRAM_MspDeInit) for HAL_SDRAM_MspDeInit
    stm32f7xx_hal_sdram.o(i.HAL_SDRAM_DeInit) refers to stm32f7xx_ll_fmc.o(i.FMC_SDRAM_DeInit) for FMC_SDRAM_DeInit
    stm32f7xx_hal_sdram.o(i.HAL_SDRAM_GetModeStatus) refers to stm32f7xx_ll_fmc.o(i.FMC_SDRAM_GetModeStatus) for FMC_SDRAM_GetModeStatus
    stm32f7xx_hal_sdram.o(i.HAL_SDRAM_IRQHandler) refers to stm32f7xx_hal_sdram.o(i.HAL_SDRAM_RefreshErrorCallback) for HAL_SDRAM_RefreshErrorCallback
    stm32f7xx_hal_sdram.o(i.HAL_SDRAM_Init) refers to stm32f7xx_hal_sdram.o(i.HAL_SDRAM_MspInit) for HAL_SDRAM_MspInit
    stm32f7xx_hal_sdram.o(i.HAL_SDRAM_Init) refers to stm32f7xx_ll_fmc.o(i.FMC_SDRAM_Init) for FMC_SDRAM_Init
    stm32f7xx_hal_sdram.o(i.HAL_SDRAM_Init) refers to stm32f7xx_ll_fmc.o(i.FMC_SDRAM_Timing_Init) for FMC_SDRAM_Timing_Init
    stm32f7xx_hal_sdram.o(i.HAL_SDRAM_ProgramRefreshRate) refers to stm32f7xx_ll_fmc.o(i.FMC_SDRAM_ProgramRefreshRate) for FMC_SDRAM_ProgramRefreshRate
    stm32f7xx_hal_sdram.o(i.HAL_SDRAM_Read_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_sdram.o(i.HAL_SDRAM_Read_DMA) refers to stm32f7xx_hal_sdram.o(i.HAL_SDRAM_DMA_XferCpltCallback) for HAL_SDRAM_DMA_XferCpltCallback
    stm32f7xx_hal_sdram.o(i.HAL_SDRAM_Read_DMA) refers to stm32f7xx_hal_sdram.o(i.HAL_SDRAM_DMA_XferErrorCallback) for HAL_SDRAM_DMA_XferErrorCallback
    stm32f7xx_hal_sdram.o(i.HAL_SDRAM_SendCommand) refers to stm32f7xx_ll_fmc.o(i.FMC_SDRAM_SendCommand) for FMC_SDRAM_SendCommand
    stm32f7xx_hal_sdram.o(i.HAL_SDRAM_SetAutoRefreshNumber) refers to stm32f7xx_ll_fmc.o(i.FMC_SDRAM_SetAutoRefreshNumber) for FMC_SDRAM_SetAutoRefreshNumber
    stm32f7xx_hal_sdram.o(i.HAL_SDRAM_WriteProtection_Disable) refers to stm32f7xx_ll_fmc.o(i.FMC_SDRAM_WriteProtection_Disable) for FMC_SDRAM_WriteProtection_Disable
    stm32f7xx_hal_sdram.o(i.HAL_SDRAM_WriteProtection_Enable) refers to stm32f7xx_ll_fmc.o(i.FMC_SDRAM_WriteProtection_Enable) for FMC_SDRAM_WriteProtection_Enable
    stm32f7xx_hal_sdram.o(i.HAL_SDRAM_Write_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_sdram.o(i.HAL_SDRAM_Write_DMA) refers to stm32f7xx_hal_sdram.o(i.HAL_SDRAM_DMA_XferCpltCallback) for HAL_SDRAM_DMA_XferCpltCallback
    stm32f7xx_hal_sdram.o(i.HAL_SDRAM_Write_DMA) refers to stm32f7xx_hal_sdram.o(i.HAL_SDRAM_DMA_XferErrorCallback) for HAL_SDRAM_DMA_XferErrorCallback
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Abort) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_AbortReceive) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_AbortReceive_IT) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_AbortReceive_IT) refers to stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_AbortReceiveCpltCallback) for HAL_SMARTCARD_AbortReceiveCpltCallback
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_AbortReceive_IT) refers to stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMARxOnlyAbortCallback) for SMARTCARD_DMARxOnlyAbortCallback
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_AbortTransmit) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_AbortTransmit_IT) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_AbortTransmit_IT) refers to stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_AbortTransmitCpltCallback) for HAL_SMARTCARD_AbortTransmitCpltCallback
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_AbortTransmit_IT) refers to stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMATxOnlyAbortCallback) for SMARTCARD_DMATxOnlyAbortCallback
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Abort_IT) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Abort_IT) refers to stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_AbortCpltCallback) for HAL_SMARTCARD_AbortCpltCallback
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Abort_IT) refers to stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMATxAbortCallback) for SMARTCARD_DMATxAbortCallback
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Abort_IT) refers to stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMARxAbortCallback) for SMARTCARD_DMARxAbortCallback
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_DeInit) refers to stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_MspDeInit) for HAL_SMARTCARD_MspDeInit
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_IRQHandler) refers to stm32f7xx_hal_smartcard.o(i.SMARTCARD_Receive_IT) for SMARTCARD_Receive_IT
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_IRQHandler) refers to stm32f7xx_hal_smartcard.o(i.SMARTCARD_EndRxTransfer) for SMARTCARD_EndRxTransfer
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_IRQHandler) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_IRQHandler) refers to stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_ErrorCallback) for HAL_SMARTCARD_ErrorCallback
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_IRQHandler) refers to stm32f7xx_hal_smartcard.o(i.SMARTCARD_EndTxTransfer) for SMARTCARD_EndTxTransfer
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_IRQHandler) refers to stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_RxCpltCallback) for HAL_SMARTCARD_RxCpltCallback
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_IRQHandler) refers to stm32f7xx_hal_smartcard.o(i.SMARTCARD_Transmit_IT) for SMARTCARD_Transmit_IT
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_IRQHandler) refers to stm32f7xx_hal_smartcard.o(i.SMARTCARD_EndTransmit_IT) for SMARTCARD_EndTransmit_IT
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_IRQHandler) refers to stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMAAbortOnError) for SMARTCARD_DMAAbortOnError
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Init) refers to stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_MspInit) for HAL_SMARTCARD_MspInit
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Init) refers to stm32f7xx_hal_smartcard.o(i.SMARTCARD_SetConfig) for SMARTCARD_SetConfig
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Init) refers to stm32f7xx_hal_smartcard.o(i.SMARTCARD_AdvFeatureConfig) for SMARTCARD_AdvFeatureConfig
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Init) refers to stm32f7xx_hal_smartcard.o(i.SMARTCARD_CheckIdleState) for SMARTCARD_CheckIdleState
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Receive) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Receive) refers to stm32f7xx_hal_smartcard.o(i.SMARTCARD_WaitOnFlagUntilTimeout) for SMARTCARD_WaitOnFlagUntilTimeout
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Receive_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Receive_DMA) refers to stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMAReceiveCplt) for SMARTCARD_DMAReceiveCplt
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Receive_DMA) refers to stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMAError) for SMARTCARD_DMAError
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Transmit) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Transmit) refers to stm32f7xx_hal_smartcard.o(i.SMARTCARD_WaitOnFlagUntilTimeout) for SMARTCARD_WaitOnFlagUntilTimeout
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Transmit_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Transmit_DMA) refers to stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMATransmitCplt) for SMARTCARD_DMATransmitCplt
    stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Transmit_DMA) refers to stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMAError) for SMARTCARD_DMAError
    stm32f7xx_hal_smartcard.o(i.SMARTCARD_CheckIdleState) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_smartcard.o(i.SMARTCARD_CheckIdleState) refers to stm32f7xx_hal_smartcard.o(i.SMARTCARD_WaitOnFlagUntilTimeout) for SMARTCARD_WaitOnFlagUntilTimeout
    stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMAAbortOnError) refers to stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_ErrorCallback) for HAL_SMARTCARD_ErrorCallback
    stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMAError) refers to stm32f7xx_hal_smartcard.o(i.SMARTCARD_EndTxTransfer) for SMARTCARD_EndTxTransfer
    stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMAError) refers to stm32f7xx_hal_smartcard.o(i.SMARTCARD_EndRxTransfer) for SMARTCARD_EndRxTransfer
    stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMAError) refers to stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_ErrorCallback) for HAL_SMARTCARD_ErrorCallback
    stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMAReceiveCplt) refers to stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_RxCpltCallback) for HAL_SMARTCARD_RxCpltCallback
    stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMARxAbortCallback) refers to stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_AbortCpltCallback) for HAL_SMARTCARD_AbortCpltCallback
    stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMARxOnlyAbortCallback) refers to stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_AbortReceiveCpltCallback) for HAL_SMARTCARD_AbortReceiveCpltCallback
    stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMATxAbortCallback) refers to stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_AbortCpltCallback) for HAL_SMARTCARD_AbortCpltCallback
    stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMATxOnlyAbortCallback) refers to stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_AbortTransmitCpltCallback) for HAL_SMARTCARD_AbortTransmitCpltCallback
    stm32f7xx_hal_smartcard.o(i.SMARTCARD_EndTransmit_IT) refers to stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_TxCpltCallback) for HAL_SMARTCARD_TxCpltCallback
    stm32f7xx_hal_smartcard.o(i.SMARTCARD_Receive_IT) refers to stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_RxCpltCallback) for HAL_SMARTCARD_RxCpltCallback
    stm32f7xx_hal_smartcard.o(i.SMARTCARD_SetConfig) refers to stm32f7xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq) for HAL_RCC_GetPCLK1Freq
    stm32f7xx_hal_smartcard.o(i.SMARTCARD_SetConfig) refers to stm32f7xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq) for HAL_RCC_GetPCLK2Freq
    stm32f7xx_hal_smartcard.o(i.SMARTCARD_SetConfig) refers to stm32f7xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq) for HAL_RCC_GetSysClockFreq
    stm32f7xx_hal_smartcard.o(i.SMARTCARD_WaitOnFlagUntilTimeout) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_DeInit) refers to stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_MspDeInit) for HAL_SPDIFRX_MspDeInit
    stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_IRQHandler) refers to stm32f7xx_hal_spdifrx.o(i.SPDIFRX_ReceiveDataFlow_IT) for SPDIFRX_ReceiveDataFlow_IT
    stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_IRQHandler) refers to stm32f7xx_hal_spdifrx.o(i.SPDIFRX_ReceiveControlFlow_IT) for SPDIFRX_ReceiveControlFlow_IT
    stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_IRQHandler) refers to stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ErrorCallback) for HAL_SPDIFRX_ErrorCallback
    stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_Init) refers to stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_MspInit) for HAL_SPDIFRX_MspInit
    stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveControlFlow) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveControlFlow) refers to stm32f7xx_hal_spdifrx.o(i.SPDIFRX_WaitOnFlagUntilTimeout) for SPDIFRX_WaitOnFlagUntilTimeout
    stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveControlFlow_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveControlFlow_DMA) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveControlFlow_DMA) refers to stm32f7xx_hal_spdifrx.o(i.SPDIFRX_WaitOnFlagUntilTimeout) for SPDIFRX_WaitOnFlagUntilTimeout
    stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveControlFlow_DMA) refers to stm32f7xx_hal_spdifrx.o(i.SPDIFRX_DMACxHalfCplt) for SPDIFRX_DMACxHalfCplt
    stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveControlFlow_DMA) refers to stm32f7xx_hal_spdifrx.o(i.SPDIFRX_DMACxCplt) for SPDIFRX_DMACxCplt
    stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveControlFlow_DMA) refers to stm32f7xx_hal_spdifrx.o(i.SPDIFRX_DMAError) for SPDIFRX_DMAError
    stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveControlFlow_IT) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveControlFlow_IT) refers to stm32f7xx_hal_spdifrx.o(i.SPDIFRX_WaitOnFlagUntilTimeout) for SPDIFRX_WaitOnFlagUntilTimeout
    stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveDataFlow) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveDataFlow) refers to stm32f7xx_hal_spdifrx.o(i.SPDIFRX_WaitOnFlagUntilTimeout) for SPDIFRX_WaitOnFlagUntilTimeout
    stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveDataFlow_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveDataFlow_DMA) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveDataFlow_DMA) refers to stm32f7xx_hal_spdifrx.o(i.SPDIFRX_WaitOnFlagUntilTimeout) for SPDIFRX_WaitOnFlagUntilTimeout
    stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveDataFlow_DMA) refers to stm32f7xx_hal_spdifrx.o(i.SPDIFRX_DMARxHalfCplt) for SPDIFRX_DMARxHalfCplt
    stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveDataFlow_DMA) refers to stm32f7xx_hal_spdifrx.o(i.SPDIFRX_DMARxCplt) for SPDIFRX_DMARxCplt
    stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveDataFlow_DMA) refers to stm32f7xx_hal_spdifrx.o(i.SPDIFRX_DMAError) for SPDIFRX_DMAError
    stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveDataFlow_IT) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveDataFlow_IT) refers to stm32f7xx_hal_spdifrx.o(i.SPDIFRX_WaitOnFlagUntilTimeout) for SPDIFRX_WaitOnFlagUntilTimeout
    stm32f7xx_hal_spdifrx.o(i.SPDIFRX_DMACxCplt) refers to stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_CxCpltCallback) for HAL_SPDIFRX_CxCpltCallback
    stm32f7xx_hal_spdifrx.o(i.SPDIFRX_DMACxHalfCplt) refers to stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_CxHalfCpltCallback) for HAL_SPDIFRX_CxHalfCpltCallback
    stm32f7xx_hal_spdifrx.o(i.SPDIFRX_DMAError) refers to stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ErrorCallback) for HAL_SPDIFRX_ErrorCallback
    stm32f7xx_hal_spdifrx.o(i.SPDIFRX_DMARxCplt) refers to stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_RxCpltCallback) for HAL_SPDIFRX_RxCpltCallback
    stm32f7xx_hal_spdifrx.o(i.SPDIFRX_DMARxHalfCplt) refers to stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_RxHalfCpltCallback) for HAL_SPDIFRX_RxHalfCpltCallback
    stm32f7xx_hal_spdifrx.o(i.SPDIFRX_ReceiveControlFlow_IT) refers to stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_CxCpltCallback) for HAL_SPDIFRX_CxCpltCallback
    stm32f7xx_hal_spdifrx.o(i.SPDIFRX_ReceiveDataFlow_IT) refers to stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_RxCpltCallback) for HAL_SPDIFRX_RxCpltCallback
    stm32f7xx_hal_spdifrx.o(i.SPDIFRX_WaitOnFlagUntilTimeout) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_spi.o(i.HAL_SPI_Abort) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f7xx_hal_spi.o(i.HAL_SPI_Abort) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_spi.o(i.HAL_SPI_Abort) refers to stm32f7xx_hal_spi.o(i.SPI_EndRxTxTransaction) for SPI_EndRxTxTransaction
    stm32f7xx_hal_spi.o(i.HAL_SPI_Abort) refers to stm32f7xx_hal_spi.o(i.SPI_WaitFifoStateUntilTimeout) for SPI_WaitFifoStateUntilTimeout
    stm32f7xx_hal_spi.o(i.HAL_SPI_Abort) refers to stm32f7xx_hal_spi.o(i.SPI_WaitFlagStateUntilTimeout) for SPI_WaitFlagStateUntilTimeout
    stm32f7xx_hal_spi.o(i.HAL_SPI_Abort) refers to stm32f7xx_hal_spi.o(i.SPI_AbortTx_ISR) for SPI_AbortTx_ISR
    stm32f7xx_hal_spi.o(i.HAL_SPI_Abort) refers to stm32f7xx_hal_spi.o(i.SPI_AbortRx_ISR) for SPI_AbortRx_ISR
    stm32f7xx_hal_spi.o(i.HAL_SPI_Abort_IT) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32f7xx_hal_spi.o(i.HAL_SPI_Abort_IT) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_AbortCpltCallback) for HAL_SPI_AbortCpltCallback
    stm32f7xx_hal_spi.o(i.HAL_SPI_Abort_IT) refers to stm32f7xx_hal_spi.o(i.SPI_AbortTx_ISR) for SPI_AbortTx_ISR
    stm32f7xx_hal_spi.o(i.HAL_SPI_Abort_IT) refers to stm32f7xx_hal_spi.o(i.SPI_AbortRx_ISR) for SPI_AbortRx_ISR
    stm32f7xx_hal_spi.o(i.HAL_SPI_Abort_IT) refers to stm32f7xx_hal_spi.o(i.SPI_DMATxAbortCallback) for SPI_DMATxAbortCallback
    stm32f7xx_hal_spi.o(i.HAL_SPI_Abort_IT) refers to stm32f7xx_hal_spi.o(i.SPI_DMARxAbortCallback) for SPI_DMARxAbortCallback
    stm32f7xx_hal_spi.o(i.HAL_SPI_DMAStop) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f7xx_hal_spi.o(i.HAL_SPI_DeInit) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_MspDeInit) for HAL_SPI_MspDeInit
    stm32f7xx_hal_spi.o(i.HAL_SPI_IRQHandler) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32f7xx_hal_spi.o(i.HAL_SPI_IRQHandler) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_ErrorCallback) for HAL_SPI_ErrorCallback
    stm32f7xx_hal_spi.o(i.HAL_SPI_IRQHandler) refers to stm32f7xx_hal_spi.o(i.SPI_DMAAbortOnError) for SPI_DMAAbortOnError
    stm32f7xx_hal_spi.o(i.HAL_SPI_Init) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_MspInit) for HAL_SPI_MspInit
    stm32f7xx_hal_spi.o(i.HAL_SPI_Receive) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_spi.o(i.HAL_SPI_Receive) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_TransmitReceive) for HAL_SPI_TransmitReceive
    stm32f7xx_hal_spi.o(i.HAL_SPI_Receive) refers to stm32f7xx_hal_spi.o(i.SPI_WaitFlagStateUntilTimeout) for SPI_WaitFlagStateUntilTimeout
    stm32f7xx_hal_spi.o(i.HAL_SPI_Receive) refers to stm32f7xx_hal_spi.o(i.SPI_EndRxTransaction) for SPI_EndRxTransaction
    stm32f7xx_hal_spi.o(i.HAL_SPI_Receive_DMA) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA) for HAL_SPI_TransmitReceive_DMA
    stm32f7xx_hal_spi.o(i.HAL_SPI_Receive_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_spi.o(i.HAL_SPI_Receive_DMA) refers to stm32f7xx_hal_spi.o(i.SPI_DMAHalfReceiveCplt) for SPI_DMAHalfReceiveCplt
    stm32f7xx_hal_spi.o(i.HAL_SPI_Receive_DMA) refers to stm32f7xx_hal_spi.o(i.SPI_DMAReceiveCplt) for SPI_DMAReceiveCplt
    stm32f7xx_hal_spi.o(i.HAL_SPI_Receive_DMA) refers to stm32f7xx_hal_spi.o(i.SPI_DMAError) for SPI_DMAError
    stm32f7xx_hal_spi.o(i.HAL_SPI_Receive_IT) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_TransmitReceive_IT) for HAL_SPI_TransmitReceive_IT
    stm32f7xx_hal_spi.o(i.HAL_SPI_Receive_IT) refers to stm32f7xx_hal_spi.o(i.SPI_RxISR_16BIT) for SPI_RxISR_16BIT
    stm32f7xx_hal_spi.o(i.HAL_SPI_Receive_IT) refers to stm32f7xx_hal_spi.o(i.SPI_RxISR_8BIT) for SPI_RxISR_8BIT
    stm32f7xx_hal_spi.o(i.HAL_SPI_Transmit) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_spi.o(i.HAL_SPI_Transmit) refers to stm32f7xx_hal_spi.o(i.SPI_EndRxTxTransaction) for SPI_EndRxTxTransaction
    stm32f7xx_hal_spi.o(i.HAL_SPI_TransmitReceive) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_spi.o(i.HAL_SPI_TransmitReceive) refers to stm32f7xx_hal_spi.o(i.SPI_WaitFlagStateUntilTimeout) for SPI_WaitFlagStateUntilTimeout
    stm32f7xx_hal_spi.o(i.HAL_SPI_TransmitReceive) refers to stm32f7xx_hal_spi.o(i.SPI_EndRxTxTransaction) for SPI_EndRxTxTransaction
    stm32f7xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA) refers to stm32f7xx_hal_spi.o(i.SPI_DMAHalfTransmitReceiveCplt) for SPI_DMAHalfTransmitReceiveCplt
    stm32f7xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA) refers to stm32f7xx_hal_spi.o(i.SPI_DMATransmitReceiveCplt) for SPI_DMATransmitReceiveCplt
    stm32f7xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA) refers to stm32f7xx_hal_spi.o(i.SPI_DMAError) for SPI_DMAError
    stm32f7xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA) refers to stm32f7xx_hal_spi.o(i.SPI_DMAHalfReceiveCplt) for SPI_DMAHalfReceiveCplt
    stm32f7xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA) refers to stm32f7xx_hal_spi.o(i.SPI_DMAReceiveCplt) for SPI_DMAReceiveCplt
    stm32f7xx_hal_spi.o(i.HAL_SPI_TransmitReceive_IT) refers to stm32f7xx_hal_spi.o(i.SPI_2linesRxISR_16BIT) for SPI_2linesRxISR_16BIT
    stm32f7xx_hal_spi.o(i.HAL_SPI_TransmitReceive_IT) refers to stm32f7xx_hal_spi.o(i.SPI_2linesTxISR_16BIT) for SPI_2linesTxISR_16BIT
    stm32f7xx_hal_spi.o(i.HAL_SPI_TransmitReceive_IT) refers to stm32f7xx_hal_spi.o(i.SPI_2linesRxISR_8BIT) for SPI_2linesRxISR_8BIT
    stm32f7xx_hal_spi.o(i.HAL_SPI_TransmitReceive_IT) refers to stm32f7xx_hal_spi.o(i.SPI_2linesTxISR_8BIT) for SPI_2linesTxISR_8BIT
    stm32f7xx_hal_spi.o(i.HAL_SPI_Transmit_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_spi.o(i.HAL_SPI_Transmit_DMA) refers to stm32f7xx_hal_spi.o(i.SPI_DMAHalfTransmitCplt) for SPI_DMAHalfTransmitCplt
    stm32f7xx_hal_spi.o(i.HAL_SPI_Transmit_DMA) refers to stm32f7xx_hal_spi.o(i.SPI_DMATransmitCplt) for SPI_DMATransmitCplt
    stm32f7xx_hal_spi.o(i.HAL_SPI_Transmit_DMA) refers to stm32f7xx_hal_spi.o(i.SPI_DMAError) for SPI_DMAError
    stm32f7xx_hal_spi.o(i.HAL_SPI_Transmit_IT) refers to stm32f7xx_hal_spi.o(i.SPI_TxISR_16BIT) for SPI_TxISR_16BIT
    stm32f7xx_hal_spi.o(i.HAL_SPI_Transmit_IT) refers to stm32f7xx_hal_spi.o(i.SPI_TxISR_8BIT) for SPI_TxISR_8BIT
    stm32f7xx_hal_spi.o(i.SPI_2linesRxISR_16BIT) refers to stm32f7xx_hal_spi.o(i.SPI_CloseRxTx_ISR) for SPI_CloseRxTx_ISR
    stm32f7xx_hal_spi.o(i.SPI_2linesRxISR_16BIT) refers to stm32f7xx_hal_spi.o(i.SPI_2linesRxISR_16BITCRC) for SPI_2linesRxISR_16BITCRC
    stm32f7xx_hal_spi.o(i.SPI_2linesRxISR_16BITCRC) refers to stm32f7xx_hal_spi.o(i.SPI_CloseRxTx_ISR) for SPI_CloseRxTx_ISR
    stm32f7xx_hal_spi.o(i.SPI_2linesRxISR_8BIT) refers to stm32f7xx_hal_spi.o(i.SPI_CloseRxTx_ISR) for SPI_CloseRxTx_ISR
    stm32f7xx_hal_spi.o(i.SPI_2linesRxISR_8BIT) refers to stm32f7xx_hal_spi.o(i.SPI_2linesRxISR_8BITCRC) for SPI_2linesRxISR_8BITCRC
    stm32f7xx_hal_spi.o(i.SPI_2linesRxISR_8BITCRC) refers to stm32f7xx_hal_spi.o(i.SPI_CloseRxTx_ISR) for SPI_CloseRxTx_ISR
    stm32f7xx_hal_spi.o(i.SPI_2linesTxISR_16BIT) refers to stm32f7xx_hal_spi.o(i.SPI_CloseRxTx_ISR) for SPI_CloseRxTx_ISR
    stm32f7xx_hal_spi.o(i.SPI_2linesTxISR_8BIT) refers to stm32f7xx_hal_spi.o(i.SPI_CloseRxTx_ISR) for SPI_CloseRxTx_ISR
    stm32f7xx_hal_spi.o(i.SPI_AbortRx_ISR) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_spi.o(i.SPI_AbortRx_ISR) refers to stm32f7xx_hal_spi.o(i.SPI_WaitFlagStateUntilTimeout) for SPI_WaitFlagStateUntilTimeout
    stm32f7xx_hal_spi.o(i.SPI_AbortRx_ISR) refers to stm32f7xx_hal_spi.o(i.SPI_WaitFifoStateUntilTimeout) for SPI_WaitFifoStateUntilTimeout
    stm32f7xx_hal_spi.o(i.SPI_AbortTx_ISR) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_spi.o(i.SPI_AbortTx_ISR) refers to stm32f7xx_hal_spi.o(i.SPI_EndRxTxTransaction) for SPI_EndRxTxTransaction
    stm32f7xx_hal_spi.o(i.SPI_AbortTx_ISR) refers to stm32f7xx_hal_spi.o(i.SPI_WaitFifoStateUntilTimeout) for SPI_WaitFifoStateUntilTimeout
    stm32f7xx_hal_spi.o(i.SPI_CloseRxTx_ISR) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_spi.o(i.SPI_CloseRxTx_ISR) refers to stm32f7xx_hal_spi.o(i.SPI_EndRxTxTransaction) for SPI_EndRxTxTransaction
    stm32f7xx_hal_spi.o(i.SPI_CloseRxTx_ISR) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_ErrorCallback) for HAL_SPI_ErrorCallback
    stm32f7xx_hal_spi.o(i.SPI_CloseRxTx_ISR) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_TxRxCpltCallback) for HAL_SPI_TxRxCpltCallback
    stm32f7xx_hal_spi.o(i.SPI_CloseRxTx_ISR) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_RxCpltCallback) for HAL_SPI_RxCpltCallback
    stm32f7xx_hal_spi.o(i.SPI_CloseRx_ISR) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_spi.o(i.SPI_CloseRx_ISR) refers to stm32f7xx_hal_spi.o(i.SPI_EndRxTransaction) for SPI_EndRxTransaction
    stm32f7xx_hal_spi.o(i.SPI_CloseRx_ISR) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_ErrorCallback) for HAL_SPI_ErrorCallback
    stm32f7xx_hal_spi.o(i.SPI_CloseRx_ISR) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_RxCpltCallback) for HAL_SPI_RxCpltCallback
    stm32f7xx_hal_spi.o(i.SPI_CloseTx_ISR) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_spi.o(i.SPI_CloseTx_ISR) refers to stm32f7xx_hal_spi.o(i.SPI_EndRxTxTransaction) for SPI_EndRxTxTransaction
    stm32f7xx_hal_spi.o(i.SPI_CloseTx_ISR) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_ErrorCallback) for HAL_SPI_ErrorCallback
    stm32f7xx_hal_spi.o(i.SPI_CloseTx_ISR) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_TxCpltCallback) for HAL_SPI_TxCpltCallback
    stm32f7xx_hal_spi.o(i.SPI_DMAAbortOnError) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_ErrorCallback) for HAL_SPI_ErrorCallback
    stm32f7xx_hal_spi.o(i.SPI_DMAError) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_ErrorCallback) for HAL_SPI_ErrorCallback
    stm32f7xx_hal_spi.o(i.SPI_DMAHalfReceiveCplt) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_RxHalfCpltCallback) for HAL_SPI_RxHalfCpltCallback
    stm32f7xx_hal_spi.o(i.SPI_DMAHalfTransmitCplt) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_TxHalfCpltCallback) for HAL_SPI_TxHalfCpltCallback
    stm32f7xx_hal_spi.o(i.SPI_DMAHalfTransmitReceiveCplt) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_TxRxHalfCpltCallback) for HAL_SPI_TxRxHalfCpltCallback
    stm32f7xx_hal_spi.o(i.SPI_DMAReceiveCplt) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_spi.o(i.SPI_DMAReceiveCplt) refers to stm32f7xx_hal_spi.o(i.SPI_WaitFlagStateUntilTimeout) for SPI_WaitFlagStateUntilTimeout
    stm32f7xx_hal_spi.o(i.SPI_DMAReceiveCplt) refers to stm32f7xx_hal_spi.o(i.SPI_EndRxTransaction) for SPI_EndRxTransaction
    stm32f7xx_hal_spi.o(i.SPI_DMAReceiveCplt) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_ErrorCallback) for HAL_SPI_ErrorCallback
    stm32f7xx_hal_spi.o(i.SPI_DMAReceiveCplt) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_RxCpltCallback) for HAL_SPI_RxCpltCallback
    stm32f7xx_hal_spi.o(i.SPI_DMARxAbortCallback) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_spi.o(i.SPI_DMARxAbortCallback) refers to stm32f7xx_hal_spi.o(i.SPI_WaitFlagStateUntilTimeout) for SPI_WaitFlagStateUntilTimeout
    stm32f7xx_hal_spi.o(i.SPI_DMARxAbortCallback) refers to stm32f7xx_hal_spi.o(i.SPI_WaitFifoStateUntilTimeout) for SPI_WaitFifoStateUntilTimeout
    stm32f7xx_hal_spi.o(i.SPI_DMARxAbortCallback) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_AbortCpltCallback) for HAL_SPI_AbortCpltCallback
    stm32f7xx_hal_spi.o(i.SPI_DMATransmitCplt) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_spi.o(i.SPI_DMATransmitCplt) refers to stm32f7xx_hal_spi.o(i.SPI_EndRxTxTransaction) for SPI_EndRxTxTransaction
    stm32f7xx_hal_spi.o(i.SPI_DMATransmitCplt) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_ErrorCallback) for HAL_SPI_ErrorCallback
    stm32f7xx_hal_spi.o(i.SPI_DMATransmitCplt) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_TxCpltCallback) for HAL_SPI_TxCpltCallback
    stm32f7xx_hal_spi.o(i.SPI_DMATransmitReceiveCplt) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_spi.o(i.SPI_DMATransmitReceiveCplt) refers to stm32f7xx_hal_spi.o(i.SPI_WaitFifoStateUntilTimeout) for SPI_WaitFifoStateUntilTimeout
    stm32f7xx_hal_spi.o(i.SPI_DMATransmitReceiveCplt) refers to stm32f7xx_hal_spi.o(i.SPI_EndRxTxTransaction) for SPI_EndRxTxTransaction
    stm32f7xx_hal_spi.o(i.SPI_DMATransmitReceiveCplt) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_ErrorCallback) for HAL_SPI_ErrorCallback
    stm32f7xx_hal_spi.o(i.SPI_DMATransmitReceiveCplt) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_TxRxCpltCallback) for HAL_SPI_TxRxCpltCallback
    stm32f7xx_hal_spi.o(i.SPI_DMATxAbortCallback) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_spi.o(i.SPI_DMATxAbortCallback) refers to stm32f7xx_hal_spi.o(i.SPI_EndRxTxTransaction) for SPI_EndRxTxTransaction
    stm32f7xx_hal_spi.o(i.SPI_DMATxAbortCallback) refers to stm32f7xx_hal_spi.o(i.SPI_WaitFifoStateUntilTimeout) for SPI_WaitFifoStateUntilTimeout
    stm32f7xx_hal_spi.o(i.SPI_DMATxAbortCallback) refers to stm32f7xx_hal_spi.o(i.HAL_SPI_AbortCpltCallback) for HAL_SPI_AbortCpltCallback
    stm32f7xx_hal_spi.o(i.SPI_EndRxTransaction) refers to stm32f7xx_hal_spi.o(i.SPI_WaitFlagStateUntilTimeout) for SPI_WaitFlagStateUntilTimeout
    stm32f7xx_hal_spi.o(i.SPI_EndRxTransaction) refers to stm32f7xx_hal_spi.o(i.SPI_WaitFifoStateUntilTimeout) for SPI_WaitFifoStateUntilTimeout
    stm32f7xx_hal_spi.o(i.SPI_EndRxTxTransaction) refers to stm32f7xx_hal_spi.o(i.SPI_WaitFifoStateUntilTimeout) for SPI_WaitFifoStateUntilTimeout
    stm32f7xx_hal_spi.o(i.SPI_EndRxTxTransaction) refers to stm32f7xx_hal_spi.o(i.SPI_WaitFlagStateUntilTimeout) for SPI_WaitFlagStateUntilTimeout
    stm32f7xx_hal_spi.o(i.SPI_RxISR_16BIT) refers to stm32f7xx_hal_spi.o(i.SPI_CloseRx_ISR) for SPI_CloseRx_ISR
    stm32f7xx_hal_spi.o(i.SPI_RxISR_16BIT) refers to stm32f7xx_hal_spi.o(i.SPI_RxISR_16BITCRC) for SPI_RxISR_16BITCRC
    stm32f7xx_hal_spi.o(i.SPI_RxISR_16BITCRC) refers to stm32f7xx_hal_spi.o(i.SPI_CloseRx_ISR) for SPI_CloseRx_ISR
    stm32f7xx_hal_spi.o(i.SPI_RxISR_8BIT) refers to stm32f7xx_hal_spi.o(i.SPI_CloseRx_ISR) for SPI_CloseRx_ISR
    stm32f7xx_hal_spi.o(i.SPI_RxISR_8BIT) refers to stm32f7xx_hal_spi.o(i.SPI_RxISR_8BITCRC) for SPI_RxISR_8BITCRC
    stm32f7xx_hal_spi.o(i.SPI_RxISR_8BITCRC) refers to stm32f7xx_hal_spi.o(i.SPI_CloseRx_ISR) for SPI_CloseRx_ISR
    stm32f7xx_hal_spi.o(i.SPI_TxISR_16BIT) refers to stm32f7xx_hal_spi.o(i.SPI_CloseTx_ISR) for SPI_CloseTx_ISR
    stm32f7xx_hal_spi.o(i.SPI_TxISR_8BIT) refers to stm32f7xx_hal_spi.o(i.SPI_CloseTx_ISR) for SPI_CloseTx_ISR
    stm32f7xx_hal_spi.o(i.SPI_WaitFifoStateUntilTimeout) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_spi.o(i.SPI_WaitFlagStateUntilTimeout) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_sram.o(i.HAL_SRAM_DeInit) refers to stm32f7xx_hal_sram.o(i.HAL_SRAM_MspDeInit) for HAL_SRAM_MspDeInit
    stm32f7xx_hal_sram.o(i.HAL_SRAM_DeInit) refers to stm32f7xx_ll_fmc.o(i.FMC_NORSRAM_DeInit) for FMC_NORSRAM_DeInit
    stm32f7xx_hal_sram.o(i.HAL_SRAM_Init) refers to stm32f7xx_hal_sram.o(i.HAL_SRAM_MspInit) for HAL_SRAM_MspInit
    stm32f7xx_hal_sram.o(i.HAL_SRAM_Init) refers to stm32f7xx_ll_fmc.o(i.FMC_NORSRAM_Init) for FMC_NORSRAM_Init
    stm32f7xx_hal_sram.o(i.HAL_SRAM_Init) refers to stm32f7xx_ll_fmc.o(i.FMC_NORSRAM_Timing_Init) for FMC_NORSRAM_Timing_Init
    stm32f7xx_hal_sram.o(i.HAL_SRAM_Init) refers to stm32f7xx_ll_fmc.o(i.FMC_NORSRAM_Extended_Timing_Init) for FMC_NORSRAM_Extended_Timing_Init
    stm32f7xx_hal_sram.o(i.HAL_SRAM_Read_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_sram.o(i.HAL_SRAM_Read_DMA) refers to stm32f7xx_hal_sram.o(i.HAL_SRAM_DMA_XferCpltCallback) for HAL_SRAM_DMA_XferCpltCallback
    stm32f7xx_hal_sram.o(i.HAL_SRAM_Read_DMA) refers to stm32f7xx_hal_sram.o(i.HAL_SRAM_DMA_XferErrorCallback) for HAL_SRAM_DMA_XferErrorCallback
    stm32f7xx_hal_sram.o(i.HAL_SRAM_WriteOperation_Disable) refers to stm32f7xx_ll_fmc.o(i.FMC_NORSRAM_WriteOperation_Disable) for FMC_NORSRAM_WriteOperation_Disable
    stm32f7xx_hal_sram.o(i.HAL_SRAM_WriteOperation_Enable) refers to stm32f7xx_ll_fmc.o(i.FMC_NORSRAM_WriteOperation_Enable) for FMC_NORSRAM_WriteOperation_Enable
    stm32f7xx_hal_sram.o(i.HAL_SRAM_Write_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_sram.o(i.HAL_SRAM_Write_DMA) refers to stm32f7xx_hal_sram.o(i.HAL_SRAM_DMA_XferCpltCallback) for HAL_SRAM_DMA_XferCpltCallback
    stm32f7xx_hal_sram.o(i.HAL_SRAM_Write_DMA) refers to stm32f7xx_hal_sram.o(i.HAL_SRAM_DMA_XferErrorCallback) for HAL_SRAM_DMA_XferErrorCallback
    stm32f7xx_hal_tim.o(i.HAL_TIM_Base_DeInit) refers to stm32f7xx_hal_tim.o(i.HAL_TIM_Base_MspDeInit) for HAL_TIM_Base_MspDeInit
    stm32f7xx_hal_tim.o(i.HAL_TIM_Base_Init) refers to stm32f7xx_hal_tim.o(i.HAL_TIM_Base_MspInit) for HAL_TIM_Base_MspInit
    stm32f7xx_hal_tim.o(i.HAL_TIM_Base_Init) refers to stm32f7xx_hal_tim.o(i.TIM_Base_SetConfig) for TIM_Base_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_Base_Start_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_tim.o(i.HAL_TIM_Base_Start_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_DMAPeriodElapsedCplt) for TIM_DMAPeriodElapsedCplt
    stm32f7xx_hal_tim.o(i.HAL_TIM_Base_Start_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_DMAError) for TIM_DMAError
    stm32f7xx_hal_tim.o(i.HAL_TIM_ConfigClockSource) refers to stm32f7xx_hal_tim.o(i.TIM_ETR_SetConfig) for TIM_ETR_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_ConfigClockSource) refers to stm32f7xx_hal_tim.o(i.TIM_TI1_ConfigInputStage) for TIM_TI1_ConfigInputStage
    stm32f7xx_hal_tim.o(i.HAL_TIM_ConfigClockSource) refers to stm32f7xx_hal_tim.o(i.TIM_ITRx_SetConfig) for TIM_ITRx_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_ConfigClockSource) refers to stm32f7xx_hal_tim.o(i.TIM_TI2_ConfigInputStage) for TIM_TI2_ConfigInputStage
    stm32f7xx_hal_tim.o(i.HAL_TIM_ConfigOCrefClear) refers to stm32f7xx_hal_tim.o(i.TIM_ETR_SetConfig) for TIM_ETR_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_DMABurst_ReadStart) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_tim.o(i.HAL_TIM_DMABurst_ReadStart) refers to stm32f7xx_hal_tim.o(i.TIM_DMAError) for TIM_DMAError
    stm32f7xx_hal_tim.o(i.HAL_TIM_DMABurst_ReadStart) refers to stm32f7xx_hal_tim.o(i.TIM_DMACaptureCplt) for TIM_DMACaptureCplt
    stm32f7xx_hal_tim.o(i.HAL_TIM_DMABurst_ReadStart) refers to stm32f7xx_hal_tim.o(i.TIM_DMAPeriodElapsedCplt) for TIM_DMAPeriodElapsedCplt
    stm32f7xx_hal_tim.o(i.HAL_TIM_DMABurst_ReadStart) refers to stm32f7xx_hal_tim_ex.o(i.TIMEx_DMACommutationCplt) for TIMEx_DMACommutationCplt
    stm32f7xx_hal_tim.o(i.HAL_TIM_DMABurst_ReadStart) refers to stm32f7xx_hal_tim.o(i.TIM_DMATriggerCplt) for TIM_DMATriggerCplt
    stm32f7xx_hal_tim.o(i.HAL_TIM_DMABurst_ReadStop) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f7xx_hal_tim.o(i.HAL_TIM_DMABurst_WriteStart) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_tim.o(i.HAL_TIM_DMABurst_WriteStart) refers to stm32f7xx_hal_tim.o(i.TIM_DMAError) for TIM_DMAError
    stm32f7xx_hal_tim.o(i.HAL_TIM_DMABurst_WriteStart) refers to stm32f7xx_hal_tim.o(i.TIM_DMADelayPulseCplt) for TIM_DMADelayPulseCplt
    stm32f7xx_hal_tim.o(i.HAL_TIM_DMABurst_WriteStart) refers to stm32f7xx_hal_tim.o(i.TIM_DMAPeriodElapsedCplt) for TIM_DMAPeriodElapsedCplt
    stm32f7xx_hal_tim.o(i.HAL_TIM_DMABurst_WriteStart) refers to stm32f7xx_hal_tim_ex.o(i.TIMEx_DMACommutationCplt) for TIMEx_DMACommutationCplt
    stm32f7xx_hal_tim.o(i.HAL_TIM_DMABurst_WriteStart) refers to stm32f7xx_hal_tim.o(i.TIM_DMATriggerCplt) for TIM_DMATriggerCplt
    stm32f7xx_hal_tim.o(i.HAL_TIM_DMABurst_WriteStop) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f7xx_hal_tim.o(i.HAL_TIM_Encoder_DeInit) refers to stm32f7xx_hal_tim.o(i.HAL_TIM_Encoder_MspDeInit) for HAL_TIM_Encoder_MspDeInit
    stm32f7xx_hal_tim.o(i.HAL_TIM_Encoder_Init) refers to stm32f7xx_hal_tim.o(i.HAL_TIM_Encoder_MspInit) for HAL_TIM_Encoder_MspInit
    stm32f7xx_hal_tim.o(i.HAL_TIM_Encoder_Init) refers to stm32f7xx_hal_tim.o(i.TIM_Base_SetConfig) for TIM_Base_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_Encoder_Start) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_Encoder_Start_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_tim.o(i.HAL_TIM_Encoder_Start_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_Encoder_Start_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_DMACaptureCplt) for TIM_DMACaptureCplt
    stm32f7xx_hal_tim.o(i.HAL_TIM_Encoder_Start_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_DMAError) for TIM_DMAError
    stm32f7xx_hal_tim.o(i.HAL_TIM_Encoder_Start_IT) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_Encoder_Stop) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_Encoder_Stop_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_Encoder_Stop_IT) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_IC_ConfigChannel) refers to stm32f7xx_hal_tim.o(i.TIM_TI4_SetConfig) for TIM_TI4_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_IC_ConfigChannel) refers to stm32f7xx_hal_tim.o(i.TIM_TI1_SetConfig) for TIM_TI1_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_IC_ConfigChannel) refers to stm32f7xx_hal_tim.o(i.TIM_TI2_SetConfig) for TIM_TI2_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_IC_ConfigChannel) refers to stm32f7xx_hal_tim.o(i.TIM_TI3_SetConfig) for TIM_TI3_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_IC_DeInit) refers to stm32f7xx_hal_tim.o(i.HAL_TIM_IC_MspDeInit) for HAL_TIM_IC_MspDeInit
    stm32f7xx_hal_tim.o(i.HAL_TIM_IC_Init) refers to stm32f7xx_hal_tim.o(i.HAL_TIM_IC_MspInit) for HAL_TIM_IC_MspInit
    stm32f7xx_hal_tim.o(i.HAL_TIM_IC_Init) refers to stm32f7xx_hal_tim.o(i.TIM_Base_SetConfig) for TIM_Base_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_IC_Start) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_IC_Start_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_tim.o(i.HAL_TIM_IC_Start_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_IC_Start_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_DMACaptureCplt) for TIM_DMACaptureCplt
    stm32f7xx_hal_tim.o(i.HAL_TIM_IC_Start_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_DMAError) for TIM_DMAError
    stm32f7xx_hal_tim.o(i.HAL_TIM_IC_Start_IT) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_IC_Stop) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_IC_Stop_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_IC_Stop_IT) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_IRQHandler) refers to stm32f7xx_hal_tim.o(i.HAL_TIM_IC_CaptureCallback) for HAL_TIM_IC_CaptureCallback
    stm32f7xx_hal_tim.o(i.HAL_TIM_IRQHandler) refers to stm32f7xx_hal_tim.o(i.HAL_TIM_OC_DelayElapsedCallback) for HAL_TIM_OC_DelayElapsedCallback
    stm32f7xx_hal_tim.o(i.HAL_TIM_IRQHandler) refers to stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_PulseFinishedCallback) for HAL_TIM_PWM_PulseFinishedCallback
    stm32f7xx_hal_tim.o(i.HAL_TIM_IRQHandler) refers to stm32f7xx_hal_tim.o(i.HAL_TIM_PeriodElapsedCallback) for HAL_TIM_PeriodElapsedCallback
    stm32f7xx_hal_tim.o(i.HAL_TIM_IRQHandler) refers to stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_BreakCallback) for HAL_TIMEx_BreakCallback
    stm32f7xx_hal_tim.o(i.HAL_TIM_IRQHandler) refers to stm32f7xx_hal_tim.o(i.HAL_TIM_TriggerCallback) for HAL_TIM_TriggerCallback
    stm32f7xx_hal_tim.o(i.HAL_TIM_IRQHandler) refers to stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_CommutationCallback) for HAL_TIMEx_CommutationCallback
    stm32f7xx_hal_tim.o(i.HAL_TIM_OC_ConfigChannel) refers to stm32f7xx_hal_tim.o(i.TIM_OC1_SetConfig) for TIM_OC1_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_OC_ConfigChannel) refers to stm32f7xx_hal_tim.o(i.TIM_OC2_SetConfig) for TIM_OC2_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_OC_ConfigChannel) refers to stm32f7xx_hal_tim.o(i.TIM_OC3_SetConfig) for TIM_OC3_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_OC_ConfigChannel) refers to stm32f7xx_hal_tim.o(i.TIM_OC4_SetConfig) for TIM_OC4_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_OC_DeInit) refers to stm32f7xx_hal_tim.o(i.HAL_TIM_OC_MspDeInit) for HAL_TIM_OC_MspDeInit
    stm32f7xx_hal_tim.o(i.HAL_TIM_OC_Init) refers to stm32f7xx_hal_tim.o(i.HAL_TIM_OC_MspInit) for HAL_TIM_OC_MspInit
    stm32f7xx_hal_tim.o(i.HAL_TIM_OC_Init) refers to stm32f7xx_hal_tim.o(i.TIM_Base_SetConfig) for TIM_Base_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_OC_Start) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_OC_Start_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_tim.o(i.HAL_TIM_OC_Start_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_OC_Start_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_DMADelayPulseCplt) for TIM_DMADelayPulseCplt
    stm32f7xx_hal_tim.o(i.HAL_TIM_OC_Start_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_DMAError) for TIM_DMAError
    stm32f7xx_hal_tim.o(i.HAL_TIM_OC_Start_IT) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_OC_Stop) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_OC_Stop_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_OC_Stop_IT) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_OnePulse_ConfigChannel) refers to stm32f7xx_hal_tim.o(i.TIM_OC1_SetConfig) for TIM_OC1_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_OnePulse_ConfigChannel) refers to stm32f7xx_hal_tim.o(i.TIM_OC2_SetConfig) for TIM_OC2_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_OnePulse_ConfigChannel) refers to stm32f7xx_hal_tim.o(i.TIM_TI1_SetConfig) for TIM_TI1_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_OnePulse_ConfigChannel) refers to stm32f7xx_hal_tim.o(i.TIM_TI2_SetConfig) for TIM_TI2_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_OnePulse_DeInit) refers to stm32f7xx_hal_tim.o(i.HAL_TIM_OnePulse_MspDeInit) for HAL_TIM_OnePulse_MspDeInit
    stm32f7xx_hal_tim.o(i.HAL_TIM_OnePulse_Init) refers to stm32f7xx_hal_tim.o(i.HAL_TIM_OnePulse_MspInit) for HAL_TIM_OnePulse_MspInit
    stm32f7xx_hal_tim.o(i.HAL_TIM_OnePulse_Init) refers to stm32f7xx_hal_tim.o(i.TIM_Base_SetConfig) for TIM_Base_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_OnePulse_Start) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_OnePulse_Start_IT) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_OnePulse_Stop) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_OnePulse_Stop_IT) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_ConfigChannel) refers to stm32f7xx_hal_tim.o(i.TIM_OC1_SetConfig) for TIM_OC1_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_ConfigChannel) refers to stm32f7xx_hal_tim.o(i.TIM_OC2_SetConfig) for TIM_OC2_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_ConfigChannel) refers to stm32f7xx_hal_tim.o(i.TIM_OC3_SetConfig) for TIM_OC3_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_ConfigChannel) refers to stm32f7xx_hal_tim.o(i.TIM_OC4_SetConfig) for TIM_OC4_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_DeInit) refers to stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_MspDeInit) for HAL_TIM_PWM_MspDeInit
    stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_Init) refers to stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_MspInit) for HAL_TIM_PWM_MspInit
    stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_Init) refers to stm32f7xx_hal_tim.o(i.TIM_Base_SetConfig) for TIM_Base_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_Start) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_Start_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_Start_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_Start_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_DMADelayPulseCplt) for TIM_DMADelayPulseCplt
    stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_Start_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_DMAError) for TIM_DMAError
    stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_Start_IT) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_Stop) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_Stop_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_Stop_IT) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim.o(i.HAL_TIM_SlaveConfigSynchronization) refers to stm32f7xx_hal_tim.o(i.TIM_ETR_SetConfig) for TIM_ETR_SetConfig
    stm32f7xx_hal_tim.o(i.HAL_TIM_SlaveConfigSynchronization) refers to stm32f7xx_hal_tim.o(i.TIM_TI1_ConfigInputStage) for TIM_TI1_ConfigInputStage
    stm32f7xx_hal_tim.o(i.HAL_TIM_SlaveConfigSynchronization) refers to stm32f7xx_hal_tim.o(i.TIM_TI2_ConfigInputStage) for TIM_TI2_ConfigInputStage
    stm32f7xx_hal_tim.o(i.HAL_TIM_SlaveConfigSynchronization_IT) refers to stm32f7xx_hal_tim.o(i.TIM_SlaveTimer_SetConfig) for TIM_SlaveTimer_SetConfig
    stm32f7xx_hal_tim.o(i.TIM_DMACaptureCplt) refers to stm32f7xx_hal_tim.o(i.HAL_TIM_IC_CaptureCallback) for HAL_TIM_IC_CaptureCallback
    stm32f7xx_hal_tim.o(i.TIM_DMADelayPulseCplt) refers to stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_PulseFinishedCallback) for HAL_TIM_PWM_PulseFinishedCallback
    stm32f7xx_hal_tim.o(i.TIM_DMAError) refers to stm32f7xx_hal_tim.o(i.HAL_TIM_ErrorCallback) for HAL_TIM_ErrorCallback
    stm32f7xx_hal_tim.o(i.TIM_DMAPeriodElapsedCplt) refers to stm32f7xx_hal_tim.o(i.HAL_TIM_PeriodElapsedCallback) for HAL_TIM_PeriodElapsedCallback
    stm32f7xx_hal_tim.o(i.TIM_DMATriggerCplt) refers to stm32f7xx_hal_tim.o(i.HAL_TIM_TriggerCallback) for HAL_TIM_TriggerCallback
    stm32f7xx_hal_tim.o(i.TIM_SlaveTimer_SetConfig) refers to stm32f7xx_hal_tim.o(i.TIM_ETR_SetConfig) for TIM_ETR_SetConfig
    stm32f7xx_hal_tim.o(i.TIM_SlaveTimer_SetConfig) refers to stm32f7xx_hal_tim.o(i.TIM_TI1_ConfigInputStage) for TIM_TI1_ConfigInputStage
    stm32f7xx_hal_tim.o(i.TIM_SlaveTimer_SetConfig) refers to stm32f7xx_hal_tim.o(i.TIM_TI2_ConfigInputStage) for TIM_TI2_ConfigInputStage
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_ConfigCommutationEvent_DMA) refers to stm32f7xx_hal_tim_ex.o(i.TIMEx_DMACommutationCplt) for TIMEx_DMACommutationCplt
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_ConfigCommutationEvent_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_DMAError) for TIM_DMAError
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_DeInit) refers to stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_MspDeInit) for HAL_TIMEx_HallSensor_MspDeInit
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_Init) refers to stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_MspInit) for HAL_TIMEx_HallSensor_MspInit
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_Init) refers to stm32f7xx_hal_tim.o(i.TIM_Base_SetConfig) for TIM_Base_SetConfig
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_Init) refers to stm32f7xx_hal_tim.o(i.TIM_TI1_SetConfig) for TIM_TI1_SetConfig
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_Init) refers to stm32f7xx_hal_tim.o(i.TIM_OC2_SetConfig) for TIM_OC2_SetConfig
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_Start) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_Start_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_Start_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_Start_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_DMACaptureCplt) for TIM_DMACaptureCplt
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_Start_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_DMAError) for TIM_DMAError
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_Start_IT) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_Stop) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_Stop_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_Stop_IT) refers to stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd) for TIM_CCxChannelCmd
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_OCN_Start) refers to stm32f7xx_hal_tim_ex.o(i.TIM_CCxNChannelCmd) for TIM_CCxNChannelCmd
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_OCN_Start_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_OCN_Start_DMA) refers to stm32f7xx_hal_tim_ex.o(i.TIM_CCxNChannelCmd) for TIM_CCxNChannelCmd
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_OCN_Start_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_DMADelayPulseCplt) for TIM_DMADelayPulseCplt
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_OCN_Start_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_DMAError) for TIM_DMAError
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_OCN_Start_IT) refers to stm32f7xx_hal_tim_ex.o(i.TIM_CCxNChannelCmd) for TIM_CCxNChannelCmd
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_OCN_Stop) refers to stm32f7xx_hal_tim_ex.o(i.TIM_CCxNChannelCmd) for TIM_CCxNChannelCmd
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_OCN_Stop_DMA) refers to stm32f7xx_hal_tim_ex.o(i.TIM_CCxNChannelCmd) for TIM_CCxNChannelCmd
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_OCN_Stop_IT) refers to stm32f7xx_hal_tim_ex.o(i.TIM_CCxNChannelCmd) for TIM_CCxNChannelCmd
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_OnePulseN_Start) refers to stm32f7xx_hal_tim_ex.o(i.TIM_CCxNChannelCmd) for TIM_CCxNChannelCmd
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_OnePulseN_Start_IT) refers to stm32f7xx_hal_tim_ex.o(i.TIM_CCxNChannelCmd) for TIM_CCxNChannelCmd
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_OnePulseN_Stop) refers to stm32f7xx_hal_tim_ex.o(i.TIM_CCxNChannelCmd) for TIM_CCxNChannelCmd
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_OnePulseN_Stop_IT) refers to stm32f7xx_hal_tim_ex.o(i.TIM_CCxNChannelCmd) for TIM_CCxNChannelCmd
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_PWMN_Start) refers to stm32f7xx_hal_tim_ex.o(i.TIM_CCxNChannelCmd) for TIM_CCxNChannelCmd
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_PWMN_Start_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_PWMN_Start_DMA) refers to stm32f7xx_hal_tim_ex.o(i.TIM_CCxNChannelCmd) for TIM_CCxNChannelCmd
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_PWMN_Start_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_DMADelayPulseCplt) for TIM_DMADelayPulseCplt
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_PWMN_Start_DMA) refers to stm32f7xx_hal_tim.o(i.TIM_DMAError) for TIM_DMAError
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_PWMN_Start_IT) refers to stm32f7xx_hal_tim_ex.o(i.TIM_CCxNChannelCmd) for TIM_CCxNChannelCmd
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_PWMN_Stop) refers to stm32f7xx_hal_tim_ex.o(i.TIM_CCxNChannelCmd) for TIM_CCxNChannelCmd
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_PWMN_Stop_DMA) refers to stm32f7xx_hal_tim_ex.o(i.TIM_CCxNChannelCmd) for TIM_CCxNChannelCmd
    stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_PWMN_Stop_IT) refers to stm32f7xx_hal_tim_ex.o(i.TIM_CCxNChannelCmd) for TIM_CCxNChannelCmd
    stm32f7xx_hal_tim_ex.o(i.HAL_TIM_ConfigOCrefClear) refers to stm32f7xx_hal_tim.o(i.TIM_ETR_SetConfig) for TIM_ETR_SetConfig
    stm32f7xx_hal_tim_ex.o(i.HAL_TIM_OC_ConfigChannel) refers to stm32f7xx_hal_tim.o(i.TIM_OC1_SetConfig) for TIM_OC1_SetConfig
    stm32f7xx_hal_tim_ex.o(i.HAL_TIM_OC_ConfigChannel) refers to stm32f7xx_hal_tim.o(i.TIM_OC2_SetConfig) for TIM_OC2_SetConfig
    stm32f7xx_hal_tim_ex.o(i.HAL_TIM_OC_ConfigChannel) refers to stm32f7xx_hal_tim.o(i.TIM_OC3_SetConfig) for TIM_OC3_SetConfig
    stm32f7xx_hal_tim_ex.o(i.HAL_TIM_OC_ConfigChannel) refers to stm32f7xx_hal_tim.o(i.TIM_OC4_SetConfig) for TIM_OC4_SetConfig
    stm32f7xx_hal_tim_ex.o(i.HAL_TIM_OC_ConfigChannel) refers to stm32f7xx_hal_tim_ex.o(i.TIM_OC5_SetConfig) for TIM_OC5_SetConfig
    stm32f7xx_hal_tim_ex.o(i.HAL_TIM_OC_ConfigChannel) refers to stm32f7xx_hal_tim_ex.o(i.TIM_OC6_SetConfig) for TIM_OC6_SetConfig
    stm32f7xx_hal_tim_ex.o(i.HAL_TIM_PWM_ConfigChannel) refers to stm32f7xx_hal_tim.o(i.TIM_OC1_SetConfig) for TIM_OC1_SetConfig
    stm32f7xx_hal_tim_ex.o(i.HAL_TIM_PWM_ConfigChannel) refers to stm32f7xx_hal_tim.o(i.TIM_OC2_SetConfig) for TIM_OC2_SetConfig
    stm32f7xx_hal_tim_ex.o(i.HAL_TIM_PWM_ConfigChannel) refers to stm32f7xx_hal_tim.o(i.TIM_OC3_SetConfig) for TIM_OC3_SetConfig
    stm32f7xx_hal_tim_ex.o(i.HAL_TIM_PWM_ConfigChannel) refers to stm32f7xx_hal_tim.o(i.TIM_OC4_SetConfig) for TIM_OC4_SetConfig
    stm32f7xx_hal_tim_ex.o(i.HAL_TIM_PWM_ConfigChannel) refers to stm32f7xx_hal_tim_ex.o(i.TIM_OC5_SetConfig) for TIM_OC5_SetConfig
    stm32f7xx_hal_tim_ex.o(i.HAL_TIM_PWM_ConfigChannel) refers to stm32f7xx_hal_tim_ex.o(i.TIM_OC6_SetConfig) for TIM_OC6_SetConfig
    stm32f7xx_hal_tim_ex.o(i.TIMEx_DMACommutationCplt) refers to stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_CommutationCallback) for HAL_TIMEx_CommutationCallback
    stm32f7xx_hal_uart.o(i.HAL_HalfDuplex_Init) refers to stm32f7xx_hal_uart.o(i.HAL_UART_MspInit) for HAL_UART_MspInit
    stm32f7xx_hal_uart.o(i.HAL_HalfDuplex_Init) refers to stm32f7xx_hal_uart.o(i.UART_SetConfig) for UART_SetConfig
    stm32f7xx_hal_uart.o(i.HAL_HalfDuplex_Init) refers to stm32f7xx_hal_uart.o(i.UART_AdvFeatureConfig) for UART_AdvFeatureConfig
    stm32f7xx_hal_uart.o(i.HAL_HalfDuplex_Init) refers to stm32f7xx_hal_uart.o(i.UART_CheckIdleState) for UART_CheckIdleState
    stm32f7xx_hal_uart.o(i.HAL_LIN_Init) refers to stm32f7xx_hal_uart.o(i.HAL_UART_MspInit) for HAL_UART_MspInit
    stm32f7xx_hal_uart.o(i.HAL_LIN_Init) refers to stm32f7xx_hal_uart.o(i.UART_SetConfig) for UART_SetConfig
    stm32f7xx_hal_uart.o(i.HAL_LIN_Init) refers to stm32f7xx_hal_uart.o(i.UART_AdvFeatureConfig) for UART_AdvFeatureConfig
    stm32f7xx_hal_uart.o(i.HAL_LIN_Init) refers to stm32f7xx_hal_uart.o(i.UART_CheckIdleState) for UART_CheckIdleState
    stm32f7xx_hal_uart.o(i.HAL_MultiProcessorEx_AddressLength_Set) refers to stm32f7xx_hal_uart.o(i.UART_CheckIdleState) for UART_CheckIdleState
    stm32f7xx_hal_uart.o(i.HAL_MultiProcessor_DisableMuteMode) refers to stm32f7xx_hal_uart.o(i.UART_CheckIdleState) for UART_CheckIdleState
    stm32f7xx_hal_uart.o(i.HAL_MultiProcessor_EnableMuteMode) refers to stm32f7xx_hal_uart.o(i.UART_CheckIdleState) for UART_CheckIdleState
    stm32f7xx_hal_uart.o(i.HAL_MultiProcessor_Init) refers to stm32f7xx_hal_uart.o(i.HAL_UART_MspInit) for HAL_UART_MspInit
    stm32f7xx_hal_uart.o(i.HAL_MultiProcessor_Init) refers to stm32f7xx_hal_uart.o(i.UART_SetConfig) for UART_SetConfig
    stm32f7xx_hal_uart.o(i.HAL_MultiProcessor_Init) refers to stm32f7xx_hal_uart.o(i.UART_AdvFeatureConfig) for UART_AdvFeatureConfig
    stm32f7xx_hal_uart.o(i.HAL_MultiProcessor_Init) refers to stm32f7xx_hal_uart.o(i.UART_CheckIdleState) for UART_CheckIdleState
    stm32f7xx_hal_uart.o(i.HAL_RS485Ex_Init) refers to stm32f7xx_hal_uart.o(i.HAL_UART_MspInit) for HAL_UART_MspInit
    stm32f7xx_hal_uart.o(i.HAL_RS485Ex_Init) refers to stm32f7xx_hal_uart.o(i.UART_SetConfig) for UART_SetConfig
    stm32f7xx_hal_uart.o(i.HAL_RS485Ex_Init) refers to stm32f7xx_hal_uart.o(i.UART_AdvFeatureConfig) for UART_AdvFeatureConfig
    stm32f7xx_hal_uart.o(i.HAL_RS485Ex_Init) refers to stm32f7xx_hal_uart.o(i.UART_CheckIdleState) for UART_CheckIdleState
    stm32f7xx_hal_uart.o(i.HAL_UART_DMAStop) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f7xx_hal_uart.o(i.HAL_UART_DMAStop) refers to stm32f7xx_hal_uart.o(i.UART_EndTxTransfer) for UART_EndTxTransfer
    stm32f7xx_hal_uart.o(i.HAL_UART_DMAStop) refers to stm32f7xx_hal_uart.o(i.UART_EndRxTransfer) for UART_EndRxTransfer
    stm32f7xx_hal_uart.o(i.HAL_UART_DeInit) refers to stm32f7xx_hal_uart.o(i.HAL_UART_MspDeInit) for HAL_UART_MspDeInit
    stm32f7xx_hal_uart.o(i.HAL_UART_IRQHandler) refers to stm32f7xx_hal_uart.o(i.UART_Receive_IT) for UART_Receive_IT
    stm32f7xx_hal_uart.o(i.HAL_UART_IRQHandler) refers to stm32f7xx_hal_uart.o(i.UART_EndRxTransfer) for UART_EndRxTransfer
    stm32f7xx_hal_uart.o(i.HAL_UART_IRQHandler) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32f7xx_hal_uart.o(i.HAL_UART_IRQHandler) refers to stm32f7xx_hal_uart.o(i.HAL_UART_ErrorCallback) for HAL_UART_ErrorCallback
    stm32f7xx_hal_uart.o(i.HAL_UART_IRQHandler) refers to stm32f7xx_hal_uart.o(i.UART_Transmit_IT) for UART_Transmit_IT
    stm32f7xx_hal_uart.o(i.HAL_UART_IRQHandler) refers to stm32f7xx_hal_uart.o(i.UART_EndTransmit_IT) for UART_EndTransmit_IT
    stm32f7xx_hal_uart.o(i.HAL_UART_IRQHandler) refers to stm32f7xx_hal_uart.o(i.UART_DMAAbortOnError) for UART_DMAAbortOnError
    stm32f7xx_hal_uart.o(i.HAL_UART_Init) refers to stm32f7xx_hal_uart.o(i.HAL_UART_MspInit) for HAL_UART_MspInit
    stm32f7xx_hal_uart.o(i.HAL_UART_Init) refers to stm32f7xx_hal_uart.o(i.UART_SetConfig) for UART_SetConfig
    stm32f7xx_hal_uart.o(i.HAL_UART_Init) refers to stm32f7xx_hal_uart.o(i.UART_AdvFeatureConfig) for UART_AdvFeatureConfig
    stm32f7xx_hal_uart.o(i.HAL_UART_Init) refers to stm32f7xx_hal_uart.o(i.UART_CheckIdleState) for UART_CheckIdleState
    stm32f7xx_hal_uart.o(i.HAL_UART_Receive) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_uart.o(i.HAL_UART_Receive) refers to stm32f7xx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout) for UART_WaitOnFlagUntilTimeout
    stm32f7xx_hal_uart.o(i.HAL_UART_Receive_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_uart.o(i.HAL_UART_Receive_DMA) refers to stm32f7xx_hal_uart.o(i.UART_DMAReceiveCplt) for UART_DMAReceiveCplt
    stm32f7xx_hal_uart.o(i.HAL_UART_Receive_DMA) refers to stm32f7xx_hal_uart.o(i.UART_DMARxHalfCplt) for UART_DMARxHalfCplt
    stm32f7xx_hal_uart.o(i.HAL_UART_Receive_DMA) refers to stm32f7xx_hal_uart.o(i.UART_DMAError) for UART_DMAError
    stm32f7xx_hal_uart.o(i.HAL_UART_Transmit) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_uart.o(i.HAL_UART_Transmit) refers to stm32f7xx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout) for UART_WaitOnFlagUntilTimeout
    stm32f7xx_hal_uart.o(i.HAL_UART_Transmit_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_uart.o(i.HAL_UART_Transmit_DMA) refers to stm32f7xx_hal_uart.o(i.UART_DMATransmitCplt) for UART_DMATransmitCplt
    stm32f7xx_hal_uart.o(i.HAL_UART_Transmit_DMA) refers to stm32f7xx_hal_uart.o(i.UART_DMATxHalfCplt) for UART_DMATxHalfCplt
    stm32f7xx_hal_uart.o(i.HAL_UART_Transmit_DMA) refers to stm32f7xx_hal_uart.o(i.UART_DMAError) for UART_DMAError
    stm32f7xx_hal_uart.o(i.UART_CheckIdleState) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_uart.o(i.UART_CheckIdleState) refers to stm32f7xx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout) for UART_WaitOnFlagUntilTimeout
    stm32f7xx_hal_uart.o(i.UART_DMAAbortOnError) refers to stm32f7xx_hal_uart.o(i.HAL_UART_ErrorCallback) for HAL_UART_ErrorCallback
    stm32f7xx_hal_uart.o(i.UART_DMAError) refers to stm32f7xx_hal_uart.o(i.UART_EndTxTransfer) for UART_EndTxTransfer
    stm32f7xx_hal_uart.o(i.UART_DMAError) refers to stm32f7xx_hal_uart.o(i.UART_EndRxTransfer) for UART_EndRxTransfer
    stm32f7xx_hal_uart.o(i.UART_DMAError) refers to stm32f7xx_hal_uart.o(i.HAL_UART_ErrorCallback) for HAL_UART_ErrorCallback
    stm32f7xx_hal_uart.o(i.UART_DMAReceiveCplt) refers to stm32f7xx_hal_uart.o(i.HAL_UART_RxCpltCallback) for HAL_UART_RxCpltCallback
    stm32f7xx_hal_uart.o(i.UART_DMARxHalfCplt) refers to stm32f7xx_hal_uart.o(i.HAL_UART_RxHalfCpltCallback) for HAL_UART_RxHalfCpltCallback
    stm32f7xx_hal_uart.o(i.UART_DMATransmitCplt) refers to stm32f7xx_hal_uart.o(i.HAL_UART_TxCpltCallback) for HAL_UART_TxCpltCallback
    stm32f7xx_hal_uart.o(i.UART_DMATxHalfCplt) refers to stm32f7xx_hal_uart.o(i.HAL_UART_TxHalfCpltCallback) for HAL_UART_TxHalfCpltCallback
    stm32f7xx_hal_uart.o(i.UART_EndTransmit_IT) refers to stm32f7xx_hal_uart.o(i.HAL_UART_TxCpltCallback) for HAL_UART_TxCpltCallback
    stm32f7xx_hal_uart.o(i.UART_Receive_IT) refers to stm32f7xx_hal_uart.o(i.HAL_UART_RxCpltCallback) for HAL_UART_RxCpltCallback
    stm32f7xx_hal_uart.o(i.UART_SetConfig) refers to stm32f7xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq) for HAL_RCC_GetPCLK1Freq
    stm32f7xx_hal_uart.o(i.UART_SetConfig) refers to stm32f7xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq) for HAL_RCC_GetPCLK2Freq
    stm32f7xx_hal_uart.o(i.UART_SetConfig) refers to stm32f7xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq) for HAL_RCC_GetSysClockFreq
    stm32f7xx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_usart.o(i.HAL_USART_DMAStop) refers to stm32f7xx_hal_usart.o(i.USART_EndTxTransfer) for USART_EndTxTransfer
    stm32f7xx_hal_usart.o(i.HAL_USART_DMAStop) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort) for HAL_DMA_Abort
    stm32f7xx_hal_usart.o(i.HAL_USART_DMAStop) refers to stm32f7xx_hal_usart.o(i.USART_EndRxTransfer) for USART_EndRxTransfer
    stm32f7xx_hal_usart.o(i.HAL_USART_DeInit) refers to stm32f7xx_hal_usart.o(i.HAL_USART_MspDeInit) for HAL_USART_MspDeInit
    stm32f7xx_hal_usart.o(i.HAL_USART_IRQHandler) refers to stm32f7xx_hal_usart.o(i.USART_TransmitReceive_IT) for USART_TransmitReceive_IT
    stm32f7xx_hal_usart.o(i.HAL_USART_IRQHandler) refers to stm32f7xx_hal_usart.o(i.USART_Receive_IT) for USART_Receive_IT
    stm32f7xx_hal_usart.o(i.HAL_USART_IRQHandler) refers to stm32f7xx_hal_usart.o(i.USART_EndRxTransfer) for USART_EndRxTransfer
    stm32f7xx_hal_usart.o(i.HAL_USART_IRQHandler) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Abort_IT) for HAL_DMA_Abort_IT
    stm32f7xx_hal_usart.o(i.HAL_USART_IRQHandler) refers to stm32f7xx_hal_usart.o(i.HAL_USART_ErrorCallback) for HAL_USART_ErrorCallback
    stm32f7xx_hal_usart.o(i.HAL_USART_IRQHandler) refers to stm32f7xx_hal_usart.o(i.USART_Transmit_IT) for USART_Transmit_IT
    stm32f7xx_hal_usart.o(i.HAL_USART_IRQHandler) refers to stm32f7xx_hal_usart.o(i.USART_EndTransmit_IT) for USART_EndTransmit_IT
    stm32f7xx_hal_usart.o(i.HAL_USART_IRQHandler) refers to stm32f7xx_hal_usart.o(i.USART_DMAAbortOnError) for USART_DMAAbortOnError
    stm32f7xx_hal_usart.o(i.HAL_USART_Init) refers to stm32f7xx_hal_usart.o(i.HAL_USART_MspInit) for HAL_USART_MspInit
    stm32f7xx_hal_usart.o(i.HAL_USART_Init) refers to stm32f7xx_hal_usart.o(i.USART_SetConfig) for USART_SetConfig
    stm32f7xx_hal_usart.o(i.HAL_USART_Init) refers to stm32f7xx_hal_usart.o(i.USART_CheckIdleState) for USART_CheckIdleState
    stm32f7xx_hal_usart.o(i.HAL_USART_Receive) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_usart.o(i.HAL_USART_Receive) refers to stm32f7xx_hal_usart.o(i.USART_WaitOnFlagUntilTimeout) for USART_WaitOnFlagUntilTimeout
    stm32f7xx_hal_usart.o(i.HAL_USART_Receive_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_usart.o(i.HAL_USART_Receive_DMA) refers to stm32f7xx_hal_usart.o(i.USART_DMAReceiveCplt) for USART_DMAReceiveCplt
    stm32f7xx_hal_usart.o(i.HAL_USART_Receive_DMA) refers to stm32f7xx_hal_usart.o(i.USART_DMARxHalfCplt) for USART_DMARxHalfCplt
    stm32f7xx_hal_usart.o(i.HAL_USART_Receive_DMA) refers to stm32f7xx_hal_usart.o(i.USART_DMAError) for USART_DMAError
    stm32f7xx_hal_usart.o(i.HAL_USART_Transmit) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_usart.o(i.HAL_USART_Transmit) refers to stm32f7xx_hal_usart.o(i.USART_WaitOnFlagUntilTimeout) for USART_WaitOnFlagUntilTimeout
    stm32f7xx_hal_usart.o(i.HAL_USART_TransmitReceive) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_usart.o(i.HAL_USART_TransmitReceive) refers to stm32f7xx_hal_usart.o(i.USART_WaitOnFlagUntilTimeout) for USART_WaitOnFlagUntilTimeout
    stm32f7xx_hal_usart.o(i.HAL_USART_TransmitReceive_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_usart.o(i.HAL_USART_TransmitReceive_DMA) refers to stm32f7xx_hal_usart.o(i.USART_DMAReceiveCplt) for USART_DMAReceiveCplt
    stm32f7xx_hal_usart.o(i.HAL_USART_TransmitReceive_DMA) refers to stm32f7xx_hal_usart.o(i.USART_DMARxHalfCplt) for USART_DMARxHalfCplt
    stm32f7xx_hal_usart.o(i.HAL_USART_TransmitReceive_DMA) refers to stm32f7xx_hal_usart.o(i.USART_DMATransmitCplt) for USART_DMATransmitCplt
    stm32f7xx_hal_usart.o(i.HAL_USART_TransmitReceive_DMA) refers to stm32f7xx_hal_usart.o(i.USART_DMATxHalfCplt) for USART_DMATxHalfCplt
    stm32f7xx_hal_usart.o(i.HAL_USART_TransmitReceive_DMA) refers to stm32f7xx_hal_usart.o(i.USART_DMAError) for USART_DMAError
    stm32f7xx_hal_usart.o(i.HAL_USART_Transmit_DMA) refers to stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT) for HAL_DMA_Start_IT
    stm32f7xx_hal_usart.o(i.HAL_USART_Transmit_DMA) refers to stm32f7xx_hal_usart.o(i.USART_DMATransmitCplt) for USART_DMATransmitCplt
    stm32f7xx_hal_usart.o(i.HAL_USART_Transmit_DMA) refers to stm32f7xx_hal_usart.o(i.USART_DMATxHalfCplt) for USART_DMATxHalfCplt
    stm32f7xx_hal_usart.o(i.HAL_USART_Transmit_DMA) refers to stm32f7xx_hal_usart.o(i.USART_DMAError) for USART_DMAError
    stm32f7xx_hal_usart.o(i.USART_CheckIdleState) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_usart.o(i.USART_CheckIdleState) refers to stm32f7xx_hal_usart.o(i.USART_WaitOnFlagUntilTimeout) for USART_WaitOnFlagUntilTimeout
    stm32f7xx_hal_usart.o(i.USART_DMAAbortOnError) refers to stm32f7xx_hal_usart.o(i.HAL_USART_ErrorCallback) for HAL_USART_ErrorCallback
    stm32f7xx_hal_usart.o(i.USART_DMAError) refers to stm32f7xx_hal_usart.o(i.USART_EndTxTransfer) for USART_EndTxTransfer
    stm32f7xx_hal_usart.o(i.USART_DMAError) refers to stm32f7xx_hal_usart.o(i.USART_EndRxTransfer) for USART_EndRxTransfer
    stm32f7xx_hal_usart.o(i.USART_DMAError) refers to stm32f7xx_hal_usart.o(i.HAL_USART_ErrorCallback) for HAL_USART_ErrorCallback
    stm32f7xx_hal_usart.o(i.USART_DMAReceiveCplt) refers to stm32f7xx_hal_usart.o(i.HAL_USART_TxRxCpltCallback) for HAL_USART_TxRxCpltCallback
    stm32f7xx_hal_usart.o(i.USART_DMAReceiveCplt) refers to stm32f7xx_hal_usart.o(i.HAL_USART_RxCpltCallback) for HAL_USART_RxCpltCallback
    stm32f7xx_hal_usart.o(i.USART_DMARxHalfCplt) refers to stm32f7xx_hal_usart.o(i.HAL_USART_RxHalfCpltCallback) for HAL_USART_RxHalfCpltCallback
    stm32f7xx_hal_usart.o(i.USART_DMATransmitCplt) refers to stm32f7xx_hal_usart.o(i.HAL_USART_TxCpltCallback) for HAL_USART_TxCpltCallback
    stm32f7xx_hal_usart.o(i.USART_DMATxHalfCplt) refers to stm32f7xx_hal_usart.o(i.HAL_USART_TxHalfCpltCallback) for HAL_USART_TxHalfCpltCallback
    stm32f7xx_hal_usart.o(i.USART_EndTransmit_IT) refers to stm32f7xx_hal_usart.o(i.HAL_USART_TxCpltCallback) for HAL_USART_TxCpltCallback
    stm32f7xx_hal_usart.o(i.USART_Receive_IT) refers to stm32f7xx_hal_usart.o(i.HAL_USART_RxCpltCallback) for HAL_USART_RxCpltCallback
    stm32f7xx_hal_usart.o(i.USART_SetConfig) refers to stm32f7xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq) for HAL_RCC_GetPCLK1Freq
    stm32f7xx_hal_usart.o(i.USART_SetConfig) refers to stm32f7xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq) for HAL_RCC_GetPCLK2Freq
    stm32f7xx_hal_usart.o(i.USART_SetConfig) refers to stm32f7xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq) for HAL_RCC_GetSysClockFreq
    stm32f7xx_hal_usart.o(i.USART_TransmitReceive_IT) refers to stm32f7xx_hal_usart.o(i.HAL_USART_TxRxCpltCallback) for HAL_USART_TxRxCpltCallback
    stm32f7xx_hal_usart.o(i.USART_WaitOnFlagUntilTimeout) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_hal_wwdg.o(i.HAL_WWDG_IRQHandler) refers to stm32f7xx_hal_wwdg.o(i.HAL_WWDG_EarlyWakeupCallback) for HAL_WWDG_EarlyWakeupCallback
    stm32f7xx_hal_wwdg.o(i.HAL_WWDG_Init) refers to stm32f7xx_hal_wwdg.o(i.HAL_WWDG_MspInit) for HAL_WWDG_MspInit
    stm32f7xx_ll_fmc.o(i.FMC_NAND_GetECC) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_ll_fmc.o(i.FMC_SDRAM_SendCommand) refers to stm32f7xx_hal.o(i.HAL_GetTick) for HAL_GetTick
    stm32f7xx_ll_usb.o(i.USB_ActivateDedicatedEndpoint) refers to stm32f7xx_ll_usb.o(.data) for .data
    stm32f7xx_ll_usb.o(i.USB_CoreInit) refers to stm32f7xx_ll_usb.o(i.USB_CoreReset) for USB_CoreReset
    stm32f7xx_ll_usb.o(i.USB_DevConnect) refers to stm32f7xx_hal.o(i.HAL_Delay) for HAL_Delay
    stm32f7xx_ll_usb.o(i.USB_DevDisconnect) refers to stm32f7xx_hal.o(i.HAL_Delay) for HAL_Delay
    stm32f7xx_ll_usb.o(i.USB_DevInit) refers to stm32f7xx_ll_usb.o(i.USB_SetDevSpeed) for USB_SetDevSpeed
    stm32f7xx_ll_usb.o(i.USB_DevInit) refers to stm32f7xx_ll_usb.o(i.USB_FlushTxFifo) for USB_FlushTxFifo
    stm32f7xx_ll_usb.o(i.USB_DevInit) refers to stm32f7xx_ll_usb.o(i.USB_FlushRxFifo) for USB_FlushRxFifo
    stm32f7xx_ll_usb.o(i.USB_EPStartXfer) refers to stm32f7xx_ll_usb.o(i.USB_WritePacket) for USB_WritePacket
    stm32f7xx_ll_usb.o(i.USB_HC_StartXfer) refers to stm32f7xx_ll_usb.o(i.USB_DoPing) for USB_DoPing
    stm32f7xx_ll_usb.o(i.USB_HC_StartXfer) refers to stm32f7xx_ll_usb.o(i.USB_WritePacket) for USB_WritePacket
    stm32f7xx_ll_usb.o(i.USB_HostInit) refers to stm32f7xx_ll_usb.o(i.USB_FlushTxFifo) for USB_FlushTxFifo
    stm32f7xx_ll_usb.o(i.USB_HostInit) refers to stm32f7xx_ll_usb.o(i.USB_FlushRxFifo) for USB_FlushRxFifo
    stm32f7xx_ll_usb.o(i.USB_HostInit) refers to stm32f7xx_ll_usb.o(i.USB_DriveVbus) for USB_DriveVbus
    stm32f7xx_ll_usb.o(i.USB_HostInit) refers to stm32f7xx_hal.o(i.HAL_Delay) for HAL_Delay
    stm32f7xx_ll_usb.o(i.USB_ResetPort) refers to stm32f7xx_hal.o(i.HAL_Delay) for HAL_Delay
    stm32f7xx_ll_usb.o(i.USB_SetCurrentMode) refers to stm32f7xx_hal.o(i.HAL_Delay) for HAL_Delay
    stm32f7xx_ll_usb.o(i.USB_StopDevice) refers to stm32f7xx_ll_usb.o(i.USB_FlushRxFifo) for USB_FlushRxFifo
    stm32f7xx_ll_usb.o(i.USB_StopDevice) refers to stm32f7xx_ll_usb.o(i.USB_FlushTxFifo) for USB_FlushTxFifo
    stm32f7xx_ll_usb.o(i.USB_StopHost) refers to stm32f7xx_ll_usb.o(i.USB_DisableGlobalInt) for USB_DisableGlobalInt
    stm32f7xx_ll_usb.o(i.USB_StopHost) refers to stm32f7xx_ll_usb.o(i.USB_FlushTxFifo) for USB_FlushTxFifo
    stm32f7xx_ll_usb.o(i.USB_StopHost) refers to stm32f7xx_ll_usb.o(i.USB_FlushRxFifo) for USB_FlushRxFifo
    stm32f7xx_ll_usb.o(i.USB_StopHost) refers to stm32f7xx_ll_usb.o(i.USB_EnableGlobalInt) for USB_EnableGlobalInt
    main.o(i.SDRAM_Check) refers to printf5.o(i.__0printf$5) for __2printf
    main.o(i.SDRAM_Check) refers to main.o(.data) for .data
    main.o(i.SDRAM_Check) refers to main.o(.bss) for .bss
    main.o(i.SDRAM_Test_All) refers to printf5.o(i.__0printf$5) for __2printf
    main.o(i.SDRAM_Test_All) refers to bsp_sdram.o(i.SDRAM_Test) for SDRAM_Test
    main.o(i.SDRAM_Test_All) refers to stm32f7xx_hal_rng.o(i.HAL_RNG_Init) for HAL_RNG_Init
    main.o(i.SDRAM_Test_All) refers to stm32f7xx_hal_rng.o(i.HAL_RNG_GetRandomNumber) for HAL_RNG_GetRandomNumber
    main.o(i.SDRAM_Test_All) refers to main.o(i.SDRAM_Check) for SDRAM_Check
    main.o(i.SDRAM_Test_All) refers to main.o(.bss) for .bss
    main.o(i.SDRAM_Test_All) refers to main.o(.data) for .data
    main.o(i.SPI_Test_All) refers to printf5.o(i.__0printf$5) for __2printf
    main.o(i.SPI_Test_All) refers to bsp_qspi_flash.o(i.QSPI_FLASH_ReadDeviceID) for QSPI_FLASH_ReadDeviceID
    main.o(i.SPI_Test_All) refers to main.o(i.Delay) for Delay
    main.o(i.SPI_Test_All) refers to bsp_qspi_flash.o(i.QSPI_FLASH_ReadID) for QSPI_FLASH_ReadID
    main.o(i.SPI_Test_All) refers to bsp_qspi_flash.o(i.BSP_QSPI_Erase_Block) for BSP_QSPI_Erase_Block
    main.o(i.SPI_Test_All) refers to bsp_qspi_flash.o(i.BSP_QSPI_Write) for BSP_QSPI_Write
    main.o(i.SPI_Test_All) refers to bsp_qspi_flash.o(i.BSP_QSPI_Read) for BSP_QSPI_Read
    main.o(i.SPI_Test_All) refers to main.o(i.Buffercmp) for Buffercmp
    main.o(i.SPI_Test_All) refers to stm32f7xx_hal_gpio.o(i.HAL_GPIO_WritePin) for HAL_GPIO_WritePin
    main.o(i.SPI_Test_All) refers to main.o(.data) for .data
    main.o(i.SPI_Test_All) refers to main.o(.bss) for .bss
    main.o(i.SystemClock_Config) refers to stm32f7xx_hal_rcc.o(i.HAL_RCC_OscConfig) for HAL_RCC_OscConfig
    main.o(i.SystemClock_Config) refers to stm32f7xx_hal_pwr_ex.o(i.HAL_PWREx_EnableOverDrive) for HAL_PWREx_EnableOverDrive
    main.o(i.SystemClock_Config) refers to stm32f7xx_hal_rcc.o(i.HAL_RCC_ClockConfig) for HAL_RCC_ClockConfig
    main.o(i.main) refers to main.o(i.SystemClock_Config) for SystemClock_Config
    main.o(i.main) refers to bsp_key.o(i.Key_GPIO_Config) for Key_GPIO_Config
    main.o(i.main) refers to bsp_led.o(i.LED_GPIO_Config) for LED_GPIO_Config
    main.o(i.main) refers to bsp_qspi_flash.o(i.QSPI_FLASH_Init) for QSPI_FLASH_Init
    main.o(i.main) refers to bsp_debug_usart.o(i.DEBUG_USART_Config) for DEBUG_USART_Config
    main.o(i.main) refers to bsp_sdram.o(i.SDRAM_Init) for SDRAM_Init
    main.o(i.main) refers to main.o(i.SDRAM_Test_All) for SDRAM_Test_All
    main.o(i.main) refers to bsp_key.o(i.Key_Scan) for Key_Scan
    main.o(i.main) refers to main.o(i.SPI_Test_All) for SPI_Test_All
    stm32f7xx_it.o(i.SysTick_Handler) refers to stm32f7xx_hal.o(i.HAL_IncTick) for HAL_IncTick
    bsp_qspi_flash.o(i.BSP_QSPI_Erase_Block) refers to bsp_qspi_flash.o(i.QSPI_WriteEnable) for QSPI_WriteEnable
    bsp_qspi_flash.o(i.BSP_QSPI_Erase_Block) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_Command) for HAL_QSPI_Command
    bsp_qspi_flash.o(i.BSP_QSPI_Erase_Block) refers to bsp_qspi_flash.o(i.QSPI_AutoPollingMemReady) for QSPI_AutoPollingMemReady
    bsp_qspi_flash.o(i.BSP_QSPI_Erase_Block) refers to bsp_qspi_flash.o(.bss) for .bss
    bsp_qspi_flash.o(i.BSP_QSPI_Erase_Chip) refers to bsp_qspi_flash.o(i.QSPI_WriteEnable) for QSPI_WriteEnable
    bsp_qspi_flash.o(i.BSP_QSPI_Erase_Chip) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_Command) for HAL_QSPI_Command
    bsp_qspi_flash.o(i.BSP_QSPI_Erase_Chip) refers to bsp_qspi_flash.o(i.QSPI_AutoPollingMemReady) for QSPI_AutoPollingMemReady
    bsp_qspi_flash.o(i.BSP_QSPI_Erase_Chip) refers to bsp_qspi_flash.o(.bss) for .bss
    bsp_qspi_flash.o(i.BSP_QSPI_GetStatus) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_Command) for HAL_QSPI_Command
    bsp_qspi_flash.o(i.BSP_QSPI_GetStatus) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_Receive) for HAL_QSPI_Receive
    bsp_qspi_flash.o(i.BSP_QSPI_GetStatus) refers to bsp_qspi_flash.o(.bss) for .bss
    bsp_qspi_flash.o(i.BSP_QSPI_Init) refers to bsp_qspi_flash.o(i.QSPI_ResetMemory) for QSPI_ResetMemory
    bsp_qspi_flash.o(i.BSP_QSPI_Init) refers to bsp_qspi_flash.o(i.QSPI_WriteEnable) for QSPI_WriteEnable
    bsp_qspi_flash.o(i.BSP_QSPI_Init) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_Command) for HAL_QSPI_Command
    bsp_qspi_flash.o(i.BSP_QSPI_Init) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_Transmit) for HAL_QSPI_Transmit
    bsp_qspi_flash.o(i.BSP_QSPI_Init) refers to bsp_qspi_flash.o(i.QSPI_AutoPollingMemReady) for QSPI_AutoPollingMemReady
    bsp_qspi_flash.o(i.BSP_QSPI_Init) refers to bsp_qspi_flash.o(.bss) for .bss
    bsp_qspi_flash.o(i.BSP_QSPI_Read) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_Command) for HAL_QSPI_Command
    bsp_qspi_flash.o(i.BSP_QSPI_Read) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_Receive) for HAL_QSPI_Receive
    bsp_qspi_flash.o(i.BSP_QSPI_Read) refers to bsp_qspi_flash.o(.bss) for .bss
    bsp_qspi_flash.o(i.BSP_QSPI_Write) refers to bsp_qspi_flash.o(i.QSPI_WriteEnable) for QSPI_WriteEnable
    bsp_qspi_flash.o(i.BSP_QSPI_Write) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_Command) for HAL_QSPI_Command
    bsp_qspi_flash.o(i.BSP_QSPI_Write) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_Transmit) for HAL_QSPI_Transmit
    bsp_qspi_flash.o(i.BSP_QSPI_Write) refers to bsp_qspi_flash.o(i.QSPI_AutoPollingMemReady) for QSPI_AutoPollingMemReady
    bsp_qspi_flash.o(i.BSP_QSPI_Write) refers to bsp_qspi_flash.o(.bss) for .bss
    bsp_qspi_flash.o(i.QSPI_AutoPollingMemReady) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_AutoPolling) for HAL_QSPI_AutoPolling
    bsp_qspi_flash.o(i.QSPI_AutoPollingMemReady) refers to bsp_qspi_flash.o(.bss) for .bss
    bsp_qspi_flash.o(i.QSPI_FLASH_Init) refers to stm32f7xx_hal_gpio.o(i.HAL_GPIO_Init) for HAL_GPIO_Init
    bsp_qspi_flash.o(i.QSPI_FLASH_Init) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_Init) for HAL_QSPI_Init
    bsp_qspi_flash.o(i.QSPI_FLASH_Init) refers to bsp_qspi_flash.o(i.BSP_QSPI_Init) for BSP_QSPI_Init
    bsp_qspi_flash.o(i.QSPI_FLASH_Init) refers to bsp_qspi_flash.o(.bss) for .bss
    bsp_qspi_flash.o(i.QSPI_FLASH_ReadDeviceID) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_Command) for HAL_QSPI_Command
    bsp_qspi_flash.o(i.QSPI_FLASH_ReadDeviceID) refers to printf5.o(i.__0printf$5) for __2printf
    bsp_qspi_flash.o(i.QSPI_FLASH_ReadDeviceID) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_Receive) for HAL_QSPI_Receive
    bsp_qspi_flash.o(i.QSPI_FLASH_ReadDeviceID) refers to bsp_qspi_flash.o(.bss) for .bss
    bsp_qspi_flash.o(i.QSPI_FLASH_ReadID) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_Command) for HAL_QSPI_Command
    bsp_qspi_flash.o(i.QSPI_FLASH_ReadID) refers to printf5.o(i.__0printf$5) for __2printf
    bsp_qspi_flash.o(i.QSPI_FLASH_ReadID) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_Receive) for HAL_QSPI_Receive
    bsp_qspi_flash.o(i.QSPI_FLASH_ReadID) refers to bsp_qspi_flash.o(.bss) for .bss
    bsp_qspi_flash.o(i.QSPI_ResetMemory) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_Command) for HAL_QSPI_Command
    bsp_qspi_flash.o(i.QSPI_ResetMemory) refers to bsp_qspi_flash.o(i.QSPI_AutoPollingMemReady) for QSPI_AutoPollingMemReady
    bsp_qspi_flash.o(i.QSPI_ResetMemory) refers to bsp_qspi_flash.o(.bss) for .bss
    bsp_qspi_flash.o(i.QSPI_WriteEnable) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_Command) for HAL_QSPI_Command
    bsp_qspi_flash.o(i.QSPI_WriteEnable) refers to stm32f7xx_hal_qspi.o(i.HAL_QSPI_AutoPolling) for HAL_QSPI_AutoPolling
    bsp_qspi_flash.o(i.QSPI_WriteEnable) refers to bsp_qspi_flash.o(.bss) for .bss
    bsp_key.o(i.Key_GPIO_Config) refers to stm32f7xx_hal_gpio.o(i.HAL_GPIO_Init) for HAL_GPIO_Init
    bsp_key.o(i.Key_Scan) refers to stm32f7xx_hal_gpio.o(i.HAL_GPIO_ReadPin) for HAL_GPIO_ReadPin
    bsp_led.o(i.LED_GPIO_Config) refers to stm32f7xx_hal_gpio.o(i.HAL_GPIO_Init) for HAL_GPIO_Init
    bsp_led.o(i.LED_GPIO_Config) refers to stm32f7xx_hal_gpio.o(i.HAL_GPIO_WritePin) for HAL_GPIO_WritePin
    bsp_sdram.o(i.SDRAM_GPIO_Config) refers to stm32f7xx_hal_gpio.o(i.HAL_GPIO_Init) for HAL_GPIO_Init
    bsp_sdram.o(i.SDRAM_Init) refers to bsp_sdram.o(i.SDRAM_GPIO_Config) for SDRAM_GPIO_Config
    bsp_sdram.o(i.SDRAM_Init) refers to stm32f7xx_hal_sdram.o(i.HAL_SDRAM_Init) for HAL_SDRAM_Init
    bsp_sdram.o(i.SDRAM_Init) refers to bsp_sdram.o(i.SDRAM_InitSequence) for SDRAM_InitSequence
    bsp_sdram.o(i.SDRAM_Init) refers to bsp_sdram.o(.bss) for .bss
    bsp_sdram.o(i.SDRAM_InitSequence) refers to stm32f7xx_hal_sdram.o(i.HAL_SDRAM_SendCommand) for HAL_SDRAM_SendCommand
    bsp_sdram.o(i.SDRAM_InitSequence) refers to bsp_sdram.o(i.SDRAM_delay) for SDRAM_delay
    bsp_sdram.o(i.SDRAM_InitSequence) refers to stm32f7xx_hal_sdram.o(i.HAL_SDRAM_ProgramRefreshRate) for HAL_SDRAM_ProgramRefreshRate
    bsp_sdram.o(i.SDRAM_InitSequence) refers to bsp_sdram.o(.bss) for .bss
    bsp_sdram.o(i.SDRAM_ReadBuffer) refers to stm32f7xx_hal_sdram.o(i.HAL_SDRAM_GetState) for HAL_SDRAM_GetState
    bsp_sdram.o(i.SDRAM_ReadBuffer) refers to bsp_sdram.o(.bss) for .bss
    bsp_sdram.o(i.SDRAM_Test) refers to printf5.o(i.__0printf$5) for __2printf
    bsp_sdram.o(i.SDRAM_Test) refers to bsp_sdram.o(.conststring) for .conststring
    bsp_sdram.o(i.SDRAM_WriteBuffer) refers to stm32f7xx_hal_sdram.o(i.HAL_SDRAM_WriteProtection_Disable) for HAL_SDRAM_WriteProtection_Disable
    bsp_sdram.o(i.SDRAM_WriteBuffer) refers to stm32f7xx_hal_sdram.o(i.HAL_SDRAM_GetState) for HAL_SDRAM_GetState
    bsp_sdram.o(i.SDRAM_WriteBuffer) refers to bsp_sdram.o(.bss) for .bss
    bsp_debug_usart.o(i.DEBUG_USART_Config) refers to stm32f7xx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig) for HAL_RCCEx_PeriphCLKConfig
    bsp_debug_usart.o(i.DEBUG_USART_Config) refers to stm32f7xx_hal_gpio.o(i.HAL_GPIO_Init) for HAL_GPIO_Init
    bsp_debug_usart.o(i.DEBUG_USART_Config) refers to stm32f7xx_hal_uart.o(i.HAL_UART_Init) for HAL_UART_Init
    bsp_debug_usart.o(i.DEBUG_USART_Config) refers to stm32f7xx_hal_cortex.o(i.HAL_NVIC_SetPriority) for HAL_NVIC_SetPriority
    bsp_debug_usart.o(i.DEBUG_USART_Config) refers to stm32f7xx_hal_cortex.o(i.HAL_NVIC_EnableIRQ) for HAL_NVIC_EnableIRQ
    bsp_debug_usart.o(i.DEBUG_USART_Config) refers to bsp_debug_usart.o(.bss) for .bss
    bsp_debug_usart.o(i.Usart_SendString) refers to stm32f7xx_hal_uart.o(i.HAL_UART_Transmit) for HAL_UART_Transmit
    bsp_debug_usart.o(i.Usart_SendString) refers to bsp_debug_usart.o(.bss) for .bss
    bsp_debug_usart.o(i.fgetc) refers to stm32f7xx_hal_uart.o(i.HAL_UART_Receive) for HAL_UART_Receive
    bsp_debug_usart.o(i.fgetc) refers to bsp_debug_usart.o(.bss) for .bss
    bsp_debug_usart.o(i.fputc) refers to stm32f7xx_hal_uart.o(i.HAL_UART_Transmit) for HAL_UART_Transmit
    bsp_debug_usart.o(i.fputc) refers to bsp_debug_usart.o(.bss) for .bss
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry10a.o(.ARM.Collect$$$$0000000D) for __rt_final_cpp
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry11a.o(.ARM.Collect$$$$0000000F) for __rt_final_exit
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry7b.o(.ARM.Collect$$$$00000008) for _main_clock
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry8b.o(.ARM.Collect$$$$0000000A) for _main_cpp_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry9a.o(.ARM.Collect$$$$0000000B) for _main_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry5.o(.ARM.Collect$$$$00000004) for _main_scatterload
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry2.o(.ARM.Collect$$$$00000001) for _main_stk
    printfb.o(i.__0fprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0fprintf$bare) refers to bsp_debug_usart.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0printf$bare) refers to bsp_debug_usart.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printfb.o(i.__0vfprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vfprintf$bare) refers to bsp_debug_usart.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vprintf$bare) refers to bsp_debug_usart.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to stdout.o(.data) for __stdout
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printf0.o(i.__0fprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0fprintf$0) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0printf$0) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf0.o(i.__0vfprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vfprintf$0) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vprintf$0) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to stdout.o(.data) for __stdout
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf1.o(i.__0fprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0fprintf$1) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0printf$1) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i.__0vfprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vfprintf$1) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vprintf$1) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to stdout.o(.data) for __stdout
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf2.o(i.__0fprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0fprintf$2) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0printf$2) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf2.o(i.__0vfprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vfprintf$2) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vprintf$2) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to stdout.o(.data) for __stdout
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf3.o(i.__0fprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0fprintf$3) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0printf$3) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i.__0vfprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vfprintf$3) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vprintf$3) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to stdout.o(.data) for __stdout
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf4.o(i.__0fprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0fprintf$4) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0printf$4) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i.__0vfprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vfprintf$4) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vprintf$4) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to stdout.o(.data) for __stdout
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf5.o(i.__0fprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0fprintf$5) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0printf$5) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i.__0vfprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vfprintf$5) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vprintf$5) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to stdout.o(.data) for __stdout
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf6.o(i.__0fprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0fprintf$6) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0printf$6) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i.__0vfprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vfprintf$6) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vprintf$6) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to stdout.o(.data) for __stdout
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i._printf_core) refers to printf6.o(i._printf_pre_padding) for _printf_pre_padding
    printf6.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf6.o(i._printf_core) refers to printf6.o(i._printf_post_padding) for _printf_post_padding
    printf7.o(i.__0fprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0fprintf$7) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0printf$7) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i.__0vfprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vfprintf$7) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vprintf$7) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to stdout.o(.data) for __stdout
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i._printf_core) refers to printf7.o(i._printf_pre_padding) for _printf_pre_padding
    printf7.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf7.o(i._printf_core) refers to printf7.o(i._printf_post_padding) for _printf_post_padding
    printf8.o(i.__0fprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0fprintf$8) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0printf$8) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i.__0vfprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vfprintf$8) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vprintf$8) refers to bsp_debug_usart.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to stdout.o(.data) for __stdout
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i._printf_core) refers to printf8.o(i._printf_pre_padding) for _printf_pre_padding
    printf8.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf8.o(i._printf_core) refers to printf8.o(i._printf_post_padding) for _printf_post_padding
    printfa.o(i.__0fprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0fprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0fprintf) refers to bsp_debug_usart.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0printf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0printf) refers to bsp_debug_usart.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0snprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0snprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0snprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0sprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0sprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0sprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i.__0vfprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vfprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vfprintf) refers to bsp_debug_usart.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vprintf) refers to bsp_debug_usart.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers to stdout.o(.data) for __stdout
    printfa.o(i.__0vsnprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0vsprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i._fp_digits) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._fp_digits) refers to dmul.o(.text) for __aeabi_dmul
    printfa.o(i._fp_digits) refers to ddiv.o(.text) for __aeabi_ddiv
    printfa.o(i._fp_digits) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    printfa.o(i._fp_digits) refers to dadd.o(.text) for __aeabi_dadd
    printfa.o(i._fp_digits) refers to dfixul.o(.text) for __aeabi_d2ulz
    printfa.o(i._fp_digits) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_core) refers to printfa.o(i._printf_pre_padding) for _printf_pre_padding
    printfa.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers to printfa.o(i._printf_post_padding) for _printf_post_padding
    printfa.o(i._printf_core) refers to printfa.o(i._fp_digits) for _fp_digits
    printfa.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfa.o(i._printf_post_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_pre_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._snputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._sputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    entry2.o(.ARM.Collect$$$$00000001) refers to entry2.o(.ARM.Collect$$$$00002712) for __lit__00000000
    entry2.o(.ARM.Collect$$$$00002712) refers to startup_stm32f767xx.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to startup_stm32f767xx.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    entry5.o(.ARM.Collect$$$$00000004) refers to init.o(.text) for __scatterload
    entry9a.o(.ARM.Collect$$$$0000000B) refers to main.o(i.main) for main
    entry9b.o(.ARM.Collect$$$$0000000C) refers to main.o(i.main) for main
    uldiv.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    uldiv.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    dadd.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    dadd.o(.text) refers to llsshr.o(.text) for __aeabi_lasr
    dadd.o(.text) refers to depilogue.o(.text) for _double_epilogue
    dmul.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ddiv.o(.text) refers to depilogue.o(.text) for _double_round
    dfixul.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixul.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    init.o(.text) refers to entry5.o(.ARM.Collect$$$$00000004) for __main_after_scatterload
    depilogue.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to llushr.o(.text) for __aeabi_llsr


==============================================================================

Removing Unused input sections from the image.

    Removing startup_stm32f767xx.o(HEAP), (512 bytes).
    Removing system_stm32f7xx.o(.rev16_text), (4 bytes).
    Removing system_stm32f7xx.o(.revsh_text), (4 bytes).
    Removing system_stm32f7xx.o(.rrx_text), (6 bytes).
    Removing system_stm32f7xx.o(i.SystemCoreClockUpdate), (140 bytes).
    Removing stm32f7xx_hal.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal.o(i.HAL_DBGMCU_DisableDBGSleepMode), (16 bytes).
    Removing stm32f7xx_hal.o(i.HAL_DBGMCU_DisableDBGStandbyMode), (16 bytes).
    Removing stm32f7xx_hal.o(i.HAL_DBGMCU_DisableDBGStopMode), (16 bytes).
    Removing stm32f7xx_hal.o(i.HAL_DBGMCU_EnableDBGSleepMode), (16 bytes).
    Removing stm32f7xx_hal.o(i.HAL_DBGMCU_EnableDBGStandbyMode), (16 bytes).
    Removing stm32f7xx_hal.o(i.HAL_DBGMCU_EnableDBGStopMode), (16 bytes).
    Removing stm32f7xx_hal.o(i.HAL_DeInit), (52 bytes).
    Removing stm32f7xx_hal.o(i.HAL_Delay), (22 bytes).
    Removing stm32f7xx_hal.o(i.HAL_DisableCompensationCell), (16 bytes).
    Removing stm32f7xx_hal.o(i.HAL_DisableFMCMemorySwapping), (16 bytes).
    Removing stm32f7xx_hal.o(i.HAL_DisableMemorySwappingBank), (16 bytes).
    Removing stm32f7xx_hal.o(i.HAL_EnableCompensationCell), (16 bytes).
    Removing stm32f7xx_hal.o(i.HAL_EnableFMCMemorySwapping), (16 bytes).
    Removing stm32f7xx_hal.o(i.HAL_EnableMemorySwappingBank), (16 bytes).
    Removing stm32f7xx_hal.o(i.HAL_GetDEVID), (16 bytes).
    Removing stm32f7xx_hal.o(i.HAL_GetHalVersion), (8 bytes).
    Removing stm32f7xx_hal.o(i.HAL_GetREVID), (12 bytes).
    Removing stm32f7xx_hal.o(i.HAL_Init), (36 bytes).
    Removing stm32f7xx_hal.o(i.HAL_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal.o(i.HAL_MspInit), (2 bytes).
    Removing stm32f7xx_hal.o(i.HAL_ResumeTick), (14 bytes).
    Removing stm32f7xx_hal.o(i.HAL_SuspendTick), (14 bytes).
    Removing stm32f7xx_hal_adc.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_adc.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_adc.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_adc.o(i.ADC_DMAConvCplt), (98 bytes).
    Removing stm32f7xx_hal_adc.o(i.ADC_DMAError), (22 bytes).
    Removing stm32f7xx_hal_adc.o(i.ADC_DMAHalfConvCplt), (10 bytes).
    Removing stm32f7xx_hal_adc.o(i.ADC_Init), (312 bytes).
    Removing stm32f7xx_hal_adc.o(i.HAL_ADC_AnalogWDGConfig), (116 bytes).
    Removing stm32f7xx_hal_adc.o(i.HAL_ADC_ConfigChannel), (368 bytes).
    Removing stm32f7xx_hal_adc.o(i.HAL_ADC_ConvCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_adc.o(i.HAL_ADC_ConvHalfCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_adc.o(i.HAL_ADC_DeInit), (62 bytes).
    Removing stm32f7xx_hal_adc.o(i.HAL_ADC_ErrorCallback), (2 bytes).
    Removing stm32f7xx_hal_adc.o(i.HAL_ADC_GetError), (4 bytes).
    Removing stm32f7xx_hal_adc.o(i.HAL_ADC_GetState), (4 bytes).
    Removing stm32f7xx_hal_adc.o(i.HAL_ADC_GetValue), (6 bytes).
    Removing stm32f7xx_hal_adc.o(i.HAL_ADC_IRQHandler), (318 bytes).
    Removing stm32f7xx_hal_adc.o(i.HAL_ADC_Init), (84 bytes).
    Removing stm32f7xx_hal_adc.o(i.HAL_ADC_LevelOutOfWindowCallback), (2 bytes).
    Removing stm32f7xx_hal_adc.o(i.HAL_ADC_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_adc.o(i.HAL_ADC_MspInit), (2 bytes).
    Removing stm32f7xx_hal_adc.o(i.HAL_ADC_PollForConversion), (162 bytes).
    Removing stm32f7xx_hal_adc.o(i.HAL_ADC_PollForEvent), (114 bytes).
    Removing stm32f7xx_hal_adc.o(i.HAL_ADC_Start), (212 bytes).
    Removing stm32f7xx_hal_adc.o(i.HAL_ADC_Start_DMA), (284 bytes).
    Removing stm32f7xx_hal_adc.o(i.HAL_ADC_Start_IT), (224 bytes).
    Removing stm32f7xx_hal_adc.o(i.HAL_ADC_Stop), (60 bytes).
    Removing stm32f7xx_hal_adc.o(i.HAL_ADC_Stop_DMA), (88 bytes).
    Removing stm32f7xx_hal_adc.o(i.HAL_ADC_Stop_IT), (72 bytes).
    Removing stm32f7xx_hal_adc_ex.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_adc_ex.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_adc_ex.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_adc_ex.o(i.ADC_MultiModeDMAConvCplt), (90 bytes).
    Removing stm32f7xx_hal_adc_ex.o(i.ADC_MultiModeDMAError), (18 bytes).
    Removing stm32f7xx_hal_adc_ex.o(i.ADC_MultiModeDMAHalfConvCplt), (6 bytes).
    Removing stm32f7xx_hal_adc_ex.o(i.HAL_ADCEx_InjectedConfigChannel), (472 bytes).
    Removing stm32f7xx_hal_adc_ex.o(i.HAL_ADCEx_InjectedConvCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_adc_ex.o(i.HAL_ADCEx_InjectedGetValue), (62 bytes).
    Removing stm32f7xx_hal_adc_ex.o(i.HAL_ADCEx_InjectedPollForConversion), (136 bytes).
    Removing stm32f7xx_hal_adc_ex.o(i.HAL_ADCEx_InjectedStart), (220 bytes).
    Removing stm32f7xx_hal_adc_ex.o(i.HAL_ADCEx_InjectedStart_IT), (232 bytes).
    Removing stm32f7xx_hal_adc_ex.o(i.HAL_ADCEx_InjectedStop), (86 bytes).
    Removing stm32f7xx_hal_adc_ex.o(i.HAL_ADCEx_InjectedStop_IT), (94 bytes).
    Removing stm32f7xx_hal_adc_ex.o(i.HAL_ADCEx_MultiModeConfigChannel), (84 bytes).
    Removing stm32f7xx_hal_adc_ex.o(i.HAL_ADCEx_MultiModeGetValue), (12 bytes).
    Removing stm32f7xx_hal_adc_ex.o(i.HAL_ADCEx_MultiModeStart_DMA), (268 bytes).
    Removing stm32f7xx_hal_adc_ex.o(i.HAL_ADCEx_MultiModeStop_DMA), (96 bytes).
    Removing stm32f7xx_hal_can.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_can.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_can.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_can.o(i.CAN_Receive_IT), (266 bytes).
    Removing stm32f7xx_hal_can.o(i.CAN_Transmit_IT), (60 bytes).
    Removing stm32f7xx_hal_can.o(i.HAL_CAN_ConfigFilter), (260 bytes).
    Removing stm32f7xx_hal_can.o(i.HAL_CAN_DeInit), (34 bytes).
    Removing stm32f7xx_hal_can.o(i.HAL_CAN_ErrorCallback), (2 bytes).
    Removing stm32f7xx_hal_can.o(i.HAL_CAN_GetError), (4 bytes).
    Removing stm32f7xx_hal_can.o(i.HAL_CAN_GetState), (6 bytes).
    Removing stm32f7xx_hal_can.o(i.HAL_CAN_IRQHandler), (392 bytes).
    Removing stm32f7xx_hal_can.o(i.HAL_CAN_Init), (388 bytes).
    Removing stm32f7xx_hal_can.o(i.HAL_CAN_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_can.o(i.HAL_CAN_MspInit), (2 bytes).
    Removing stm32f7xx_hal_can.o(i.HAL_CAN_Receive), (342 bytes).
    Removing stm32f7xx_hal_can.o(i.HAL_CAN_Receive_IT), (104 bytes).
    Removing stm32f7xx_hal_can.o(i.HAL_CAN_RxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_can.o(i.HAL_CAN_Sleep), (118 bytes).
    Removing stm32f7xx_hal_can.o(i.HAL_CAN_Transmit), (432 bytes).
    Removing stm32f7xx_hal_can.o(i.HAL_CAN_Transmit_IT), (300 bytes).
    Removing stm32f7xx_hal_can.o(i.HAL_CAN_TxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_can.o(i.HAL_CAN_WakeUp), (106 bytes).
    Removing stm32f7xx_hal_cec.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_cec.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_cec.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_cec.o(i.HAL_CEC_ChangeRxBuffer), (4 bytes).
    Removing stm32f7xx_hal_cec.o(i.HAL_CEC_DeInit), (74 bytes).
    Removing stm32f7xx_hal_cec.o(i.HAL_CEC_ErrorCallback), (2 bytes).
    Removing stm32f7xx_hal_cec.o(i.HAL_CEC_GetError), (4 bytes).
    Removing stm32f7xx_hal_cec.o(i.HAL_CEC_GetLastReceivedFrameSize), (4 bytes).
    Removing stm32f7xx_hal_cec.o(i.HAL_CEC_GetState), (12 bytes).
    Removing stm32f7xx_hal_cec.o(i.HAL_CEC_IRQHandler), (264 bytes).
    Removing stm32f7xx_hal_cec.o(i.HAL_CEC_Init), (130 bytes).
    Removing stm32f7xx_hal_cec.o(i.HAL_CEC_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_cec.o(i.HAL_CEC_MspInit), (2 bytes).
    Removing stm32f7xx_hal_cec.o(i.HAL_CEC_RxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_cec.o(i.HAL_CEC_SetDeviceAddress), (112 bytes).
    Removing stm32f7xx_hal_cec.o(i.HAL_CEC_Transmit_IT), (98 bytes).
    Removing stm32f7xx_hal_cec.o(i.HAL_CEC_TxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_cortex.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_cortex.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_cortex.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_cortex.o(i.HAL_MPU_ConfigRegion), (88 bytes).
    Removing stm32f7xx_hal_cortex.o(i.HAL_MPU_Disable), (28 bytes).
    Removing stm32f7xx_hal_cortex.o(i.HAL_MPU_Enable), (36 bytes).
    Removing stm32f7xx_hal_cortex.o(i.HAL_NVIC_ClearPendingIRQ), (22 bytes).
    Removing stm32f7xx_hal_cortex.o(i.HAL_NVIC_DisableIRQ), (22 bytes).
    Removing stm32f7xx_hal_cortex.o(i.HAL_NVIC_GetActive), (32 bytes).
    Removing stm32f7xx_hal_cortex.o(i.HAL_NVIC_GetPendingIRQ), (32 bytes).
    Removing stm32f7xx_hal_cortex.o(i.HAL_NVIC_GetPriority), (86 bytes).
    Removing stm32f7xx_hal_cortex.o(i.HAL_NVIC_GetPriorityGrouping), (16 bytes).
    Removing stm32f7xx_hal_cortex.o(i.HAL_NVIC_SetPendingIRQ), (22 bytes).
    Removing stm32f7xx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping), (36 bytes).
    Removing stm32f7xx_hal_cortex.o(i.HAL_NVIC_SystemReset), (36 bytes).
    Removing stm32f7xx_hal_cortex.o(i.HAL_SYSTICK_CLKSourceConfig), (28 bytes).
    Removing stm32f7xx_hal_cortex.o(i.HAL_SYSTICK_Callback), (2 bytes).
    Removing stm32f7xx_hal_cortex.o(i.HAL_SYSTICK_IRQHandler), (8 bytes).
    Removing stm32f7xx_hal_crc.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_crc.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_crc.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_crc.o(i.CRC_Handle_16), (54 bytes).
    Removing stm32f7xx_hal_crc.o(i.CRC_Handle_8), (122 bytes).
    Removing stm32f7xx_hal_crc.o(i.HAL_CRC_Accumulate), (90 bytes).
    Removing stm32f7xx_hal_crc.o(i.HAL_CRC_Calculate), (104 bytes).
    Removing stm32f7xx_hal_crc.o(i.HAL_CRC_DeInit), (58 bytes).
    Removing stm32f7xx_hal_crc.o(i.HAL_CRC_GetState), (4 bytes).
    Removing stm32f7xx_hal_crc.o(i.HAL_CRC_Init), (128 bytes).
    Removing stm32f7xx_hal_crc.o(i.HAL_CRC_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_crc.o(i.HAL_CRC_MspInit), (2 bytes).
    Removing stm32f7xx_hal_crc_ex.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_crc_ex.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_crc_ex.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_crc_ex.o(i.HAL_CRCEx_Input_Data_Reverse), (24 bytes).
    Removing stm32f7xx_hal_crc_ex.o(i.HAL_CRCEx_Output_Data_Reverse), (24 bytes).
    Removing stm32f7xx_hal_crc_ex.o(i.HAL_CRCEx_Polynomial_Set), (78 bytes).
    Removing stm32f7xx_hal_cryp.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_cryp.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_cryp.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_cryp_ex.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_cryp_ex.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_cryp_ex.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_dac.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_dac.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_dac.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_dac.o(i.DAC_DMAConvCpltCh1), (16 bytes).
    Removing stm32f7xx_hal_dac.o(i.DAC_DMAErrorCh1), (24 bytes).
    Removing stm32f7xx_hal_dac.o(i.DAC_DMAHalfConvCpltCh1), (10 bytes).
    Removing stm32f7xx_hal_dac.o(i.HAL_DAC_ConfigChannel), (66 bytes).
    Removing stm32f7xx_hal_dac.o(i.HAL_DAC_ConvCpltCallbackCh1), (2 bytes).
    Removing stm32f7xx_hal_dac.o(i.HAL_DAC_ConvHalfCpltCallbackCh1), (2 bytes).
    Removing stm32f7xx_hal_dac.o(i.HAL_DAC_DMAUnderrunCallbackCh1), (2 bytes).
    Removing stm32f7xx_hal_dac.o(i.HAL_DAC_DeInit), (32 bytes).
    Removing stm32f7xx_hal_dac.o(i.HAL_DAC_ErrorCallbackCh1), (2 bytes).
    Removing stm32f7xx_hal_dac.o(i.HAL_DAC_GetError), (4 bytes).
    Removing stm32f7xx_hal_dac.o(i.HAL_DAC_GetState), (4 bytes).
    Removing stm32f7xx_hal_dac.o(i.HAL_DAC_GetValue), (14 bytes).
    Removing stm32f7xx_hal_dac.o(i.HAL_DAC_IRQHandler), (92 bytes).
    Removing stm32f7xx_hal_dac.o(i.HAL_DAC_Init), (42 bytes).
    Removing stm32f7xx_hal_dac.o(i.HAL_DAC_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_dac.o(i.HAL_DAC_MspInit), (2 bytes).
    Removing stm32f7xx_hal_dac.o(i.HAL_DAC_SetValue), (32 bytes).
    Removing stm32f7xx_hal_dac.o(i.HAL_DAC_Start), (112 bytes).
    Removing stm32f7xx_hal_dac.o(i.HAL_DAC_Start_DMA), (264 bytes).
    Removing stm32f7xx_hal_dac.o(i.HAL_DAC_Stop), (22 bytes).
    Removing stm32f7xx_hal_dac.o(i.HAL_DAC_Stop_DMA), (62 bytes).
    Removing stm32f7xx_hal_dac_ex.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_dac_ex.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_dac_ex.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_dac_ex.o(i.DAC_DMAConvCpltCh2), (16 bytes).
    Removing stm32f7xx_hal_dac_ex.o(i.DAC_DMAErrorCh2), (24 bytes).
    Removing stm32f7xx_hal_dac_ex.o(i.DAC_DMAHalfConvCpltCh2), (10 bytes).
    Removing stm32f7xx_hal_dac_ex.o(i.HAL_DACEx_ConvCpltCallbackCh2), (2 bytes).
    Removing stm32f7xx_hal_dac_ex.o(i.HAL_DACEx_ConvHalfCpltCallbackCh2), (2 bytes).
    Removing stm32f7xx_hal_dac_ex.o(i.HAL_DACEx_DMAUnderrunCallbackCh2), (2 bytes).
    Removing stm32f7xx_hal_dac_ex.o(i.HAL_DACEx_DualGetValue), (12 bytes).
    Removing stm32f7xx_hal_dac_ex.o(i.HAL_DACEx_DualSetValue), (24 bytes).
    Removing stm32f7xx_hal_dac_ex.o(i.HAL_DACEx_ErrorCallbackCh2), (2 bytes).
    Removing stm32f7xx_hal_dac_ex.o(i.HAL_DACEx_NoiseWaveGenerate), (52 bytes).
    Removing stm32f7xx_hal_dac_ex.o(i.HAL_DACEx_TriangleWaveGenerate), (52 bytes).
    Removing stm32f7xx_hal_dcmi.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_dcmi.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_dcmi.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_dcmi.o(i.DCMI_DMAError), (32 bytes).
    Removing stm32f7xx_hal_dcmi.o(i.DCMI_DMAXferCplt), (146 bytes).
    Removing stm32f7xx_hal_dcmi.o(i.HAL_DCMI_ConfigCrop), (84 bytes).
    Removing stm32f7xx_hal_dcmi.o(i.HAL_DCMI_DeInit), (22 bytes).
    Removing stm32f7xx_hal_dcmi.o(i.HAL_DCMI_DisableCrop), (44 bytes).
    Removing stm32f7xx_hal_dcmi.o(i.HAL_DCMI_EnableCrop), (44 bytes).
    Removing stm32f7xx_hal_dcmi.o(i.HAL_DCMI_ErrorCallback), (2 bytes).
    Removing stm32f7xx_hal_dcmi.o(i.HAL_DCMI_FrameEventCallback), (2 bytes).
    Removing stm32f7xx_hal_dcmi.o(i.HAL_DCMI_GetError), (4 bytes).
    Removing stm32f7xx_hal_dcmi.o(i.HAL_DCMI_GetState), (6 bytes).
    Removing stm32f7xx_hal_dcmi.o(i.HAL_DCMI_IRQHandler), (160 bytes).
    Removing stm32f7xx_hal_dcmi.o(i.HAL_DCMI_Init), (188 bytes).
    Removing stm32f7xx_hal_dcmi.o(i.HAL_DCMI_LineEventCallback), (2 bytes).
    Removing stm32f7xx_hal_dcmi.o(i.HAL_DCMI_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_dcmi.o(i.HAL_DCMI_MspInit), (2 bytes).
    Removing stm32f7xx_hal_dcmi.o(i.HAL_DCMI_Resume), (54 bytes).
    Removing stm32f7xx_hal_dcmi.o(i.HAL_DCMI_Start_DMA), (184 bytes).
    Removing stm32f7xx_hal_dcmi.o(i.HAL_DCMI_Stop), (116 bytes).
    Removing stm32f7xx_hal_dcmi.o(i.HAL_DCMI_Suspend), (108 bytes).
    Removing stm32f7xx_hal_dcmi.o(i.HAL_DCMI_VsyncEventCallback), (2 bytes).
    Removing stm32f7xx_hal_dcmi_ex.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_dcmi_ex.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_dcmi_ex.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_dma.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_dma.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_dma.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_dma.o(i.DMA_CalcBaseAndBitshift), (44 bytes).
    Removing stm32f7xx_hal_dma.o(i.DMA_CheckFifoParam), (136 bytes).
    Removing stm32f7xx_hal_dma.o(i.DMA_SetConfig), (42 bytes).
    Removing stm32f7xx_hal_dma.o(i.HAL_DMA_Abort), (142 bytes).
    Removing stm32f7xx_hal_dma.o(i.HAL_DMA_Abort_IT), (36 bytes).
    Removing stm32f7xx_hal_dma.o(i.HAL_DMA_DeInit), (90 bytes).
    Removing stm32f7xx_hal_dma.o(i.HAL_DMA_GetError), (4 bytes).
    Removing stm32f7xx_hal_dma.o(i.HAL_DMA_GetState), (6 bytes).
    Removing stm32f7xx_hal_dma.o(i.HAL_DMA_IRQHandler), (472 bytes).
    Removing stm32f7xx_hal_dma.o(i.HAL_DMA_Init), (208 bytes).
    Removing stm32f7xx_hal_dma.o(i.HAL_DMA_PollForTransfer), (292 bytes).
    Removing stm32f7xx_hal_dma.o(i.HAL_DMA_RegisterCallback), (80 bytes).
    Removing stm32f7xx_hal_dma.o(i.HAL_DMA_Start), (70 bytes).
    Removing stm32f7xx_hal_dma.o(i.HAL_DMA_Start_IT), (120 bytes).
    Removing stm32f7xx_hal_dma.o(i.HAL_DMA_UnRegisterCallback), (100 bytes).
    Removing stm32f7xx_hal_dma.o(.constdata), (8 bytes).
    Removing stm32f7xx_hal_dma_ex.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_dma_ex.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_dma_ex.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_dma_ex.o(i.DMA_MultiBufferSetConfig), (32 bytes).
    Removing stm32f7xx_hal_dma_ex.o(i.HAL_DMAEx_ChangeMemory), (16 bytes).
    Removing stm32f7xx_hal_dma_ex.o(i.HAL_DMAEx_MultiBufferStart), (100 bytes).
    Removing stm32f7xx_hal_dma_ex.o(i.HAL_DMAEx_MultiBufferStart_IT), (2824 bytes).
    Removing stm32f7xx_hal_dma2d.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_dma2d.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_dma2d.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.DMA2D_SetConfig), (172 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_Abort), (94 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_BlendingStart), (62 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_BlendingStart_IT), (72 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_CLUTLoad), (152 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_CLUTLoad_IT), (172 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_CLUTLoadingCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_CLUTLoading_Abort), (102 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_CLUTLoading_Resume), (54 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_CLUTLoading_Suspend), (110 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_ConfigCLUT), (140 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_ConfigDeadTime), (62 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_ConfigLayer), (224 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_DeInit), (128 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_DisableDeadTime), (44 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_EnableCLUT), (52 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_EnableDeadTime), (44 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_GetError), (4 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_GetState), (6 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_IRQHandler), (286 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_Init), (148 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_LineEventCallback), (2 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_MspInit), (2 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_PollForTransfer), (302 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_ProgramLineEvent), (60 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_Resume), (28 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_Start), (52 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_Start_IT), (62 bytes).
    Removing stm32f7xx_hal_dma2d.o(i.HAL_DMA2D_Suspend), (96 bytes).
    Removing stm32f7xx_hal_eth.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_eth.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_eth.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_eth.o(i.ETH_DMAReceptionDisable), (16 bytes).
    Removing stm32f7xx_hal_eth.o(i.ETH_DMAReceptionEnable), (16 bytes).
    Removing stm32f7xx_hal_eth.o(i.ETH_DMATransmissionDisable), (16 bytes).
    Removing stm32f7xx_hal_eth.o(i.ETH_DMATransmissionEnable), (16 bytes).
    Removing stm32f7xx_hal_eth.o(i.ETH_FlushTransmitFIFO), (46 bytes).
    Removing stm32f7xx_hal_eth.o(i.ETH_MACAddressConfig), (44 bytes).
    Removing stm32f7xx_hal_eth.o(i.ETH_MACDMAConfig), (400 bytes).
    Removing stm32f7xx_hal_eth.o(i.ETH_MACReceptionDisable), (34 bytes).
    Removing stm32f7xx_hal_eth.o(i.ETH_MACReceptionEnable), (34 bytes).
    Removing stm32f7xx_hal_eth.o(i.ETH_MACTransmissionDisable), (34 bytes).
    Removing stm32f7xx_hal_eth.o(i.ETH_MACTransmissionEnable), (34 bytes).
    Removing stm32f7xx_hal_eth.o(i.HAL_ETH_ConfigDMA), (184 bytes).
    Removing stm32f7xx_hal_eth.o(i.HAL_ETH_ConfigMAC), (304 bytes).
    Removing stm32f7xx_hal_eth.o(i.HAL_ETH_DMARxDescListInit), (110 bytes).
    Removing stm32f7xx_hal_eth.o(i.HAL_ETH_DMATxDescListInit), (122 bytes).
    Removing stm32f7xx_hal_eth.o(i.HAL_ETH_DeInit), (26 bytes).
    Removing stm32f7xx_hal_eth.o(i.HAL_ETH_ErrorCallback), (2 bytes).
    Removing stm32f7xx_hal_eth.o(i.HAL_ETH_GetReceivedFrame), (126 bytes).
    Removing stm32f7xx_hal_eth.o(i.HAL_ETH_GetReceivedFrame_IT), (142 bytes).
    Removing stm32f7xx_hal_eth.o(i.HAL_ETH_GetState), (6 bytes).
    Removing stm32f7xx_hal_eth.o(i.HAL_ETH_IRQHandler), (130 bytes).
    Removing stm32f7xx_hal_eth.o(i.HAL_ETH_Init), (560 bytes).
    Removing stm32f7xx_hal_eth.o(i.HAL_ETH_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_eth.o(i.HAL_ETH_MspInit), (2 bytes).
    Removing stm32f7xx_hal_eth.o(i.HAL_ETH_ReadPHYRegister), (130 bytes).
    Removing stm32f7xx_hal_eth.o(i.HAL_ETH_RxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_eth.o(i.HAL_ETH_Start), (68 bytes).
    Removing stm32f7xx_hal_eth.o(i.HAL_ETH_Stop), (68 bytes).
    Removing stm32f7xx_hal_eth.o(i.HAL_ETH_TransmitFrame), (274 bytes).
    Removing stm32f7xx_hal_eth.o(i.HAL_ETH_TxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_eth.o(i.HAL_ETH_WritePHYRegister), (122 bytes).
    Removing stm32f7xx_hal_flash.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_flash.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_flash.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_flash.o(i.FLASH_Program_Byte), (36 bytes).
    Removing stm32f7xx_hal_flash.o(i.FLASH_Program_DoubleWord), (44 bytes).
    Removing stm32f7xx_hal_flash.o(i.FLASH_Program_HalfWord), (40 bytes).
    Removing stm32f7xx_hal_flash.o(i.FLASH_Program_Word), (40 bytes).
    Removing stm32f7xx_hal_flash.o(i.FLASH_SetErrorCode), (88 bytes).
    Removing stm32f7xx_hal_flash.o(i.FLASH_WaitForLastOperation), (84 bytes).
    Removing stm32f7xx_hal_flash.o(i.HAL_FLASH_EndOfOperationCallback), (2 bytes).
    Removing stm32f7xx_hal_flash.o(i.HAL_FLASH_GetError), (12 bytes).
    Removing stm32f7xx_hal_flash.o(i.HAL_FLASH_IRQHandler), (240 bytes).
    Removing stm32f7xx_hal_flash.o(i.HAL_FLASH_Lock), (20 bytes).
    Removing stm32f7xx_hal_flash.o(i.HAL_FLASH_OB_Launch), (24 bytes).
    Removing stm32f7xx_hal_flash.o(i.HAL_FLASH_OB_Lock), (20 bytes).
    Removing stm32f7xx_hal_flash.o(i.HAL_FLASH_OB_Unlock), (40 bytes).
    Removing stm32f7xx_hal_flash.o(i.HAL_FLASH_OperationErrorCallback), (2 bytes).
    Removing stm32f7xx_hal_flash.o(i.HAL_FLASH_Program), (132 bytes).
    Removing stm32f7xx_hal_flash.o(i.HAL_FLASH_Program_IT), (116 bytes).
    Removing stm32f7xx_hal_flash.o(i.HAL_FLASH_Unlock), (40 bytes).
    Removing stm32f7xx_hal_flash.o(.bss), (28 bytes).
    Removing stm32f7xx_hal_flash_ex.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_flash_ex.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_flash_ex.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_flash_ex.o(i.FLASH_Erase_Sector), (100 bytes).
    Removing stm32f7xx_hal_flash_ex.o(i.FLASH_MassErase), (72 bytes).
    Removing stm32f7xx_hal_flash_ex.o(i.FLASH_OB_BOR_LevelConfig), (20 bytes).
    Removing stm32f7xx_hal_flash_ex.o(i.FLASH_OB_BootAddressConfig), (52 bytes).
    Removing stm32f7xx_hal_flash_ex.o(i.FLASH_OB_DisableWRP), (32 bytes).
    Removing stm32f7xx_hal_flash_ex.o(i.FLASH_OB_EnableWRP), (32 bytes).
    Removing stm32f7xx_hal_flash_ex.o(i.FLASH_OB_GetBOR), (16 bytes).
    Removing stm32f7xx_hal_flash_ex.o(i.FLASH_OB_GetBootAddress), (24 bytes).
    Removing stm32f7xx_hal_flash_ex.o(i.FLASH_OB_GetRDP), (28 bytes).
    Removing stm32f7xx_hal_flash_ex.o(i.FLASH_OB_GetUser), (20 bytes).
    Removing stm32f7xx_hal_flash_ex.o(i.FLASH_OB_GetWRP), (20 bytes).
    Removing stm32f7xx_hal_flash_ex.o(i.FLASH_OB_RDP_LevelConfig), (28 bytes).
    Removing stm32f7xx_hal_flash_ex.o(i.FLASH_OB_UserConfig), (80 bytes).
    Removing stm32f7xx_hal_flash_ex.o(i.HAL_FLASHEx_Erase), (148 bytes).
    Removing stm32f7xx_hal_flash_ex.o(i.HAL_FLASHEx_Erase_IT), (100 bytes).
    Removing stm32f7xx_hal_flash_ex.o(i.HAL_FLASHEx_OBGetConfig), (50 bytes).
    Removing stm32f7xx_hal_flash_ex.o(i.HAL_FLASHEx_OBProgram), (164 bytes).
    Removing stm32f7xx_hal_gpio.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_gpio.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_gpio.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_gpio.o(i.HAL_GPIO_DeInit), (348 bytes).
    Removing stm32f7xx_hal_gpio.o(i.HAL_GPIO_EXTI_Callback), (2 bytes).
    Removing stm32f7xx_hal_gpio.o(i.HAL_GPIO_EXTI_IRQHandler), (24 bytes).
    Removing stm32f7xx_hal_gpio.o(i.HAL_GPIO_LockPin), (36 bytes).
    Removing stm32f7xx_hal_gpio.o(i.HAL_GPIO_TogglePin), (8 bytes).
    Removing stm32f7xx_hal_hash.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_hash.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_hash.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_hash_ex.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_hash_ex.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_hash_ex.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_hcd.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_hcd.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_hcd.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_hcd.o(i.HAL_HCD_Connect_Callback), (2 bytes).
    Removing stm32f7xx_hal_hcd.o(i.HAL_HCD_DeInit), (38 bytes).
    Removing stm32f7xx_hal_hcd.o(i.HAL_HCD_Disconnect_Callback), (2 bytes).
    Removing stm32f7xx_hal_hcd.o(i.HAL_HCD_GetCurrentFrame), (6 bytes).
    Removing stm32f7xx_hal_hcd.o(i.HAL_HCD_GetCurrentSpeed), (6 bytes).
    Removing stm32f7xx_hal_hcd.o(i.HAL_HCD_GetState), (6 bytes).
    Removing stm32f7xx_hal_hcd.o(i.HAL_HCD_HC_GetState), (14 bytes).
    Removing stm32f7xx_hal_hcd.o(i.HAL_HCD_HC_GetURBState), (14 bytes).
    Removing stm32f7xx_hal_hcd.o(i.HAL_HCD_HC_GetXferCount), (12 bytes).
    Removing stm32f7xx_hal_hcd.o(i.HAL_HCD_HC_Halt), (36 bytes).
    Removing stm32f7xx_hal_hcd.o(i.HAL_HCD_HC_Init), (80 bytes).
    Removing stm32f7xx_hal_hcd.o(i.HAL_HCD_HC_NotifyURBChange_Callback), (2 bytes).
    Removing stm32f7xx_hal_hcd.o(i.HAL_HCD_HC_SubmitRequest), (244 bytes).
    Removing stm32f7xx_hal_hcd.o(i.HAL_HCD_IRQHandler), (304 bytes).
    Removing stm32f7xx_hal_hcd.o(i.HAL_HCD_Init), (92 bytes).
    Removing stm32f7xx_hal_hcd.o(i.HAL_HCD_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_hcd.o(i.HAL_HCD_MspInit), (2 bytes).
    Removing stm32f7xx_hal_hcd.o(i.HAL_HCD_ResetPort), (6 bytes).
    Removing stm32f7xx_hal_hcd.o(i.HAL_HCD_SOF_Callback), (2 bytes).
    Removing stm32f7xx_hal_hcd.o(i.HAL_HCD_Start), (44 bytes).
    Removing stm32f7xx_hal_hcd.o(i.HAL_HCD_Stop), (36 bytes).
    Removing stm32f7xx_hal_hcd.o(i.HCD_HC_IN_IRQHandler), (558 bytes).
    Removing stm32f7xx_hal_hcd.o(i.HCD_HC_OUT_IRQHandler), (538 bytes).
    Removing stm32f7xx_hal_hcd.o(i.HCD_Port_IRQHandler), (184 bytes).
    Removing stm32f7xx_hal_hcd.o(i.HCD_RXQLVL_IRQHandler), (112 bytes).
    Removing stm32f7xx_hal_i2c.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_i2c.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_i2c.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_AbortCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_AddrCallback), (2 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_DeInit), (50 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_DisableListen_IT), (50 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_ER_IRQHandler), (98 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_EV_IRQHandler), (16 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_EnableListen_IT), (40 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_ErrorCallback), (2 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_GetError), (4 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_GetMode), (6 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_GetState), (6 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_Init), (192 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_IsDeviceReady), (320 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_ListenCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_MasterRxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_MasterTxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Abort_IT), (92 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Receive), (348 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Receive_DMA), (220 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Receive_IT), (140 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Sequential_Receive_IT), (128 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Sequential_Transmit_IT), (128 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Transmit), (348 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Transmit_DMA), (204 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_Master_Transmit_IT), (140 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_MemRxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_MemTxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Read), (396 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Read_DMA), (272 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Read_IT), (216 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Write), (400 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Write_DMA), (268 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_Mem_Write_IT), (212 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_MspInit), (2 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_SlaveRxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_SlaveTxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Receive), (348 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Receive_DMA), (168 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Receive_IT), (96 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Sequential_Receive_IT), (132 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Sequential_Transmit_IT), (132 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Transmit), (368 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Transmit_DMA), (160 bytes).
    Removing stm32f7xx_hal_i2c.o(i.HAL_I2C_Slave_Transmit_IT), (96 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_DMAAbort), (50 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_DMAError), (18 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_DMAMasterReceiveCplt), (80 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_DMAMasterTransmitCplt), (80 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_DMASlaveReceiveCplt), (2 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_DMASlaveTransmitCplt), (2 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_Disable_IRQ), (100 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_Enable_IRQ), (104 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_Flush_TXDR), (34 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_ITAddrCplt), (160 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_ITError), (224 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_ITListenCplt), (92 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_ITMasterCplt), (192 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_ITMasterSequentialCplt), (80 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_ITSlaveCplt), (272 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_ITSlaveSequentialCplt), (84 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_IsAcknowledgeFailed), (128 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_Master_ISR_DMA), (202 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_Master_ISR_IT), (324 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_RequestMemoryRead), (132 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_RequestMemoryWrite), (132 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_Slave_ISR_DMA), (114 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_Slave_ISR_IT), (284 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_TransferConfig), (36 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_WaitOnFlagUntilTimeout), (78 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_WaitOnRXNEFlagUntilTimeout), (132 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_WaitOnSTOPFlagUntilTimeout), (76 bytes).
    Removing stm32f7xx_hal_i2c.o(i.I2C_WaitOnTXISFlagUntilTimeout), (80 bytes).
    Removing stm32f7xx_hal_i2c_ex.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_i2c_ex.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_i2c_ex.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_i2c_ex.o(i.HAL_I2CEx_ConfigAnalogFilter), (90 bytes).
    Removing stm32f7xx_hal_i2c_ex.o(i.HAL_I2CEx_ConfigDigitalFilter), (86 bytes).
    Removing stm32f7xx_hal_i2c_ex.o(i.HAL_I2CEx_DisableFastModePlus), (40 bytes).
    Removing stm32f7xx_hal_i2c_ex.o(i.HAL_I2CEx_EnableFastModePlus), (40 bytes).
    Removing stm32f7xx_hal_i2s.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_i2s.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_i2s.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_i2s.o(i.HAL_I2S_DMAPause), (110 bytes).
    Removing stm32f7xx_hal_i2s.o(i.HAL_I2S_DMAResume), (84 bytes).
    Removing stm32f7xx_hal_i2s.o(i.HAL_I2S_DMAStop), (104 bytes).
    Removing stm32f7xx_hal_i2s.o(i.HAL_I2S_DeInit), (36 bytes).
    Removing stm32f7xx_hal_i2s.o(i.HAL_I2S_ErrorCallback), (2 bytes).
    Removing stm32f7xx_hal_i2s.o(i.HAL_I2S_GetError), (4 bytes).
    Removing stm32f7xx_hal_i2s.o(i.HAL_I2S_GetState), (6 bytes).
    Removing stm32f7xx_hal_i2s.o(i.HAL_I2S_IRQHandler), (156 bytes).
    Removing stm32f7xx_hal_i2s.o(i.HAL_I2S_Init), (244 bytes).
    Removing stm32f7xx_hal_i2s.o(i.HAL_I2S_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_i2s.o(i.HAL_I2S_MspInit), (2 bytes).
    Removing stm32f7xx_hal_i2s.o(i.HAL_I2S_Receive), (238 bytes).
    Removing stm32f7xx_hal_i2s.o(i.HAL_I2S_Receive_DMA), (200 bytes).
    Removing stm32f7xx_hal_i2s.o(i.HAL_I2S_Receive_IT), (122 bytes).
    Removing stm32f7xx_hal_i2s.o(i.HAL_I2S_RxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_i2s.o(i.HAL_I2S_RxHalfCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_i2s.o(i.HAL_I2S_Transmit), (274 bytes).
    Removing stm32f7xx_hal_i2s.o(i.HAL_I2S_Transmit_DMA), (176 bytes).
    Removing stm32f7xx_hal_i2s.o(i.HAL_I2S_Transmit_IT), (122 bytes).
    Removing stm32f7xx_hal_i2s.o(i.HAL_I2S_TxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_i2s.o(i.HAL_I2S_TxHalfCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_i2s.o(i.I2S_DMAError), (40 bytes).
    Removing stm32f7xx_hal_i2s.o(i.I2S_DMARxCplt), (60 bytes).
    Removing stm32f7xx_hal_i2s.o(i.I2S_DMARxHalfCplt), (10 bytes).
    Removing stm32f7xx_hal_i2s.o(i.I2S_DMATxCplt), (60 bytes).
    Removing stm32f7xx_hal_i2s.o(i.I2S_DMATxHalfCplt), (10 bytes).
    Removing stm32f7xx_hal_i2s.o(i.I2S_GetClockFreq), (92 bytes).
    Removing stm32f7xx_hal_i2s.o(i.I2S_Receive_IT), (48 bytes).
    Removing stm32f7xx_hal_i2s.o(i.I2S_Transmit_IT), (48 bytes).
    Removing stm32f7xx_hal_i2s.o(i.I2S_WaitFlagStateUntilTimeout), (118 bytes).
    Removing stm32f7xx_hal_irda.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_irda.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_irda.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_Abort), (110 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_AbortCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_AbortReceive), (74 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_AbortReceiveCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_AbortReceive_IT), (116 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_AbortTransmit), (58 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_AbortTransmitCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_AbortTransmit_IT), (96 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_Abort_IT), (184 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_DMAPause), (98 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_DMAResume), (92 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_DMAStop), (84 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_DeInit), (50 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_ErrorCallback), (2 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_GetError), (4 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_GetState), (12 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_IRQHandler), (316 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_Init), (112 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_MspInit), (2 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_Receive), (224 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_Receive_DMA), (148 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_Receive_IT), (144 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_RxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_RxHalfCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_Transmit), (180 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_Transmit_DMA), (136 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_Transmit_IT), (66 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_TxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_irda.o(i.HAL_IRDA_TxHalfCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_irda.o(i.IRDA_CheckIdleState), (92 bytes).
    Removing stm32f7xx_hal_irda.o(i.IRDA_DMAAbortOnError), (16 bytes).
    Removing stm32f7xx_hal_irda.o(i.IRDA_DMAError), (70 bytes).
    Removing stm32f7xx_hal_irda.o(i.IRDA_DMAReceiveCplt), (60 bytes).
    Removing stm32f7xx_hal_irda.o(i.IRDA_DMAReceiveHalfCplt), (10 bytes).
    Removing stm32f7xx_hal_irda.o(i.IRDA_DMARxAbortCallback), (50 bytes).
    Removing stm32f7xx_hal_irda.o(i.IRDA_DMARxOnlyAbortCallback), (26 bytes).
    Removing stm32f7xx_hal_irda.o(i.IRDA_DMATransmitCplt), (46 bytes).
    Removing stm32f7xx_hal_irda.o(i.IRDA_DMATransmitHalfCplt), (10 bytes).
    Removing stm32f7xx_hal_irda.o(i.IRDA_DMATxAbortCallback), (50 bytes).
    Removing stm32f7xx_hal_irda.o(i.IRDA_DMATxOnlyAbortCallback), (20 bytes).
    Removing stm32f7xx_hal_irda.o(i.IRDA_EndRxTransfer), (28 bytes).
    Removing stm32f7xx_hal_irda.o(i.IRDA_EndTransmit_IT), (26 bytes).
    Removing stm32f7xx_hal_irda.o(i.IRDA_EndTxTransfer), (18 bytes).
    Removing stm32f7xx_hal_irda.o(i.IRDA_Receive_IT), (116 bytes).
    Removing stm32f7xx_hal_irda.o(i.IRDA_SetConfig), (404 bytes).
    Removing stm32f7xx_hal_irda.o(i.IRDA_Transmit_IT), (96 bytes).
    Removing stm32f7xx_hal_irda.o(i.IRDA_WaitOnFlagUntilTimeout), (100 bytes).
    Removing stm32f7xx_hal_iwdg.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_iwdg.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_iwdg.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_iwdg.o(i.HAL_IWDG_Init), (94 bytes).
    Removing stm32f7xx_hal_iwdg.o(i.HAL_IWDG_Refresh), (12 bytes).
    Removing stm32f7xx_hal_lptim.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_lptim.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_lptim.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_AutoReloadMatchCallback), (2 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_AutoReloadWriteCallback), (2 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_CompareMatchCallback), (2 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_CompareWriteCallback), (2 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_Counter_Start), (64 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_Counter_Start_IT), (112 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_Counter_Stop), (26 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_Counter_Stop_IT), (72 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_DeInit), (44 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_DirectionDownCallback), (2 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_DirectionUpCallback), (2 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_Encoder_Start), (66 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_Encoder_Start_IT), (86 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_Encoder_Stop), (36 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_Encoder_Stop_IT), (56 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_GetState), (6 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_IRQHandler), (216 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_Init), (144 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_MspInit), (2 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_OnePulse_Start), (56 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_OnePulse_Start_IT), (116 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_OnePulse_Stop), (26 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_OnePulse_Stop_IT), (86 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_PWM_Start), (56 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_PWM_Start_IT), (116 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_PWM_Stop), (26 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_PWM_Stop_IT), (86 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_ReadAutoReload), (6 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_ReadCompare), (6 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_ReadCounter), (6 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_SetOnce_Start), (56 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_SetOnce_Start_IT), (116 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_SetOnce_Stop), (26 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_SetOnce_Stop_IT), (86 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_TimeOut_Start), (56 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_TimeOut_Start_IT), (92 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_TimeOut_Stop), (36 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_TimeOut_Stop_IT), (72 bytes).
    Removing stm32f7xx_hal_lptim.o(i.HAL_LPTIM_TriggerCallback), (2 bytes).
    Removing stm32f7xx_hal_ltdc.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_ltdc.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_ltdc.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_ConfigCLUT), (132 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_ConfigColorKeying), (64 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_ConfigColorKeying_NoReload), (58 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_ConfigLayer), (84 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_ConfigLayer_NoReload), (78 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_DeInit), (22 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_DisableCLUT), (58 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_DisableCLUT_NoReload), (52 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_DisableColorKeying), (58 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_DisableColorKeying_NoReload), (52 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_DisableDither), (48 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_EnableCLUT), (58 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_EnableCLUT_NoReload), (52 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_EnableColorKeying), (58 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_EnableColorKeying_NoReload), (52 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_EnableDither), (48 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_ErrorCallback), (2 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_GetError), (6 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_GetState), (6 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_IRQHandler), (202 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_Init), (256 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_LineEventCallback), (2 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_MspInit), (2 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_ProgramLineEvent), (56 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_Reload), (52 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_ReloadEventCallback), (2 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_SetAddress), (68 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_SetAddress_NoReload), (62 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_SetAlpha), (68 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_SetAlpha_NoReload), (62 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_SetPitch), (144 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_SetPitch_NoReload), (124 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_SetPixelFormat), (68 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_SetPixelFormat_NoReload), (62 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_SetWindowPosition), (86 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_SetWindowPosition_NoReload), (80 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_SetWindowSize), (88 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.HAL_LTDC_SetWindowSize_NoReload), (82 bytes).
    Removing stm32f7xx_hal_ltdc.o(i.LTDC_SetConfig), (350 bytes).
    Removing stm32f7xx_hal_msp_template.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_msp_template.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_msp_template.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_msp_template.o(i.HAL_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_msp_template.o(i.HAL_MspInit), (2 bytes).
    Removing stm32f7xx_hal_msp_template.o(i.HAL_PPP_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_msp_template.o(i.HAL_PPP_MspInit), (2 bytes).
    Removing stm32f7xx_hal_nand.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_nand.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_nand.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_nand.o(i.HAL_NAND_Address_Inc), (66 bytes).
    Removing stm32f7xx_hal_nand.o(i.HAL_NAND_DeInit), (30 bytes).
    Removing stm32f7xx_hal_nand.o(i.HAL_NAND_ECC_Disable), (40 bytes).
    Removing stm32f7xx_hal_nand.o(i.HAL_NAND_ECC_Enable), (40 bytes).
    Removing stm32f7xx_hal_nand.o(i.HAL_NAND_Erase_Block), (188 bytes).
    Removing stm32f7xx_hal_nand.o(i.HAL_NAND_GetECC), (40 bytes).
    Removing stm32f7xx_hal_nand.o(i.HAL_NAND_GetState), (6 bytes).
    Removing stm32f7xx_hal_nand.o(i.HAL_NAND_IRQHandler), (102 bytes).
    Removing stm32f7xx_hal_nand.o(i.HAL_NAND_ITCallback), (2 bytes).
    Removing stm32f7xx_hal_nand.o(i.HAL_NAND_Init), (84 bytes).
    Removing stm32f7xx_hal_nand.o(i.HAL_NAND_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_nand.o(i.HAL_NAND_MspInit), (2 bytes).
    Removing stm32f7xx_hal_nand.o(i.HAL_NAND_Read_ID), (144 bytes).
    Removing stm32f7xx_hal_nand.o(i.HAL_NAND_Read_Page_16b), (230 bytes).
    Removing stm32f7xx_hal_nand.o(i.HAL_NAND_Read_Page_8b), (256 bytes).
    Removing stm32f7xx_hal_nand.o(i.HAL_NAND_Read_SpareArea_16b), (228 bytes).
    Removing stm32f7xx_hal_nand.o(i.HAL_NAND_Read_SpareArea_8b), (228 bytes).
    Removing stm32f7xx_hal_nand.o(i.HAL_NAND_Read_Status), (36 bytes).
    Removing stm32f7xx_hal_nand.o(i.HAL_NAND_Reset), (56 bytes).
    Removing stm32f7xx_hal_nand.o(i.HAL_NAND_Write_Page_16b), (266 bytes).
    Removing stm32f7xx_hal_nand.o(i.HAL_NAND_Write_Page_8b), (294 bytes).
    Removing stm32f7xx_hal_nand.o(i.HAL_NAND_Write_SpareArea_16b), (266 bytes).
    Removing stm32f7xx_hal_nand.o(i.HAL_NAND_Write_SpareArea_8b), (266 bytes).
    Removing stm32f7xx_hal_nor.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_nor.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_nor.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_nor.o(i.HAL_NOR_DeInit), (30 bytes).
    Removing stm32f7xx_hal_nor.o(i.HAL_NOR_Erase_Block), (232 bytes).
    Removing stm32f7xx_hal_nor.o(i.HAL_NOR_Erase_Chip), (236 bytes).
    Removing stm32f7xx_hal_nor.o(i.HAL_NOR_GetState), (6 bytes).
    Removing stm32f7xx_hal_nor.o(i.HAL_NOR_GetStatus), (108 bytes).
    Removing stm32f7xx_hal_nor.o(i.HAL_NOR_Init), (116 bytes).
    Removing stm32f7xx_hal_nor.o(i.HAL_NOR_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_nor.o(i.HAL_NOR_MspInit), (2 bytes).
    Removing stm32f7xx_hal_nor.o(i.HAL_NOR_MspWait), (2 bytes).
    Removing stm32f7xx_hal_nor.o(i.HAL_NOR_Program), (172 bytes).
    Removing stm32f7xx_hal_nor.o(i.HAL_NOR_ProgramBuffer), (260 bytes).
    Removing stm32f7xx_hal_nor.o(i.HAL_NOR_Read), (168 bytes).
    Removing stm32f7xx_hal_nor.o(i.HAL_NOR_ReadBuffer), (188 bytes).
    Removing stm32f7xx_hal_nor.o(i.HAL_NOR_Read_CFI), (192 bytes).
    Removing stm32f7xx_hal_nor.o(i.HAL_NOR_Read_ID), (228 bytes).
    Removing stm32f7xx_hal_nor.o(i.HAL_NOR_ReturnToReadMode), (84 bytes).
    Removing stm32f7xx_hal_nor.o(i.HAL_NOR_WriteOperation_Disable), (48 bytes).
    Removing stm32f7xx_hal_nor.o(i.HAL_NOR_WriteOperation_Enable), (42 bytes).
    Removing stm32f7xx_hal_nor.o(.data), (4 bytes).
    Removing stm32f7xx_hal_pcd.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_pcd.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_pcd.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_ActivateRemoteWakeup), (26 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_ConnectCallback), (2 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_DataInStageCallback), (2 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_DataOutStageCallback), (2 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_DeActivateRemoteWakeup), (18 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_DeInit), (38 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_DevConnect), (36 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_DevDisconnect), (36 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_DisconnectCallback), (2 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_EP_Close), (68 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_EP_ClrStall), (80 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_EP_Flush), (52 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_EP_GetRxCount), (20 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_EP_Open), (84 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_EP_Receive), (90 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_EP_SetStall), (96 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_EP_Transmit), (88 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_GetState), (6 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_IRQHandler), (1360 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_ISOINIncompleteCallback), (2 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_ISOOUTIncompleteCallback), (2 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_Init), (200 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_MspInit), (2 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_ResetCallback), (2 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_ResumeCallback), (2 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_SOFCallback), (2 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_SetAddress), (36 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_SetupStageCallback), (2 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_Start), (42 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_Stop), (48 bytes).
    Removing stm32f7xx_hal_pcd.o(i.HAL_PCD_SuspendCallback), (2 bytes).
    Removing stm32f7xx_hal_pcd.o(i.PCD_WriteEmptyTxFifo), (152 bytes).
    Removing stm32f7xx_hal_pcd_ex.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_pcd_ex.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_pcd_ex.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_pcd_ex.o(i.HAL_PCDEx_ActivateLPM), (40 bytes).
    Removing stm32f7xx_hal_pcd_ex.o(i.HAL_PCDEx_DeActivateLPM), (32 bytes).
    Removing stm32f7xx_hal_pcd_ex.o(i.HAL_PCDEx_LPM_Callback), (2 bytes).
    Removing stm32f7xx_hal_pcd_ex.o(i.HAL_PCDEx_SetRxFiFo), (8 bytes).
    Removing stm32f7xx_hal_pcd_ex.o(i.HAL_PCDEx_SetTxFiFo), (66 bytes).
    Removing stm32f7xx_hal_pwr.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_pwr.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_pwr.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_pwr.o(i.HAL_PWR_ConfigPVD), (124 bytes).
    Removing stm32f7xx_hal_pwr.o(i.HAL_PWR_DeInit), (24 bytes).
    Removing stm32f7xx_hal_pwr.o(i.HAL_PWR_DisableBkUpAccess), (16 bytes).
    Removing stm32f7xx_hal_pwr.o(i.HAL_PWR_DisablePVD), (16 bytes).
    Removing stm32f7xx_hal_pwr.o(i.HAL_PWR_DisableSEVOnPend), (16 bytes).
    Removing stm32f7xx_hal_pwr.o(i.HAL_PWR_DisableSleepOnExit), (16 bytes).
    Removing stm32f7xx_hal_pwr.o(i.HAL_PWR_DisableWakeUpPin), (16 bytes).
    Removing stm32f7xx_hal_pwr.o(i.HAL_PWR_EnableBkUpAccess), (16 bytes).
    Removing stm32f7xx_hal_pwr.o(i.HAL_PWR_EnablePVD), (16 bytes).
    Removing stm32f7xx_hal_pwr.o(i.HAL_PWR_EnableSEVOnPend), (16 bytes).
    Removing stm32f7xx_hal_pwr.o(i.HAL_PWR_EnableSleepOnExit), (16 bytes).
    Removing stm32f7xx_hal_pwr.o(i.HAL_PWR_EnableWakeUpPin), (28 bytes).
    Removing stm32f7xx_hal_pwr.o(i.HAL_PWR_EnterSLEEPMode), (32 bytes).
    Removing stm32f7xx_hal_pwr.o(i.HAL_PWR_EnterSTANDBYMode), (32 bytes).
    Removing stm32f7xx_hal_pwr.o(i.HAL_PWR_EnterSTOPMode), (56 bytes).
    Removing stm32f7xx_hal_pwr.o(i.HAL_PWR_PVDCallback), (2 bytes).
    Removing stm32f7xx_hal_pwr.o(i.HAL_PWR_PVD_IRQHandler), (28 bytes).
    Removing stm32f7xx_hal_pwr_ex.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_pwr_ex.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_pwr_ex.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_pwr_ex.o(i.HAL_PWREx_ControlVoltageScaling), (184 bytes).
    Removing stm32f7xx_hal_pwr_ex.o(i.HAL_PWREx_DisableBkUpReg), (64 bytes).
    Removing stm32f7xx_hal_pwr_ex.o(i.HAL_PWREx_DisableFlashPowerDown), (16 bytes).
    Removing stm32f7xx_hal_pwr_ex.o(i.HAL_PWREx_DisableLowRegulatorLowVoltage), (16 bytes).
    Removing stm32f7xx_hal_pwr_ex.o(i.HAL_PWREx_DisableMainRegulatorLowVoltage), (16 bytes).
    Removing stm32f7xx_hal_pwr_ex.o(i.HAL_PWREx_DisableOverDrive), (112 bytes).
    Removing stm32f7xx_hal_pwr_ex.o(i.HAL_PWREx_EnableBkUpReg), (64 bytes).
    Removing stm32f7xx_hal_pwr_ex.o(i.HAL_PWREx_EnableFlashPowerDown), (16 bytes).
    Removing stm32f7xx_hal_pwr_ex.o(i.HAL_PWREx_EnableLowRegulatorLowVoltage), (16 bytes).
    Removing stm32f7xx_hal_pwr_ex.o(i.HAL_PWREx_EnableMainRegulatorLowVoltage), (16 bytes).
    Removing stm32f7xx_hal_pwr_ex.o(i.HAL_PWREx_EnterUnderDriveSTOPMode), (140 bytes).
    Removing stm32f7xx_hal_pwr_ex.o(i.HAL_PWREx_GetVoltageRange), (16 bytes).
    Removing stm32f7xx_hal_qspi.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_qspi.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_qspi.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_Abort), (124 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_AbortCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_Abort_IT), (96 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_AutoPolling_IT), (168 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_CmdCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_Command_IT), (138 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_DeInit), (58 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_ErrorCallback), (2 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_FifoThresholdCallback), (2 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_GetError), (4 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_GetFifoThreshold), (26 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_GetState), (6 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_IRQHandler), (456 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_MemoryMapped), (144 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_Receive_DMA), (296 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_Receive_IT), (124 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_RxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_RxHalfCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_SetFifoThreshold), (74 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_StatusMatchCallback), (2 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_TimeOutCallback), (2 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_Transmit_DMA), (288 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_Transmit_IT), (114 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_TxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_qspi.o(i.HAL_QSPI_TxHalfCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_qspi.o(i.QSPI_DMAAbortCplt), (58 bytes).
    Removing stm32f7xx_hal_qspi.o(i.QSPI_DMAError), (48 bytes).
    Removing stm32f7xx_hal_qspi.o(i.QSPI_DMARxCplt), (18 bytes).
    Removing stm32f7xx_hal_qspi.o(i.QSPI_DMARxHalfCplt), (10 bytes).
    Removing stm32f7xx_hal_qspi.o(i.QSPI_DMATxCplt), (18 bytes).
    Removing stm32f7xx_hal_qspi.o(i.QSPI_DMATxHalfCplt), (10 bytes).
    Removing stm32f7xx_hal_rcc.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_rcc.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_rcc.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_rcc.o(i.HAL_RCC_CSSCallback), (2 bytes).
    Removing stm32f7xx_hal_rcc.o(i.HAL_RCC_DeInit), (100 bytes).
    Removing stm32f7xx_hal_rcc.o(i.HAL_RCC_DisableCSS), (16 bytes).
    Removing stm32f7xx_hal_rcc.o(i.HAL_RCC_EnableCSS), (16 bytes).
    Removing stm32f7xx_hal_rcc.o(i.HAL_RCC_GetClockConfig), (60 bytes).
    Removing stm32f7xx_hal_rcc.o(i.HAL_RCC_GetOscConfig), (232 bytes).
    Removing stm32f7xx_hal_rcc.o(i.HAL_RCC_MCOConfig), (144 bytes).
    Removing stm32f7xx_hal_rcc.o(i.HAL_RCC_NMI_IRQHandler), (28 bytes).
    Removing stm32f7xx_hal_rcc_ex.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_rcc_ex.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_rcc_ex.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKConfig), (472 bytes).
    Removing stm32f7xx_hal_rcc_ex.o(i.HAL_RCCEx_GetPeriphCLKFreq), (400 bytes).
    Removing stm32f7xx_hal_rng.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_rng.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_rng.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_rng.o(i.HAL_RNG_DeInit), (46 bytes).
    Removing stm32f7xx_hal_rng.o(i.HAL_RNG_ErrorCallback), (2 bytes).
    Removing stm32f7xx_hal_rng.o(i.HAL_RNG_GenerateRandomNumber_IT), (50 bytes).
    Removing stm32f7xx_hal_rng.o(i.HAL_RNG_GetRandomNumber_IT), (32 bytes).
    Removing stm32f7xx_hal_rng.o(i.HAL_RNG_GetState), (4 bytes).
    Removing stm32f7xx_hal_rng.o(i.HAL_RNG_IRQHandler), (82 bytes).
    Removing stm32f7xx_hal_rng.o(i.HAL_RNG_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_rng.o(i.HAL_RNG_ReadLastRandomNumber), (4 bytes).
    Removing stm32f7xx_hal_rng.o(i.HAL_RNG_ReadyDataCallback), (2 bytes).
    Removing stm32f7xx_hal_rtc.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_rtc.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_rtc.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_rtc.o(i.HAL_RTC_AlarmAEventCallback), (2 bytes).
    Removing stm32f7xx_hal_rtc.o(i.HAL_RTC_AlarmIRQHandler), (92 bytes).
    Removing stm32f7xx_hal_rtc.o(i.HAL_RTC_DeInit), (220 bytes).
    Removing stm32f7xx_hal_rtc.o(i.HAL_RTC_DeactivateAlarm), (196 bytes).
    Removing stm32f7xx_hal_rtc.o(i.HAL_RTC_GetAlarm), (130 bytes).
    Removing stm32f7xx_hal_rtc.o(i.HAL_RTC_GetDate), (68 bytes).
    Removing stm32f7xx_hal_rtc.o(i.HAL_RTC_GetState), (4 bytes).
    Removing stm32f7xx_hal_rtc.o(i.HAL_RTC_GetTime), (88 bytes).
    Removing stm32f7xx_hal_rtc.o(i.HAL_RTC_Init), (160 bytes).
    Removing stm32f7xx_hal_rtc.o(i.HAL_RTC_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_rtc.o(i.HAL_RTC_MspInit), (2 bytes).
    Removing stm32f7xx_hal_rtc.o(i.HAL_RTC_PollForAlarmAEvent), (66 bytes).
    Removing stm32f7xx_hal_rtc.o(i.HAL_RTC_SetAlarm), (394 bytes).
    Removing stm32f7xx_hal_rtc.o(i.HAL_RTC_SetAlarm_IT), (448 bytes).
    Removing stm32f7xx_hal_rtc.o(i.HAL_RTC_SetDate), (228 bytes).
    Removing stm32f7xx_hal_rtc.o(i.HAL_RTC_SetTime), (256 bytes).
    Removing stm32f7xx_hal_rtc.o(i.HAL_RTC_WaitForSynchro), (52 bytes).
    Removing stm32f7xx_hal_rtc.o(i.RTC_Bcd2ToByte), (18 bytes).
    Removing stm32f7xx_hal_rtc.o(i.RTC_ByteToBcd2), (22 bytes).
    Removing stm32f7xx_hal_rtc.o(i.RTC_EnterInitMode), (56 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_AlarmBEventCallback), (2 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_BKUPRead), (12 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_BKUPWrite), (12 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_DeactivateCalibrationOutPut), (56 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_DeactivateInternalTimeStamp), (56 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_DeactivateRefClock), (92 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_DeactivateTamper), (92 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_DeactivateTimeStamp), (70 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_DeactivateWakeUpTimer), (122 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_DisableBypassShadow), (56 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_EnableBypassShadow), (56 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_GetTimeStamp), (152 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_GetWakeUpTimer), (8 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_PollForAlarmBEvent), (66 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_PollForTamper1Event), (66 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_PollForTamper2Event), (66 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_PollForTamper3Event), (68 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_PollForTimeStampEvent), (80 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_PollForWakeUpTimerEvent), (66 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_SetCalibrationOutPut), (76 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_SetInternalTimeStamp), (56 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_SetRefClock), (92 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_SetSmoothCalib), (134 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_SetSynchroShift), (164 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_SetTamper), (188 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_SetTamper_IT), (280 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_SetTimeStamp), (90 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_SetTimeStamp_IT), (140 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_SetWakeUpTimer), (162 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_SetWakeUpTimer_IT), (212 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_Tamper1EventCallback), (2 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_Tamper2EventCallback), (2 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_Tamper3EventCallback), (2 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_TamperTimeStampIRQHandler), (180 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_TimeStampEventCallback), (2 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_WakeUpTimerEventCallback), (2 bytes).
    Removing stm32f7xx_hal_rtc_ex.o(i.HAL_RTCEx_WakeUpTimerIRQHandler), (56 bytes).
    Removing stm32f7xx_hal_sai.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_sai.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_sai.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_Abort), (106 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_DMAPause), (38 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_DMAResume), (54 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_DMAStop), (76 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_DeInit), (64 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_DisableRxMuteMode), (30 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_DisableTxMuteMode), (26 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_EnableRxMuteMode), (62 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_EnableTxMuteMode), (38 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_ErrorCallback), (2 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_GetError), (6 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_GetState), (6 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_IRQHandler), (372 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_Init), (464 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_InitProtocol), (52 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_MspInit), (2 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_Receive), (266 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_Receive_DMA), (172 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_Receive_IT), (148 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_RxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_RxHalfCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_Transmit), (276 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_Transmit_DMA), (172 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_Transmit_IT), (156 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_TxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_sai.o(i.HAL_SAI_TxHalfCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_sai.o(i.SAI_DMAAbort), (68 bytes).
    Removing stm32f7xx_hal_sai.o(i.SAI_DMAError), (68 bytes).
    Removing stm32f7xx_hal_sai.o(i.SAI_DMARxCplt), (60 bytes).
    Removing stm32f7xx_hal_sai.o(i.SAI_DMARxHalfCplt), (10 bytes).
    Removing stm32f7xx_hal_sai.o(i.SAI_DMATxCplt), (60 bytes).
    Removing stm32f7xx_hal_sai.o(i.SAI_DMATxHalfCplt), (10 bytes).
    Removing stm32f7xx_hal_sai.o(i.SAI_Disable), (64 bytes).
    Removing stm32f7xx_hal_sai.o(i.SAI_FillFifo), (86 bytes).
    Removing stm32f7xx_hal_sai.o(i.SAI_InitI2S), (178 bytes).
    Removing stm32f7xx_hal_sai.o(i.SAI_InitPCM), (132 bytes).
    Removing stm32f7xx_hal_sai.o(i.SAI_InterruptFlag), (48 bytes).
    Removing stm32f7xx_hal_sai.o(i.SAI_Receive_IT16Bit), (70 bytes).
    Removing stm32f7xx_hal_sai.o(i.SAI_Receive_IT32Bit), (70 bytes).
    Removing stm32f7xx_hal_sai.o(i.SAI_Receive_IT8Bit), (68 bytes).
    Removing stm32f7xx_hal_sai.o(i.SAI_Transmit_IT16Bit), (70 bytes).
    Removing stm32f7xx_hal_sai.o(i.SAI_Transmit_IT32Bit), (70 bytes).
    Removing stm32f7xx_hal_sai.o(i.SAI_Transmit_IT8Bit), (68 bytes).
    Removing stm32f7xx_hal_sai_ex.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_sai_ex.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_sai_ex.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_sd.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_sd.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_sd.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_sd.o(i.HAL_SD_CheckReadOperation), (102 bytes).
    Removing stm32f7xx_hal_sd.o(i.HAL_SD_CheckWriteOperation), (112 bytes).
    Removing stm32f7xx_hal_sd.o(i.HAL_SD_DMA_RxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_sd.o(i.HAL_SD_DMA_RxErrorCallback), (2 bytes).
    Removing stm32f7xx_hal_sd.o(i.HAL_SD_DMA_TxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_sd.o(i.HAL_SD_DMA_TxErrorCallback), (2 bytes).
    Removing stm32f7xx_hal_sd.o(i.HAL_SD_DeInit), (20 bytes).
    Removing stm32f7xx_hal_sd.o(i.HAL_SD_Erase), (272 bytes).
    Removing stm32f7xx_hal_sd.o(i.HAL_SD_GetCardStatus), (158 bytes).
    Removing stm32f7xx_hal_sd.o(i.HAL_SD_GetStatus), (26 bytes).
    Removing stm32f7xx_hal_sd.o(i.HAL_SD_Get_CardInfo), (666 bytes).
    Removing stm32f7xx_hal_sd.o(i.HAL_SD_HighSpeed), (308 bytes).
    Removing stm32f7xx_hal_sd.o(i.HAL_SD_IRQHandler), (132 bytes).
    Removing stm32f7xx_hal_sd.o(i.HAL_SD_Init), (148 bytes).
    Removing stm32f7xx_hal_sd.o(i.HAL_SD_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_sd.o(i.HAL_SD_MspInit), (2 bytes).
    Removing stm32f7xx_hal_sd.o(i.HAL_SD_ReadBlocks), (384 bytes).
    Removing stm32f7xx_hal_sd.o(i.HAL_SD_ReadBlocks_DMA), (264 bytes).
    Removing stm32f7xx_hal_sd.o(i.HAL_SD_SendSDStatus), (288 bytes).
    Removing stm32f7xx_hal_sd.o(i.HAL_SD_StopTransfer), (44 bytes).
    Removing stm32f7xx_hal_sd.o(i.HAL_SD_WideBusOperation_Config), (122 bytes).
    Removing stm32f7xx_hal_sd.o(i.HAL_SD_WriteBlocks), (502 bytes).
    Removing stm32f7xx_hal_sd.o(i.HAL_SD_WriteBlocks_DMA), (264 bytes).
    Removing stm32f7xx_hal_sd.o(i.HAL_SD_XferCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_sd.o(i.HAL_SD_XferErrorCallback), (2 bytes).
    Removing stm32f7xx_hal_sd.o(i.SD_CmdError), (46 bytes).
    Removing stm32f7xx_hal_sd.o(i.SD_CmdResp1Error), (248 bytes).
    Removing stm32f7xx_hal_sd.o(i.SD_CmdResp2Error), (48 bytes).
    Removing stm32f7xx_hal_sd.o(i.SD_CmdResp3Error), (36 bytes).
    Removing stm32f7xx_hal_sd.o(i.SD_CmdResp6Error), (124 bytes).
    Removing stm32f7xx_hal_sd.o(i.SD_CmdResp7Error), (72 bytes).
    Removing stm32f7xx_hal_sd.o(i.SD_DMA_RxCplt), (26 bytes).
    Removing stm32f7xx_hal_sd.o(i.SD_DMA_RxError), (12 bytes).
    Removing stm32f7xx_hal_sd.o(i.SD_DMA_TxCplt), (26 bytes).
    Removing stm32f7xx_hal_sd.o(i.SD_DMA_TxError), (12 bytes).
    Removing stm32f7xx_hal_sd.o(i.SD_FindSCR), (310 bytes).
    Removing stm32f7xx_hal_sd.o(i.SD_GetState), (26 bytes).
    Removing stm32f7xx_hal_sd.o(i.SD_Initialize_Cards), (250 bytes).
    Removing stm32f7xx_hal_sd.o(i.SD_IsCardProgramming), (332 bytes).
    Removing stm32f7xx_hal_sd.o(i.SD_PowerOFF), (14 bytes).
    Removing stm32f7xx_hal_sd.o(i.SD_PowerON), (352 bytes).
    Removing stm32f7xx_hal_sd.o(i.SD_Select_Deselect), (46 bytes).
    Removing stm32f7xx_hal_sd.o(i.SD_SendStatus), (80 bytes).
    Removing stm32f7xx_hal_sd.o(i.SD_WideBus_Disable), (116 bytes).
    Removing stm32f7xx_hal_sd.o(i.SD_WideBus_Enable), (118 bytes).
    Removing stm32f7xx_hal_sdram.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_sdram.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_sdram.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_sdram.o(i.HAL_SDRAM_DMA_XferCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_sdram.o(i.HAL_SDRAM_DMA_XferErrorCallback), (2 bytes).
    Removing stm32f7xx_hal_sdram.o(i.HAL_SDRAM_DeInit), (30 bytes).
    Removing stm32f7xx_hal_sdram.o(i.HAL_SDRAM_GetModeStatus), (6 bytes).
    Removing stm32f7xx_hal_sdram.o(i.HAL_SDRAM_GetState), (6 bytes).
    Removing stm32f7xx_hal_sdram.o(i.HAL_SDRAM_IRQHandler), (30 bytes).
    Removing stm32f7xx_hal_sdram.o(i.HAL_SDRAM_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_sdram.o(i.HAL_SDRAM_Read_16b), (70 bytes).
    Removing stm32f7xx_hal_sdram.o(i.HAL_SDRAM_Read_32b), (66 bytes).
    Removing stm32f7xx_hal_sdram.o(i.HAL_SDRAM_Read_8b), (70 bytes).
    Removing stm32f7xx_hal_sdram.o(i.HAL_SDRAM_Read_DMA), (76 bytes).
    Removing stm32f7xx_hal_sdram.o(i.HAL_SDRAM_RefreshErrorCallback), (2 bytes).
    Removing stm32f7xx_hal_sdram.o(i.HAL_SDRAM_SetAutoRefreshNumber), (38 bytes).
    Removing stm32f7xx_hal_sdram.o(i.HAL_SDRAM_WriteProtection_Disable), (40 bytes).
    Removing stm32f7xx_hal_sdram.o(i.HAL_SDRAM_WriteProtection_Enable), (40 bytes).
    Removing stm32f7xx_hal_sdram.o(i.HAL_SDRAM_Write_16b), (70 bytes).
    Removing stm32f7xx_hal_sdram.o(i.HAL_SDRAM_Write_32b), (66 bytes).
    Removing stm32f7xx_hal_sdram.o(i.HAL_SDRAM_Write_8b), (70 bytes).
    Removing stm32f7xx_hal_sdram.o(i.HAL_SDRAM_Write_DMA), (88 bytes).
    Removing stm32f7xx_hal_smartcard.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_smartcard.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_smartcard.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Abort), (116 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_AbortCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_AbortReceive), (92 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_AbortReceiveCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_AbortReceive_IT), (132 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_AbortTransmit), (84 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_AbortTransmitCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_AbortTransmit_IT), (124 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Abort_IT), (192 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_DeInit), (70 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_ErrorCallback), (2 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_GetError), (6 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_GetState), (12 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_IRQHandler), (528 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Init), (130 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_MspInit), (2 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Receive), (140 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Receive_DMA), (140 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Receive_IT), (80 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_RxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Transmit), (250 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Transmit_DMA), (200 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_Transmit_IT), (142 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.HAL_SMARTCARD_TxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.SMARTCARD_AdvFeatureConfig), (156 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.SMARTCARD_CheckIdleState), (94 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMAAbortOnError), (20 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMAError), (78 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMAReceiveCplt), (52 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMARxAbortCallback), (54 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMARxOnlyAbortCallback), (30 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMATransmitCplt), (84 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMATxAbortCallback), (54 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.SMARTCARD_DMATxOnlyAbortCallback), (28 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.SMARTCARD_EndRxTransfer), (28 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.SMARTCARD_EndTransmit_IT), (120 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.SMARTCARD_EndTxTransfer), (28 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.SMARTCARD_Receive_IT), (106 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.SMARTCARD_SetConfig), (488 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.SMARTCARD_Transmit_IT), (122 bytes).
    Removing stm32f7xx_hal_smartcard.o(i.SMARTCARD_WaitOnFlagUntilTimeout), (100 bytes).
    Removing stm32f7xx_hal_smartcard_ex.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_smartcard_ex.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_smartcard_ex.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_smartcard_ex.o(i.HAL_SMARTCARDEx_BlockLength_Config), (12 bytes).
    Removing stm32f7xx_hal_smartcard_ex.o(i.HAL_SMARTCARDEx_DisableReceiverTimeOut), (46 bytes).
    Removing stm32f7xx_hal_smartcard_ex.o(i.HAL_SMARTCARDEx_EnableReceiverTimeOut), (46 bytes).
    Removing stm32f7xx_hal_smartcard_ex.o(i.HAL_SMARTCARDEx_TimeOut_Config), (14 bytes).
    Removing stm32f7xx_hal_spdifrx.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_spdifrx.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_spdifrx.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_CxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_CxHalfCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_DMAStop), (92 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_DeInit), (46 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ErrorCallback), (2 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_GetError), (4 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_GetState), (6 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_IRQHandler), (134 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_Init), (116 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_MspInit), (2 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveControlFlow), (154 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveControlFlow_DMA), (200 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveControlFlow_IT), (172 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveDataFlow), (154 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveDataFlow_DMA), (200 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_ReceiveDataFlow_IT), (172 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_RxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_RxHalfCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.HAL_SPDIFRX_SetDataFormat), (88 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.SPDIFRX_DMACxCplt), (32 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.SPDIFRX_DMACxHalfCplt), (10 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.SPDIFRX_DMAError), (40 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.SPDIFRX_DMARxCplt), (42 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.SPDIFRX_DMARxHalfCplt), (10 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.SPDIFRX_ReceiveControlFlow_IT), (56 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.SPDIFRX_ReceiveDataFlow_IT), (56 bytes).
    Removing stm32f7xx_hal_spdifrx.o(i.SPDIFRX_WaitOnFlagUntilTimeout), (278 bytes).
    Removing stm32f7xx_hal_spi.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_spi.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_spi.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_Abort), (284 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_AbortCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_Abort_IT), (292 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_DMAPause), (38 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_DMAResume), (38 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_DMAStop), (42 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_DeInit), (46 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_ErrorCallback), (2 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_GetError), (4 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_GetState), (6 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_IRQHandler), (228 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_Init), (222 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_MspInit), (2 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_Receive), (606 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_Receive_DMA), (312 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_Receive_IT), (252 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_RxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_RxHalfCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_Transmit), (370 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_TransmitReceive), (814 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA), (476 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_TransmitReceive_IT), (264 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_Transmit_DMA), (292 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_Transmit_IT), (180 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_TxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_TxHalfCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_TxRxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_spi.o(i.HAL_SPI_TxRxHalfCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_2linesRxISR_16BIT), (72 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_2linesRxISR_16BITCRC), (30 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_2linesRxISR_8BIT), (124 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_2linesRxISR_8BITCRC), (50 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_2linesTxISR_16BIT), (78 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_2linesTxISR_8BIT), (100 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_AbortRx_ISR), (88 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_AbortTx_ISR), (84 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_CloseRxTx_ISR), (126 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_CloseRx_ISR), (96 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_CloseTx_ISR), (76 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_DMAAbortOnError), (18 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_DMAError), (34 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_DMAHalfReceiveCplt), (10 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_DMAHalfTransmitCplt), (10 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_DMAHalfTransmitReceiveCplt), (10 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_DMAReceiveCplt), (218 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_DMARxAbortCallback), (128 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_DMATransmitCplt), (100 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_DMATransmitReceiveCplt), (218 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_DMATxAbortCallback), (124 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_EndRxTransaction), (126 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_EndRxTxTransaction), (100 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_RxISR_16BIT), (80 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_RxISR_16BITCRC), (30 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_RxISR_8BIT), (80 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_RxISR_8BITCRC), (36 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_TxISR_16BIT), (50 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_TxISR_8BIT), (48 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_WaitFifoStateUntilTimeout), (156 bytes).
    Removing stm32f7xx_hal_spi.o(i.SPI_WaitFlagStateUntilTimeout), (134 bytes).
    Removing stm32f7xx_hal_sram.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_sram.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_sram.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_sram.o(i.HAL_SRAM_DMA_XferCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_sram.o(i.HAL_SRAM_DMA_XferErrorCallback), (2 bytes).
    Removing stm32f7xx_hal_sram.o(i.HAL_SRAM_DeInit), (30 bytes).
    Removing stm32f7xx_hal_sram.o(i.HAL_SRAM_GetState), (6 bytes).
    Removing stm32f7xx_hal_sram.o(i.HAL_SRAM_Init), (88 bytes).
    Removing stm32f7xx_hal_sram.o(i.HAL_SRAM_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_sram.o(i.HAL_SRAM_MspInit), (2 bytes).
    Removing stm32f7xx_hal_sram.o(i.HAL_SRAM_Read_16b), (54 bytes).
    Removing stm32f7xx_hal_sram.o(i.HAL_SRAM_Read_32b), (50 bytes).
    Removing stm32f7xx_hal_sram.o(i.HAL_SRAM_Read_8b), (54 bytes).
    Removing stm32f7xx_hal_sram.o(i.HAL_SRAM_Read_DMA), (60 bytes).
    Removing stm32f7xx_hal_sram.o(i.HAL_SRAM_WriteOperation_Disable), (48 bytes).
    Removing stm32f7xx_hal_sram.o(i.HAL_SRAM_WriteOperation_Enable), (42 bytes).
    Removing stm32f7xx_hal_sram.o(i.HAL_SRAM_Write_16b), (66 bytes).
    Removing stm32f7xx_hal_sram.o(i.HAL_SRAM_Write_32b), (62 bytes).
    Removing stm32f7xx_hal_sram.o(i.HAL_SRAM_Write_8b), (66 bytes).
    Removing stm32f7xx_hal_sram.o(i.HAL_SRAM_Write_DMA), (80 bytes).
    Removing stm32f7xx_hal_tim.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_tim.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_tim.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_Base_DeInit), (54 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_Base_GetState), (6 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_Base_Init), (50 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_Base_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_Base_MspInit), (2 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_Base_Start), (26 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_Base_Start_DMA), (96 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_Base_Start_IT), (24 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_Base_Stop), (44 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_Base_Stop_DMA), (48 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_Base_Stop_IT), (42 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_ConfigClockSource), (276 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_ConfigOCrefClear), (188 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_ConfigTI1Input), (16 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_DMABurst_ReadStart), (328 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_DMABurst_ReadStop), (120 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_DMABurst_WriteStart), (328 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_DMABurst_WriteStop), (120 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_Encoder_DeInit), (54 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_Encoder_GetState), (6 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_Encoder_Init), (168 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_Encoder_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_Encoder_MspInit), (2 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_Encoder_Start), (66 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_Encoder_Start_DMA), (288 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_Encoder_Start_IT), (106 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_Encoder_Stop), (84 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_Encoder_Stop_DMA), (130 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_Encoder_Stop_IT), (130 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_ErrorCallback), (2 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_GenerateEvent), (38 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_IC_CaptureCallback), (2 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_IC_ConfigChannel), (188 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_IC_DeInit), (54 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_IC_GetState), (6 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_IC_Init), (56 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_IC_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_IC_MspInit), (2 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_IC_Start), (26 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_IC_Start_DMA), (212 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_IC_Start_IT), (84 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_IC_Stop), (44 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_IC_Stop_DMA), (108 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_IC_Stop_IT), (102 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_IRQHandler), (392 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_OC_ConfigChannel), (84 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_OC_DeInit), (54 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_OC_DelayElapsedCallback), (2 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_OC_GetState), (6 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_OC_Init), (56 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_OC_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_OC_MspInit), (2 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_OC_Start), (56 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_OC_Start_DMA), (244 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_OC_Start_IT), (116 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_OC_Stop), (88 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_OC_Stop_DMA), (152 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_OC_Stop_IT), (144 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_OnePulse_ConfigChannel), (248 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_OnePulse_DeInit), (54 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_OnePulse_GetState), (6 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_OnePulse_Init), (76 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_OnePulse_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_OnePulse_MspInit), (2 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_OnePulse_Start), (60 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_OnePulse_Start_IT), (80 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_OnePulse_Stop), (100 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_OnePulse_Stop_IT), (120 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_ConfigChannel), (218 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_DeInit), (54 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_GetState), (6 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_Init), (56 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_MspInit), (2 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_PulseFinishedCallback), (2 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_Start), (56 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_Start_DMA), (244 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_Start_IT), (116 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_Stop), (92 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_Stop_DMA), (152 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_PWM_Stop_IT), (144 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_PeriodElapsedCallback), (2 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_ReadCapturedValue), (68 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_SlaveConfigSynchronization), (164 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_SlaveConfigSynchronization_IT), (66 bytes).
    Removing stm32f7xx_hal_tim.o(i.HAL_TIM_TriggerCallback), (2 bytes).
    Removing stm32f7xx_hal_tim.o(i.TIM_Base_SetConfig), (196 bytes).
    Removing stm32f7xx_hal_tim.o(i.TIM_CCxChannelCmd), (22 bytes).
    Removing stm32f7xx_hal_tim.o(i.TIM_DMACaptureCplt), (66 bytes).
    Removing stm32f7xx_hal_tim.o(i.TIM_DMADelayPulseCplt), (66 bytes).
    Removing stm32f7xx_hal_tim.o(i.TIM_DMAError), (16 bytes).
    Removing stm32f7xx_hal_tim.o(i.TIM_DMAPeriodElapsedCplt), (16 bytes).
    Removing stm32f7xx_hal_tim.o(i.TIM_DMATriggerCplt), (16 bytes).
    Removing stm32f7xx_hal_tim.o(i.TIM_ETR_SetConfig), (20 bytes).
    Removing stm32f7xx_hal_tim.o(i.TIM_ITRx_SetConfig), (16 bytes).
    Removing stm32f7xx_hal_tim.o(i.TIM_OC1_SetConfig), (100 bytes).
    Removing stm32f7xx_hal_tim.o(i.TIM_OC2_SetConfig), (112 bytes).
    Removing stm32f7xx_hal_tim.o(i.TIM_OC3_SetConfig), (108 bytes).
    Removing stm32f7xx_hal_tim.o(i.TIM_OC4_SetConfig), (88 bytes).
    Removing stm32f7xx_hal_tim.o(i.TIM_SlaveTimer_SetConfig), (128 bytes).
    Removing stm32f7xx_hal_tim.o(i.TIM_TI1_ConfigInputStage), (34 bytes).
    Removing stm32f7xx_hal_tim.o(i.TIM_TI1_SetConfig), (128 bytes).
    Removing stm32f7xx_hal_tim.o(i.TIM_TI2_ConfigInputStage), (36 bytes).
    Removing stm32f7xx_hal_tim.o(i.TIM_TI2_SetConfig), (54 bytes).
    Removing stm32f7xx_hal_tim.o(i.TIM_TI3_SetConfig), (50 bytes).
    Removing stm32f7xx_hal_tim.o(i.TIM_TI4_SetConfig), (56 bytes).
    Removing stm32f7xx_hal_tim_ex.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_tim_ex.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_tim_ex.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_BreakCallback), (2 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_CommutationCallback), (2 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_ConfigBreakDeadTime), (84 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_ConfigBreakInput), (100 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_ConfigCommutationEvent), (92 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_ConfigCommutationEvent_DMA), (124 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_ConfigCommutationEvent_IT), (102 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_GroupChannel5), (56 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_DeInit), (54 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_GetState), (6 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_Init), (184 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_MspInit), (2 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_Start), (28 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_Start_DMA), (112 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_Start_IT), (38 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_Stop), (46 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_Stop_DMA), (56 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_HallSensor_Stop_IT), (56 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_MasterConfigSynchronization), (88 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_OCN_Start), (36 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_OCN_Start_DMA), (224 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_OCN_Start_IT), (104 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_OCN_Stop), (68 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_OCN_Stop_DMA), (132 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_OCN_Stop_IT), (142 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_OnePulseN_Start), (26 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_OnePulseN_Start_IT), (46 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_OnePulseN_Stop), (68 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_OnePulseN_Stop_IT), (88 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_PWMN_Start), (36 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_PWMN_Start_DMA), (224 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_PWMN_Start_IT), (104 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_PWMN_Stop), (68 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_PWMN_Stop_DMA), (132 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_PWMN_Stop_IT), (142 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIMEx_RemapConfig), (34 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIM_ConfigOCrefClear), (292 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIM_OC_ConfigChannel), (112 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.HAL_TIM_PWM_ConfigChannel), (312 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.TIMEx_DMACommutationCplt), (16 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.TIM_CCxNChannelCmd), (22 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.TIM_OC5_SetConfig), (80 bytes).
    Removing stm32f7xx_hal_tim_ex.o(i.TIM_OC6_SetConfig), (84 bytes).
    Removing stm32f7xx_hal_uart.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_uart.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_uart.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_HalfDuplex_EnableReceiver), (58 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_HalfDuplex_EnableTransmitter), (58 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_HalfDuplex_Init), (122 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_LIN_Init), (136 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_LIN_SendBreak), (46 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_MultiProcessorEx_AddressLength_Set), (50 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_MultiProcessor_DisableMuteMode), (44 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_MultiProcessor_EnableMuteMode), (44 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_MultiProcessor_EnterMuteMode), (12 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_MultiProcessor_Init), (146 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_RS485Ex_Init), (148 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_UART_DMAPause), (98 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_UART_DMAResume), (102 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_UART_DMAStop), (84 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_UART_DeInit), (62 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_UART_ErrorCallback), (2 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_UART_GetError), (4 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_UART_GetState), (12 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_UART_IRQHandler), (296 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_UART_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_UART_Receive), (246 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_UART_Receive_DMA), (148 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_UART_Receive_IT), (160 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_UART_RxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_UART_RxHalfCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_UART_Transmit_DMA), (140 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_UART_Transmit_IT), (66 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_UART_TxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_uart.o(i.HAL_UART_TxHalfCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_uart.o(i.UART_DMAAbortOnError), (20 bytes).
    Removing stm32f7xx_hal_uart.o(i.UART_DMAError), (72 bytes).
    Removing stm32f7xx_hal_uart.o(i.UART_DMAReceiveCplt), (62 bytes).
    Removing stm32f7xx_hal_uart.o(i.UART_DMARxHalfCplt), (10 bytes).
    Removing stm32f7xx_hal_uart.o(i.UART_DMATransmitCplt), (48 bytes).
    Removing stm32f7xx_hal_uart.o(i.UART_DMATxHalfCplt), (10 bytes).
    Removing stm32f7xx_hal_uart.o(i.UART_EndRxTransfer), (28 bytes).
    Removing stm32f7xx_hal_uart.o(i.UART_EndTransmit_IT), (26 bytes).
    Removing stm32f7xx_hal_uart.o(i.UART_EndTxTransfer), (18 bytes).
    Removing stm32f7xx_hal_uart.o(i.UART_Receive_IT), (122 bytes).
    Removing stm32f7xx_hal_uart.o(i.UART_Transmit_IT), (100 bytes).
    Removing stm32f7xx_hal_usart.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_usart.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_usart.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_usart.o(i.HAL_USART_DMAPause), (110 bytes).
    Removing stm32f7xx_hal_usart.o(i.HAL_USART_DMAResume), (120 bytes).
    Removing stm32f7xx_hal_usart.o(i.HAL_USART_DMAStop), (88 bytes).
    Removing stm32f7xx_hal_usart.o(i.HAL_USART_DeInit), (50 bytes).
    Removing stm32f7xx_hal_usart.o(i.HAL_USART_ErrorCallback), (2 bytes).
    Removing stm32f7xx_hal_usart.o(i.HAL_USART_GetError), (4 bytes).
    Removing stm32f7xx_hal_usart.o(i.HAL_USART_GetState), (6 bytes).
    Removing stm32f7xx_hal_usart.o(i.HAL_USART_IRQHandler), (336 bytes).
    Removing stm32f7xx_hal_usart.o(i.HAL_USART_Init), (102 bytes).
    Removing stm32f7xx_hal_usart.o(i.HAL_USART_MspDeInit), (2 bytes).
    Removing stm32f7xx_hal_usart.o(i.HAL_USART_MspInit), (2 bytes).
    Removing stm32f7xx_hal_usart.o(i.HAL_USART_Receive), (252 bytes).
    Removing stm32f7xx_hal_usart.o(i.HAL_USART_Receive_DMA), (208 bytes).
    Removing stm32f7xx_hal_usart.o(i.HAL_USART_Receive_IT), (162 bytes).
    Removing stm32f7xx_hal_usart.o(i.HAL_USART_RxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_usart.o(i.HAL_USART_RxHalfCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_usart.o(i.HAL_USART_Transmit), (184 bytes).
    Removing stm32f7xx_hal_usart.o(i.HAL_USART_TransmitReceive), (292 bytes).
    Removing stm32f7xx_hal_usart.o(i.HAL_USART_TransmitReceive_DMA), (232 bytes).
    Removing stm32f7xx_hal_usart.o(i.HAL_USART_TransmitReceive_IT), (174 bytes).
    Removing stm32f7xx_hal_usart.o(i.HAL_USART_Transmit_DMA), (152 bytes).
    Removing stm32f7xx_hal_usart.o(i.HAL_USART_Transmit_IT), (66 bytes).
    Removing stm32f7xx_hal_usart.o(i.HAL_USART_TxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_usart.o(i.HAL_USART_TxHalfCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_usart.o(i.HAL_USART_TxRxCpltCallback), (2 bytes).
    Removing stm32f7xx_hal_usart.o(i.USART_CheckIdleState), (106 bytes).
    Removing stm32f7xx_hal_usart.o(i.USART_DMAAbortOnError), (16 bytes).
    Removing stm32f7xx_hal_usart.o(i.USART_DMAError), (76 bytes).
    Removing stm32f7xx_hal_usart.o(i.USART_DMAReceiveCplt), (110 bytes).
    Removing stm32f7xx_hal_usart.o(i.USART_DMARxHalfCplt), (10 bytes).
    Removing stm32f7xx_hal_usart.o(i.USART_DMATransmitCplt), (62 bytes).
    Removing stm32f7xx_hal_usart.o(i.USART_DMATxHalfCplt), (10 bytes).
    Removing stm32f7xx_hal_usart.o(i.USART_EndRxTransfer), (28 bytes).
    Removing stm32f7xx_hal_usart.o(i.USART_EndTransmit_IT), (36 bytes).
    Removing stm32f7xx_hal_usart.o(i.USART_EndTxTransfer), (18 bytes).
    Removing stm32f7xx_hal_usart.o(i.USART_Receive_IT), (126 bytes).
    Removing stm32f7xx_hal_usart.o(i.USART_SetConfig), (416 bytes).
    Removing stm32f7xx_hal_usart.o(i.USART_TransmitReceive_IT), (204 bytes).
    Removing stm32f7xx_hal_usart.o(i.USART_Transmit_IT), (96 bytes).
    Removing stm32f7xx_hal_usart.o(i.USART_WaitOnFlagUntilTimeout), (116 bytes).
    Removing stm32f7xx_hal_wwdg.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_hal_wwdg.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_hal_wwdg.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_hal_wwdg.o(i.HAL_WWDG_EarlyWakeupCallback), (2 bytes).
    Removing stm32f7xx_hal_wwdg.o(i.HAL_WWDG_IRQHandler), (30 bytes).
    Removing stm32f7xx_hal_wwdg.o(i.HAL_WWDG_Init), (46 bytes).
    Removing stm32f7xx_hal_wwdg.o(i.HAL_WWDG_MspInit), (2 bytes).
    Removing stm32f7xx_hal_wwdg.o(i.HAL_WWDG_Refresh), (10 bytes).
    Removing stm32f7xx_ll_fmc.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_ll_fmc.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_ll_fmc.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_ll_fmc.o(i.FMC_NAND_AttributeSpace_Timing_Init), (28 bytes).
    Removing stm32f7xx_ll_fmc.o(i.FMC_NAND_CommonSpace_Timing_Init), (28 bytes).
    Removing stm32f7xx_ll_fmc.o(i.FMC_NAND_DeInit), (28 bytes).
    Removing stm32f7xx_ll_fmc.o(i.FMC_NAND_ECC_Disable), (12 bytes).
    Removing stm32f7xx_ll_fmc.o(i.FMC_NAND_ECC_Enable), (12 bytes).
    Removing stm32f7xx_ll_fmc.o(i.FMC_NAND_GetECC), (56 bytes).
    Removing stm32f7xx_ll_fmc.o(i.FMC_NAND_Init), (52 bytes).
    Removing stm32f7xx_ll_fmc.o(i.FMC_NORSRAM_DeInit), (52 bytes).
    Removing stm32f7xx_ll_fmc.o(i.FMC_NORSRAM_Extended_Timing_Init), (64 bytes).
    Removing stm32f7xx_ll_fmc.o(i.FMC_NORSRAM_Init), (120 bytes).
    Removing stm32f7xx_ll_fmc.o(i.FMC_NORSRAM_Timing_Init), (84 bytes).
    Removing stm32f7xx_ll_fmc.o(i.FMC_NORSRAM_WriteOperation_Disable), (16 bytes).
    Removing stm32f7xx_ll_fmc.o(i.FMC_NORSRAM_WriteOperation_Enable), (16 bytes).
    Removing stm32f7xx_ll_fmc.o(i.FMC_SDRAM_DeInit), (30 bytes).
    Removing stm32f7xx_ll_fmc.o(i.FMC_SDRAM_GetModeStatus), (22 bytes).
    Removing stm32f7xx_ll_fmc.o(i.FMC_SDRAM_SetAutoRefreshNumber), (12 bytes).
    Removing stm32f7xx_ll_fmc.o(i.FMC_SDRAM_WriteProtection_Disable), (16 bytes).
    Removing stm32f7xx_ll_fmc.o(i.FMC_SDRAM_WriteProtection_Enable), (16 bytes).
    Removing stm32f7xx_ll_sdmmc.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_ll_sdmmc.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_ll_sdmmc.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_ll_sdmmc.o(i.SDMMC_DataConfig), (36 bytes).
    Removing stm32f7xx_ll_sdmmc.o(i.SDMMC_GetCommandResponse), (6 bytes).
    Removing stm32f7xx_ll_sdmmc.o(i.SDMMC_GetDataCounter), (4 bytes).
    Removing stm32f7xx_ll_sdmmc.o(i.SDMMC_GetFIFOCount), (6 bytes).
    Removing stm32f7xx_ll_sdmmc.o(i.SDMMC_GetPowerState), (8 bytes).
    Removing stm32f7xx_ll_sdmmc.o(i.SDMMC_GetResponse), (14 bytes).
    Removing stm32f7xx_ll_sdmmc.o(i.SDMMC_Init), (42 bytes).
    Removing stm32f7xx_ll_sdmmc.o(i.SDMMC_PowerState_OFF), (8 bytes).
    Removing stm32f7xx_ll_sdmmc.o(i.SDMMC_PowerState_ON), (8 bytes).
    Removing stm32f7xx_ll_sdmmc.o(i.SDMMC_ReadFIFO), (6 bytes).
    Removing stm32f7xx_ll_sdmmc.o(i.SDMMC_SendCommand), (32 bytes).
    Removing stm32f7xx_ll_sdmmc.o(i.SDMMC_SetSDMMCReadWaitMode), (14 bytes).
    Removing stm32f7xx_ll_sdmmc.o(i.SDMMC_WriteFIFO), (10 bytes).
    Removing stm32f7xx_ll_usb.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_ll_usb.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_ll_usb.o(.rrx_text), (6 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_ActivateDedicatedEndpoint), (216 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_ActivateEndpoint), (132 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_ActivateSetup), (52 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_ClearInterrupts), (8 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_CoreInit), (116 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_CoreReset), (56 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_DeactivateDedicatedEndpoint), (78 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_DeactivateEndpoint), (114 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_DevConnect), (24 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_DevDisconnect), (24 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_DevInit), (340 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_DisableGlobalInt), (12 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_DoPing), (64 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_DriveVbus), (66 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_EP0StartXfer), (328 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_EP0_OutStart), (56 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_EPClearStall), (100 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_EPSetStall), (94 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_EPStartXfer), (572 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_EnableGlobalInt), (12 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_FlushRxFifo), (32 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_FlushTxFifo), (36 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_GetCurrentFrame), (8 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_GetDevSpeed), (60 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_GetHostSpeed), (16 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_GetMode), (8 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_HC_Halt), (376 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_HC_Init), (252 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_HC_ReadInterrupt), (12 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_HC_StartXfer), (392 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_HostInit), (208 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_InitFSLSPClkSel), (58 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_ReadDevAllInEpInterrupt), (14 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_ReadDevAllOutEpInterrupt), (14 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_ReadDevInEPInterrupt), (30 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_ReadDevOutEPInterrupt), (16 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_ReadInterrupts), (8 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_ReadPacket), (32 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_ResetPort), (54 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_SetCurrentMode), (46 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_SetDevAddress), (30 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_SetDevSpeed), (14 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_StopDevice), (66 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_StopHost), (174 bytes).
    Removing stm32f7xx_ll_usb.o(i.USB_WritePacket), (40 bytes).
    Removing stm32f7xx_ll_usb.o(.data), (4 bytes).
    Removing main.o(.rev16_text), (4 bytes).
    Removing main.o(.revsh_text), (4 bytes).
    Removing main.o(.rrx_text), (6 bytes).
    Removing main.o(.bss), (40000 bytes).
    Removing stm32f7xx_it.o(.rev16_text), (4 bytes).
    Removing stm32f7xx_it.o(.revsh_text), (4 bytes).
    Removing stm32f7xx_it.o(.rrx_text), (6 bytes).
    Removing bsp_qspi_flash.o(.rev16_text), (4 bytes).
    Removing bsp_qspi_flash.o(.revsh_text), (4 bytes).
    Removing bsp_qspi_flash.o(.rrx_text), (6 bytes).
    Removing bsp_qspi_flash.o(i.BSP_QSPI_Erase_Chip), (84 bytes).
    Removing bsp_qspi_flash.o(i.BSP_QSPI_GetInfo), (24 bytes).
    Removing bsp_qspi_flash.o(i.BSP_QSPI_GetStatus), (96 bytes).
    Removing bsp_key.o(.rev16_text), (4 bytes).
    Removing bsp_key.o(.revsh_text), (4 bytes).
    Removing bsp_key.o(.rrx_text), (6 bytes).
    Removing bsp_led.o(.rev16_text), (4 bytes).
    Removing bsp_led.o(.revsh_text), (4 bytes).
    Removing bsp_led.o(.rrx_text), (6 bytes).
    Removing bsp_sdram.o(.rev16_text), (4 bytes).
    Removing bsp_sdram.o(.revsh_text), (4 bytes).
    Removing bsp_sdram.o(.rrx_text), (6 bytes).
    Removing bsp_sdram.o(i.SDRAM_ReadBuffer), (52 bytes).
    Removing bsp_sdram.o(i.SDRAM_WriteBuffer), (56 bytes).
    Removing bsp_debug_usart.o(.rev16_text), (4 bytes).
    Removing bsp_debug_usart.o(.revsh_text), (4 bytes).
    Removing bsp_debug_usart.o(.rrx_text), (6 bytes).
    Removing bsp_debug_usart.o(i.Usart_SendString), (36 bytes).
    Removing bsp_debug_usart.o(i.fgetc), (24 bytes).
    Removing dadd.o(.text), (334 bytes).
    Removing dmul.o(.text), (228 bytes).
    Removing ddiv.o(.text), (222 bytes).
    Removing dfixul.o(.text), (48 bytes).
    Removing cdrcmple.o(.text), (48 bytes).
    Removing depilogue.o(.text), (186 bytes).

1573 unused section(s) (total 158870 bytes) removed from the image.

==============================================================================

Image Symbol Table

    Local Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    ../clib/microlib/division.c              0x00000000   Number         0  uidiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uldiv.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry5.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry2.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11b.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llushr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llsshr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llshl.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf0.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfb.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfa.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf8.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf3.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf7.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf6.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf1.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf2.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf4.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf5.o ABSOLUTE
    ../clib/microlib/printf/stubs.s          0x00000000   Number         0  stubs.o ABSOLUTE
    ../clib/microlib/stdio/streams.c         0x00000000   Number         0  stdout.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpya.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpyb.o ABSOLUTE
    ../clib/microlib/string/memset.c         0x00000000   Number         0  memseta.o ABSOLUTE
    ../clib/microlib/stubs.s                 0x00000000   Number         0  iusefp.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  dadd.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  ddiv.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  depilogue.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixul.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  dmul.o ABSOLUTE
    ..\..\Libraries\CMSIS\Device\ST\STM32F7xx\Source\Templates\arm\startup_stm32f767xx.s 0x00000000   Number         0  startup_stm32f767xx.o ABSOLUTE
    ..\..\Libraries\CMSIS\Device\ST\STM32F7xx\Source\Templates\system_stm32f7xx.c 0x00000000   Number         0  system_stm32f7xx.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal.c 0x00000000   Number         0  stm32f7xx_hal.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_adc.c 0x00000000   Number         0  stm32f7xx_hal_adc.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_adc_ex.c 0x00000000   Number         0  stm32f7xx_hal_adc_ex.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_can.c 0x00000000   Number         0  stm32f7xx_hal_can.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_cec.c 0x00000000   Number         0  stm32f7xx_hal_cec.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_cortex.c 0x00000000   Number         0  stm32f7xx_hal_cortex.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_crc.c 0x00000000   Number         0  stm32f7xx_hal_crc.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_crc_ex.c 0x00000000   Number         0  stm32f7xx_hal_crc_ex.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_cryp.c 0x00000000   Number         0  stm32f7xx_hal_cryp.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_cryp_ex.c 0x00000000   Number         0  stm32f7xx_hal_cryp_ex.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_dac.c 0x00000000   Number         0  stm32f7xx_hal_dac.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_dac_ex.c 0x00000000   Number         0  stm32f7xx_hal_dac_ex.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_dcmi.c 0x00000000   Number         0  stm32f7xx_hal_dcmi.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_dcmi_ex.c 0x00000000   Number         0  stm32f7xx_hal_dcmi_ex.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_dma.c 0x00000000   Number         0  stm32f7xx_hal_dma.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_dma2d.c 0x00000000   Number         0  stm32f7xx_hal_dma2d.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_dma_ex.c 0x00000000   Number         0  stm32f7xx_hal_dma_ex.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_eth.c 0x00000000   Number         0  stm32f7xx_hal_eth.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_flash.c 0x00000000   Number         0  stm32f7xx_hal_flash.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_flash_ex.c 0x00000000   Number         0  stm32f7xx_hal_flash_ex.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_gpio.c 0x00000000   Number         0  stm32f7xx_hal_gpio.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_hash.c 0x00000000   Number         0  stm32f7xx_hal_hash.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_hash_ex.c 0x00000000   Number         0  stm32f7xx_hal_hash_ex.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_hcd.c 0x00000000   Number         0  stm32f7xx_hal_hcd.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_i2c.c 0x00000000   Number         0  stm32f7xx_hal_i2c.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_i2c_ex.c 0x00000000   Number         0  stm32f7xx_hal_i2c_ex.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_i2s.c 0x00000000   Number         0  stm32f7xx_hal_i2s.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_irda.c 0x00000000   Number         0  stm32f7xx_hal_irda.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_iwdg.c 0x00000000   Number         0  stm32f7xx_hal_iwdg.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_lptim.c 0x00000000   Number         0  stm32f7xx_hal_lptim.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_ltdc.c 0x00000000   Number         0  stm32f7xx_hal_ltdc.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_msp_template.c 0x00000000   Number         0  stm32f7xx_hal_msp_template.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_nand.c 0x00000000   Number         0  stm32f7xx_hal_nand.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_nor.c 0x00000000   Number         0  stm32f7xx_hal_nor.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_pcd.c 0x00000000   Number         0  stm32f7xx_hal_pcd.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_pcd_ex.c 0x00000000   Number         0  stm32f7xx_hal_pcd_ex.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_pwr.c 0x00000000   Number         0  stm32f7xx_hal_pwr.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_pwr_ex.c 0x00000000   Number         0  stm32f7xx_hal_pwr_ex.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_qspi.c 0x00000000   Number         0  stm32f7xx_hal_qspi.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_rcc.c 0x00000000   Number         0  stm32f7xx_hal_rcc.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_rcc_ex.c 0x00000000   Number         0  stm32f7xx_hal_rcc_ex.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_rng.c 0x00000000   Number         0  stm32f7xx_hal_rng.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_rtc.c 0x00000000   Number         0  stm32f7xx_hal_rtc.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_rtc_ex.c 0x00000000   Number         0  stm32f7xx_hal_rtc_ex.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_sai.c 0x00000000   Number         0  stm32f7xx_hal_sai.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_sai_ex.c 0x00000000   Number         0  stm32f7xx_hal_sai_ex.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_sd.c 0x00000000   Number         0  stm32f7xx_hal_sd.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_sdram.c 0x00000000   Number         0  stm32f7xx_hal_sdram.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_smartcard.c 0x00000000   Number         0  stm32f7xx_hal_smartcard.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_smartcard_ex.c 0x00000000   Number         0  stm32f7xx_hal_smartcard_ex.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_spdifrx.c 0x00000000   Number         0  stm32f7xx_hal_spdifrx.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_spi.c 0x00000000   Number         0  stm32f7xx_hal_spi.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_sram.c 0x00000000   Number         0  stm32f7xx_hal_sram.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_tim.c 0x00000000   Number         0  stm32f7xx_hal_tim.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_tim_ex.c 0x00000000   Number         0  stm32f7xx_hal_tim_ex.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_uart.c 0x00000000   Number         0  stm32f7xx_hal_uart.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_usart.c 0x00000000   Number         0  stm32f7xx_hal_usart.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_hal_wwdg.c 0x00000000   Number         0  stm32f7xx_hal_wwdg.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_ll_fmc.c 0x00000000   Number         0  stm32f7xx_ll_fmc.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_ll_sdmmc.c 0x00000000   Number         0  stm32f7xx_ll_sdmmc.o ABSOLUTE
    ..\..\Libraries\STM32F7xx_HAL_Driver\Src\stm32f7xx_ll_usb.c 0x00000000   Number         0  stm32f7xx_ll_usb.o ABSOLUTE
    ..\..\User\flash\bsp_qspi_flash.c        0x00000000   Number         0  bsp_qspi_flash.o ABSOLUTE
    ..\..\User\key\bsp_key.c                 0x00000000   Number         0  bsp_key.o ABSOLUTE
    ..\..\User\led\bsp_led.c                 0x00000000   Number         0  bsp_led.o ABSOLUTE
    ..\..\User\main.c                        0x00000000   Number         0  main.o ABSOLUTE
    ..\..\User\sdram\bsp_sdram.c             0x00000000   Number         0  bsp_sdram.o ABSOLUTE
    ..\..\User\stm32f7xx_it.c                0x00000000   Number         0  stm32f7xx_it.o ABSOLUTE
    ..\..\User\usart\bsp_debug_usart.c       0x00000000   Number         0  bsp_debug_usart.o ABSOLUTE
    ..\\..\\Libraries\\CMSIS\\Device\\ST\\STM32F7xx\\Source\\Templates\\system_stm32f7xx.c 0x00000000   Number         0  system_stm32f7xx.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal.c 0x00000000   Number         0  stm32f7xx_hal.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_adc.c 0x00000000   Number         0  stm32f7xx_hal_adc.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_adc_ex.c 0x00000000   Number         0  stm32f7xx_hal_adc_ex.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_can.c 0x00000000   Number         0  stm32f7xx_hal_can.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_cec.c 0x00000000   Number         0  stm32f7xx_hal_cec.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_cortex.c 0x00000000   Number         0  stm32f7xx_hal_cortex.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_crc.c 0x00000000   Number         0  stm32f7xx_hal_crc.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_crc_ex.c 0x00000000   Number         0  stm32f7xx_hal_crc_ex.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_cryp.c 0x00000000   Number         0  stm32f7xx_hal_cryp.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_cryp_ex.c 0x00000000   Number         0  stm32f7xx_hal_cryp_ex.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_dac.c 0x00000000   Number         0  stm32f7xx_hal_dac.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_dac_ex.c 0x00000000   Number         0  stm32f7xx_hal_dac_ex.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_dcmi.c 0x00000000   Number         0  stm32f7xx_hal_dcmi.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_dcmi_ex.c 0x00000000   Number         0  stm32f7xx_hal_dcmi_ex.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_dma.c 0x00000000   Number         0  stm32f7xx_hal_dma.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_dma2d.c 0x00000000   Number         0  stm32f7xx_hal_dma2d.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_dma_ex.c 0x00000000   Number         0  stm32f7xx_hal_dma_ex.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_eth.c 0x00000000   Number         0  stm32f7xx_hal_eth.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_flash.c 0x00000000   Number         0  stm32f7xx_hal_flash.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_flash_ex.c 0x00000000   Number         0  stm32f7xx_hal_flash_ex.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_gpio.c 0x00000000   Number         0  stm32f7xx_hal_gpio.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_hash.c 0x00000000   Number         0  stm32f7xx_hal_hash.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_hash_ex.c 0x00000000   Number         0  stm32f7xx_hal_hash_ex.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_hcd.c 0x00000000   Number         0  stm32f7xx_hal_hcd.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_i2c.c 0x00000000   Number         0  stm32f7xx_hal_i2c.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_i2c_ex.c 0x00000000   Number         0  stm32f7xx_hal_i2c_ex.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_i2s.c 0x00000000   Number         0  stm32f7xx_hal_i2s.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_irda.c 0x00000000   Number         0  stm32f7xx_hal_irda.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_iwdg.c 0x00000000   Number         0  stm32f7xx_hal_iwdg.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_lptim.c 0x00000000   Number         0  stm32f7xx_hal_lptim.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_ltdc.c 0x00000000   Number         0  stm32f7xx_hal_ltdc.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_msp_template.c 0x00000000   Number         0  stm32f7xx_hal_msp_template.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_nand.c 0x00000000   Number         0  stm32f7xx_hal_nand.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_nor.c 0x00000000   Number         0  stm32f7xx_hal_nor.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_pcd.c 0x00000000   Number         0  stm32f7xx_hal_pcd.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_pcd_ex.c 0x00000000   Number         0  stm32f7xx_hal_pcd_ex.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_pwr.c 0x00000000   Number         0  stm32f7xx_hal_pwr.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_pwr_ex.c 0x00000000   Number         0  stm32f7xx_hal_pwr_ex.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_qspi.c 0x00000000   Number         0  stm32f7xx_hal_qspi.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_rcc.c 0x00000000   Number         0  stm32f7xx_hal_rcc.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_rcc_ex.c 0x00000000   Number         0  stm32f7xx_hal_rcc_ex.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_rng.c 0x00000000   Number         0  stm32f7xx_hal_rng.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_rtc.c 0x00000000   Number         0  stm32f7xx_hal_rtc.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_rtc_ex.c 0x00000000   Number         0  stm32f7xx_hal_rtc_ex.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_sai.c 0x00000000   Number         0  stm32f7xx_hal_sai.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_sai_ex.c 0x00000000   Number         0  stm32f7xx_hal_sai_ex.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_sd.c 0x00000000   Number         0  stm32f7xx_hal_sd.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_sdram.c 0x00000000   Number         0  stm32f7xx_hal_sdram.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_smartcard.c 0x00000000   Number         0  stm32f7xx_hal_smartcard.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_smartcard_ex.c 0x00000000   Number         0  stm32f7xx_hal_smartcard_ex.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_spdifrx.c 0x00000000   Number         0  stm32f7xx_hal_spdifrx.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_spi.c 0x00000000   Number         0  stm32f7xx_hal_spi.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_sram.c 0x00000000   Number         0  stm32f7xx_hal_sram.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_tim.c 0x00000000   Number         0  stm32f7xx_hal_tim.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_tim_ex.c 0x00000000   Number         0  stm32f7xx_hal_tim_ex.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_uart.c 0x00000000   Number         0  stm32f7xx_hal_uart.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_usart.c 0x00000000   Number         0  stm32f7xx_hal_usart.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_hal_wwdg.c 0x00000000   Number         0  stm32f7xx_hal_wwdg.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_ll_fmc.c 0x00000000   Number         0  stm32f7xx_ll_fmc.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_ll_sdmmc.c 0x00000000   Number         0  stm32f7xx_ll_sdmmc.o ABSOLUTE
    ..\\..\\Libraries\\STM32F7xx_HAL_Driver\\Src\\stm32f7xx_ll_usb.c 0x00000000   Number         0  stm32f7xx_ll_usb.o ABSOLUTE
    ..\\..\\User\\flash\\bsp_qspi_flash.c    0x00000000   Number         0  bsp_qspi_flash.o ABSOLUTE
    ..\\..\\User\\key\\bsp_key.c             0x00000000   Number         0  bsp_key.o ABSOLUTE
    ..\\..\\User\\led\\bsp_led.c             0x00000000   Number         0  bsp_led.o ABSOLUTE
    ..\\..\\User\\main.c                     0x00000000   Number         0  main.o ABSOLUTE
    ..\\..\\User\\sdram\\bsp_sdram.c         0x00000000   Number         0  bsp_sdram.o ABSOLUTE
    ..\\..\\User\\stm32f7xx_it.c             0x00000000   Number         0  stm32f7xx_it.o ABSOLUTE
    ..\\..\\User\\usart\\bsp_debug_usart.c   0x00000000   Number         0  bsp_debug_usart.o ABSOLUTE
    cdrcmple.s                               0x00000000   Number         0  cdrcmple.o ABSOLUTE
    dc.s                                     0x00000000   Number         0  dc.o ABSOLUTE
    handlers.s                               0x00000000   Number         0  handlers.o ABSOLUTE
    init.s                                   0x00000000   Number         0  init.o ABSOLUTE
    RESET                                    0x08000000   Section      504  startup_stm32f767xx.o(RESET)
    .ARM.Collect$$$$00000000                 0x080001f8   Section        0  entry.o(.ARM.Collect$$$$00000000)
    .ARM.Collect$$$$00000001                 0x080001f8   Section        4  entry2.o(.ARM.Collect$$$$00000001)
    .ARM.Collect$$$$00000004                 0x080001fc   Section        4  entry5.o(.ARM.Collect$$$$00000004)
    .ARM.Collect$$$$00000008                 0x08000200   Section        0  entry7b.o(.ARM.Collect$$$$00000008)
    .ARM.Collect$$$$0000000A                 0x08000200   Section        0  entry8b.o(.ARM.Collect$$$$0000000A)
    .ARM.Collect$$$$0000000B                 0x08000200   Section        8  entry9a.o(.ARM.Collect$$$$0000000B)
    .ARM.Collect$$$$0000000D                 0x08000208   Section        0  entry10a.o(.ARM.Collect$$$$0000000D)
    .ARM.Collect$$$$0000000F                 0x08000208   Section        0  entry11a.o(.ARM.Collect$$$$0000000F)
    .ARM.Collect$$$$00002712                 0x08000208   Section        4  entry2.o(.ARM.Collect$$$$00002712)
    __lit__00000000                          0x08000208   Data           4  entry2.o(.ARM.Collect$$$$00002712)
    .text                                    0x0800020c   Section       36  startup_stm32f767xx.o(.text)
    $v0                                      0x0800020c   Number         0  startup_stm32f767xx.o(.text)
    .text                                    0x08000230   Section        0  uldiv.o(.text)
    .text                                    0x08000294   Section       36  init.o(.text)
    .text                                    0x080002b8   Section        0  llshl.o(.text)
    .text                                    0x080002d6   Section        0  llushr.o(.text)
    i.BSP_QSPI_Erase_Block                   0x080002f8   Section        0  bsp_qspi_flash.o(i.BSP_QSPI_Erase_Block)
    i.BSP_QSPI_Init                          0x08000354   Section        0  bsp_qspi_flash.o(i.BSP_QSPI_Init)
    i.BSP_QSPI_Read                          0x080003d0   Section        0  bsp_qspi_flash.o(i.BSP_QSPI_Read)
    i.BSP_QSPI_Write                         0x08000430   Section        0  bsp_qspi_flash.o(i.BSP_QSPI_Write)
    i.Buffercmp                              0x080004d8   Section        0  main.o(i.Buffercmp)
    i.BusFault_Handler                       0x080004f6   Section        0  stm32f7xx_it.o(i.BusFault_Handler)
    i.DEBUG_USART_Config                     0x080004f8   Section        0  bsp_debug_usart.o(i.DEBUG_USART_Config)
    i.DebugMon_Handler                       0x080005c0   Section        0  stm32f7xx_it.o(i.DebugMon_Handler)
    i.Delay                                  0x080005c2   Section        0  main.o(i.Delay)
    i.FMC_SDRAM_Init                         0x080005d4   Section        0  stm32f7xx_ll_fmc.o(i.FMC_SDRAM_Init)
    i.FMC_SDRAM_ProgramRefreshRate           0x08000626   Section        0  stm32f7xx_ll_fmc.o(i.FMC_SDRAM_ProgramRefreshRate)
    i.FMC_SDRAM_SendCommand                  0x08000632   Section        0  stm32f7xx_ll_fmc.o(i.FMC_SDRAM_SendCommand)
    i.FMC_SDRAM_Timing_Init                  0x08000678   Section        0  stm32f7xx_ll_fmc.o(i.FMC_SDRAM_Timing_Init)
    i.HAL_GPIO_Init                          0x080006e8   Section        0  stm32f7xx_hal_gpio.o(i.HAL_GPIO_Init)
    i.HAL_GPIO_ReadPin                       0x080008c8   Section        0  stm32f7xx_hal_gpio.o(i.HAL_GPIO_ReadPin)
    i.HAL_GPIO_WritePin                      0x080008d6   Section        0  stm32f7xx_hal_gpio.o(i.HAL_GPIO_WritePin)
    i.HAL_GetTick                            0x080008e4   Section        0  stm32f7xx_hal.o(i.HAL_GetTick)
    i.HAL_IncTick                            0x080008f0   Section        0  stm32f7xx_hal.o(i.HAL_IncTick)
    i.HAL_InitTick                           0x08000900   Section        0  stm32f7xx_hal.o(i.HAL_InitTick)
    i.HAL_NVIC_EnableIRQ                     0x08000928   Section        0  stm32f7xx_hal_cortex.o(i.HAL_NVIC_EnableIRQ)
    i.HAL_NVIC_SetPriority                   0x08000940   Section        0  stm32f7xx_hal_cortex.o(i.HAL_NVIC_SetPriority)
    i.HAL_PWREx_EnableOverDrive              0x08000980   Section        0  stm32f7xx_hal_pwr_ex.o(i.HAL_PWREx_EnableOverDrive)
    i.HAL_QSPI_AutoPolling                   0x080009f0   Section        0  stm32f7xx_hal_qspi.o(i.HAL_QSPI_AutoPolling)
    i.HAL_QSPI_Command                       0x08000a9a   Section        0  stm32f7xx_hal_qspi.o(i.HAL_QSPI_Command)
    i.HAL_QSPI_Init                          0x08000b2c   Section        0  stm32f7xx_hal_qspi.o(i.HAL_QSPI_Init)
    i.HAL_QSPI_MspInit                       0x08000be4   Section        0  stm32f7xx_hal_qspi.o(i.HAL_QSPI_MspInit)
    i.HAL_QSPI_Receive                       0x08000be6   Section        0  stm32f7xx_hal_qspi.o(i.HAL_QSPI_Receive)
    i.HAL_QSPI_SetTimeout                    0x08000cb4   Section        0  stm32f7xx_hal_qspi.o(i.HAL_QSPI_SetTimeout)
    i.HAL_QSPI_Transmit                      0x08000cb8   Section        0  stm32f7xx_hal_qspi.o(i.HAL_QSPI_Transmit)
    i.HAL_RCCEx_PeriphCLKConfig              0x08000d7c   Section        0  stm32f7xx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig)
    i.HAL_RCC_ClockConfig                    0x08001438   Section        0  stm32f7xx_hal_rcc.o(i.HAL_RCC_ClockConfig)
    i.HAL_RCC_GetHCLKFreq                    0x080015ac   Section        0  stm32f7xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq)
    i.HAL_RCC_GetPCLK1Freq                   0x080015b8   Section        0  stm32f7xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq)
    i.HAL_RCC_GetPCLK2Freq                   0x080015e4   Section        0  stm32f7xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq)
    i.HAL_RCC_GetSysClockFreq                0x08001610   Section        0  stm32f7xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq)
    i.HAL_RCC_OscConfig                      0x08001694   Section        0  stm32f7xx_hal_rcc.o(i.HAL_RCC_OscConfig)
    i.HAL_RNG_GenerateRandomNumber           0x08001a5c   Section        0  stm32f7xx_hal_rng.o(i.HAL_RNG_GenerateRandomNumber)
    i.HAL_RNG_GetRandomNumber                0x08001ac2   Section        0  stm32f7xx_hal_rng.o(i.HAL_RNG_GetRandomNumber)
    i.HAL_RNG_Init                           0x08001ad8   Section        0  stm32f7xx_hal_rng.o(i.HAL_RNG_Init)
    i.HAL_RNG_MspInit                        0x08001b18   Section        0  stm32f7xx_hal_rng.o(i.HAL_RNG_MspInit)
    i.HAL_SDRAM_Init                         0x08001b1a   Section        0  stm32f7xx_hal_sdram.o(i.HAL_SDRAM_Init)
    i.HAL_SDRAM_MspInit                      0x08001b5e   Section        0  stm32f7xx_hal_sdram.o(i.HAL_SDRAM_MspInit)
    i.HAL_SDRAM_ProgramRefreshRate           0x08001b60   Section        0  stm32f7xx_hal_sdram.o(i.HAL_SDRAM_ProgramRefreshRate)
    i.HAL_SDRAM_SendCommand                  0x08001b86   Section        0  stm32f7xx_hal_sdram.o(i.HAL_SDRAM_SendCommand)
    i.HAL_SYSTICK_Config                     0x08001bbe   Section        0  stm32f7xx_hal_cortex.o(i.HAL_SYSTICK_Config)
    i.HAL_UART_Init                          0x08001be6   Section        0  stm32f7xx_hal_uart.o(i.HAL_UART_Init)
    i.HAL_UART_MspInit                       0x08001c56   Section        0  stm32f7xx_hal_uart.o(i.HAL_UART_MspInit)
    i.HAL_UART_Transmit                      0x08001c58   Section        0  stm32f7xx_hal_uart.o(i.HAL_UART_Transmit)
    i.HardFault_Handler                      0x08001d12   Section        0  stm32f7xx_it.o(i.HardFault_Handler)
    i.Key_GPIO_Config                        0x08001d14   Section        0  bsp_key.o(i.Key_GPIO_Config)
    i.Key_Scan                               0x08001d48   Section        0  bsp_key.o(i.Key_Scan)
    i.LED_GPIO_Config                        0x08001d70   Section        0  bsp_led.o(i.LED_GPIO_Config)
    i.MemManage_Handler                      0x08001db8   Section        0  stm32f7xx_it.o(i.MemManage_Handler)
    i.NMI_Handler                            0x08001dba   Section        0  stm32f7xx_it.o(i.NMI_Handler)
    i.NVIC_SetPriority                       0x08001dbc   Section        0  stm32f7xx_hal_cortex.o(i.NVIC_SetPriority)
    NVIC_SetPriority                         0x08001dbd   Thumb Code    32  stm32f7xx_hal_cortex.o(i.NVIC_SetPriority)
    i.PendSV_Handler                         0x08001ddc   Section        0  stm32f7xx_it.o(i.PendSV_Handler)
    i.QSPI_AutoPollingMemReady               0x08001de0   Section        0  bsp_qspi_flash.o(i.QSPI_AutoPollingMemReady)
    QSPI_AutoPollingMemReady                 0x08001de1   Thumb Code    76  bsp_qspi_flash.o(i.QSPI_AutoPollingMemReady)
    i.QSPI_Config                            0x08001e30   Section        0  stm32f7xx_hal_qspi.o(i.QSPI_Config)
    QSPI_Config                              0x08001e31   Thumb Code   434  stm32f7xx_hal_qspi.o(i.QSPI_Config)
    i.QSPI_FLASH_Init                        0x08001fe4   Section        0  bsp_qspi_flash.o(i.QSPI_FLASH_Init)
    i.QSPI_FLASH_ReadDeviceID                0x08002114   Section        0  bsp_qspi_flash.o(i.QSPI_FLASH_ReadDeviceID)
    i.QSPI_FLASH_ReadID                      0x0800219c   Section        0  bsp_qspi_flash.o(i.QSPI_FLASH_ReadID)
    i.QSPI_ResetMemory                       0x08002228   Section        0  bsp_qspi_flash.o(i.QSPI_ResetMemory)
    QSPI_ResetMemory                         0x08002229   Thumb Code    88  bsp_qspi_flash.o(i.QSPI_ResetMemory)
    i.QSPI_WaitFlagStateUntilTimeout         0x08002284   Section        0  stm32f7xx_hal_qspi.o(i.QSPI_WaitFlagStateUntilTimeout)
    QSPI_WaitFlagStateUntilTimeout           0x08002285   Thumb Code    76  stm32f7xx_hal_qspi.o(i.QSPI_WaitFlagStateUntilTimeout)
    i.QSPI_WriteEnable                       0x080022d0   Section        0  bsp_qspi_flash.o(i.QSPI_WriteEnable)
    QSPI_WriteEnable                         0x080022d1   Thumb Code   104  bsp_qspi_flash.o(i.QSPI_WriteEnable)
    i.SDRAM_Check                            0x0800233c   Section        0  main.o(i.SDRAM_Check)
    i.SDRAM_GPIO_Config                      0x080024f8   Section        0  bsp_sdram.o(i.SDRAM_GPIO_Config)
    SDRAM_GPIO_Config                        0x080024f9   Thumb Code  1126  bsp_sdram.o(i.SDRAM_GPIO_Config)
    i.SDRAM_Init                             0x0800296c   Section        0  bsp_sdram.o(i.SDRAM_Init)
    i.SDRAM_InitSequence                     0x080029e0   Section        0  bsp_sdram.o(i.SDRAM_InitSequence)
    SDRAM_InitSequence                       0x080029e1   Thumb Code   134  bsp_sdram.o(i.SDRAM_InitSequence)
    i.SDRAM_Test                             0x08002a6c   Section        0  bsp_sdram.o(i.SDRAM_Test)
    i.SDRAM_Test_All                         0x08002b8c   Section        0  main.o(i.SDRAM_Test_All)
    i.SDRAM_delay                            0x08002c8c   Section        0  bsp_sdram.o(i.SDRAM_delay)
    SDRAM_delay                              0x08002c8d   Thumb Code    28  bsp_sdram.o(i.SDRAM_delay)
    i.SPI_Test_All                           0x08002cac   Section        0  main.o(i.SPI_Test_All)
    i.SVC_Handler                            0x08002f08   Section        0  stm32f7xx_it.o(i.SVC_Handler)
    i.SysTick_Handler                        0x08002f0a   Section        0  stm32f7xx_it.o(i.SysTick_Handler)
    i.SystemClock_Config                     0x08002f0e   Section        0  main.o(i.SystemClock_Config)
    SystemClock_Config                       0x08002f0f   Thumb Code    94  main.o(i.SystemClock_Config)
    i.SystemInit                             0x08002f6c   Section        0  system_stm32f7xx.o(i.SystemInit)
    i.UART_AdvFeatureConfig                  0x08002fc0   Section        0  stm32f7xx_hal_uart.o(i.UART_AdvFeatureConfig)
    i.UART_CheckIdleState                    0x08003088   Section        0  stm32f7xx_hal_uart.o(i.UART_CheckIdleState)
    i.UART_SetConfig                         0x080030e4   Section        0  stm32f7xx_hal_uart.o(i.UART_SetConfig)
    i.UART_WaitOnFlagUntilTimeout            0x080033e0   Section        0  stm32f7xx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout)
    i.UsageFault_Handler                     0x08003444   Section        0  stm32f7xx_it.o(i.UsageFault_Handler)
    i.__0printf$5                            0x08003448   Section        0  printf5.o(i.__0printf$5)
    i.__scatterload_copy                     0x08003468   Section       14  handlers.o(i.__scatterload_copy)
    i.__scatterload_null                     0x08003476   Section        2  handlers.o(i.__scatterload_null)
    i.__scatterload_zeroinit                 0x08003478   Section       14  handlers.o(i.__scatterload_zeroinit)
    i._printf_core                           0x08003488   Section        0  printf5.o(i._printf_core)
    _printf_core                             0x08003489   Thumb Code   658  printf5.o(i._printf_core)
    i.fputc                                  0x08003748   Section        0  bsp_debug_usart.o(i.fputc)
    i.main                                   0x08003760   Section        0  main.o(i.main)
    .constdata                               0x08003794   Section       16  system_stm32f7xx.o(.constdata)
    .constdata                               0x080037a4   Section        8  system_stm32f7xx.o(.constdata)
    .conststring                             0x080037ac   Section       67  bsp_sdram.o(.conststring)
    .data                                    0x20020000   Section        4  system_stm32f7xx.o(.data)
    .data                                    0x20020004   Section        4  stm32f7xx_hal.o(.data)
    .data                                    0x20020008   Section       92  main.o(.data)
    .data                                    0x20020064   Section        4  stdout.o(.data)
    .bss                                     0x20020068   Section    40071  main.o(.bss)
    .bss                                     0x20029cf0   Section       68  bsp_qspi_flash.o(.bss)
    .bss                                     0x20029d34   Section       68  bsp_sdram.o(.bss)
    Command                                  0x20029d34   Data          16  bsp_sdram.o(.bss)
    .bss                                     0x20029d78   Section      112  bsp_debug_usart.o(.bss)
    STACK                                    0x20029de8   Section     1024  startup_stm32f767xx.o(STACK)
    .ARM.__AT_0xD0000000                     0xd0000000   Section        1  main.o(.ARM.__AT_0xD0000000)

    Global Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    BuildAttributes$$THM_ISAv4$E$P$D$K$B$S$7EM$VFPv5_D16$PE$PLD8$A:L22UL41UL21$X:L11$S22US41US21$IEEE1$IW$USESV6$~STKCKD$USESV7$~SHL$OSPACE$ROPI$EBA8$MICROLIB$REQ8$PRES8$EABIv2 0x00000000   Number         0  anon$$obj.o ABSOLUTE
    __ARM_use_no_argv                        0x00000000   Number         0  main.o ABSOLUTE
    _printf_a                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_c                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_charcount                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_d                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_e                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_f                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_flags                            0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_dec                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_fp_hex                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_g                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_i                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_int_dec                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_l                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ll                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lld                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_lli                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llo                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llu                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_llx                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_dec                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_hex                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_longlong_oct                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_ls                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_mbtowc                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_n                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_o                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_p                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_percent                          0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_pre_padding                      0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_return_value                     0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_s                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_sizespec                         0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_str                              0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_signed                  0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_truncate_unsigned                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_u                                0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wc                               0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_wctomb                           0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_widthprec                        0x00000000   Number         0  stubs.o ABSOLUTE
    _printf_x                                0x00000000   Number         0  stubs.o ABSOLUTE
    __cpp_initialize__aeabi_                  - Undefined Weak Reference
    __cxa_finalize                            - Undefined Weak Reference
    __decompress                              - Undefined Weak Reference
    _clock_init                               - Undefined Weak Reference
    _microlib_exit                            - Undefined Weak Reference
    __Vectors_Size                           0x000001f8   Number         0  startup_stm32f767xx.o ABSOLUTE
    __Vectors                                0x08000000   Data           4  startup_stm32f767xx.o(RESET)
    __Vectors_End                            0x080001f8   Data           0  startup_stm32f767xx.o(RESET)
    __main                                   0x080001f9   Thumb Code     0  entry.o(.ARM.Collect$$$$00000000)
    _main_stk                                0x080001f9   Thumb Code     0  entry2.o(.ARM.Collect$$$$00000001)
    _main_scatterload                        0x080001fd   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    __main_after_scatterload                 0x08000201   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    _main_clock                              0x08000201   Thumb Code     0  entry7b.o(.ARM.Collect$$$$00000008)
    _main_cpp_init                           0x08000201   Thumb Code     0  entry8b.o(.ARM.Collect$$$$0000000A)
    _main_init                               0x08000201   Thumb Code     0  entry9a.o(.ARM.Collect$$$$0000000B)
    __rt_final_cpp                           0x08000209   Thumb Code     0  entry10a.o(.ARM.Collect$$$$0000000D)
    __rt_final_exit                          0x08000209   Thumb Code     0  entry11a.o(.ARM.Collect$$$$0000000F)
    Reset_Handler                            0x0800020d   Thumb Code     8  startup_stm32f767xx.o(.text)
    ADC_IRQHandler                           0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    CAN1_RX0_IRQHandler                      0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    CAN1_RX1_IRQHandler                      0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    CAN1_SCE_IRQHandler                      0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    CAN1_TX_IRQHandler                       0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    CAN2_RX0_IRQHandler                      0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    CAN2_RX1_IRQHandler                      0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    CAN2_SCE_IRQHandler                      0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    CAN2_TX_IRQHandler                       0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    CAN3_RX0_IRQHandler                      0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    CAN3_RX1_IRQHandler                      0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    CAN3_SCE_IRQHandler                      0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    CAN3_TX_IRQHandler                       0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    CEC_IRQHandler                           0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    DCMI_IRQHandler                          0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    DFSDM1_FLT0_IRQHandler                   0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    DFSDM1_FLT1_IRQHandler                   0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    DFSDM1_FLT2_IRQHandler                   0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    DFSDM1_FLT3_IRQHandler                   0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    DMA1_Stream0_IRQHandler                  0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    DMA1_Stream1_IRQHandler                  0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    DMA1_Stream2_IRQHandler                  0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    DMA1_Stream3_IRQHandler                  0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    DMA1_Stream4_IRQHandler                  0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    DMA1_Stream5_IRQHandler                  0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    DMA1_Stream6_IRQHandler                  0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    DMA1_Stream7_IRQHandler                  0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    DMA2D_IRQHandler                         0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    DMA2_Stream0_IRQHandler                  0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    DMA2_Stream1_IRQHandler                  0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    DMA2_Stream2_IRQHandler                  0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    DMA2_Stream3_IRQHandler                  0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    DMA2_Stream4_IRQHandler                  0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    DMA2_Stream5_IRQHandler                  0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    DMA2_Stream6_IRQHandler                  0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    DMA2_Stream7_IRQHandler                  0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    ETH_IRQHandler                           0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    ETH_WKUP_IRQHandler                      0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    EXTI0_IRQHandler                         0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    EXTI15_10_IRQHandler                     0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    EXTI1_IRQHandler                         0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    EXTI2_IRQHandler                         0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    EXTI3_IRQHandler                         0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    EXTI4_IRQHandler                         0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    EXTI9_5_IRQHandler                       0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    FLASH_IRQHandler                         0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    FMC_IRQHandler                           0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    FPU_IRQHandler                           0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    I2C1_ER_IRQHandler                       0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    I2C1_EV_IRQHandler                       0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    I2C2_ER_IRQHandler                       0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    I2C2_EV_IRQHandler                       0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    I2C3_ER_IRQHandler                       0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    I2C3_EV_IRQHandler                       0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    I2C4_ER_IRQHandler                       0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    I2C4_EV_IRQHandler                       0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    JPEG_IRQHandler                          0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    LPTIM1_IRQHandler                        0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    LTDC_ER_IRQHandler                       0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    LTDC_IRQHandler                          0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    MDIOS_IRQHandler                         0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    OTG_FS_IRQHandler                        0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    OTG_FS_WKUP_IRQHandler                   0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    OTG_HS_EP1_IN_IRQHandler                 0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    OTG_HS_EP1_OUT_IRQHandler                0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    OTG_HS_IRQHandler                        0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    OTG_HS_WKUP_IRQHandler                   0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    PVD_IRQHandler                           0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    QUADSPI_IRQHandler                       0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    RCC_IRQHandler                           0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    RNG_IRQHandler                           0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    RTC_Alarm_IRQHandler                     0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    RTC_WKUP_IRQHandler                      0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    SAI1_IRQHandler                          0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    SAI2_IRQHandler                          0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    SDMMC1_IRQHandler                        0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    SDMMC2_IRQHandler                        0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    SPDIF_RX_IRQHandler                      0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    SPI1_IRQHandler                          0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    SPI2_IRQHandler                          0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    SPI3_IRQHandler                          0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    SPI4_IRQHandler                          0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    SPI5_IRQHandler                          0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    SPI6_IRQHandler                          0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    TAMP_STAMP_IRQHandler                    0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    TIM1_BRK_TIM9_IRQHandler                 0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    TIM1_CC_IRQHandler                       0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    TIM1_TRG_COM_TIM11_IRQHandler            0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    TIM1_UP_TIM10_IRQHandler                 0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    TIM2_IRQHandler                          0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    TIM3_IRQHandler                          0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    TIM4_IRQHandler                          0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    TIM5_IRQHandler                          0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    TIM6_DAC_IRQHandler                      0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    TIM7_IRQHandler                          0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    TIM8_BRK_TIM12_IRQHandler                0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    TIM8_CC_IRQHandler                       0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    TIM8_TRG_COM_TIM14_IRQHandler            0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    TIM8_UP_TIM13_IRQHandler                 0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    UART4_IRQHandler                         0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    UART5_IRQHandler                         0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    UART7_IRQHandler                         0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    UART8_IRQHandler                         0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    USART1_IRQHandler                        0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    USART2_IRQHandler                        0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    USART3_IRQHandler                        0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    USART6_IRQHandler                        0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    WWDG_IRQHandler                          0x08000227   Thumb Code     0  startup_stm32f767xx.o(.text)
    __aeabi_uldivmod                         0x08000231   Thumb Code    98  uldiv.o(.text)
    __scatterload                            0x08000295   Thumb Code    28  init.o(.text)
    __scatterload_rt2                        0x08000295   Thumb Code     0  init.o(.text)
    __aeabi_llsl                             0x080002b9   Thumb Code    30  llshl.o(.text)
    _ll_shift_l                              0x080002b9   Thumb Code     0  llshl.o(.text)
    __aeabi_llsr                             0x080002d7   Thumb Code    32  llushr.o(.text)
    _ll_ushift_r                             0x080002d7   Thumb Code     0  llushr.o(.text)
    BSP_QSPI_Erase_Block                     0x080002f9   Thumb Code    86  bsp_qspi_flash.o(i.BSP_QSPI_Erase_Block)
    BSP_QSPI_Init                            0x08000355   Thumb Code   118  bsp_qspi_flash.o(i.BSP_QSPI_Init)
    BSP_QSPI_Read                            0x080003d1   Thumb Code    90  bsp_qspi_flash.o(i.BSP_QSPI_Read)
    BSP_QSPI_Write                           0x08000431   Thumb Code   164  bsp_qspi_flash.o(i.BSP_QSPI_Write)
    Buffercmp                                0x080004d9   Thumb Code    30  main.o(i.Buffercmp)
    BusFault_Handler                         0x080004f7   Thumb Code     2  stm32f7xx_it.o(i.BusFault_Handler)
    DEBUG_USART_Config                       0x080004f9   Thumb Code   182  bsp_debug_usart.o(i.DEBUG_USART_Config)
    DebugMon_Handler                         0x080005c1   Thumb Code     2  stm32f7xx_it.o(i.DebugMon_Handler)
    Delay                                    0x080005c3   Thumb Code    18  main.o(i.Delay)
    FMC_SDRAM_Init                           0x080005d5   Thumb Code    82  stm32f7xx_ll_fmc.o(i.FMC_SDRAM_Init)
    FMC_SDRAM_ProgramRefreshRate             0x08000627   Thumb Code    12  stm32f7xx_ll_fmc.o(i.FMC_SDRAM_ProgramRefreshRate)
    FMC_SDRAM_SendCommand                    0x08000633   Thumb Code    70  stm32f7xx_ll_fmc.o(i.FMC_SDRAM_SendCommand)
    FMC_SDRAM_Timing_Init                    0x08000679   Thumb Code   108  stm32f7xx_ll_fmc.o(i.FMC_SDRAM_Timing_Init)
    HAL_GPIO_Init                            0x080006e9   Thumb Code   426  stm32f7xx_hal_gpio.o(i.HAL_GPIO_Init)
    HAL_GPIO_ReadPin                         0x080008c9   Thumb Code    14  stm32f7xx_hal_gpio.o(i.HAL_GPIO_ReadPin)
    HAL_GPIO_WritePin                        0x080008d7   Thumb Code    14  stm32f7xx_hal_gpio.o(i.HAL_GPIO_WritePin)
    HAL_GetTick                              0x080008e5   Thumb Code     6  stm32f7xx_hal.o(i.HAL_GetTick)
    HAL_IncTick                              0x080008f1   Thumb Code    10  stm32f7xx_hal.o(i.HAL_IncTick)
    HAL_InitTick                             0x08000901   Thumb Code    34  stm32f7xx_hal.o(i.HAL_InitTick)
    HAL_NVIC_EnableIRQ                       0x08000929   Thumb Code    22  stm32f7xx_hal_cortex.o(i.HAL_NVIC_EnableIRQ)
    HAL_NVIC_SetPriority                     0x08000941   Thumb Code    60  stm32f7xx_hal_cortex.o(i.HAL_NVIC_SetPriority)
    HAL_PWREx_EnableOverDrive                0x08000981   Thumb Code   102  stm32f7xx_hal_pwr_ex.o(i.HAL_PWREx_EnableOverDrive)
    HAL_QSPI_AutoPolling                     0x080009f1   Thumb Code   170  stm32f7xx_hal_qspi.o(i.HAL_QSPI_AutoPolling)
    HAL_QSPI_Command                         0x08000a9b   Thumb Code   146  stm32f7xx_hal_qspi.o(i.HAL_QSPI_Command)
    HAL_QSPI_Init                            0x08000b2d   Thumb Code   174  stm32f7xx_hal_qspi.o(i.HAL_QSPI_Init)
    HAL_QSPI_MspInit                         0x08000be5   Thumb Code     2  stm32f7xx_hal_qspi.o(i.HAL_QSPI_MspInit)
    HAL_QSPI_Receive                         0x08000be7   Thumb Code   206  stm32f7xx_hal_qspi.o(i.HAL_QSPI_Receive)
    HAL_QSPI_SetTimeout                      0x08000cb5   Thumb Code     4  stm32f7xx_hal_qspi.o(i.HAL_QSPI_SetTimeout)
    HAL_QSPI_Transmit                        0x08000cb9   Thumb Code   196  stm32f7xx_hal_qspi.o(i.HAL_QSPI_Transmit)
    HAL_RCCEx_PeriphCLKConfig                0x08000d7d   Thumb Code  1714  stm32f7xx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig)
    HAL_RCC_ClockConfig                      0x08001439   Thumb Code   354  stm32f7xx_hal_rcc.o(i.HAL_RCC_ClockConfig)
    HAL_RCC_GetHCLKFreq                      0x080015ad   Thumb Code     6  stm32f7xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq)
    HAL_RCC_GetPCLK1Freq                     0x080015b9   Thumb Code    36  stm32f7xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq)
    HAL_RCC_GetPCLK2Freq                     0x080015e5   Thumb Code    36  stm32f7xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq)
    HAL_RCC_GetSysClockFreq                  0x08001611   Thumb Code   120  stm32f7xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq)
    HAL_RCC_OscConfig                        0x08001695   Thumb Code   960  stm32f7xx_hal_rcc.o(i.HAL_RCC_OscConfig)
    HAL_RNG_GenerateRandomNumber             0x08001a5d   Thumb Code   102  stm32f7xx_hal_rng.o(i.HAL_RNG_GenerateRandomNumber)
    HAL_RNG_GetRandomNumber                  0x08001ac3   Thumb Code    22  stm32f7xx_hal_rng.o(i.HAL_RNG_GetRandomNumber)
    HAL_RNG_Init                             0x08001ad9   Thumb Code    64  stm32f7xx_hal_rng.o(i.HAL_RNG_Init)
    HAL_RNG_MspInit                          0x08001b19   Thumb Code     2  stm32f7xx_hal_rng.o(i.HAL_RNG_MspInit)
    HAL_SDRAM_Init                           0x08001b1b   Thumb Code    68  stm32f7xx_hal_sdram.o(i.HAL_SDRAM_Init)
    HAL_SDRAM_MspInit                        0x08001b5f   Thumb Code     2  stm32f7xx_hal_sdram.o(i.HAL_SDRAM_MspInit)
    HAL_SDRAM_ProgramRefreshRate             0x08001b61   Thumb Code    38  stm32f7xx_hal_sdram.o(i.HAL_SDRAM_ProgramRefreshRate)
    HAL_SDRAM_SendCommand                    0x08001b87   Thumb Code    56  stm32f7xx_hal_sdram.o(i.HAL_SDRAM_SendCommand)
    HAL_SYSTICK_Config                       0x08001bbf   Thumb Code    40  stm32f7xx_hal_cortex.o(i.HAL_SYSTICK_Config)
    HAL_UART_Init                            0x08001be7   Thumb Code   112  stm32f7xx_hal_uart.o(i.HAL_UART_Init)
    HAL_UART_MspInit                         0x08001c57   Thumb Code     2  stm32f7xx_hal_uart.o(i.HAL_UART_MspInit)
    HAL_UART_Transmit                        0x08001c59   Thumb Code   186  stm32f7xx_hal_uart.o(i.HAL_UART_Transmit)
    HardFault_Handler                        0x08001d13   Thumb Code     2  stm32f7xx_it.o(i.HardFault_Handler)
    Key_GPIO_Config                          0x08001d15   Thumb Code    44  bsp_key.o(i.Key_GPIO_Config)
    Key_Scan                                 0x08001d49   Thumb Code    38  bsp_key.o(i.Key_Scan)
    LED_GPIO_Config                          0x08001d71   Thumb Code    62  bsp_led.o(i.LED_GPIO_Config)
    MemManage_Handler                        0x08001db9   Thumb Code     2  stm32f7xx_it.o(i.MemManage_Handler)
    NMI_Handler                              0x08001dbb   Thumb Code     2  stm32f7xx_it.o(i.NMI_Handler)
    PendSV_Handler                           0x08001ddd   Thumb Code     2  stm32f7xx_it.o(i.PendSV_Handler)
    QSPI_FLASH_Init                          0x08001fe5   Thumb Code   282  bsp_qspi_flash.o(i.QSPI_FLASH_Init)
    QSPI_FLASH_ReadDeviceID                  0x08002115   Thumb Code   108  bsp_qspi_flash.o(i.QSPI_FLASH_ReadDeviceID)
    QSPI_FLASH_ReadID                        0x0800219d   Thumb Code   110  bsp_qspi_flash.o(i.QSPI_FLASH_ReadID)
    SDRAM_Check                              0x0800233d   Thumb Code   278  main.o(i.SDRAM_Check)
    SDRAM_Init                               0x0800296d   Thumb Code   104  bsp_sdram.o(i.SDRAM_Init)
    SDRAM_Test                               0x08002a6d   Thumb Code   162  bsp_sdram.o(i.SDRAM_Test)
    SDRAM_Test_All                           0x08002b8d   Thumb Code   114  main.o(i.SDRAM_Test_All)
    SPI_Test_All                             0x08002cad   Thumb Code   296  main.o(i.SPI_Test_All)
    SVC_Handler                              0x08002f09   Thumb Code     2  stm32f7xx_it.o(i.SVC_Handler)
    SysTick_Handler                          0x08002f0b   Thumb Code     4  stm32f7xx_it.o(i.SysTick_Handler)
    SystemInit                               0x08002f6d   Thumb Code    66  system_stm32f7xx.o(i.SystemInit)
    UART_AdvFeatureConfig                    0x08002fc1   Thumb Code   200  stm32f7xx_hal_uart.o(i.UART_AdvFeatureConfig)
    UART_CheckIdleState                      0x08003089   Thumb Code    92  stm32f7xx_hal_uart.o(i.UART_CheckIdleState)
    UART_SetConfig                           0x080030e5   Thumb Code   716  stm32f7xx_hal_uart.o(i.UART_SetConfig)
    UART_WaitOnFlagUntilTimeout              0x080033e1   Thumb Code   100  stm32f7xx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout)
    UsageFault_Handler                       0x08003445   Thumb Code     2  stm32f7xx_it.o(i.UsageFault_Handler)
    __0printf$5                              0x08003449   Thumb Code    22  printf5.o(i.__0printf$5)
    __1printf$5                              0x08003449   Thumb Code     0  printf5.o(i.__0printf$5)
    __2printf                                0x08003449   Thumb Code     0  printf5.o(i.__0printf$5)
    __scatterload_copy                       0x08003469   Thumb Code    14  handlers.o(i.__scatterload_copy)
    __scatterload_null                       0x08003477   Thumb Code     2  handlers.o(i.__scatterload_null)
    __scatterload_zeroinit                   0x08003479   Thumb Code    14  handlers.o(i.__scatterload_zeroinit)
    fputc                                    0x08003749   Thumb Code    20  bsp_debug_usart.o(i.fputc)
    main                                     0x08003761   Thumb Code    48  main.o(i.main)
    AHBPrescTable                            0x08003794   Data          16  system_stm32f7xx.o(.constdata)
    APBPrescTable                            0x080037a4   Data           8  system_stm32f7xx.o(.constdata)
    Region$$Table$$Base                      0x080037f0   Number         0  anon$$obj.o(Region$$Table)
    Region$$Table$$Limit                     0x08003810   Number         0  anon$$obj.o(Region$$Table)
    SystemCoreClock                          0x20020000   Data           4  system_stm32f7xx.o(.data)
    uwTick                                   0x20020004   Data           4  stm32f7xx_hal.o(.data)
    TransferStatus1                          0x20020008   Data           1  main.o(.data)
    DeviceID                                 0x2002000c   Data           4  main.o(.data)
    FlashID                                  0x20020010   Data           4  main.o(.data)
    pSDRAM                                   0x20020014   Data           4  main.o(.data)
    count                                    0x20020018   Data           8  main.o(.data)
    sdram_count                              0x20020020   Data           8  main.o(.data)
    Tx_Buffer                                0x20020028   Data          60  main.o(.data)
    __stdout                                 0x20020064   Data           4  stdout.o(.data)
    RadomBuffer                              0x20020068   Data       40000  main.o(.bss)
    hrng                                     0x20029ca8   Data          12  main.o(.bss)
    Rx_Buffer                                0x20029cb4   Data          59  main.o(.bss)
    hqspi                                    0x20029cf0   Data          68  bsp_qspi_flash.o(.bss)
    hsdram1                                  0x20029d44   Data          52  bsp_sdram.o(.bss)
    UartHandle                               0x20029d78   Data         112  bsp_debug_usart.o(.bss)
    __initial_sp                             0x2002a1e8   Data           0  startup_stm32f767xx.o(STACK)
    testValue                                0xd0000000   Data           1  main.o(.ARM.__AT_0xD0000000)



==============================================================================

Memory Map of the image

  Image Entry point : 0x080001f9

  Load Region LR_IROM1 (Base: 0x08000000, Size: 0x00003878, Max: 0x00100000, ABSOLUTE)

    Execution Region ER_IROM1 (Base: 0x08000000, Size: 0x00003810, Max: 0x00100000, ABSOLUTE)

    Base Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x08000000   0x000001f8   Data   RO            3    RESET               startup_stm32f767xx.o
    0x080001f8   0x00000000   Code   RO         9923  * .ARM.Collect$$$$00000000  mc_w.l(entry.o)
    0x080001f8   0x00000004   Code   RO        10193    .ARM.Collect$$$$00000001  mc_w.l(entry2.o)
    0x080001fc   0x00000004   Code   RO        10196    .ARM.Collect$$$$00000004  mc_w.l(entry5.o)
    0x08000200   0x00000000   Code   RO        10198    .ARM.Collect$$$$00000008  mc_w.l(entry7b.o)
    0x08000200   0x00000000   Code   RO        10200    .ARM.Collect$$$$0000000A  mc_w.l(entry8b.o)
    0x08000200   0x00000008   Code   RO        10201    .ARM.Collect$$$$0000000B  mc_w.l(entry9a.o)
    0x08000208   0x00000000   Code   RO        10203    .ARM.Collect$$$$0000000D  mc_w.l(entry10a.o)
    0x08000208   0x00000000   Code   RO        10205    .ARM.Collect$$$$0000000F  mc_w.l(entry11a.o)
    0x08000208   0x00000004   Code   RO        10194    .ARM.Collect$$$$00002712  mc_w.l(entry2.o)
    0x0800020c   0x00000024   Code   RO            4    .text               startup_stm32f767xx.o
    0x08000230   0x00000062   Code   RO        10210    .text               mc_w.l(uldiv.o)
    0x08000292   0x00000002   PAD
    0x08000294   0x00000024   Code   RO        10223    .text               mc_w.l(init.o)
    0x080002b8   0x0000001e   Code   RO        10225    .text               mc_w.l(llshl.o)
    0x080002d6   0x00000020   Code   RO        10227    .text               mc_w.l(llushr.o)
    0x080002f6   0x00000002   PAD
    0x080002f8   0x0000005c   Code   RO         9663    i.BSP_QSPI_Erase_Block  bsp_qspi_flash.o
    0x08000354   0x0000007c   Code   RO         9667    i.BSP_QSPI_Init     bsp_qspi_flash.o
    0x080003d0   0x00000060   Code   RO         9668    i.BSP_QSPI_Read     bsp_qspi_flash.o
    0x08000430   0x000000a8   Code   RO         9669    i.BSP_QSPI_Write    bsp_qspi_flash.o
    0x080004d8   0x0000001e   Code   RO         9500    i.Buffercmp         main.o
    0x080004f6   0x00000002   Code   RO         9588    i.BusFault_Handler  stm32f7xx_it.o
    0x080004f8   0x000000c8   Code   RO         9877    i.DEBUG_USART_Config  bsp_debug_usart.o
    0x080005c0   0x00000002   Code   RO         9589    i.DebugMon_Handler  stm32f7xx_it.o
    0x080005c2   0x00000012   Code   RO         9501    i.Delay             main.o
    0x080005d4   0x00000052   Code   RO         8981    i.FMC_SDRAM_Init    stm32f7xx_ll_fmc.o
    0x08000626   0x0000000c   Code   RO         8982    i.FMC_SDRAM_ProgramRefreshRate  stm32f7xx_ll_fmc.o
    0x08000632   0x00000046   Code   RO         8983    i.FMC_SDRAM_SendCommand  stm32f7xx_ll_fmc.o
    0x08000678   0x00000070   Code   RO         8985    i.FMC_SDRAM_Timing_Init  stm32f7xx_ll_fmc.o
    0x080006e8   0x000001e0   Code   RO         2387    i.HAL_GPIO_Init     stm32f7xx_hal_gpio.o
    0x080008c8   0x0000000e   Code   RO         2389    i.HAL_GPIO_ReadPin  stm32f7xx_hal_gpio.o
    0x080008d6   0x0000000e   Code   RO         2391    i.HAL_GPIO_WritePin  stm32f7xx_hal_gpio.o
    0x080008e4   0x0000000c   Code   RO          296    i.HAL_GetTick       stm32f7xx_hal.o
    0x080008f0   0x00000010   Code   RO          297    i.HAL_IncTick       stm32f7xx_hal.o
    0x08000900   0x00000028   Code   RO          299    i.HAL_InitTick      stm32f7xx_hal.o
    0x08000928   0x00000016   Code   RO          969    i.HAL_NVIC_EnableIRQ  stm32f7xx_hal_cortex.o
    0x0800093e   0x00000002   PAD
    0x08000940   0x00000040   Code   RO          975    i.HAL_NVIC_SetPriority  stm32f7xx_hal_cortex.o
    0x08000980   0x00000070   Code   RO         4861    i.HAL_PWREx_EnableOverDrive  stm32f7xx_hal_pwr_ex.o
    0x080009f0   0x000000aa   Code   RO         4950    i.HAL_QSPI_AutoPolling  stm32f7xx_hal_qspi.o
    0x08000a9a   0x00000092   Code   RO         4953    i.HAL_QSPI_Command  stm32f7xx_hal_qspi.o
    0x08000b2c   0x000000b8   Code   RO         4962    i.HAL_QSPI_Init     stm32f7xx_hal_qspi.o
    0x08000be4   0x00000002   Code   RO         4965    i.HAL_QSPI_MspInit  stm32f7xx_hal_qspi.o
    0x08000be6   0x000000ce   Code   RO         4966    i.HAL_QSPI_Receive  stm32f7xx_hal_qspi.o
    0x08000cb4   0x00000004   Code   RO         4972    i.HAL_QSPI_SetTimeout  stm32f7xx_hal_qspi.o
    0x08000cb8   0x000000c4   Code   RO         4975    i.HAL_QSPI_Transmit  stm32f7xx_hal_qspi.o
    0x08000d7c   0x000006bc   Code   RO         5307    i.HAL_RCCEx_PeriphCLKConfig  stm32f7xx_hal_rcc_ex.o
    0x08001438   0x00000174   Code   RO         5204    i.HAL_RCC_ClockConfig  stm32f7xx_hal_rcc.o
    0x080015ac   0x0000000c   Code   RO         5209    i.HAL_RCC_GetHCLKFreq  stm32f7xx_hal_rcc.o
    0x080015b8   0x0000002c   Code   RO         5211    i.HAL_RCC_GetPCLK1Freq  stm32f7xx_hal_rcc.o
    0x080015e4   0x0000002c   Code   RO         5212    i.HAL_RCC_GetPCLK2Freq  stm32f7xx_hal_rcc.o
    0x08001610   0x00000084   Code   RO         5213    i.HAL_RCC_GetSysClockFreq  stm32f7xx_hal_rcc.o
    0x08001694   0x000003c8   Code   RO         5216    i.HAL_RCC_OscConfig  stm32f7xx_hal_rcc.o
    0x08001a5c   0x00000066   Code   RO         5343    i.HAL_RNG_GenerateRandomNumber  stm32f7xx_hal_rng.o
    0x08001ac2   0x00000016   Code   RO         5345    i.HAL_RNG_GetRandomNumber  stm32f7xx_hal_rng.o
    0x08001ad8   0x00000040   Code   RO         5349    i.HAL_RNG_Init      stm32f7xx_hal_rng.o
    0x08001b18   0x00000002   Code   RO         5351    i.HAL_RNG_MspInit   stm32f7xx_hal_rng.o
    0x08001b1a   0x00000044   Code   RO         6372    i.HAL_SDRAM_Init    stm32f7xx_hal_sdram.o
    0x08001b5e   0x00000002   Code   RO         6374    i.HAL_SDRAM_MspInit  stm32f7xx_hal_sdram.o
    0x08001b60   0x00000026   Code   RO         6375    i.HAL_SDRAM_ProgramRefreshRate  stm32f7xx_hal_sdram.o
    0x08001b86   0x00000038   Code   RO         6381    i.HAL_SDRAM_SendCommand  stm32f7xx_hal_sdram.o
    0x08001bbe   0x00000028   Code   RO          980    i.HAL_SYSTICK_Config  stm32f7xx_hal_cortex.o
    0x08001be6   0x00000070   Code   RO         8405    i.HAL_UART_Init     stm32f7xx_hal_uart.o
    0x08001c56   0x00000002   Code   RO         8407    i.HAL_UART_MspInit  stm32f7xx_hal_uart.o
    0x08001c58   0x000000ba   Code   RO         8413    i.HAL_UART_Transmit  stm32f7xx_hal_uart.o
    0x08001d12   0x00000002   Code   RO         9590    i.HardFault_Handler  stm32f7xx_it.o
    0x08001d14   0x00000034   Code   RO         9759    i.Key_GPIO_Config   bsp_key.o
    0x08001d48   0x00000026   Code   RO         9760    i.Key_Scan          bsp_key.o
    0x08001d6e   0x00000002   PAD
    0x08001d70   0x00000048   Code   RO         9792    i.LED_GPIO_Config   bsp_led.o
    0x08001db8   0x00000002   Code   RO         9591    i.MemManage_Handler  stm32f7xx_it.o
    0x08001dba   0x00000002   Code   RO         9592    i.NMI_Handler       stm32f7xx_it.o
    0x08001dbc   0x00000020   Code   RO          982    i.NVIC_SetPriority  stm32f7xx_hal_cortex.o
    0x08001ddc   0x00000002   Code   RO         9593    i.PendSV_Handler    stm32f7xx_it.o
    0x08001dde   0x00000002   PAD
    0x08001de0   0x00000050   Code   RO         9670    i.QSPI_AutoPollingMemReady  bsp_qspi_flash.o
    0x08001e30   0x000001b2   Code   RO         4980    i.QSPI_Config       stm32f7xx_hal_qspi.o
    0x08001fe2   0x00000002   PAD
    0x08001fe4   0x00000130   Code   RO         9671    i.QSPI_FLASH_Init   bsp_qspi_flash.o
    0x08002114   0x00000088   Code   RO         9672    i.QSPI_FLASH_ReadDeviceID  bsp_qspi_flash.o
    0x0800219c   0x0000008c   Code   RO         9673    i.QSPI_FLASH_ReadID  bsp_qspi_flash.o
    0x08002228   0x0000005c   Code   RO         9674    i.QSPI_ResetMemory  bsp_qspi_flash.o
    0x08002284   0x0000004c   Code   RO         4987    i.QSPI_WaitFlagStateUntilTimeout  stm32f7xx_hal_qspi.o
    0x080022d0   0x0000006c   Code   RO         9675    i.QSPI_WriteEnable  bsp_qspi_flash.o
    0x0800233c   0x000001bc   Code   RO         9502    i.SDRAM_Check       main.o
    0x080024f8   0x00000474   Code   RO         9816    i.SDRAM_GPIO_Config  bsp_sdram.o
    0x0800296c   0x00000074   Code   RO         9817    i.SDRAM_Init        bsp_sdram.o
    0x080029e0   0x0000008c   Code   RO         9818    i.SDRAM_InitSequence  bsp_sdram.o
    0x08002a6c   0x00000120   Code   RO         9820    i.SDRAM_Test        bsp_sdram.o
    0x08002b8c   0x00000100   Code   RO         9503    i.SDRAM_Test_All    main.o
    0x08002c8c   0x00000020   Code   RO         9822    i.SDRAM_delay       bsp_sdram.o
    0x08002cac   0x0000025c   Code   RO         9504    i.SPI_Test_All      main.o
    0x08002f08   0x00000002   Code   RO         9594    i.SVC_Handler       stm32f7xx_it.o
    0x08002f0a   0x00000004   Code   RO         9595    i.SysTick_Handler   stm32f7xx_it.o
    0x08002f0e   0x0000005e   Code   RO         9505    i.SystemClock_Config  main.o
    0x08002f6c   0x00000054   Code   RO           14    i.SystemInit        system_stm32f7xx.o
    0x08002fc0   0x000000c8   Code   RO         8418    i.UART_AdvFeatureConfig  stm32f7xx_hal_uart.o
    0x08003088   0x0000005c   Code   RO         8419    i.UART_CheckIdleState  stm32f7xx_hal_uart.o
    0x080030e4   0x000002fc   Code   RO         8430    i.UART_SetConfig    stm32f7xx_hal_uart.o
    0x080033e0   0x00000064   Code   RO         8432    i.UART_WaitOnFlagUntilTimeout  stm32f7xx_hal_uart.o
    0x08003444   0x00000002   Code   RO         9596    i.UsageFault_Handler  stm32f7xx_it.o
    0x08003446   0x00000002   PAD
    0x08003448   0x00000020   Code   RO        10065    i.__0printf$5       mc_w.l(printf5.o)
    0x08003468   0x0000000e   Code   RO        10235    i.__scatterload_copy  mc_w.l(handlers.o)
    0x08003476   0x00000002   Code   RO        10236    i.__scatterload_null  mc_w.l(handlers.o)
    0x08003478   0x0000000e   Code   RO        10237    i.__scatterload_zeroinit  mc_w.l(handlers.o)
    0x08003486   0x00000002   PAD
    0x08003488   0x000002c0   Code   RO        10072    i._printf_core      mc_w.l(printf5.o)
    0x08003748   0x00000018   Code   RO         9880    i.fputc             bsp_debug_usart.o
    0x08003760   0x00000034   Code   RO         9506    i.main              main.o
    0x08003794   0x00000010   Data   RO           15    .constdata          system_stm32f7xx.o
    0x080037a4   0x00000008   Data   RO           16    .constdata          system_stm32f7xx.o
    0x080037ac   0x00000043   Data   RO         9824    .conststring        bsp_sdram.o
    0x080037ef   0x00000001   PAD
    0x080037f0   0x00000020   Data   RO        10233    Region$$Table       anon$$obj.o


    Execution Region RW_IRAM1 (Base: 0x20020000, Size: 0x0000a1e8, Max: 0x00060000, ABSOLUTE)

    Base Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x20020000   0x00000004   Data   RW           17    .data               system_stm32f7xx.o
    0x20020004   0x00000004   Data   RW          304    .data               stm32f7xx_hal.o
    0x20020008   0x0000005c   Data   RW         9510    .data               main.o
    0x20020064   0x00000004   Data   RW        10207    .data               mc_w.l(stdout.o)
    0x20020068   0x00009c87   Zero   RW         9508    .bss                main.o
    0x20029cef   0x00000001   PAD
    0x20029cf0   0x00000044   Zero   RW         9676    .bss                bsp_qspi_flash.o
    0x20029d34   0x00000044   Zero   RW         9823    .bss                bsp_sdram.o
    0x20029d78   0x00000070   Zero   RW         9881    .bss                bsp_debug_usart.o
    0x20029de8   0x00000400   Zero   RW            1    STACK               startup_stm32f767xx.o



  Load Region LR$$.ARM.__AT_0xD0000000 (Base: 0xd0000000, Size: 0x00000000, Max: 0x00000004, ABSOLUTE)

    Execution Region ER$$.ARM.__AT_0xD0000000 (Base: 0xd0000000, Size: 0x00000004, Max: 0x00000004, ABSOLUTE, UNINIT)

    Base Addr    Size         Type   Attr      Idx    E Section Name        Object

    0xd0000000   0x00000001   Zero   RW         9507    .ARM.__AT_0xD0000000  main.o


==============================================================================

Image component sizes


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Object Name

       224         22          0          0        112       2495   bsp_debug_usart.o
        90          8          0          0          0       1921   bsp_key.o
        72         10          0          0          0       1154   bsp_led.o
      1340        114          0          0         68      10080   bsp_qspi_flash.o
      1716        190         67          0         68       6532   bsp_sdram.o
      1498        620          0         92      40072      42230   main.o
        36          8        504          0       1024       1052   startup_stm32f767xx.o
        68         18          0          4          0       3336   stm32f7xx_hal.o
       158          4          0          0          0      35472   stm32f7xx_hal_cortex.o
       508         54          0          0          0       3879   stm32f7xx_hal_gpio.o
       112         10          0          0          0       1588   stm32f7xx_hal_pwr_ex.o
      1418         10          0          0          0      10626   stm32f7xx_hal_qspi.o
      1572         60          0          0          0       7140   stm32f7xx_hal_rcc.o
      1724         36          0          0          0       2888   stm32f7xx_hal_rcc_ex.o
       190          0          0          0          0       3970   stm32f7xx_hal_rng.o
       164          0          0          0          0       4068   stm32f7xx_hal_sdram.o
      1456         68          0          0          0       7616   stm32f7xx_hal_uart.o
        20          0          0          0          0       5338   stm32f7xx_it.o
       276          4          0          0          0       4340   stm32f7xx_ll_fmc.o
        84         18         24          4          0     421779   system_stm32f7xx.o

    ----------------------------------------------------------------------
     12736       1254        628        100      41348     577504   Object Totals
         0          0         32          0          0          0   (incl. Generated)
        10          0          1          0          4          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Member Name

         0          0          0          0          0          0   entry.o
         0          0          0          0          0          0   entry10a.o
         0          0          0          0          0          0   entry11a.o
         8          4          0          0          0          0   entry2.o
         4          0          0          0          0          0   entry5.o
         0          0          0          0          0          0   entry7b.o
         0          0          0          0          0          0   entry8b.o
         8          4          0          0          0          0   entry9a.o
        30          0          0          0          0          0   handlers.o
        36          8          0          0          0         68   init.o
        30          0          0          0          0         68   llshl.o
        32          0          0          0          0         68   llushr.o
       736         56          0          0          0        184   printf5.o
         0          0          0          4          0          0   stdout.o
        98          0          0          0          0         92   uldiv.o

    ----------------------------------------------------------------------
       988         72          0          4          0        480   Library Totals
         6          0          0          0          0          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Name

       982         72          0          4          0        480   mc_w.l

    ----------------------------------------------------------------------
       988         72          0          4          0        480   Library Totals

    ----------------------------------------------------------------------

==============================================================================


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   

     13724       1326        628        104      41348     570432   Grand Totals
     13724       1326        628        104      41348     570432   ELF Image Totals
     13724       1326        628        104          0          0   ROM Totals

==============================================================================

    Total RO  Size (Code + RO Data)                14352 (  14.02kB)
    Total RW  Size (RW Data + ZI Data)             41452 (  40.48kB)
    Total ROM Size (Code + RO Data + RW Data)      14456 (  14.12kB)

==============================================================================

