# Static Call Graph for image ..\..\Output\STM32F767_Test.axf

#<CALLGRAPH># ARM Linker, 5060300: Last Updated: Tue Apr 10 10:05:25 2018

### Maximum Stack Usage = 360 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ QSPI_FLASH_Init ⇒ BSP_QSPI_Init ⇒ QSPI_ResetMemory ⇒ QSPI_AutoPollingMemReady ⇒ HAL_QSPI_AutoPolling ⇒ QSPI_WaitFlagStateUntilTimeout

### Mutually Recursive functions

- ADC_IRQHandler ⇒ ADC_IRQHandler
- BusFault_Handler ⇒ BusFault_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- UsageFault_Handler ⇒ UsageFault_Handler

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - BusFault_Handler from stm32f7xx_it.o(i.BusFault_Handler) referenced from startup_stm32f767xx.o(RESET)
  - CAN1_RX0_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - CAN1_TX_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - CAN2_RX0_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - CAN2_RX1_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - CAN2_SCE_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - CAN2_TX_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - CAN3_RX0_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - CAN3_RX1_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - CAN3_SCE_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - CAN3_TX_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - CEC_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - DCMI_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - DFSDM1_FLT0_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - DFSDM1_FLT1_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - DFSDM1_FLT2_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - DFSDM1_FLT3_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - DMA2D_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - DebugMon_Handler from stm32f7xx_it.o(i.DebugMon_Handler) referenced from startup_stm32f767xx.o(RESET)
  - ETH_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - ETH_WKUP_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - FLASH_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - FMC_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - FPU_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - HardFault_Handler from stm32f7xx_it.o(i.HardFault_Handler) referenced from startup_stm32f767xx.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - I2C4_ER_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - I2C4_EV_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - JPEG_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - LPTIM1_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - LTDC_ER_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - LTDC_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - MDIOS_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - MemManage_Handler from stm32f7xx_it.o(i.MemManage_Handler) referenced from startup_stm32f767xx.o(RESET)
  - NMI_Handler from stm32f7xx_it.o(i.NMI_Handler) referenced from startup_stm32f767xx.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - OTG_HS_EP1_IN_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - OTG_HS_EP1_OUT_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - OTG_HS_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - OTG_HS_WKUP_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - PVD_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - PendSV_Handler from stm32f7xx_it.o(i.PendSV_Handler) referenced from startup_stm32f767xx.o(RESET)
  - QUADSPI_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - RCC_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - RNG_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - Reset_Handler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - SAI1_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - SAI2_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - SDMMC1_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - SDMMC2_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - SPDIF_RX_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - SPI1_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - SPI2_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - SPI3_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - SPI4_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - SPI5_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - SPI6_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - SVC_Handler from stm32f7xx_it.o(i.SVC_Handler) referenced from startup_stm32f767xx.o(RESET)
  - SysTick_Handler from stm32f7xx_it.o(i.SysTick_Handler) referenced from startup_stm32f767xx.o(RESET)
  - SystemInit from system_stm32f7xx.o(i.SystemInit) referenced from startup_stm32f767xx.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - TIM2_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - TIM3_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - TIM4_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - TIM5_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - TIM7_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - TIM8_BRK_TIM12_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - TIM8_TRG_COM_TIM14_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - TIM8_UP_TIM13_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - UART4_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - UART5_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - UART7_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - UART8_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - USART1_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - USART2_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - USART3_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - USART6_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - UsageFault_Handler from stm32f7xx_it.o(i.UsageFault_Handler) referenced from startup_stm32f767xx.o(RESET)
  - WWDG_IRQHandler from startup_stm32f767xx.o(.text) referenced from startup_stm32f767xx.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f767xx.o(.text)
  - fputc from bsp_debug_usart.o(i.fputc) referenced from printf5.o(i.__0printf$5)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f767xx.o(RESET)

  CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  CAN2_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  CAN2_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  CAN2_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  CAN2_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  CAN3_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  CAN3_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  CAN3_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  CAN3_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  CEC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  DCMI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  DFSDM1_FLT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  DFSDM1_FLT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  DFSDM1_FLT2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  DFSDM1_FLT3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  DMA2D_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  FMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  I2C4_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  I2C4_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  JPEG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  LPTIM1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  LTDC_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  LTDC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  MDIOS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  OTG_HS_EP1_IN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  OTG_HS_EP1_OUT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  OTG_HS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  OTG_HS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  QUADSPI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  SAI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  SAI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  SDMMC1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  SDMMC2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  SPDIF_RX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  SPI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  SPI5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  SPI6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  TIM8_BRK_TIM12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  TIM8_TRG_COM_TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  TIM8_UP_TIM13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  UART7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  UART8_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f767xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _printf_core

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  BSP_QSPI_Erase_Block (Thumb, 86 bytes, Stack size 64 bytes, bsp_qspi_flash.o(i.BSP_QSPI_Erase_Block))
  [Stack]

  - Max Depth = 232
  - Call Chain = BSP_QSPI_Erase_Block ⇒ QSPI_WriteEnable ⇒ HAL_QSPI_Command ⇒ QSPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_QSPI_Command
  - >> QSPI_WriteEnable
  - >> QSPI_AutoPollingMemReady
  [Called By]
  - >> SPI_Test_All

  BSP_QSPI_Init (Thumb, 118 bytes, Stack size 72 bytes, bsp_qspi_flash.o(i.BSP_QSPI_Init))
  [Stack]

  - Max Depth = 296
  - Call Chain = BSP_QSPI_Init ⇒ QSPI_ResetMemory ⇒ QSPI_AutoPollingMemReady ⇒ HAL_QSPI_AutoPolling ⇒ QSPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_QSPI_Transmit
  - >> HAL_QSPI_Command
  - >> QSPI_WriteEnable
  - >> QSPI_ResetMemory
  - >> QSPI_AutoPollingMemReady
  [Called By]
  - >> QSPI_FLASH_Init

  BSP_QSPI_Read (Thumb, 90 bytes, Stack size 72 bytes, bsp_qspi_flash.o(i.BSP_QSPI_Read))
  [Stack]

  - Max Depth = 144
  - Call Chain = BSP_QSPI_Read ⇒ HAL_QSPI_Receive ⇒ QSPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_QSPI_Receive
  - >> HAL_QSPI_Command
  [Called By]
  - >> SPI_Test_All

  BSP_QSPI_Write (Thumb, 164 bytes, Stack size 88 bytes, bsp_qspi_flash.o(i.BSP_QSPI_Write))
  [Stack]

  - Max Depth = 256
  - Call Chain = BSP_QSPI_Write ⇒ QSPI_WriteEnable ⇒ HAL_QSPI_Command ⇒ QSPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_QSPI_Transmit
  - >> HAL_QSPI_Command
  - >> QSPI_WriteEnable
  - >> QSPI_AutoPollingMemReady
  [Called By]
  - >> SPI_Test_All

  Buffercmp (Thumb, 30 bytes, Stack size 8 bytes, main.o(i.Buffercmp))
  [Stack]

  - Max Depth = 8
  - Call Chain = Buffercmp
  [Called By]
  - >> SPI_Test_All

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f7xx_it.o(i.BusFault_Handler))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f767xx.o(RESET)

  DEBUG_USART_Config (Thumb, 182 bytes, Stack size 184 bytes, bsp_debug_usart.o(i.DEBUG_USART_Config))
  [Stack]

  - Max Depth = 240
  - Call Chain = DEBUG_USART_Config ⇒ HAL_UART_Init ⇒ UART_CheckIdleState ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> HAL_GPIO_Init
  - >> HAL_UART_Init
  [Called By]
  - >> main

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f7xx_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  Delay (Thumb, 18 bytes, Stack size 8 bytes, main.o(i.Delay))
  [Stack]

  - Max Depth = 8
  - Call Chain = Delay
  [Called By]
  - >> SPI_Test_All

  FMC_SDRAM_Init (Thumb, 82 bytes, Stack size 12 bytes, stm32f7xx_ll_fmc.o(i.FMC_SDRAM_Init))
  [Stack]

  - Max Depth = 12
  - Call Chain = FMC_SDRAM_Init
  [Called By]
  - >> HAL_SDRAM_Init

  FMC_SDRAM_ProgramRefreshRate (Thumb, 12 bytes, Stack size 0 bytes, stm32f7xx_ll_fmc.o(i.FMC_SDRAM_ProgramRefreshRate))
  [Called By]

  - >> HAL_SDRAM_ProgramRefreshRate

  FMC_SDRAM_SendCommand (Thumb, 70 bytes, Stack size 24 bytes, stm32f7xx_ll_fmc.o(i.FMC_SDRAM_SendCommand))
  [Stack]

  - Max Depth = 24
  - Call Chain = FMC_SDRAM_SendCommand
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_SDRAM_SendCommand

  FMC_SDRAM_Timing_Init (Thumb, 108 bytes, Stack size 20 bytes, stm32f7xx_ll_fmc.o(i.FMC_SDRAM_Timing_Init))
  [Stack]

  - Max Depth = 20
  - Call Chain = FMC_SDRAM_Timing_Init
  [Called By]
  - >> HAL_SDRAM_Init

  HAL_GPIO_Init (Thumb, 426 bytes, Stack size 40 bytes, stm32f7xx_hal_gpio.o(i.HAL_GPIO_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_GPIO_Init
  [Called By]
  - >> QSPI_FLASH_Init
  - >> LED_GPIO_Config
  - >> Key_GPIO_Config
  - >> DEBUG_USART_Config
  - >> SDRAM_GPIO_Config

  HAL_GPIO_ReadPin (Thumb, 14 bytes, Stack size 0 bytes, stm32f7xx_hal_gpio.o(i.HAL_GPIO_ReadPin))
  [Called By]

  - >> Key_Scan

  HAL_GPIO_WritePin (Thumb, 14 bytes, Stack size 0 bytes, stm32f7xx_hal_gpio.o(i.HAL_GPIO_WritePin))
  [Called By]

  - >> LED_GPIO_Config
  - >> SPI_Test_All

  HAL_GetTick (Thumb, 6 bytes, Stack size 0 bytes, stm32f7xx_hal.o(i.HAL_GetTick))
  [Called By]

  - >> HAL_RNG_GenerateRandomNumber
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> HAL_QSPI_Transmit
  - >> HAL_QSPI_Receive
  - >> HAL_QSPI_Init
  - >> HAL_QSPI_Command
  - >> HAL_QSPI_AutoPolling
  - >> QSPI_WaitFlagStateUntilTimeout
  - >> HAL_PWREx_EnableOverDrive
  - >> UART_WaitOnFlagUntilTimeout
  - >> UART_CheckIdleState
  - >> HAL_UART_Transmit
  - >> FMC_SDRAM_SendCommand

  HAL_IncTick (Thumb, 10 bytes, Stack size 0 bytes, stm32f7xx_hal.o(i.HAL_IncTick))
  [Called By]

  - >> SysTick_Handler

  HAL_InitTick (Thumb, 34 bytes, Stack size 8 bytes, stm32f7xx_hal.o(i.HAL_InitTick))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_SYSTICK_Config
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> HAL_RCC_ClockConfig

  HAL_NVIC_EnableIRQ (Thumb, 22 bytes, Stack size 0 bytes, stm32f7xx_hal_cortex.o(i.HAL_NVIC_EnableIRQ))
  [Called By]

  - >> DEBUG_USART_Config

  HAL_NVIC_SetPriority (Thumb, 60 bytes, Stack size 16 bytes, stm32f7xx_hal_cortex.o(i.HAL_NVIC_SetPriority))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_NVIC_SetPriority
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> HAL_InitTick
  - >> DEBUG_USART_Config

  HAL_PWREx_EnableOverDrive (Thumb, 102 bytes, Stack size 24 bytes, stm32f7xx_hal_pwr_ex.o(i.HAL_PWREx_EnableOverDrive))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_PWREx_EnableOverDrive
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_QSPI_AutoPolling (Thumb, 170 bytes, Stack size 40 bytes, stm32f7xx_hal_qspi.o(i.HAL_QSPI_AutoPolling))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_QSPI_AutoPolling ⇒ QSPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> QSPI_WaitFlagStateUntilTimeout
  - >> QSPI_Config
  [Called By]
  - >> QSPI_WriteEnable
  - >> QSPI_AutoPollingMemReady

  HAL_QSPI_Command (Thumb, 146 bytes, Stack size 40 bytes, stm32f7xx_hal_qspi.o(i.HAL_QSPI_Command))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_QSPI_Command ⇒ QSPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> QSPI_WaitFlagStateUntilTimeout
  - >> QSPI_Config
  [Called By]
  - >> QSPI_WriteEnable
  - >> QSPI_ResetMemory
  - >> QSPI_FLASH_ReadID
  - >> QSPI_FLASH_ReadDeviceID
  - >> BSP_QSPI_Write
  - >> BSP_QSPI_Read
  - >> BSP_QSPI_Erase_Block
  - >> BSP_QSPI_Init

  HAL_QSPI_Init (Thumb, 174 bytes, Stack size 24 bytes, stm32f7xx_hal_qspi.o(i.HAL_QSPI_Init))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_QSPI_Init ⇒ QSPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> HAL_QSPI_MspInit
  - >> HAL_QSPI_SetTimeout
  - >> QSPI_WaitFlagStateUntilTimeout
  [Called By]
  - >> QSPI_FLASH_Init

  HAL_QSPI_MspInit (Thumb, 2 bytes, Stack size 0 bytes, stm32f7xx_hal_qspi.o(i.HAL_QSPI_MspInit))
  [Called By]

  - >> HAL_QSPI_Init

  HAL_QSPI_Receive (Thumb, 206 bytes, Stack size 40 bytes, stm32f7xx_hal_qspi.o(i.HAL_QSPI_Receive))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_QSPI_Receive ⇒ QSPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> QSPI_WaitFlagStateUntilTimeout
  [Called By]
  - >> QSPI_FLASH_ReadID
  - >> QSPI_FLASH_ReadDeviceID
  - >> BSP_QSPI_Read

  HAL_QSPI_SetTimeout (Thumb, 4 bytes, Stack size 0 bytes, stm32f7xx_hal_qspi.o(i.HAL_QSPI_SetTimeout))
  [Called By]

  - >> HAL_QSPI_Init

  HAL_QSPI_Transmit (Thumb, 196 bytes, Stack size 40 bytes, stm32f7xx_hal_qspi.o(i.HAL_QSPI_Transmit))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_QSPI_Transmit ⇒ QSPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> QSPI_WaitFlagStateUntilTimeout
  [Called By]
  - >> BSP_QSPI_Write
  - >> BSP_QSPI_Init

  HAL_RCCEx_PeriphCLKConfig (Thumb, 1714 bytes, Stack size 40 bytes, stm32f7xx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_RCCEx_PeriphCLKConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> DEBUG_USART_Config

  HAL_RCC_ClockConfig (Thumb, 354 bytes, Stack size 32 bytes, stm32f7xx_hal_rcc.o(i.HAL_RCC_ClockConfig))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_InitTick
  - >> HAL_GetTick
  - >> HAL_RCC_GetSysClockFreq
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_GetHCLKFreq (Thumb, 6 bytes, Stack size 0 bytes, stm32f7xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq))
  [Called By]

  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_RCC_GetPCLK1Freq

  HAL_RCC_GetPCLK1Freq (Thumb, 36 bytes, Stack size 4 bytes, stm32f7xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_RCC_GetPCLK1Freq
  [Calls]
  - >> HAL_RCC_GetHCLKFreq
  [Called By]
  - >> UART_SetConfig

  HAL_RCC_GetPCLK2Freq (Thumb, 36 bytes, Stack size 4 bytes, stm32f7xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq))
  [Stack]

  - Max Depth = 4
  - Call Chain = HAL_RCC_GetPCLK2Freq
  [Calls]
  - >> HAL_RCC_GetHCLKFreq
  [Called By]
  - >> UART_SetConfig

  HAL_RCC_GetSysClockFreq (Thumb, 120 bytes, Stack size 12 bytes, stm32f7xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq))
  [Stack]

  - Max Depth = 12
  - Call Chain = HAL_RCC_GetSysClockFreq
  [Called By]
  - >> HAL_RCC_ClockConfig
  - >> UART_SetConfig

  HAL_RCC_OscConfig (Thumb, 960 bytes, Stack size 40 bytes, stm32f7xx_hal_rcc.o(i.HAL_RCC_OscConfig))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_RCC_OscConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_RNG_GenerateRandomNumber (Thumb, 102 bytes, Stack size 32 bytes, stm32f7xx_hal_rng.o(i.HAL_RNG_GenerateRandomNumber))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_RNG_GenerateRandomNumber
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_RNG_GetRandomNumber

  HAL_RNG_GetRandomNumber (Thumb, 22 bytes, Stack size 8 bytes, stm32f7xx_hal_rng.o(i.HAL_RNG_GetRandomNumber))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_RNG_GetRandomNumber ⇒ HAL_RNG_GenerateRandomNumber
  [Calls]
  - >> HAL_RNG_GenerateRandomNumber
  [Called By]
  - >> SDRAM_Test_All

  HAL_RNG_Init (Thumb, 64 bytes, Stack size 16 bytes, stm32f7xx_hal_rng.o(i.HAL_RNG_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_RNG_Init
  [Calls]
  - >> HAL_RNG_MspInit
  [Called By]
  - >> SDRAM_Test_All

  HAL_RNG_MspInit (Thumb, 2 bytes, Stack size 0 bytes, stm32f7xx_hal_rng.o(i.HAL_RNG_MspInit))
  [Called By]

  - >> HAL_RNG_Init

  HAL_SDRAM_Init (Thumb, 68 bytes, Stack size 16 bytes, stm32f7xx_hal_sdram.o(i.HAL_SDRAM_Init))
  [Stack]

  - Max Depth = 36
  - Call Chain = HAL_SDRAM_Init ⇒ FMC_SDRAM_Timing_Init
  [Calls]
  - >> HAL_SDRAM_MspInit
  - >> FMC_SDRAM_Timing_Init
  - >> FMC_SDRAM_Init
  [Called By]
  - >> SDRAM_Init

  HAL_SDRAM_MspInit (Thumb, 2 bytes, Stack size 0 bytes, stm32f7xx_hal_sdram.o(i.HAL_SDRAM_MspInit))
  [Called By]

  - >> HAL_SDRAM_Init

  HAL_SDRAM_ProgramRefreshRate (Thumb, 38 bytes, Stack size 8 bytes, stm32f7xx_hal_sdram.o(i.HAL_SDRAM_ProgramRefreshRate))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SDRAM_ProgramRefreshRate
  [Calls]
  - >> FMC_SDRAM_ProgramRefreshRate
  [Called By]
  - >> SDRAM_InitSequence

  HAL_SDRAM_SendCommand (Thumb, 56 bytes, Stack size 16 bytes, stm32f7xx_hal_sdram.o(i.HAL_SDRAM_SendCommand))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_SDRAM_SendCommand ⇒ FMC_SDRAM_SendCommand
  [Calls]
  - >> FMC_SDRAM_SendCommand
  [Called By]
  - >> SDRAM_InitSequence

  HAL_SYSTICK_Config (Thumb, 40 bytes, Stack size 8 bytes, stm32f7xx_hal_cortex.o(i.HAL_SYSTICK_Config))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_Config
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> HAL_InitTick

  HAL_UART_Init (Thumb, 112 bytes, Stack size 8 bytes, stm32f7xx_hal_uart.o(i.HAL_UART_Init))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_UART_Init ⇒ UART_CheckIdleState ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_UART_MspInit
  - >> UART_SetConfig
  - >> UART_CheckIdleState
  - >> UART_AdvFeatureConfig
  [Called By]
  - >> DEBUG_USART_Config

  HAL_UART_MspInit (Thumb, 2 bytes, Stack size 0 bytes, stm32f7xx_hal_uart.o(i.HAL_UART_MspInit))
  [Called By]

  - >> HAL_UART_Init

  HAL_UART_Transmit (Thumb, 186 bytes, Stack size 32 bytes, stm32f7xx_hal_uart.o(i.HAL_UART_Transmit))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> UART_WaitOnFlagUntilTimeout
  [Called By]
  - >> fputc

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f7xx_it.o(i.HardFault_Handler))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f767xx.o(RESET)

  Key_GPIO_Config (Thumb, 44 bytes, Stack size 32 bytes, bsp_key.o(i.Key_GPIO_Config))
  [Stack]

  - Max Depth = 72
  - Call Chain = Key_GPIO_Config ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> main

  Key_Scan (Thumb, 38 bytes, Stack size 16 bytes, bsp_key.o(i.Key_Scan))
  [Stack]

  - Max Depth = 16
  - Call Chain = Key_Scan
  [Calls]
  - >> HAL_GPIO_ReadPin
  [Called By]
  - >> main

  LED_GPIO_Config (Thumb, 62 bytes, Stack size 40 bytes, bsp_led.o(i.LED_GPIO_Config))
  [Stack]

  - Max Depth = 80
  - Call Chain = LED_GPIO_Config ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> HAL_GPIO_Init
  [Called By]
  - >> main

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f7xx_it.o(i.MemManage_Handler))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f767xx.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f7xx_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f7xx_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  QSPI_FLASH_Init (Thumb, 282 bytes, Stack size 64 bytes, bsp_qspi_flash.o(i.QSPI_FLASH_Init))
  [Stack]

  - Max Depth = 360
  - Call Chain = QSPI_FLASH_Init ⇒ BSP_QSPI_Init ⇒ QSPI_ResetMemory ⇒ QSPI_AutoPollingMemReady ⇒ HAL_QSPI_AutoPolling ⇒ QSPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_QSPI_Init
  - >> HAL_GPIO_Init
  - >> BSP_QSPI_Init
  [Called By]
  - >> main

  QSPI_FLASH_ReadDeviceID (Thumb, 108 bytes, Stack size 72 bytes, bsp_qspi_flash.o(i.QSPI_FLASH_ReadDeviceID))
  [Stack]

  - Max Depth = 144
  - Call Chain = QSPI_FLASH_ReadDeviceID ⇒ HAL_QSPI_Receive ⇒ QSPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_QSPI_Receive
  - >> HAL_QSPI_Command
  - >> __2printf
  [Called By]
  - >> SPI_Test_All

  QSPI_FLASH_ReadID (Thumb, 110 bytes, Stack size 72 bytes, bsp_qspi_flash.o(i.QSPI_FLASH_ReadID))
  [Stack]

  - Max Depth = 144
  - Call Chain = QSPI_FLASH_ReadID ⇒ HAL_QSPI_Receive ⇒ QSPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_QSPI_Receive
  - >> HAL_QSPI_Command
  - >> __2printf
  [Called By]
  - >> SPI_Test_All

  SDRAM_Check (Thumb, 278 bytes, Stack size 24 bytes, main.o(i.SDRAM_Check))
  [Stack]

  - Max Depth = 48
  - Call Chain = SDRAM_Check ⇒ __2printf
  [Calls]
  - >> __2printf
  [Called By]
  - >> SDRAM_Test_All

  SDRAM_Init (Thumb, 104 bytes, Stack size 40 bytes, bsp_sdram.o(i.SDRAM_Init))
  [Stack]

  - Max Depth = 144
  - Call Chain = SDRAM_Init ⇒ SDRAM_GPIO_Config ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_SDRAM_Init
  - >> SDRAM_InitSequence
  - >> SDRAM_GPIO_Config
  [Called By]
  - >> main

  SDRAM_Test (Thumb, 162 bytes, Stack size 16 bytes, bsp_sdram.o(i.SDRAM_Test))
  [Stack]

  - Max Depth = 40
  - Call Chain = SDRAM_Test ⇒ __2printf
  [Calls]
  - >> __2printf
  [Called By]
  - >> SDRAM_Test_All

  SDRAM_Test_All (Thumb, 114 bytes, Stack size 16 bytes, main.o(i.SDRAM_Test_All))
  [Stack]

  - Max Depth = 64
  - Call Chain = SDRAM_Test_All ⇒ SDRAM_Check ⇒ __2printf
  [Calls]
  - >> HAL_RNG_Init
  - >> HAL_RNG_GetRandomNumber
  - >> SDRAM_Test
  - >> SDRAM_Check
  - >> __2printf
  [Called By]
  - >> main

  SPI_Test_All (Thumb, 296 bytes, Stack size 32 bytes, main.o(i.SPI_Test_All))
  [Stack]

  - Max Depth = 288
  - Call Chain = SPI_Test_All ⇒ BSP_QSPI_Write ⇒ QSPI_WriteEnable ⇒ HAL_QSPI_Command ⇒ QSPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> QSPI_FLASH_ReadID
  - >> QSPI_FLASH_ReadDeviceID
  - >> BSP_QSPI_Write
  - >> BSP_QSPI_Read
  - >> BSP_QSPI_Erase_Block
  - >> Delay
  - >> Buffercmp
  - >> __2printf
  [Called By]
  - >> main

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f7xx_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(RESET)

  SysTick_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f7xx_it.o(i.SysTick_Handler))
  [Calls]

  - >> HAL_IncTick
  [Address Reference Count : 1]
  - startup_stm32f767xx.o(RESET)

  SystemInit (Thumb, 66 bytes, Stack size 0 bytes, system_stm32f7xx.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_stm32f767xx.o(.text)

  UART_AdvFeatureConfig (Thumb, 200 bytes, Stack size 0 bytes, stm32f7xx_hal_uart.o(i.UART_AdvFeatureConfig))
  [Called By]

  - >> HAL_UART_Init

  UART_CheckIdleState (Thumb, 92 bytes, Stack size 24 bytes, stm32f7xx_hal_uart.o(i.UART_CheckIdleState))
  [Stack]

  - Max Depth = 48
  - Call Chain = UART_CheckIdleState ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> UART_WaitOnFlagUntilTimeout
  [Called By]
  - >> HAL_UART_Init

  UART_SetConfig (Thumb, 716 bytes, Stack size 24 bytes, stm32f7xx_hal_uart.o(i.UART_SetConfig))
  [Stack]

  - Max Depth = 36
  - Call Chain = UART_SetConfig ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_RCC_GetPCLK1Freq
  [Called By]
  - >> HAL_UART_Init

  UART_WaitOnFlagUntilTimeout (Thumb, 100 bytes, Stack size 24 bytes, stm32f7xx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout))
  [Stack]

  - Max Depth = 24
  - Call Chain = UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> UART_CheckIdleState
  - >> HAL_UART_Transmit

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f7xx_it.o(i.UsageFault_Handler))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f767xx.o(RESET)

  __0printf$5 (Thumb, 22 bytes, Stack size 24 bytes, printf5.o(i.__0printf$5), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf$5 (Thumb, 0 bytes, Stack size 24 bytes, printf5.o(i.__0printf$5), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printf5.o(i.__0printf$5))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> SDRAM_Test
  - >> QSPI_FLASH_ReadID
  - >> QSPI_FLASH_ReadDeviceID
  - >> SPI_Test_All
  - >> SDRAM_Test_All
  - >> SDRAM_Check

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  fputc (Thumb, 20 bytes, Stack size 16 bytes, bsp_debug_usart.o(i.fputc))
  [Stack]

  - Max Depth = 72
  - Call Chain = fputc ⇒ HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_UART_Transmit
  [Address Reference Count : 1]
  - printf5.o(i.__0printf$5)

  main (Thumb, 48 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 360
  - Call Chain = main ⇒ QSPI_FLASH_Init ⇒ BSP_QSPI_Init ⇒ QSPI_ResetMemory ⇒ QSPI_AutoPollingMemReady ⇒ HAL_QSPI_AutoPolling ⇒ QSPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SDRAM_Init
  - >> QSPI_FLASH_Init
  - >> LED_GPIO_Config
  - >> Key_Scan
  - >> Key_GPIO_Config
  - >> DEBUG_USART_Config
  - >> SPI_Test_All
  - >> SDRAM_Test_All
  - >> SystemClock_Config
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  ### Local Symbols

  NVIC_SetPriority (Thumb, 32 bytes, Stack size 0 bytes, stm32f7xx_hal_cortex.o(i.NVIC_SetPriority))
  [Called By]

  - >> HAL_SYSTICK_Config
  - >> HAL_NVIC_SetPriority

  QSPI_Config (Thumb, 434 bytes, Stack size 20 bytes, stm32f7xx_hal_qspi.o(i.QSPI_Config))
  [Stack]

  - Max Depth = 20
  - Call Chain = QSPI_Config
  [Called By]
  - >> HAL_QSPI_Command
  - >> HAL_QSPI_AutoPolling

  QSPI_WaitFlagStateUntilTimeout (Thumb, 76 bytes, Stack size 32 bytes, stm32f7xx_hal_qspi.o(i.QSPI_WaitFlagStateUntilTimeout))
  [Stack]

  - Max Depth = 32
  - Call Chain = QSPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_QSPI_Transmit
  - >> HAL_QSPI_Receive
  - >> HAL_QSPI_Init
  - >> HAL_QSPI_Command
  - >> HAL_QSPI_AutoPolling

  SystemClock_Config (Thumb, 94 bytes, Stack size 80 bytes, main.o(i.SystemClock_Config))
  [Stack]

  - Max Depth = 136
  - Call Chain = SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> HAL_PWREx_EnableOverDrive
  [Called By]
  - >> main

  QSPI_AutoPollingMemReady (Thumb, 76 bytes, Stack size 88 bytes, bsp_qspi_flash.o(i.QSPI_AutoPollingMemReady))
  [Stack]

  - Max Depth = 160
  - Call Chain = QSPI_AutoPollingMemReady ⇒ HAL_QSPI_AutoPolling ⇒ QSPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_QSPI_AutoPolling
  [Called By]
  - >> QSPI_ResetMemory
  - >> BSP_QSPI_Write
  - >> BSP_QSPI_Erase_Block
  - >> BSP_QSPI_Init

  QSPI_ResetMemory (Thumb, 88 bytes, Stack size 64 bytes, bsp_qspi_flash.o(i.QSPI_ResetMemory))
  [Stack]

  - Max Depth = 224
  - Call Chain = QSPI_ResetMemory ⇒ QSPI_AutoPollingMemReady ⇒ HAL_QSPI_AutoPolling ⇒ QSPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_QSPI_Command
  - >> QSPI_AutoPollingMemReady
  [Called By]
  - >> BSP_QSPI_Init

  QSPI_WriteEnable (Thumb, 104 bytes, Stack size 96 bytes, bsp_qspi_flash.o(i.QSPI_WriteEnable))
  [Stack]

  - Max Depth = 168
  - Call Chain = QSPI_WriteEnable ⇒ HAL_QSPI_Command ⇒ QSPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_QSPI_Command
  - >> HAL_QSPI_AutoPolling
  [Called By]
  - >> BSP_QSPI_Write
  - >> BSP_QSPI_Erase_Block
  - >> BSP_QSPI_Init

  SDRAM_GPIO_Config (Thumb, 1126 bytes, Stack size 64 bytes, bsp_sdram.o(i.SDRAM_GPIO_Config))
  [Stack]

  - Max Depth = 104
  - Call Chain = SDRAM_GPIO_Config ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> SDRAM_Init

  SDRAM_InitSequence (Thumb, 134 bytes, Stack size 32 bytes, bsp_sdram.o(i.SDRAM_InitSequence))
  [Stack]

  - Max Depth = 72
  - Call Chain = SDRAM_InitSequence ⇒ HAL_SDRAM_SendCommand ⇒ FMC_SDRAM_SendCommand
  [Calls]
  - >> HAL_SDRAM_SendCommand
  - >> HAL_SDRAM_ProgramRefreshRate
  - >> SDRAM_delay
  [Called By]
  - >> SDRAM_Init

  SDRAM_delay (Thumb, 28 bytes, Stack size 12 bytes, bsp_sdram.o(i.SDRAM_delay))
  [Stack]

  - Max Depth = 12
  - Call Chain = SDRAM_delay
  [Called By]
  - >> SDRAM_InitSequence

  _printf_core (Thumb, 658 bytes, Stack size 104 bytes, printf5.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  [Called By]
  - >> __0printf$5

  ### Undefined Global Symbols