Static Call Graph - [..\OBJ\TOUCH.axf]

# Static Call Graph for image ..\OBJ\TOUCH.axf

#<CALLGRAPH># ARM Linker, 5040049: Last Updated: Tue Oct 31 15:58:04 2017

### Maximum Stack Usage = 316 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

TP_Init ⇒ TP_Adjust ⇒ TP_Adj_Info_Show ⇒ LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - BusFault_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DebugMon_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - FLASH_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - HardFault_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - MemManage_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - NMI_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - PVD_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - PendSV_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - RCC_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - RTCAlarm_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - RTC_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - Reset_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - SPI1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - SPI2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - SVC_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - SysTick_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - SystemInit from system_stm32f10x.o(.text) referenced from startup_stm32f10x_md.o(.text)
  - TAMPER_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM3_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM4_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TP_Adjust from touch.o(.text) referenced from touch.o(.data)
  - TP_Init from touch.o(.text) referenced from touch.o(.data)
  - TP_Scan from touch.o(.text) referenced from touch.o(.data)
  - USART1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USART2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USART3_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - UsageFault_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - WWDG_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32f10x_md.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __rt_entry
  - >> __scatterload

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002A))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000008))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000F))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000031))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000006))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000009))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000003))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000B))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __main
  - >> __scatterload_rt2

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 300 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ Test_FillRec ⇒ DrawTestPage ⇒ Gui_StrCenter ⇒ Show_Str ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  main (Thumb, 50 bytes, Stack size 0 bytes, main.o(.text))
  [Stack]

  - Max Depth = 300
  - Call Chain = main ⇒ Test_FillRec ⇒ DrawTestPage ⇒ Gui_StrCenter ⇒ Show_Str ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> main_test
  - >> delay_init
  - >> Test_FillRec
  - >> Test_Color
  - >> Test_Circle
  - >> SystemInit
  - >> Pic_test
  - >> LCD_Init
  - >> English_Font_test
  - >> Chinese_Font_test
  [Called By]
  - >> __rt_entry_main

  DrawTestPage (Thumb, 134 bytes, Stack size 24 bytes, test.o(.text))
  [Stack]

  - Max Depth = 268
  - Call Chain = DrawTestPage ⇒ Gui_StrCenter ⇒ Show_Str ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_Fill
  - >> Gui_StrCenter
  [Called By]
  - >> Touch_Test
  - >> main_test
  - >> Test_FillRec
  - >> Test_Color
  - >> Test_Circle
  - >> Pic_test
  - >> English_Font_test
  - >> Chinese_Font_test

  main_test (Thumb, 124 bytes, Stack size 16 bytes, test.o(.text))
  [Stack]

  - Max Depth = 284
  - Call Chain = main_test ⇒ DrawTestPage ⇒ Gui_StrCenter ⇒ Show_Str ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> delay_ms
  - >> Gui_StrCenter
  - >> DrawTestPage
  [Called By]
  - >> main

  Test_Color (Thumb, 338 bytes, Stack size 16 bytes, test.o(.text))
  [Stack]

  - Max Depth = 284
  - Call Chain = Test_Color ⇒ DrawTestPage ⇒ Gui_StrCenter ⇒ Show_Str ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> delay_ms
  - >> Show_Str
  - >> LCD_Fill
  - >> DrawTestPage
  [Called By]
  - >> main

  Test_FillRec (Thumb, 392 bytes, Stack size 32 bytes, test.o(.text))
  [Stack]

  - Max Depth = 300
  - Call Chain = Test_FillRec ⇒ DrawTestPage ⇒ Gui_StrCenter ⇒ Show_Str ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> delay_ms
  - >> LCD_Fill
  - >> LCD_DrawRectangle
  - >> LCD_DrawFillRectangle
  - >> DrawTestPage
  [Called By]
  - >> main

  Test_Circle (Thumb, 440 bytes, Stack size 24 bytes, test.o(.text))
  [Stack]

  - Max Depth = 292
  - Call Chain = Test_Circle ⇒ DrawTestPage ⇒ Gui_StrCenter ⇒ Show_Str ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> gui_circle
  - >> delay_ms
  - >> LCD_Fill
  - >> DrawTestPage
  [Called By]
  - >> main

  English_Font_test (Thumb, 128 bytes, Stack size 8 bytes, test.o(.text))
  [Stack]

  - Max Depth = 276
  - Call Chain = English_Font_test ⇒ DrawTestPage ⇒ Gui_StrCenter ⇒ Show_Str ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> delay_ms
  - >> LCD_ShowString
  - >> DrawTestPage
  [Called By]
  - >> main

  Chinese_Font_test (Thumb, 122 bytes, Stack size 16 bytes, test.o(.text))
  [Stack]

  - Max Depth = 284
  - Call Chain = Chinese_Font_test ⇒ DrawTestPage ⇒ Gui_StrCenter ⇒ Show_Str ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> delay_ms
  - >> Show_Str
  - >> DrawTestPage
  [Called By]
  - >> main

  Pic_test (Thumb, 152 bytes, Stack size 16 bytes, test.o(.text))
  [Stack]

  - Max Depth = 284
  - Call Chain = Pic_test ⇒ DrawTestPage ⇒ Gui_StrCenter ⇒ Show_Str ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> delay_ms
  - >> Show_Str
  - >> LCD_Fill
  - >> Gui_Drawbmp16
  - >> DrawTestPage
  [Called By]
  - >> main

  Touch_Test (Thumb, 892 bytes, Stack size 32 bytes, test.o(.text), UNUSED)
  [Calls]

  - >> delay_ms
  - >> TP_Save_Adjdata
  - >> TP_Init
  - >> TP_Draw_Big_Point
  - >> TP_Adjust
  - >> LCD_ShowString
  - >> LCD_Fill
  - >> LCD_Clear
  - >> KEY_Scan
  - >> KEY_Init
  - >> DrawTestPage

  GUI_DrawPoint (Thumb, 24 bytes, Stack size 16 bytes, gui.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = GUI_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_SetCursor
  - >> LCD_DrawPoint_16Bit
  [Called By]
  - >> _draw_circle_8

  LCD_Fill (Thumb, 164 bytes, Stack size 40 bytes, gui.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = LCD_Fill ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_SetWindows
  [Called By]
  - >> LCD_DrawFillRectangle
  - >> Touch_Test
  - >> DrawTestPage
  - >> Test_FillRec
  - >> Test_Color
  - >> Test_Circle
  - >> Pic_test

  LCD_DrawLine (Thumb, 176 bytes, Stack size 72 bytes, gui.o(.text))
  [Stack]

  - Max Depth = 124
  - Call Chain = LCD_DrawLine ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_DrawPoint
  [Called By]
  - >> TP_Drow_Touch_Point
  - >> LCD_DrawRectangle

  LCD_DrawRectangle (Thumb, 64 bytes, Stack size 24 bytes, gui.o(.text))
  [Stack]

  - Max Depth = 148
  - Call Chain = LCD_DrawRectangle ⇒ LCD_DrawLine ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_DrawLine
  [Called By]
  - >> Test_FillRec

  LCD_DrawFillRectangle (Thumb, 30 bytes, Stack size 24 bytes, gui.o(.text))
  [Stack]

  - Max Depth = 92
  - Call Chain = LCD_DrawFillRectangle ⇒ LCD_Fill ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_Fill
  [Called By]
  - >> Test_FillRec

  _draw_circle_8 (Thumb, 132 bytes, Stack size 24 bytes, gui.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = _draw_circle_8 ⇒ GUI_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> GUI_DrawPoint
  [Called By]
  - >> gui_circle

  gui_circle (Thumb, 154 bytes, Stack size 56 bytes, gui.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = gui_circle ⇒ _draw_circle_8 ⇒ GUI_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> _draw_circle_8
  [Called By]
  - >> TP_Drow_Touch_Point
  - >> Test_Circle

  LCD_ShowChar (Thumb, 276 bytes, Stack size 64 bytes, gui.o(.text))
  [Stack]

  - Max Depth = 116
  - Call Chain = LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_SetWindows
  - >> LCD_DrawPoint_16Bit
  - >> LCD_DrawPoint
  [Called By]
  - >> LCD_ShowNum
  - >> Show_Str
  - >> LCD_ShowString

  LCD_ShowString (Thumb, 124 bytes, Stack size 40 bytes, gui.o(.text))
  [Stack]

  - Max Depth = 156
  - Call Chain = LCD_ShowString ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_ShowChar
  [Called By]
  - >> TP_Adj_Info_Show
  - >> TP_Adjust
  - >> Touch_Test
  - >> English_Font_test

  mypow (Thumb, 22 bytes, Stack size 8 bytes, gui.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = mypow
  [Called By]
  - >> LCD_ShowNum

  LCD_ShowNum (Thumb, 168 bytes, Stack size 64 bytes, gui.o(.text))
  [Stack]

  - Max Depth = 180
  - Call Chain = LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> mypow
  - >> LCD_ShowChar
  [Called By]
  - >> TP_Adj_Info_Show

  GUI_DrawFont16 (Thumb, 252 bytes, Stack size 48 bytes, gui.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = GUI_DrawFont16 ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_SetWindows
  - >> LCD_DrawPoint_16Bit
  - >> LCD_DrawPoint
  [Called By]
  - >> Show_Str

  GUI_DrawFont24 (Thumb, 268 bytes, Stack size 48 bytes, gui.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = GUI_DrawFont24 ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_SetWindows
  - >> LCD_DrawPoint_16Bit
  - >> LCD_DrawPoint
  [Called By]
  - >> Show_Str

  GUI_DrawFont32 (Thumb, 252 bytes, Stack size 48 bytes, gui.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = GUI_DrawFont32 ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_SetWindows
  - >> LCD_DrawPoint_16Bit
  - >> LCD_DrawPoint
  [Called By]
  - >> Show_Str

  Show_Str (Thumb, 290 bytes, Stack size 64 bytes, gui.o(.text))
  [Stack]

  - Max Depth = 180
  - Call Chain = Show_Str ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> GUI_DrawFont32
  - >> GUI_DrawFont24
  - >> GUI_DrawFont16
  - >> LCD_ShowChar
  [Called By]
  - >> Gui_StrCenter
  - >> Test_Color
  - >> Pic_test
  - >> Chinese_Font_test

  Gui_StrCenter (Thumb, 68 bytes, Stack size 64 bytes, gui.o(.text))
  [Stack]

  - Max Depth = 244
  - Call Chain = Gui_StrCenter ⇒ Show_Str ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> strlen
  - >> Show_Str
  [Called By]
  - >> DrawTestPage
  - >> main_test

  Gui_Drawbmp16 (Thumb, 90 bytes, Stack size 32 bytes, gui.o(.text))
  [Stack]

  - Max Depth = 60
  - Call Chain = Gui_Drawbmp16 ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_SetWindows
  - >> LCD_DrawPoint_16Bit
  [Called By]
  - >> Pic_test

  delay_init (Thumb, 52 bytes, Stack size 8 bytes, delay.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = delay_init
  [Calls]
  - >> SysTick_CLKSourceConfig
  [Called By]
  - >> main

  delay_ms (Thumb, 56 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> AT24CXX_WriteOneByte
  - >> LCD_RESET
  - >> TP_Adjust
  - >> KEY_Scan
  - >> Touch_Test
  - >> main_test
  - >> Test_FillRec
  - >> Test_Color
  - >> Test_Circle
  - >> Pic_test
  - >> LCD_Init
  - >> English_Font_test
  - >> Chinese_Font_test

  delay_us (Thumb, 56 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> TP_Read_AD
  - >> IIC_Read_Byte
  - >> IIC_Send_Byte
  - >> IIC_NAck
  - >> IIC_Ack
  - >> IIC_Wait_Ack
  - >> IIC_Stop
  - >> IIC_Start

  SystemInit (Thumb, 78 bytes, Stack size 8 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = SystemInit ⇒ SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClock
  [Called By]
  - >> main
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(.text)

  SystemCoreClockUpdate (Thumb, 142 bytes, Stack size 8 bytes, system_stm32f10x.o(.text), UNUSED)

  KEY_Init (Thumb, 82 bytes, Stack size 8 bytes, key.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_PinRemapConfig
  - >> GPIO_Init
  [Called By]
  - >> Touch_Test

  KEY_Scan (Thumb, 92 bytes, Stack size 8 bytes, key.o(.text), UNUSED)
  [Calls]

  - >> GPIO_ReadInputDataBit
  - >> delay_ms
  [Called By]
  - >> Touch_Test

  LCD_WR_REG (Thumb, 32 bytes, Stack size 0 bytes, lcd.o(.text))
  [Called By]

  - >> LCD_WriteRAM_Prepare
  - >> LCD_WriteReg

  LCD_WR_DATA (Thumb, 32 bytes, Stack size 0 bytes, lcd.o(.text))
  [Called By]

  - >> LCD_WriteReg

  LCD_DrawPoint_16Bit (Thumb, 46 bytes, Stack size 0 bytes, lcd.o(.text))
  [Called By]

  - >> GUI_DrawFont32
  - >> GUI_DrawFont24
  - >> GUI_DrawFont16
  - >> LCD_ShowChar
  - >> GUI_DrawPoint
  - >> Gui_Drawbmp16

  LCD_WriteReg (Thumb, 20 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_WriteReg
  [Calls]
  - >> LCD_WR_DATA
  - >> LCD_WR_REG
  [Called By]
  - >> LCD_SetParam
  - >> LCD_SetWindows
  - >> LCD_Init

  LCD_WriteRAM_Prepare (Thumb, 12 bytes, Stack size 4 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = LCD_WriteRAM_Prepare
  [Calls]
  - >> LCD_WR_REG
  [Called By]
  - >> LCD_SetWindows

  LCD_SetWindows (Thumb, 80 bytes, Stack size 20 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_WriteRAM_Prepare
  - >> LCD_WriteReg
  [Called By]
  - >> LCD_SetCursor
  - >> GUI_DrawFont32
  - >> GUI_DrawFont24
  - >> GUI_DrawFont16
  - >> LCD_ShowChar
  - >> LCD_Fill
  - >> LCD_Clear
  - >> Gui_Drawbmp16

  LCD_SetCursor (Thumb, 20 bytes, Stack size 12 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_SetWindows
  [Called By]
  - >> LCD_DrawPoint
  - >> GUI_DrawPoint

  LCD_DrawPoint (Thumb, 70 bytes, Stack size 12 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_SetCursor
  [Called By]
  - >> TP_Drow_Touch_Point
  - >> GUI_DrawFont32
  - >> GUI_DrawFont24
  - >> GUI_DrawFont16
  - >> LCD_ShowChar
  - >> LCD_DrawLine
  - >> TP_Draw_Big_Point

  LCD_Clear (Thumb, 98 bytes, Stack size 12 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = LCD_Clear ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_SetWindows
  [Called By]
  - >> TP_Init
  - >> TP_Adjust
  - >> Touch_Test

  LCD_GPIOInit (Thumb, 88 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = LCD_GPIOInit ⇒ GPIO_Init
  [Calls]
  - >> GPIO_SetBits
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_PinRemapConfig
  - >> GPIO_Init
  [Called By]
  - >> LCD_Init

  LCD_RESET (Thumb, 28 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_RESET
  [Calls]
  - >> delay_ms
  [Called By]
  - >> LCD_Init

  LCD_SetParam (Thumb, 40 bytes, Stack size 4 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = LCD_SetParam ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_WriteReg
  [Called By]
  - >> LCD_Init

  LCD_Init (Thumb, 532 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = LCD_Init ⇒ LCD_GPIOInit ⇒ GPIO_Init
  [Calls]
  - >> LCD_SetParam
  - >> LCD_RESET
  - >> LCD_GPIOInit
  - >> LCD_WriteReg
  - >> delay_ms
  [Called By]
  - >> main

  IIC_Init (Thumb, 52 bytes, Stack size 8 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = IIC_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> AT24CXX_Init

  IIC_Start (Thumb, 68 bytes, Stack size 8 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_Start
  [Calls]
  - >> delay_us
  [Called By]
  - >> AT24CXX_WriteOneByte
  - >> AT24CXX_ReadOneByte

  IIC_Stop (Thumb, 62 bytes, Stack size 8 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_Stop
  [Calls]
  - >> delay_us
  [Called By]
  - >> AT24CXX_WriteOneByte
  - >> AT24CXX_ReadOneByte
  - >> IIC_Wait_Ack

  IIC_Wait_Ack (Thumb, 86 bytes, Stack size 8 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = IIC_Wait_Ack ⇒ IIC_Stop
  [Calls]
  - >> IIC_Stop
  - >> delay_us
  [Called By]
  - >> AT24CXX_WriteOneByte
  - >> AT24CXX_ReadOneByte

  IIC_Ack (Thumb, 66 bytes, Stack size 8 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_Ack
  [Calls]
  - >> delay_us
  [Called By]
  - >> IIC_Read_Byte

  IIC_NAck (Thumb, 66 bytes, Stack size 8 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_NAck
  [Calls]
  - >> delay_us
  [Called By]
  - >> IIC_Read_Byte

  IIC_Send_Byte (Thumb, 90 bytes, Stack size 16 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = IIC_Send_Byte
  [Calls]
  - >> delay_us
  [Called By]
  - >> AT24CXX_WriteOneByte
  - >> AT24CXX_ReadOneByte

  IIC_Read_Byte (Thumb, 98 bytes, Stack size 16 bytes, myiic.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = IIC_Read_Byte ⇒ IIC_NAck
  [Calls]
  - >> IIC_NAck
  - >> IIC_Ack
  - >> delay_us
  [Called By]
  - >> AT24CXX_ReadOneByte

  AT24CXX_Init (Thumb, 8 bytes, Stack size 8 bytes, 24cxx.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = AT24CXX_Init ⇒ IIC_Init ⇒ GPIO_Init
  [Calls]
  - >> IIC_Init
  [Called By]
  - >> TP_Init

  AT24CXX_ReadOneByte (Thumb, 88 bytes, Stack size 16 bytes, 24cxx.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = AT24CXX_ReadOneByte ⇒ IIC_Read_Byte ⇒ IIC_NAck
  [Calls]
  - >> IIC_Read_Byte
  - >> IIC_Send_Byte
  - >> IIC_Wait_Ack
  - >> IIC_Stop
  - >> IIC_Start
  [Called By]
  - >> TP_Get_Adjdata
  - >> AT24CXX_Read
  - >> AT24CXX_Check
  - >> AT24CXX_ReadLenByte

  AT24CXX_WriteOneByte (Thumb, 80 bytes, Stack size 16 bytes, 24cxx.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = AT24CXX_WriteOneByte ⇒ IIC_Send_Byte
  [Calls]
  - >> IIC_Send_Byte
  - >> IIC_Wait_Ack
  - >> IIC_Stop
  - >> IIC_Start
  - >> delay_ms
  [Called By]
  - >> AT24CXX_Write
  - >> AT24CXX_Check
  - >> AT24CXX_WriteLenByte
  - >> TP_Save_Adjdata

  AT24CXX_WriteLenByte (Thumb, 42 bytes, Stack size 24 bytes, 24cxx.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = AT24CXX_WriteLenByte ⇒ AT24CXX_WriteOneByte ⇒ IIC_Send_Byte
  [Calls]
  - >> AT24CXX_WriteOneByte
  [Called By]
  - >> TP_Save_Adjdata

  AT24CXX_ReadLenByte (Thumb, 44 bytes, Stack size 24 bytes, 24cxx.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = AT24CXX_ReadLenByte ⇒ AT24CXX_ReadOneByte ⇒ IIC_Read_Byte ⇒ IIC_NAck
  [Calls]
  - >> AT24CXX_ReadOneByte
  [Called By]
  - >> TP_Get_Adjdata

  AT24CXX_Check (Thumb, 46 bytes, Stack size 8 bytes, 24cxx.o(.text), UNUSED)
  [Calls]

  - >> AT24CXX_WriteOneByte
  - >> AT24CXX_ReadOneByte

  AT24CXX_Read (Thumb, 34 bytes, Stack size 16 bytes, 24cxx.o(.text), UNUSED)
  [Calls]

  - >> AT24CXX_ReadOneByte

  AT24CXX_Write (Thumb, 36 bytes, Stack size 16 bytes, 24cxx.o(.text), UNUSED)
  [Calls]

  - >> AT24CXX_WriteOneByte

  TP_Write_Byte (Thumb, 56 bytes, Stack size 0 bytes, touch.o(.text))
  [Called By]

  - >> TP_Read_AD

  TP_Read_AD (Thumb, 132 bytes, Stack size 16 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = TP_Read_AD
  [Calls]
  - >> TP_Write_Byte
  - >> delay_us
  [Called By]
  - >> TP_Read_XOY

  TP_Read_XOY (Thumb, 120 bytes, Stack size 40 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = TP_Read_XOY ⇒ TP_Read_AD
  [Calls]
  - >> TP_Read_AD
  [Called By]
  - >> TP_Read_XY

  TP_Read_XY (Thumb, 38 bytes, Stack size 24 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = TP_Read_XY ⇒ TP_Read_XOY ⇒ TP_Read_AD
  [Calls]
  - >> TP_Read_XOY
  [Called By]
  - >> TP_Read_XY2
  - >> TP_Init

  TP_Read_XY2 (Thumb, 192 bytes, Stack size 32 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = TP_Read_XY2 ⇒ TP_Read_XY ⇒ TP_Read_XOY ⇒ TP_Read_AD
  [Calls]
  - >> TP_Read_XY
  [Called By]
  - >> TP_Scan

  TP_Drow_Touch_Point (Thumb, 116 bytes, Stack size 24 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 160
  - Call Chain = TP_Drow_Touch_Point ⇒ gui_circle ⇒ _draw_circle_8 ⇒ GUI_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_DrawPoint
  - >> LCD_DrawLine
  - >> gui_circle
  [Called By]
  - >> TP_Adjust

  TP_Draw_Big_Point (Thumb, 54 bytes, Stack size 16 bytes, touch.o(.text), UNUSED)
  [Calls]

  - >> LCD_DrawPoint
  [Called By]
  - >> Touch_Test

  TP_Scan (Thumb, 246 bytes, Stack size 24 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = TP_Scan ⇒ TP_Read_XY2 ⇒ TP_Read_XY ⇒ TP_Read_XOY ⇒ TP_Read_AD
  [Calls]
  - >> __aeabi_fmul
  - >> __aeabi_ui2f
  - >> __aeabi_i2f
  - >> __aeabi_f2uiz
  - >> __aeabi_fadd
  - >> TP_Read_XY2
  [Address Reference Count : 1]
  - touch.o(.data)

  TP_Save_Adjdata (Thumb, 148 bytes, Stack size 16 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = TP_Save_Adjdata ⇒ AT24CXX_WriteLenByte ⇒ AT24CXX_WriteOneByte ⇒ IIC_Send_Byte
  [Calls]
  - >> __aeabi_fmul
  - >> __aeabi_f2iz
  - >> AT24CXX_WriteLenByte
  - >> AT24CXX_WriteOneByte
  [Called By]
  - >> TP_Init
  - >> TP_Adjust
  - >> Touch_Test

  TP_Get_Adjdata (Thumb, 152 bytes, Stack size 16 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = TP_Get_Adjdata ⇒ AT24CXX_ReadLenByte ⇒ AT24CXX_ReadOneByte ⇒ IIC_Read_Byte ⇒ IIC_NAck
  [Calls]
  - >> __aeabi_i2f
  - >> __aeabi_fdiv
  - >> AT24CXX_ReadLenByte
  - >> AT24CXX_ReadOneByte
  [Called By]
  - >> TP_Init
  - >> TP_Adjust

  TP_Adj_Info_Show (Thumb, 322 bytes, Stack size 40 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 220
  - Call Chain = TP_Adj_Info_Show ⇒ LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> LCD_ShowNum
  - >> LCD_ShowString
  [Called By]
  - >> TP_Adjust

  TP_Adjust (Thumb, 2242 bytes, Stack size 88 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 308
  - Call Chain = TP_Adjust ⇒ TP_Adj_Info_Show ⇒ LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> sqrt
  - >> __aeabi_fmul
  - >> __aeabi_ui2f
  - >> __aeabi_i2f
  - >> __aeabi_f2uiz
  - >> __aeabi_f2iz
  - >> __aeabi_fdiv
  - >> __aeabi_fsub
  - >> __aeabi_f2d
  - >> __aeabi_cdrcmple
  - >> __aeabi_cdcmple
  - >> __aeabi_ui2d
  - >> __aeabi_d2uiz
  - >> TP_Adj_Info_Show
  - >> TP_Get_Adjdata
  - >> TP_Drow_Touch_Point
  - >> delay_ms
  - >> TP_Save_Adjdata
  - >> LCD_ShowString
  - >> LCD_Clear
  [Called By]
  - >> TP_Init
  - >> Touch_Test
  [Address Reference Count : 1]
  - touch.o(.data)

  TP_Init (Thumb, 106 bytes, Stack size 8 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 316
  - Call Chain = TP_Init ⇒ TP_Adjust ⇒ TP_Adj_Info_Show ⇒ LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_SetWindows ⇒ LCD_WriteReg
  [Calls]
  - >> TP_Get_Adjdata
  - >> TP_Read_XY
  - >> AT24CXX_Init
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  - >> TP_Save_Adjdata
  - >> TP_Adjust
  - >> LCD_Clear
  [Called By]
  - >> Touch_Test
  [Address Reference Count : 1]
  - touch.o(.data)

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f10x_md.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  NVIC_Init (Thumb, 100 bytes, Stack size 16 bytes, misc.o(.text), UNUSED)

  NVIC_SetVectorTable (Thumb, 14 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  NVIC_SystemLPConfig (Thumb, 34 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  SysTick_CLKSourceConfig (Thumb, 40 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> delay_init

  GPIO_DeInit (Thumb, 172 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_AFIODeInit (Thumb, 20 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_Init (Thumb, 278 bytes, Stack size 24 bytes, stm32f10x_gpio.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = GPIO_Init
  [Called By]
  - >> IIC_Init
  - >> LCD_GPIOInit
  - >> TP_Init
  - >> KEY_Init

  GPIO_StructInit (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Called By]

  - >> KEY_Scan

  GPIO_ReadInputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> LCD_GPIOInit

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_PinLockConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_PinRemapConfig (Thumb, 138 bytes, Stack size 20 bytes, stm32f10x_gpio.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_PinRemapConfig
  [Called By]
  - >> LCD_GPIOInit
  - >> KEY_Init

  GPIO_EXTILineConfig (Thumb, 66 bytes, Stack size 12 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ETH_MediaInterfaceConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  RCC_DeInit (Thumb, 64 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HSEConfig (Thumb, 70 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetFlagStatus (Thumb, 56 bytes, Stack size 8 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_WaitForHSEStartUp

  RCC_WaitForHSEStartUp (Thumb, 56 bytes, Stack size 16 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus

  RCC_AdjustHSICalibrationValue (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PLLConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_SYSCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetSYSCLKSource (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PCLK1Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PCLK2Config (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ITConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_USBCLKConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ADCCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_LSEConfig (Thumb, 50 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_LSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 192 bytes, Stack size 12 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_AHBPeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_APB2PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> IIC_Init
  - >> LCD_GPIOInit
  - >> TP_Init
  - >> KEY_Init

  RCC_APB1PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_APB2PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> GPIO_AFIODeInit
  - >> GPIO_DeInit

  RCC_APB1PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_BackupResetCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_MCOConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  strlen (Thumb, 62 bytes, Stack size 8 bytes, strlen.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = strlen
  [Called By]
  - >> Gui_StrCenter

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __read_errno (Thumb, 10 bytes, Stack size 8 bytes, _rserrno.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_errno_addr

  __set_errno (Thumb, 12 bytes, Stack size 8 bytes, _rserrno.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __set_errno
  [Calls]
  - >> __aeabi_errno_addr
  [Called By]
  - >> sqrt

  __aeabi_errno_addr (Thumb, 8 bytes, Stack size 0 bytes, rt_errno_addr_intlibspace.o(.text))
  [Called By]

  - >> __set_errno
  - >> __read_errno

  __errno$intlibspace (Thumb, 0 bytes, Stack size 0 bytes, rt_errno_addr_intlibspace.o(.text), UNUSED)

  __rt_errno_addr$intlibspace (Thumb, 0 bytes, Stack size 0 bytes, rt_errno_addr_intlibspace.o(.text), UNUSED)

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 12 bytes, Stack size 0 bytes, exit.o(.text))
  [Calls]

  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __semihosting_library_function (Thumb, 0 bytes, Stack size 24 bytes, indicate_semi.o(.text), UNUSED)

  sqrt (Thumb, 76 bytes, Stack size 24 bytes, sqrt.o(i.sqrt))
  [Stack]

  - Max Depth = 64
  - Call Chain = sqrt ⇒ _dsqrt ⇒ __fpl_dnaninf
  [Calls]
  - >> _dsqrt
  - >> __set_errno
  [Called By]
  - >> TP_Adjust

  __fpl_dcmp_Inf (Thumb, 24 bytes, Stack size 0 bytes, dcmpi.o(x$fpl$dcmpinf), UNUSED)
  [Called By]

  - >> _dcmple

  __aeabi_d2uiz (Thumb, 0 bytes, Stack size 32 bytes, dfixu.o(x$fpl$dfixu))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_d2uiz
  [Called By]
  - >> TP_Adjust

  _dfixu (Thumb, 90 bytes, Stack size 32 bytes, dfixu.o(x$fpl$dfixu), UNUSED)
  [Calls]

  - >> __fpl_dnaninf

  __aeabi_ui2d (Thumb, 0 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dfltu))
  [Called By]

  - >> TP_Adjust

  _dfltu (Thumb, 38 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dfltu), UNUSED)

  __aeabi_cdcmple (Thumb, 0 bytes, Stack size 32 bytes, dleqf.o(x$fpl$dleqf))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_cdcmple
  [Called By]
  - >> TP_Adjust

  _dcmple (Thumb, 120 bytes, Stack size 32 bytes, dleqf.o(x$fpl$dleqf), UNUSED)
  [Calls]

  - >> __fpl_dnaninf
  - >> __fpl_dcmp_Inf

  __fpl_dcmple_InfNaN (Thumb, 0 bytes, Stack size unknown bytes, dleqf.o(x$fpl$dleqf), UNUSED)
  [Called By]

  - >> _drcmple

  __fpl_dnaninf (Thumb, 156 bytes, Stack size 16 bytes, dnaninf.o(x$fpl$dnaninf))
  [Stack]

  - Max Depth = 16
  - Call Chain = __fpl_dnaninf
  [Called By]
  - >> _dsqrt
  - >> _dcmple
  - >> _dfixu

  __fpl_dretinf (Thumb, 12 bytes, Stack size 0 bytes, dretinf.o(x$fpl$dretinf), UNUSED)
  [Called By]

  - >> _f2d

  __aeabi_cdrcmple (Thumb, 0 bytes, Stack size 16 bytes, drleqf.o(x$fpl$drleqf))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_cdrcmple
  [Called By]
  - >> TP_Adjust

  _drcmple (Thumb, 108 bytes, Stack size 16 bytes, drleqf.o(x$fpl$drleqf), UNUSED)
  [Calls]

  - >> __fpl_dcmple_InfNaN

  _dsqrt (Thumb, 456 bytes, Stack size 24 bytes, dsqrt_noumaal.o(x$fpl$dsqrt))
  [Stack]

  - Max Depth = 40
  - Call Chain = _dsqrt ⇒ __fpl_dnaninf
  [Calls]
  - >> __fpl_dnaninf
  [Called By]
  - >> sqrt

  __aeabi_f2d (Thumb, 0 bytes, Stack size 16 bytes, f2d.o(x$fpl$f2d))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_f2d
  [Called By]
  - >> TP_Adjust

  _f2d (Thumb, 86 bytes, Stack size 16 bytes, f2d.o(x$fpl$f2d), UNUSED)
  [Calls]

  - >> __fpl_fnaninf
  - >> __fpl_dretinf

  __aeabi_fadd (Thumb, 0 bytes, Stack size 16 bytes, faddsub_clz.o(x$fpl$fadd))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_fadd
  [Called By]
  - >> TP_Scan

  _fadd (Thumb, 196 bytes, Stack size 16 bytes, faddsub_clz.o(x$fpl$fadd), UNUSED)
  [Calls]

  - >> __fpl_fretinf
  - >> __fpl_fnaninf
  - >> _fsub1

  __aeabi_fdiv (Thumb, 0 bytes, Stack size 16 bytes, fdiv.o(x$fpl$fdiv))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_fdiv
  [Called By]
  - >> TP_Get_Adjdata
  - >> TP_Adjust

  _fdiv (Thumb, 384 bytes, Stack size 16 bytes, fdiv.o(x$fpl$fdiv), UNUSED)
  [Calls]

  - >> __fpl_fretinf
  - >> __fpl_fnaninf

  __aeabi_f2iz (Thumb, 0 bytes, Stack size 16 bytes, ffix.o(x$fpl$ffix))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_f2iz
  [Called By]
  - >> TP_Save_Adjdata
  - >> TP_Adjust

  _ffix (Thumb, 54 bytes, Stack size 16 bytes, ffix.o(x$fpl$ffix), UNUSED)
  [Calls]

  - >> __fpl_fnaninf

  __aeabi_f2uiz (Thumb, 0 bytes, Stack size 16 bytes, ffixu.o(x$fpl$ffixu))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_f2uiz
  [Called By]
  - >> TP_Scan
  - >> TP_Adjust

  _ffixu (Thumb, 62 bytes, Stack size 16 bytes, ffixu.o(x$fpl$ffixu), UNUSED)
  [Calls]

  - >> __fpl_fnaninf

  __aeabi_i2f (Thumb, 0 bytes, Stack size 0 bytes, fflt_clz.o(x$fpl$fflt))
  [Called By]

  - >> TP_Get_Adjdata
  - >> TP_Scan
  - >> TP_Adjust

  _fflt (Thumb, 48 bytes, Stack size 0 bytes, fflt_clz.o(x$fpl$fflt), UNUSED)

  __aeabi_ui2f (Thumb, 0 bytes, Stack size 0 bytes, fflt_clz.o(x$fpl$ffltu))
  [Called By]

  - >> TP_Scan
  - >> TP_Adjust

  _ffltu (Thumb, 38 bytes, Stack size 0 bytes, fflt_clz.o(x$fpl$ffltu), UNUSED)

  __aeabi_fmul (Thumb, 0 bytes, Stack size 16 bytes, fmul.o(x$fpl$fmul))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_fmul
  [Called By]
  - >> TP_Scan
  - >> TP_Save_Adjdata
  - >> TP_Adjust

  _fmul (Thumb, 258 bytes, Stack size 16 bytes, fmul.o(x$fpl$fmul), UNUSED)
  [Calls]

  - >> __fpl_fretinf
  - >> __fpl_fnaninf

  __fpl_fnaninf (Thumb, 140 bytes, Stack size 8 bytes, fnaninf.o(x$fpl$fnaninf), UNUSED)
  [Called By]

  - >> _fmul
  - >> _ffixu
  - >> _ffix
  - >> _fdiv
  - >> _fsub
  - >> _fadd
  - >> _f2d

  __fpl_fretinf (Thumb, 10 bytes, Stack size 0 bytes, fretinf.o(x$fpl$fretinf), UNUSED)
  [Called By]

  - >> _fmul
  - >> _fdiv
  - >> _fadd

  __aeabi_fsub (Thumb, 0 bytes, Stack size 16 bytes, faddsub_clz.o(x$fpl$fsub))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_fsub
  [Called By]
  - >> TP_Adjust

  _fsub (Thumb, 234 bytes, Stack size 16 bytes, faddsub_clz.o(x$fpl$fsub), UNUSED)
  [Calls]

  - >> __fpl_fnaninf
  - >> _fadd1

  ### Local Symbols

  SetSysClockTo72 (Thumb, 214 bytes, Stack size 12 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClockTo72
  [Called By]
  - >> SetSysClock

  SetSysClock (Thumb, 8 bytes, Stack size 8 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClockTo72
  [Called By]
  - >> SystemInit

  _fadd1 (Thumb, 0 bytes, Stack size unknown bytes, faddsub_clz.o(x$fpl$fadd), UNUSED)
  [Called By]

  - >> _fsub

  _fsub1 (Thumb, 0 bytes, Stack size unknown bytes, faddsub_clz.o(x$fpl$fsub), UNUSED)
  [Called By]

  - >> _fadd

  ### Undefined Global Symbols