#

##

##

    礦ision Build Log
    Project:
    F:\显示屏技术资料\OLED驱动程序\中景园电子2.42寸OLED模块资料\2-42寸模块资料\中景园电子2.42OLED显示屏_STM32F103ZET6_IIC_V1.0\中景园电子0.96OLED显示屏_STM32F103ZET6_IIC_V1.0\中景园电子0.96OLED显示屏_STM32F103ZET6_IIC_V1.0\USER\OLED.uvproj
    Project File Date:  03/15/2016

    Output:
    Load "..\\OBJ\\OLED.axf"
    Set JLink Project File to "F:\显示屏技术资料\OLED驱动程序\中景园电子2.42寸OLED模块资料\2-42寸模块资料\中景园电子2.42OLED显示屏_STM32F103ZET6_IIC_V1.0\中景园电子0.96OLED显示屏_STM32F103ZET6_IIC_V1.0\中景园电子0.96OLED显示屏_STM32F103ZET6_IIC_V1.0\USER\JLinkSettings.ini"
    * JLink Info: Device "STM32F103ZE" selected (512 KB flash, 64 KB RAM).

    JLink info:
    ------------
    DLL: V4.76d, compiled Sep 13 2013 16:35:06
    Firmware: J-Link ARM V8 compiled Nov 25 2013 19:20:08
    Hardware: V8.00
    S/N : 17935099
    Feature(s) : RDI,FlashDL,FlashBP,JFlash

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103ZE
    VTarget = 2.788V
    State of Pins:
    TCK: 0, TDI: 1, TDO: 1, TMS: 1, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 4000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...