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Super Mini 5.8GHz 48CH FPV Transmitter
+700TVL FPV Camera+Brass dipole Antenna+0SD
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Brass dipole antenna

700TVL Camera Button

Video in. -
Video out-—
GND—— 3355V

Smart audio
GND.

Specification and Parameters:
= Transmitting power: 25mW.
= Frequency: 5.8G 48CH
= Input volage: 3.3-5.5V
= Current consumption: 280mA(typical)
= Camera resolution: 700TVL
= Video Format: PAL
= Field of view: 120° viewing angle
= Antenna dimensions: 35mm*4.2mm diameter
= Antenna: Brass dipole antenna
& Frequency: 5.8GHz 6 bands 48 channels,
with Race band: 5474-5945MHZ
= Size: 14*13.8mm(L"W)
= Weight: 3.99

Operation Instruc
Frequency switching: By one button,Short press the button
to change channel,1-8 adjustable Press and hold the button
for 2s to change bands,1-6 adjustable.

Two groups of LEDS:

Group 1:6 BLUE LED stand for bands

Group 2:8 RED LED stand for channels.

Blue LED1 and Red LED1 light on,indicating frequency
5865MHz(Band1 and CH1)

Blue LED1 and Red LED2 light on.indicating frequency
5845MHz(Band1 and CH2)

Biue LEDS and Red LEDS light on,indicating frequency
5600MHz(Band6 and CH8)




