--------->


**6.Screen Mirroring Connection**

Press “Source” on the remote control or press “” on the control panel of the projector, select “Screen Mirroring” from “Input Source”, and press “OK” to enter. You can choose a wireless connection or a wired connection.
**※Tips:**
 ①The fluency of screen mirroring with wireless connection will be affected by the network environment.

②Make sure your mobile device is close to the projector when using a wireless connection. A distance within 1 meter is recommended.

③Some mobile devices may not support screen mirroring due to compatibility limitations.

④Long press "OK" for 10s to delete the screen mirroring configuration information, you can reconfigure.

**Compatible systems**

|  |  |
| --- | --- |
| IOS |  IOS 7 and above, iPhone 4+,iPad 2+, iPad4+ |
| Android |  Android 4.2 and above, has 1GB storage at least. |

**Wireless Projection Method**

**For IOS Devices**

1. Tap “Settings” and turn on Wi-Fi network. Choose the Wi-Fi name “RKcast-xxxxxx”, then connect to it and enter the password “12345678”, which is visible on the Projector’s menu.
**※If you want to use Wi-Fi network, please perform the second step, otherwise skip this step.※**
2. Go to Safari, and enter “192.168.49.1”. And tap “Wi-Fi AP” ---> “Scan”, then select your Wi-Fi and enter the password, tap connect.
3. Open the “Control Center” and click the ”Screen Mirroring” icon, find the device name “RKcast-xxxxxx”, click it to connect.

**Note:** After connecting, if “No Internet Connection” is displayed, please ignore it, as it will not affect operation of the device.
 **For Android Device** Tap “Settings” and turn on the Wi-Fi network.
**※If you want to use a Wi-Fi network, please do the following:**

1.Connect to your home Wi-Fi network and enter the password;
  2.Tap “Settings”--->”Connection& Sharing” ---> “Cast”, turn on ”Cast” and connect “RKcast-xxxxxx”.
**※If you want to use a mobile cellular network, please do the following:**

1.Choose the Wi-Fi name “RKcast-xxxxxx”, connect to it and enter the password “12345678” which is on the projector’s menu.
 **2.Tap “Settings”--->”Connection& Sharing” ---> “Cast”, turn on ”Cast” and connect “RKcast-xxxxxx”.**
**Tips:** Different brand mobile phones may have a different name for the Miracast function.

 **Wired Projection Method**

**For IOS Device**

1.Connect the projector and IOS device with a USB cable;

2. "Do you trust this equipment?" is displayed, click "Trust".
**For Android Device**

1. Connect the projector and Android device with a USB cable;

2. Enter “Developer mode” and click “Developer options”, then open ”USB debugging”, a window will pop up "Allow USB debugging?" , tap "OK". After a while, the Android screen will be displayed on the projector.
**Tips:**
1.It is recommended to use the original USB cable to connect your device and the projector.
**2.Some Android mobile devices may only transfer the display without audio due to protocol restrictions.**