**MX-P150M HF POWER AMPLIFIER INSTRUCTION MANUAL**

MX-P150M hf power amplifier，for QRP transceiver，Improve signal。Can be used both as a base and mobile unit,Extremely Small Compact and light weight，The amplifier incorporates various protection circuits such as high swr，front mounted LED display.

This amplifier can be successfully used with other QRP rigs such as the ICOM IC-705 Elecraft KX3 FT-818ND and SUNSDR2.

**Specifications**

Frequency Band：80m  40m  20m  15m 10m

Operating Modes：SSB CW AM，FT8 and FM-Reduced duty cycle

Rf input：≤10W

Out power：100W-130W

Band mode：Manual

Power requirement：13.8V 20A，**RED “+”   BLACK “-”**

Cooling method:passive air cooling

Antenna connector：SO-239  50Ω

Size：260\*180\*90（mm）D\*W\*H

Weight：4KG







