;;******************** (C) COPYRIGHT 2011 STMicroelectronics ********************
;;* File Name          : STM8L_32K.STmap
;;* Author             : MCD Application Team
;;* Version            : V2.5.0
;;* Date               : 21-November-2011
;;* Description        : memory mapping
;;********************************************************************************
;;* THE PRESENT SOFTWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
;;* WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE TIME.
;;* AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
;;* INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM THE
;;* CONTENT OF SUCH SOFTWARE AND/OR THE USE MADE BY CUSTOMERS OF THE CODING
;;* INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
;;********************************************************************************

[Product]
Name=STM8L_8K
FlashSize=FFFF     
RAMSize=FFFF       		
PacketSize=80
ACKVAL=79
MAPNAME=sectors
PagesPerSector=1
family = 3

;; Erase Write Routines files /* BL_VER = FileName */
1.0 = E_W_ROUTINEs_32K_verL_1.0.s19
1.1 = E_W_ROUTINEs_32K_verL_1.0.s19

;; EEPROM information
[DataEE]
Name=DataEE
Index=08
Address=00001000
Size=00000100
Type=111
UFO=111


;; OPTION bytes information
[OptBytes]
Name=OptBytes
Address=00004800
Size=00000080
Type=101
UFO=111


;; Flash information
[SEC0]
Name=SEC0
Index=00
Address=00008000
Size=00000400
Type=111
UFO=111
[SEC1]
Name=SEC1
Index=01
Address=00008400
Size=00000400
Type=111
UFO=111
[SEC2]
Name=SEC2
Index=02
Address=00008800
Size=00000400
Type=111
UFO=111
[SEC3]
Name=SEC3
Index=03
Address=00008C00
Size=00000400
Type=111
UFO=111
[SEC4]
Name=SEC4
Index=04
Address=00009000
Size=00000400
Type=111
UFO=111
[SEC5]
Name=SEC5
Index=05
Address=00009400
Size=00000400
Type=111
UFO=111
[SEC6]
Name=SEC6
Index=06
Address=00009800
Size=00000400
Type=111
UFO=111
[SEC7]
Name=SEC7
Index=07
Address=00009C00
Size=00000400
Type=111
UFO=111
